{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Foglio1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Foglio1","index":0,"n_rows":45329,"n_cols":17,"rows_kept":4500,"cut":true,"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["CollectionName","FamilyName","SeriesName","ItemCode","code","description_NL","description_FR","description_IT","FeatureCode1","FeatureDescr1","UnitPrice","configcode","codEAN","dimX","dimY","dimZ","weight"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.","031","Chrome",720,"GPF750510G001G000","8055261445024"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",149,"Finox Brushed Nickel",973,"GPF750510G002G000","8055261445017"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",299,"Matte Black",973,"GPF750510C072G000","8055261445031"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",706,"Black Metal PVD",1067,"GPF750510P001G000","8055261444997"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",707,"Black Metal Brushed PVD",1138,"GPF750510P004G000","8055261444980"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.","030","Copper PVD",1067,"GPF750510P000G000","8055261445000"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",708,"Copper Brushed PVD",1138,"GPF750510P006G000","8055261444973"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",735,"Warm Bronze PVD",1067,"GPF750510P037G000","8055261444928"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",726,"Warm Bronze Brushed PVD",1138,"GPF750510P024G000","8055261444942"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",720,"Nickel PVD",1067,"GPF750510P014G000","8055261444959"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",761,"Coffee Bronze Brushed PVD",1210,"GPF750510E059G000","8055261571501"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",710,"Brass PVD",1067,"GPF750510P011G000","8055261444966"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",727,"Brass Brushed PVD",1138,"GPF750510P025G000","8055261444935"]
["BATHROOM","INCASTRI","INCASTRI",75051,75051,"Wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer with Stop&Go waste and connecting flexibles.",845,"Dark Bronze",1138,"GPF750510V221G000","8055261444911"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.","031","Chrome",696,"GPF750020G001G000","8055261446328"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",149,"Finox Brushed Nickel",940,"GPF750020G002G000","8055261446311"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",299,"Matte Black",940,"GPF750020C072G000","8055261446335"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",706,"Black Metal PVD",1030,"GPF750020P001G000","8055261446298"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",707,"Black Metal Brushed PVD",1100,"GPF750020P004G000","8055261446281"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.","030","Copper PVD",1030,"GPF750020P000G000","8055261446304"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",708,"Copper Brushed PVD",1100,"GPF750020P006G000","8055261446274"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",735,"Warm Bronze PVD",1030,"GPF750020P037G000","8055261446229"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",726,"Warm Bronze Brushed PVD",1100,"GPF750020P024G000","8055261446243"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",720,"Nickel PVD",1030,"GPF750020P014G000","8055261446250"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",761,"Coffee Bronze Brushed PVD",1170,"GPF750020E059G000","8055261571709"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",710,"Brass PVD",1030,"GPF750020P011G000","8055261446267"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",727,"Brass Brushed PVD",1100,"GPF750020P025G000","8055261446236"]
["BATHROOM","INCASTRI","INCASTRI",75002,75002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",845,"Dark Bronze",1100,"GPF750020V221G000","8055261446212"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.","031","Chrome",915,"GPF750530G001G000","8055261444898"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",149,"Finox Brushed Nickel",1235,"GPF750530G002G000","8055261444881"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",299,"Matte Black",1235,"GPF750530C072G000","8055261444904"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",706,"Black Metal PVD",1354,"GPF750530P001G000","8055261444867"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",707,"Black Metal Brushed PVD",1445,"GPF750530P004G000","8055261444850"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.","030","Copper PVD",1354,"GPF750530P000G000","8055261444874"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",708,"Copper Brushed PVD",1445,"GPF750530P006G000","8055261444843"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",735,"Warm Bronze PVD",1354,"GPF750530P037G000","8055261444799"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",726,"Warm Bronze Brushed PVD",1445,"GPF750530P024G000","8055261444812"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",720,"Nickel PVD",1354,"GPF750530P014G000","8055261444829"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",761,"Coffee Bronze Brushed PVD",1537,"GPF750530E059G000","8055261571488"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",710,"Brass PVD",1354,"GPF750530P011G000","8055261444836"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",727,"Brass Brushed PVD",1445,"GPF750530P025G000","8055261444805"]
["BATHROOM","INCASTRI","INCASTRI",75053,75053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",845,"Dark Bronze",1445,"GPF750530V221G000","8055261444782"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.","031","Chrome",891,"GPF750040G001G000","8055261446199"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",149,"Finox Brushed Nickel",1203,"GPF750040G002G000","8055261446182"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",299,"Matte Black",1203,"GPF750040C072G000","8055261446205"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",706,"Black Metal PVD",1319,"GPF750040P001G000","8055261446168"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",707,"Black Metal Brushed PVD",1408,"GPF750040P004G000","8055261446151"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.","030","Copper PVD",1319,"GPF750040P000G000","8055261446175"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",708,"Copper Brushed PVD",1408,"GPF750040P006G000","8055261446144"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",735,"Warm Bronze PVD",1319,"GPF750040P037G000","8055261446090"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",726,"Warm Bronze Brushed PVD",1408,"GPF750040P024G000","8055261446113"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",720,"Nickel PVD",1319,"GPF750040P014G000","8055261446120"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",761,"Coffee Bronze Brushed PVD",1497,"GPF750040E059G000","8055261571686"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",710,"Brass PVD",1319,"GPF750040P011G000","8055261446137"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",727,"Brass Brushed PVD",1408,"GPF750040P025G000","8055261446106"]
["BATHROOM","INCASTRI","INCASTRI",75004,75004,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",845,"Dark Bronze",1408,"GPF750040V221G000","8055261446083"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.","031","Chrome",891,"GPF752510G001G000","8055261440210"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",149,"Finox Brushed Nickel",1203,"GPF752510G002G000","8055261440203"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",299,"Matte Black",1203,"GPF752510C072G000","8055261440227"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",706,"Black Metal PVD",1319,"GPF752510P001G000","8055261440180"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",707,"Black Metal Brushed PVD",1408,"GPF752510P004G000","8055261440173"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.","030","Copper PVD",1319,"GPF752510P000G000","8055261440197"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",708,"Copper Brushed PVD",1408,"GPF752510P006G000","8055261440166"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",735,"Warm Bronze PVD",1319,"GPF752510P037G000","8055261440111"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",726,"Warm Bronze Brushed PVD",1408,"GPF752510P024G000","8055261440135"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",720,"Nickel PVD",1319,"GPF752510P014G000","8055261440142"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",761,"Coffee Bronze Brushed PVD",1497,"GPF752510E059G000","8055261571020"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",710,"Brass PVD",1319,"GPF752510P011G000","8055261440159"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",727,"Brass Brushed PVD",1408,"GPF752510P025G000","8055261440128"]
["BATHROOM","INCASTRI","INCASTRI",75251,75251,"Wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo Sospeso avec bonde \"Stop&Go\" et flexibles de raccordement.","Basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",845,"Dark Bronze",1408,"GPF752510V221G000","8055261440104"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.","031","Chrome",867,"GPF752020G001G000","8055261440470"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",149,"Finox Brushed Nickel",1170,"GPF752020G002G000","8055261440463"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",299,"Matte Black",1170,"GPF752020C072G000","8055261440487"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",706,"Black Metal PVD",1282,"GPF752020P001G000","8055261440449"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",707,"Black Metal Brushed PVD",1369,"GPF752020P004G000","8055261440432"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.","030","Copper PVD",1282,"GPF752020P000G000","8055261440456"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",708,"Copper Brushed PVD",1369,"GPF752020P006G000","8055261440425"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",735,"Warm Bronze PVD",1282,"GPF752020P037G000","8055261440371"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",726,"Warm Bronze Brushed PVD",1369,"GPF752020P024G000","8055261440395"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",720,"Nickel PVD",1282,"GPF752020P014G000","8055261440401"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",761,"Coffee Bronze Brushed PVD",1456,"GPF752020E059G000","8055261571068"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",710,"Brass PVD",1282,"GPF752020P011G000","8055261440418"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",727,"Brass Brushed PVD",1369,"GPF752020P025G000","8055261440388"]
["BATHROOM","INCASTRI","INCASTRI",75202,75202,"Mengkraan Wastafel Sospeso, zonder waste met buigzame aansluitslangen","Mitigeur lavabo Sospeso, sans vidage, avec flexibles de raccordement.","Basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",845,"Dark Bronze",1369,"GPF752020V221G000","8055261440364"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.","031","Chrome",976,"GPF752530G001G000","8055261440081"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",149,"Finox Brushed Nickel",1317,"GPF752530G002G000","8055261440074"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",299,"Matte Black",1317,"GPF752530C072G000","8055261440098"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",706,"Black Metal PVD",1444,"GPF752530P001G000","8055261440050"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",707,"Black Metal Brushed PVD",1542,"GPF752530P004G000","8055261440043"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.","030","Copper PVD",1444,"GPF752530P000G000","8055261440067"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",708,"Copper Brushed PVD",1542,"GPF752530P006G000","8055261440036"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",735,"Warm Bronze PVD",1444,"GPF752530P037G000","8055261439986"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",726,"Warm Bronze Brushed PVD",1542,"GPF752530P024G000","8055261440005"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",720,"Nickel PVD",1444,"GPF752530P014G000","8055261440012"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",761,"Coffee Bronze Brushed PVD",1639,"GPF752530E059G000","8055261571006"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",710,"Brass PVD",1444,"GPF752530P011G000","8055261440029"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",727,"Brass Brushed PVD",1542,"GPF752530P025G000","8055261439993"]
["BATHROOM","INCASTRI","INCASTRI",75253,75253,"Hoge versie wastafelmengkraan Sospeso, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé Sospeso, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer Sospeso, with Stop&Go waste and connecting flexibles.",845,"Dark Bronze",1542,"GPF752530V221G000","8055261439979"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.","031","Chrome",951,"GPF752040G001G000","8055261440340"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",149,"Finox Brushed Nickel",1284,"GPF752040G002G000","8055261440333"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",299,"Matte Black",1284,"GPF752040C072G000","8055261440357"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",706,"Black Metal PVD",1409,"GPF752040P001G000","8055261440319"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",707,"Black Metal Brushed PVD",1504,"GPF752040P004G000","8055261440302"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.","030","Copper PVD",1409,"GPF752040P000G000","8055261440326"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",708,"Copper Brushed PVD",1504,"GPF752040P006G000","8055261440296"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",735,"Warm Bronze PVD",1409,"GPF752040P037G000","8055261440241"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",726,"Warm Bronze Brushed PVD",1504,"GPF752040P024G000","8055261440265"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",720,"Nickel PVD",1409,"GPF752040P014G000","8055261440272"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",761,"Coffee Bronze Brushed PVD",1598,"GPF752040E059G000","8055261571044"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",710,"Brass PVD",1409,"GPF752040P011G000","8055261440289"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",727,"Brass Brushed PVD",1504,"GPF752040P025G000","8055261440258"]
["BATHROOM","INCASTRI","INCASTRI",75204,75204,"Mengkraan Wastafel hoog Sospeso, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé Sospeso, sans vidage, avec flexibles de raccordement.","High version basin mixer Sospeso, without Stop&Go waste, with connecting flexibles.",845,"Dark Bronze",1504,"GPF752040V221G000","8055261440234"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.","031","Chrome",1195,"GPF750140G001G000","8055261445932"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",149,"Finox Brushed Nickel",1614,"GPF750140G002G000","8055261445925"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",299,"Matte Black",1614,"GPF750140C072G000","8055261445949"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",706,"Black Metal PVD",1770,"GPF750140P001G000","8055261445901"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",707,"Black Metal Brushed PVD",1889,"GPF750140P004G000","8055261445895"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.","030","Copper PVD",1770,"GPF750140P000G000","8055261445918"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",708,"Copper Brushed PVD",1889,"GPF750140P006G000","8055261445888"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",735,"Warm Bronze PVD",1770,"GPF750140P037G000","8055261445833"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",726,"Warm Bronze Brushed PVD",1889,"GPF750140P024G000","8055261445857"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",720,"Nickel PVD",1770,"GPF750140P014G000","8055261445864"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",761,"Coffee Bronze Brushed PVD",2008,"GPF750140E059G000","8055261571648"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",710,"Brass PVD",1770,"GPF750140P011G000","8055261445871"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",727,"Brass Brushed PVD",1889,"GPF750140P025G000","8055261445840"]
["BATHROOM","INCASTRI","INCASTRI",75014,75014,"Extern deel Elektronische Wastafelkraan. FLESSA.","Mélangeur sans vidage, avec flexibles de raccordement.","Three-holes basin mixer, without waste, with connecting flexibles.",845,"Dark Bronze",1889,"GPF750140V221G000","8055261445826"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",63397,"Inbouwdeel Voor Mengkraan Met Uitloop","Partie encastrée pour mitigeur lavabo mural","Built-in part for mixer with spout",239,"Steel Brushed",473,"GPF633970A000G000","8056329551572"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.","031","Chrome",842,"GPF750880G001G000","8055261520165"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",149,"Finox Brushed Nickel",1137,"GPF750880G002G000","8055261520158"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",299,"Matte Black",1137,"GPF750880C072G000","8055261520172"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",706,"Black Metal PVD",1247,"GPF750880P001G000","8055261520134"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",707,"Black Metal Brushed PVD",1331,"GPF750880P004G000","8055261520127"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.","030","Copper PVD",1247,"GPF750880P000G000","8055261520141"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",708,"Copper Brushed PVD",1331,"GPF750880P006G000","8055261520110"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",735,"Warm Bronze PVD",1247,"GPF750880P037G000","8055261520066"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",726,"Warm Bronze Brushed PVD",1331,"GPF750880P024G000","8055261520080"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",720,"Nickel PVD",1247,"GPF750880P014G000","8055261520097"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",761,"Coffee Bronze Brushed PVD",1415,"GPF750880E059G000","8055261571440"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",710,"Brass PVD",1247,"GPF750880P011G000","8055261520103"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",727,"Brass Brushed PVD",1331,"GPF750880P025G000","8055261520073"]
["BATHROOM","INCASTRI","INCASTRI","63397+75088",75088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur mural.","External part for wall-mounted basin mixer.",845,"Dark Bronze",1331,"GPF750880V221G000","8055261520059"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288","09280","Inbouwdeel voor mengkraan met uitloop","Partie encastrée pour mitigeur lavabo mural","Built-in part for mixer with spout","031","Chrome",306,"GPF092800G001G000","8055261435582"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.","031","Chrome",915,"GPF752880G001G000","8055261439955"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",149,"Finox Brushed Nickel",1235,"GPF752880G002G000","8055261439948"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",299,"Matte Black",1235,"GPF752880C072G000","8055261439962"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",706,"Black Metal PVD",1354,"GPF752880P001G000","8055261439924"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",707,"Black Metal Brushed PVD",1445,"GPF752880P004G000","8055261439917"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.","030","Copper PVD",1354,"GPF752880P000G000","8055261439931"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",708,"Copper Brushed PVD",1445,"GPF752880P006G000","8055261439900"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",735,"Warm Bronze PVD",1354,"GPF752880P037G000","8055261439856"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",726,"Warm Bronze Brushed PVD",1445,"GPF752880P024G000","8055261439870"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",720,"Nickel PVD",1354,"GPF752880P014G000","8055261439887"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",761,"Coffee Bronze Brushed PVD",1537,"GPF752880E059G000","8055261570986"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",710,"Brass PVD",1354,"GPF752880P011G000","8055261439894"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",727,"Brass Brushed PVD",1445,"GPF752880P025G000","8055261439863"]
["BATHROOM","INCASTRI","INCASTRI","09280+75288",75288,"Afbouwdeel wandgemonteerde wastafelmengkraan, Sospeso.","Partie apparente mitigeur mural, Sospeso.","External part for wall-mounted basin mixer, Sospeso.",845,"Dark Bronze",1445,"GPF752880V221G000","8055261439849"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.","031","Chrome",488,"GPF751020G001G000","8055261444249"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",149,"Finox Brushed Nickel",659,"GPF751020G002G000","8055261444232"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",299,"Matte Black",659,"GPF751020C072G000","8055261444256"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",706,"Black Metal PVD",722,"GPF751020P001G000","8055261444218"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",707,"Black Metal Brushed PVD",771,"GPF751020P004G000","8055261444201"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.","030","Copper PVD",722,"GPF751020P000G000","8055261444225"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",708,"Copper Brushed PVD",771,"GPF751020P006G000","8055261444195"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",735,"Warm Bronze PVD",722,"GPF751020P037G000","8055261444140"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",726,"Warm Bronze Brushed PVD",771,"GPF751020P024G000","8055261444164"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",720,"Nickel PVD",722,"GPF751020P014G000","8055261444171"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",761,"Coffee Bronze Brushed PVD",820,"GPF751020E059G000","8055261571365"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",710,"Brass PVD",722,"GPF751020P011G000","8055261444188"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",727,"Brass Brushed PVD",771,"GPF751020P025G000","8055261444157"]
["BATHROOM","INCASTRI","INCASTRI",75102,75102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural. A compléter avec mitigeur à commande séparée.","Wall-mounted basin spout. To be completed with separate control.",845,"Dark Bronze",771,"GPF751020V221G000","8055261444133"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.","031","Chrome",1463,"GPF750990G001G000","8055261444508"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",149,"Finox Brushed Nickel",1975,"GPF750990G002G000","8055261444492"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",299,"Matte Black",1975,"GPF750990C072G000","8055261444515"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",706,"Black Metal PVD",2166,"GPF750990P001G000","8055261444478"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",707,"Black Metal Brushed PVD",2312,"GPF750990P004G000","8055261444461"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.","030","Copper PVD",2166,"GPF750990P000G000","8055261444485"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",708,"Copper Brushed PVD",2312,"GPF750990P006G000","8055261444454"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",735,"Warm Bronze PVD",2166,"GPF750990P037G000","8055261444409"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",726,"Warm Bronze Brushed PVD",2312,"GPF750990P024G000","8055261444423"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",720,"Nickel PVD",2166,"GPF750990P014G000","8055261444430"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",761,"Coffee Bronze Brushed PVD",2459,"GPF750990E059G000","8055261571402"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",710,"Brass PVD",2166,"GPF750990P011G000","8055261444447"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",727,"Brass Brushed PVD",2312,"GPF750990P025G000","8055261444416"]
["BATHROOM","INCASTRI","INCASTRI",75099,75099,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout. To be completed with separate control.",845,"Dark Bronze",2312,"GPF750990V221G000","8055261444393"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.","031","Chrome",2122,"GPF751990G001G000","8055261440609"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",149,"Finox Brushed Nickel",2865,"GPF751990G002G000","8055261440593"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",299,"Matte Black",2865,"GPF751990C072G000","8055261440616"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",706,"Black Metal PVD",3141,"GPF751990P001G000","8055261440579"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",707,"Black Metal Brushed PVD",3353,"GPF751990P004G000","8055261440562"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.","030","Copper PVD",3141,"GPF751990P000G000","8055261440586"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",708,"Copper Brushed PVD",3353,"GPF751990P006G000","8055261440555"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",735,"Warm Bronze PVD",3141,"GPF751990P037G000","8055261440500"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",726,"Warm Bronze Brushed PVD",3353,"GPF751990P024G000","8055261440524"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",720,"Nickel PVD",3141,"GPF751990P014G000","8055261440531"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",761,"Coffee Bronze Brushed PVD",3564,"GPF751990E059G000","8055261571082"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",710,"Brass PVD",3141,"GPF751990P011G000","8055261440548"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",727,"Brass Brushed PVD",3353,"GPF751990P025G000","8055261440517"]
["BATHROOM","INCASTRI","INCASTRI",75199,75199,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longeur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted basin spout, length on request. To be completed with separate control.",845,"Dark Bronze",3353,"GPF751990V221G000","8055261440494"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.","031","Chrome",476,"GPF751000G001G000","8055261444379"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",149,"Finox Brushed Nickel",644,"GPF751000G002G000","8055261444362"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",299,"Matte Black",644,"GPF751000C072G000","8055261444386"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",706,"Black Metal PVD",705,"GPF751000P001G000","8055261444348"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",707,"Black Metal Brushed PVD",753,"GPF751000P004G000","8055261444331"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.","030","Copper PVD",705,"GPF751000P000G000","8055261444355"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",708,"Copper Brushed PVD",753,"GPF751000P006G000","8055261444324"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",735,"Warm Bronze PVD",705,"GPF751000P037G000","8055261444270"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",726,"Warm Bronze Brushed PVD",753,"GPF751000P024G000","8055261444294"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",720,"Nickel PVD",705,"GPF751000P014G000","8055261444300"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",761,"Coffee Bronze Brushed PVD",801,"GPF751000E059G000","8055261571389"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",710,"Brass PVD",705,"GPF751000P011G000","8055261444317"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",727,"Brass Brushed PVD",753,"GPF751000P025G000","8055261444287"]
["BATHROOM","INCASTRI","INCASTRI",75100,75100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée.","Separate control.",845,"Dark Bronze",753,"GPF751000V221G000","8055261444263"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",63412,"Inbouwdeel Wall-Fixing Wastafel Met Separate Bediening, 1-Weg","Partie encastrée pour mitigeur lavabo/douche mural une sortie","Built-in part for wall-mounted basin mixer, one-way.",239,"Steel Brushed",271,"GPF634120A000G000","8056329551060"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.","031","Chrome",355,"GPF751090G001G000","8055261443594"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",149,"Finox Brushed Nickel",479,"GPF751090G002G000","8055261443587"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",299,"Matte Black",479,"GPF751090C072G000","8055261443600"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",706,"Black Metal PVD",525,"GPF751090P001G000","8055261443563"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",707,"Black Metal Brushed PVD",560,"GPF751090P004G000","8055261443556"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.","030","Copper PVD",525,"GPF751090P000G000","8055261443570"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",708,"Copper Brushed PVD",560,"GPF751090P006G000","8055261443549"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",735,"Warm Bronze PVD",525,"GPF751090P037G000","8055261443495"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",726,"Warm Bronze Brushed PVD",560,"GPF751090P024G000","8055261443518"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",720,"Nickel PVD",525,"GPF751090P014G000","8055261443525"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",761,"Coffee Bronze Brushed PVD",596,"GPF751090E059G000","8055261571327"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",710,"Brass PVD",525,"GPF751090P011G000","8055261443532"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",727,"Brass Brushed PVD",560,"GPF751090P025G000","8055261443501"]
["BATHROOM","INCASTRI","INCASTRI","63412+75109",75109,"Afbouwdeel wandgemonteerde 1-weg wastafelmengkraan.","Partie apparente commande séparée mural.","External part for wall-mounted separate control.",845,"Dark Bronze",560,"GPF751090V221G000","8055261443488"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",46189,"Inbouwdeel voor standaard bad","Partie encastrée tenue étanche pour mitigeur bain-douche sur pied.","Built-in part for freestanding basin/bath mixer with spout.","031","Chrome",457,"GPF461892G001G000","8022692601503"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.","031","Chrome",2012,"GPF750950G001G000","8055261444638"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",149,"Finox Brushed Nickel",2717,"GPF750950G002G000","8055261444621"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",299,"Matte Black",2717,"GPF750950C072G000","8055261444645"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",706,"Black Metal PVD",2978,"GPF750950P001G000","8055261444607"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",707,"Black Metal Brushed PVD",3179,"GPF750950P004G000","8055261444591"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.","030","Copper PVD",2978,"GPF750950P000G000","8055261444614"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",708,"Copper Brushed PVD",3179,"GPF750950P006G000","8055261444584"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",735,"Warm Bronze PVD",2978,"GPF750950P037G000","8055261444539"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",726,"Warm Bronze Brushed PVD",3179,"GPF750950P024G000","8055261444553"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",720,"Nickel PVD",2978,"GPF750950P014G000","8055261444560"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",761,"Coffee Bronze Brushed PVD",3381,"GPF750950E059G000","8055261571426"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",710,"Brass PVD",2978,"GPF750950P011G000","8055261444577"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",727,"Brass Brushed PVD",3179,"GPF750950P025G000","8055261444546"]
["BATHROOM","INCASTRI","INCASTRI","46189+75095",75095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part for freestanding basin mixer.",845,"Dark Bronze",3179,"GPF750950V221G000","8055261444522"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.","031","Chrome",720,"GPF750670G001G000","8055261576322"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",149,"Finox Brushed Nickel",973,"GPF750670G002G000","8055261576315"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",299,"Matte Black",973,"GPF750670C072G000","8055261576353"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",706,"Black Metal PVD",1067,"GPF750670P001G000","8055261576292"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",707,"Black Metal Brushed PVD",1138,"GPF750670P004G000","8055261576285"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.","030","Copper PVD",1067,"GPF750670P000G000","8055261576308"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",708,"Copper Brushed PVD",1138,"GPF750670P006G000","8055261576278"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",735,"Warm Bronze PVD",1067,"GPF750670P037G000","8055261576223"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",726,"Warm Bronze Brushed PVD",1138,"GPF750670P024G000","8055261576247"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",720,"Nickel PVD",1067,"GPF750670P014G000","8055261576254"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",761,"Coffee Bronze Brushed PVD",1210,"GPF750670E059G000","8055261576339"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",710,"Brass PVD",1067,"GPF750670P011G000","8055261576261"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",727,"Brass Brushed PVD",1138,"GPF750670P025G000","8055261576230"]
["BATHROOM","INCASTRI","INCASTRI",75067,75067,"Mengkraan Bidet met veste plug, met buigzame aansluitslangen","Mitigeur bidet avec vidage Stop&Go et flexibles de raccordement.","Bidet mixer with Stop&Go waste and connecting flexibles.",845,"Dark Bronze",1138,"GPF750670V221G000","8055261576216"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.","031","Chrome",696,"GPF750680G001G000","8055261576179"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",149,"Finox Brushed Nickel",940,"GPF750680G002G000","8055261576162"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",299,"Matte Black",940,"GPF750680C072G000","8055261576209"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",706,"Black Metal PVD",1030,"GPF750680P001G000","8055261576148"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",707,"Black Metal Brushed PVD",1100,"GPF750680P004G000","8055261576131"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.","030","Copper PVD",1030,"GPF750680P000G000","8055261576155"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",708,"Copper Brushed PVD",1100,"GPF750680P006G000","8055261576124"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",735,"Warm Bronze PVD",1030,"GPF750680P037G000","8055261576070"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",726,"Warm Bronze Brushed PVD",1100,"GPF750680P024G000","8055261576094"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",720,"Nickel PVD",1030,"GPF750680P014G000","8055261576100"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",761,"Coffee Bronze Brushed PVD",1170,"GPF750680E059G000","8055261576186"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",710,"Brass PVD",1030,"GPF750680P011G000","8055261576117"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",727,"Brass Brushed PVD",1100,"GPF750680P025G000","8055261576087"]
["BATHROOM","INCASTRI","INCASTRI",75068,75068,"Mengkraan Bidet zonder waste met buigzame aansluitslangen","Mitigeur bidet sans vidage et flexibles de raccordement.","Bidet mixer without waste and connecting flexibles.",845,"Dark Bronze",1100,"GPF750680V221G000","8055261576063"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",46189,"Inbouwdeel voor standaard bad","Partie encastrée tenue étanche pour mitigeur bain-douche sur pied.","Built-in part for freestanding basin/bath mixer with spout.","031","Chrome",457,"GPF461892G001G000","8022692601503"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.","031","Chrome",2914,"GPF750280G001G000","8055261445802"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",149,"Finox Brushed Nickel",3935,"GPF750280G002G000","8055261445796"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",299,"Matte Black",3935,"GPF750280C072G000","8055261445819"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",706,"Black Metal PVD",4314,"GPF750280P001G000","8055261445772"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",707,"Black Metal Brushed PVD",4605,"GPF750280P004G000","8055261445765"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.","030","Copper PVD",4314,"GPF750280P000G000","8055261445789"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",708,"Copper Brushed PVD",4605,"GPF750280P006G000","8055261445758"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",735,"Warm Bronze PVD",4314,"GPF750280P037G000","8055261445703"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",726,"Warm Bronze Brushed PVD",4605,"GPF750280P024G000","8055261445727"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",720,"Nickel PVD",4314,"GPF750280P014G000","8055261445734"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",761,"Coffee Bronze Brushed PVD",4897,"GPF750280E059G000","8055261571624"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",710,"Brass PVD",4314,"GPF750280P011G000","8055261445741"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",727,"Brass Brushed PVD",4605,"GPF750280P025G000","8055261445710"]
["BATHROOM","INCASTRI","INCASTRI","46189+75028",75028,"Extern deel vrijstaande badkraan","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part for freestanding bath mixer with automatic diverter and antilimestone handshower.",845,"Dark Bronze",4605,"GPF750280V221G000","8055261445697"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.","031","Chrome",586,"GPF751030G001G000","8055261444119"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",149,"Finox Brushed Nickel",791,"GPF751030G002G000","8055261444102"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",299,"Matte Black",791,"GPF751030C072G000","8055261444126"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",706,"Black Metal PVD",868,"GPF751030P001G000","8055261444089"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",707,"Black Metal Brushed PVD",926,"GPF751030P004G000","8055261444072"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.","030","Copper PVD",868,"GPF751030P000G000","8055261444096"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",708,"Copper Brushed PVD",926,"GPF751030P006G000","8055261444065"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",735,"Warm Bronze PVD",868,"GPF751030P037G000","8055261444010"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",726,"Warm Bronze Brushed PVD",926,"GPF751030P024G000","8055261444034"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",720,"Nickel PVD",868,"GPF751030P014G000","8055261444041"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",761,"Coffee Bronze Brushed PVD",984,"GPF751030E059G000","8055261571341"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",710,"Brass PVD",868,"GPF751030P011G000","8055261444058"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",727,"Brass Brushed PVD",926,"GPF751030P025G000","8055261444027"]
["BATHROOM","INCASTRI","INCASTRI",75103,75103,"Wandgemonteerde bad mengkraan.","Bec de baignoire mural.","Wall-mounted bath spout.",845,"Dark Bronze",926,"GPF751030V221G000","8055261444003"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",54139,"Inbouwdeel Mengkraan. 2-Weg","Partie encastrée mitigeur de baignoire mural deux sorties","Built-in part mixer, two-ways.",239,"Steel Brushed",572,"GPF541390A000G000","8022692841411"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.","031","Chrome",1268,"GPF750360G001G000","8055261445673"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",149,"Finox Brushed Nickel",1712,"GPF750360G002G000","8055261445666"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",299,"Matte Black",1712,"GPF750360C072G000","8055261445680"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",706,"Black Metal PVD",1878,"GPF750360P001G000","8055261445642"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",707,"Black Metal Brushed PVD",2005,"GPF750360P004G000","8055261445635"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.","030","Copper PVD",1878,"GPF750360P000G000","8055261445659"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",708,"Copper Brushed PVD",2005,"GPF750360P006G000","8055261445628"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",735,"Warm Bronze PVD",1878,"GPF750360P037G000","8055261445574"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",726,"Warm Bronze Brushed PVD",2005,"GPF750360P024G000","8055261445598"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",720,"Nickel PVD",1878,"GPF750360P014G000","8055261445604"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",761,"Coffee Bronze Brushed PVD",2131,"GPF750360E059G000","8055261571600"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",710,"Brass PVD",1878,"GPF750360P011G000","8055261445611"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",727,"Brass Brushed PVD",2005,"GPF750360P025G000","8055261445581"]
["BATHROOM","INCASTRI","INCASTRI","54139+75036",75036,"Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire.","External part wall-mounted shower mixer two-ways with handshower.",845,"Dark Bronze",2005,"GPF750360V221G000","8055261445567"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",54073,"Inbouwdeel Voor Wandgemonteerde Douche Mengkraan, 2-Weg","Partie encastrée pour mitigeur douche mura deux sorties","Built-in part for wall-mounted shower mixer, two-ways.",239,"Steel Brushed",516,"GPF540731A000G000","8022692849813"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.","031","Chrome",878,"GPF750380G001G000","8055261445543"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",149,"Finox Brushed Nickel",1186,"GPF750380G002G000","8055261445536"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",299,"Matte Black",1186,"GPF750380C072G000","8055261445550"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",706,"Black Metal PVD",1300,"GPF750380P001G000","8055261445512"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",707,"Black Metal Brushed PVD",1388,"GPF750380P004G000","8055261445505"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.","030","Copper PVD",1300,"GPF750380P000G000","8055261445529"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",708,"Copper Brushed PVD",1388,"GPF750380P006G000","8055261445499"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",735,"Warm Bronze PVD",1300,"GPF750380P037G000","8055261445444"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",726,"Warm Bronze Brushed PVD",1388,"GPF750380P024G000","8055261445468"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",720,"Nickel PVD",1300,"GPF750380P014G000","8055261445475"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",761,"Coffee Bronze Brushed PVD",1476,"GPF750380E059G000","8055261571587"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",710,"Brass PVD",1300,"GPF750380P011G000","8055261445482"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",727,"Brass Brushed PVD",1388,"GPF750380P025G000","8055261445451"]
["BATHROOM","INCASTRI","INCASTRI","54073+75038",75038,"Extern deel Wandmengkraan Douche 2-weg","Partie apparente pour mitigeur douche murale 2 sorites.","External part wall-mounted shower mixer two-ways.",845,"Dark Bronze",1388,"GPF750380V221G000","8055261445437"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",54055,"Inbouwdeel Voor Wandgemonteerde Douche/Wastafelmengkraan, 1-Weg","Partie encastrée pour mitigeur lavabo/douche mural une sortie","Built-in part for wall-mounted shower/basin mixer, one way",239,"Steel Brushed",296,"GPF540550A000G000","8022692835960"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.","031","Chrome",397,"GPF750610G001G000","8055261496538"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",149,"Finox Brushed Nickel",536,"GPF750610G002G000","8055261496521"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",299,"Matte Black",536,"GPF750610C072G000","8055261496545"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",706,"Black Metal PVD",588,"GPF750610P001G000","8055261496507"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",707,"Black Metal Brushed PVD",628,"GPF750610P004G000","8055261496491"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.","030","Copper PVD",588,"GPF750610P000G000","8055261496514"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",708,"Copper Brushed PVD",628,"GPF750610P006G000","8055261496484"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",735,"Warm Bronze PVD",588,"GPF750610P037G000","8055261496439"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",726,"Warm Bronze Brushed PVD",628,"GPF750610P024G000","8055261496453"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",720,"Nickel PVD",588,"GPF750610P014G000","8055261496460"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",761,"Coffee Bronze Brushed PVD",667,"GPF750610E059G000","8055261571464"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",710,"Brass PVD",588,"GPF750610P011G000","8055261496477"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",727,"Brass Brushed PVD",628,"GPF750610P025G000","8055261496446"]
["BATHROOM","INCASTRI","INCASTRI","54055+75061",75061,"Afbouwdeel wandgemonteerde 1-weg bath/douche mengkraan.","Partie apparente pour commande séparée douche mural une sortie.","External part wall-mounted shower mixer one-way.",845,"Dark Bronze",628,"GPF750610V221G000","8055261496422"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",54169,"Inbouwdeel Thermostatische Mengkraan Wanddouche","Partie encastrée pour mitigeur thermostatique douche mural","Built-in part for wall-mounted thermostatic shower mixer.",239,"Steel Brushed",438,"GPF541690A000G000","8022692841398"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.","031","Chrome",915,"GPF751320G001G000","8055261442818"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",149,"Finox Brushed Nickel",1235,"GPF751320G002G000","8055261442801"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",299,"Matte Black",1235,"GPF751320C072G000","8055261442825"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",706,"Black Metal PVD",1354,"GPF751320P001G000","8055261442788"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",707,"Black Metal Brushed PVD",1445,"GPF751320P004G000","8055261442771"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.","030","Copper PVD",1354,"GPF751320P000G000","8055261442795"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",708,"Copper Brushed PVD",1445,"GPF751320P006G000","8055261442764"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",735,"Warm Bronze PVD",1354,"GPF751320P037G000","8055261442719"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",726,"Warm Bronze Brushed PVD",1445,"GPF751320P024G000","8055261442733"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",720,"Nickel PVD",1354,"GPF751320P014G000","8055261442740"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",761,"Coffee Bronze Brushed PVD",1537,"GPF751320E059G000","8055261571303"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",710,"Brass PVD",1354,"GPF751320P011G000","8055261442757"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",727,"Brass Brushed PVD",1445,"GPF751320P025G000","8055261442726"]
["BATHROOM","INCASTRI","INCASTRI","54169+75132",75132,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",845,"Dark Bronze",1445,"GPF751320V221G000","8055261442702"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",54169,"Inbouwdeel Thermostatische Mengkraan Wanddouche","Partie encastrée pour mitigeur thermostatique douche mural","Built-in part for wall-mounted thermostatic shower mixer.",239,"Steel Brushed",438,"GPF541690A000G000","8022692841398"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.","031","Chrome",915,"GPF751340G001G000","8055261442559"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",149,"Finox Brushed Nickel",1235,"GPF751340G002G000","8055261442542"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",299,"Matte Black",1235,"GPF751340C072G000","8055261442566"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",706,"Black Metal PVD",1354,"GPF751340P001G000","8055261442528"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",707,"Black Metal Brushed PVD",1445,"GPF751340P004G000","8055261442511"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.","030","Copper PVD",1354,"GPF751340P000G000","8055261442535"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",708,"Copper Brushed PVD",1445,"GPF751340P006G000","8055261442504"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",735,"Warm Bronze PVD",1354,"GPF751340P037G000","8055261442450"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",726,"Warm Bronze Brushed PVD",1445,"GPF751340P024G000","8055261442474"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",720,"Nickel PVD",1354,"GPF751340P014G000","8055261442481"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",761,"Coffee Bronze Brushed PVD",1537,"GPF751340E059G000","8055261571266"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",710,"Brass PVD",1354,"GPF751340P011G000","8055261442498"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",727,"Brass Brushed PVD",1445,"GPF751340P025G000","8055261442467"]
["BATHROOM","INCASTRI","INCASTRI","54169+75134",75134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",845,"Dark Bronze",1445,"GPF751340V221G000","8055261442443"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",54169,"Inbouwdeel Thermostatische Mengkraan Wanddouche","Partie encastrée pour mitigeur thermostatique douche mural","Built-in part for wall-mounted thermostatic shower mixer.",239,"Steel Brushed",438,"GPF541690A000G000","8022692841398"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.","031","Chrome",915,"GPF751360G001G000","8055261442290"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",149,"Finox Brushed Nickel",1235,"GPF751360G002G000","8055261442283"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",299,"Matte Black",1235,"GPF751360C072G000","8055261442306"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",706,"Black Metal PVD",1354,"GPF751360P001G000","8055261442269"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",707,"Black Metal Brushed PVD",1445,"GPF751360P004G000","8055261442252"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.","030","Copper PVD",1354,"GPF751360P000G000","8055261442276"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",708,"Copper Brushed PVD",1445,"GPF751360P006G000","8055261442245"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",735,"Warm Bronze PVD",1354,"GPF751360P037G000","8055261442191"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",726,"Warm Bronze Brushed PVD",1445,"GPF751360P024G000","8055261442214"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",720,"Nickel PVD",1354,"GPF751360P014G000","8055261442221"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",761,"Coffee Bronze Brushed PVD",1537,"GPF751360E059G000","8055261571228"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",710,"Brass PVD",1354,"GPF751360P011G000","8055261442238"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",727,"Brass Brushed PVD",1445,"GPF751360P025G000","8055261442207"]
["BATHROOM","INCASTRI","INCASTRI","54169+75136",75136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",845,"Dark Bronze",1445,"GPF751360V221G000","8055261442184"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133","09269","Inbouwdeel voor thermostatische mengkraan","Partie encastrée pour mitigeur de douche thermostatique mural","Built-in part for thermostatic mixer","031","Chrome",571,"GPF092691G001G000","8022692101652"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.","031","Chrome",915,"GPF751330G001G000","8055261442689"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",149,"Finox Brushed Nickel",1235,"GPF751330G002G000","8055261442672"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",299,"Matte Black",1235,"GPF751330C072G000","8055261442696"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",706,"Black Metal PVD",1354,"GPF751330P001G000","8055261442658"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",707,"Black Metal Brushed PVD",1445,"GPF751330P004G000","8055261442641"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.","030","Copper PVD",1354,"GPF751330P000G000","8055261442665"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",708,"Copper Brushed PVD",1445,"GPF751330P006G000","8055261442634"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",735,"Warm Bronze PVD",1354,"GPF751330P037G000","8055261442580"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",726,"Warm Bronze Brushed PVD",1445,"GPF751330P024G000","8055261442603"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",720,"Nickel PVD",1354,"GPF751330P014G000","8055261442610"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",761,"Coffee Bronze Brushed PVD",1537,"GPF751330E059G000","8055261571280"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",710,"Brass PVD",1354,"GPF751330P011G000","8055261442627"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",727,"Brass Brushed PVD",1445,"GPF751330P025G000","8055261442597"]
["BATHROOM","INCASTRI","INCASTRI","09269+75133",75133,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche murale 1 sortie.","External part wall-mounted thermostatic shower mixer one-way.",845,"Dark Bronze",1445,"GPF751330V221G000","8055261442573"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135","09269","Inbouwdeel voor thermostatische mengkraan","Partie encastrée pour mitigeur de douche thermostatique mural","Built-in part for thermostatic mixer","031","Chrome",571,"GPF092691G001G000","8022692101652"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.","031","Chrome",915,"GPF751350G001G000","8055261442429"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",149,"Finox Brushed Nickel",1235,"GPF751350G002G000","8055261442412"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",299,"Matte Black",1235,"GPF751350C072G000","8055261442436"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",706,"Black Metal PVD",1354,"GPF751350P001G000","8055261442399"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",707,"Black Metal Brushed PVD",1445,"GPF751350P004G000","8055261442382"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.","030","Copper PVD",1354,"GPF751350P000G000","8055261442405"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",708,"Copper Brushed PVD",1445,"GPF751350P006G000","8055261442375"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",735,"Warm Bronze PVD",1354,"GPF751350P037G000","8055261442320"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",726,"Warm Bronze Brushed PVD",1445,"GPF751350P024G000","8055261442344"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",720,"Nickel PVD",1354,"GPF751350P014G000","8055261442351"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",761,"Coffee Bronze Brushed PVD",1537,"GPF751350E059G000","8055261571242"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",710,"Brass PVD",1354,"GPF751350P011G000","8055261442368"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",727,"Brass Brushed PVD",1445,"GPF751350P025G000","8055261442337"]
["BATHROOM","INCASTRI","INCASTRI","09269+75135",75135,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche murale 2 sorties.","External part wall-mounted thermostatic shower mixer two-ways.",845,"Dark Bronze",1445,"GPF751350V221G000","8055261442313"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137","09269","Inbouwdeel voor thermostatische mengkraan","Partie encastrée pour mitigeur de douche thermostatique mural","Built-in part for thermostatic mixer","031","Chrome",571,"GPF092691G001G000","8022692101652"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.","031","Chrome",915,"GPF751370G001G000","8055261442160"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",149,"Finox Brushed Nickel",1235,"GPF751370G002G000","8055261442153"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",299,"Matte Black",1235,"GPF751370C072G000","8055261442177"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",706,"Black Metal PVD",1354,"GPF751370P001G000","8055261442139"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",707,"Black Metal Brushed PVD",1445,"GPF751370P004G000","8055261442122"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.","030","Copper PVD",1354,"GPF751370P000G000","8055261442146"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",708,"Copper Brushed PVD",1445,"GPF751370P006G000","8055261442115"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",735,"Warm Bronze PVD",1354,"GPF751370P037G000","8055261442061"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",726,"Warm Bronze Brushed PVD",1445,"GPF751370P024G000","8055261442085"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",720,"Nickel PVD",1354,"GPF751370P014G000","8055261442092"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",761,"Coffee Bronze Brushed PVD",1537,"GPF751370E059G000","8055261571204"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",710,"Brass PVD",1354,"GPF751370P011G000","8055261442108"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",727,"Brass Brushed PVD",1445,"GPF751370P025G000","8055261442078"]
["BATHROOM","INCASTRI","INCASTRI","09269+75137",75137,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche murale 3 sorties.","External part wall-mounted thermosttic shower mixer three-ways.",845,"Dark Bronze",1445,"GPF751370V221G000","8055261442054"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334","09264","Inbouwdeel voor thermostatische mengkraan, 2 separate uitgangen","Partie encastrée du mitigeur thermostatique mural 2 sorties indépendantes","Built-in part for thermostatic mixer, TWO separate exits","031","Chrome",1053,"GPF092640G001G000","8056603620796"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.","031","Chrome",1128,"GPF753340G001G000","8055261495364"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",149,"Finox Brushed Nickel",1524,"GPF753340G002G000","8055261495357"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",299,"Matte Black",1524,"GPF753340C072G000","8055261495371"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",706,"Black Metal PVD",1670,"GPF753340P001G000","8055261495333"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",707,"Black Metal Brushed PVD",1783,"GPF753340P004G000","8055261495326"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.","030","Copper PVD",1670,"GPF753340P000G000","8055261495340"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",708,"Copper Brushed PVD",1783,"GPF753340P006G000","8055261495319"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",735,"Warm Bronze PVD",1670,"GPF753340P037G000","8055261495265"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",726,"Warm Bronze Brushed PVD",1783,"GPF753340P024G000","8055261495289"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",720,"Nickel PVD",1670,"GPF753340P014G000","8055261495296"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",761,"Coffee Bronze Brushed PVD",1896,"GPF753340E059G000","8055261570801"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",710,"Brass PVD",1670,"GPF753340P011G000","8055261495302"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",727,"Brass Brushed PVD",1783,"GPF753340P025G000","8055261495272"]
["BATHROOM","INCASTRI","INCASTRI","09264+75334",75334,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 2 sorties indépendantes.","External part wall-mounted thermostatic mixer 2 indipendent exits.",845,"Dark Bronze",1783,"GPF753340V221G000","8055261495258"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336","09266","Inbouwdeel voor thermostatische mengkraan, 3 separate uitgangen","Partie encastrée du mitigeur thermostatique mural 3 sorties indépendantes","Built-in part for thermostatic mixer, THREE separate exits","031","Chrome",1173,"GPF092660G001G000","8056603620789"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.","031","Chrome",1312,"GPF753360G001G000","8055261495234"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",149,"Finox Brushed Nickel",1771,"GPF753360G002G000","8055261495227"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",299,"Matte Black",1771,"GPF753360C072G000","8055261495241"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",706,"Black Metal PVD",1940,"GPF753360P001G000","8055261495203"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",707,"Black Metal Brushed PVD",2072,"GPF753360P004G000","8055261495197"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.","030","Copper PVD",1940,"GPF753360P000G000","8055261495210"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",708,"Copper Brushed PVD",2072,"GPF753360P006G000","8055261495180"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",735,"Warm Bronze PVD",1940,"GPF753360P037G000","8055261495135"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",726,"Warm Bronze Brushed PVD",2072,"GPF753360P024G000","8055261495159"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",720,"Nickel PVD",1940,"GPF753360P014G000","8055261495166"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",761,"Coffee Bronze Brushed PVD",2204,"GPF753360E059G000","8055261570788"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",710,"Brass PVD",1940,"GPF753360P011G000","8055261495173"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",727,"Brass Brushed PVD",2072,"GPF753360P025G000","8055261495142"]
["BATHROOM","INCASTRI","INCASTRI","09266+75336",75336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 3 sorties indépendantes.","External part wall-mounted thermostatic mixer 3 indipendent exits.",845,"Dark Bronze",2072,"GPF753360V221G000","8055261495128"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338","09268","Inbouwdeel voor thermostatische mengkraan, 4 separate uitgangen","Partie encastrée du mitigeur thermostatique mural 4 sorties indépendantes","Built-in part for thermostatic mixer, FOUR separate exits","031","Chrome",1378,"GPF092680G001G000","8056603620772"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.","031","Chrome",1482,"GPF753380G001G000","8055261495104"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",149,"Finox Brushed Nickel",2002,"GPF753380G002G000","8055261495098"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",299,"Matte Black",2002,"GPF753380C072G000","8055261495111"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",706,"Black Metal PVD",2194,"GPF753380P001G000","8055261495074"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",707,"Black Metal Brushed PVD",2341,"GPF753380P004G000","8055261495067"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.","030","Copper PVD",2194,"GPF753380P000G000","8055261495081"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",708,"Copper Brushed PVD",2341,"GPF753380P006G000","8055261495050"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",735,"Warm Bronze PVD",2194,"GPF753380P037G000","8055261495005"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",726,"Warm Bronze Brushed PVD",2341,"GPF753380P024G000","8055261495029"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",720,"Nickel PVD",2194,"GPF753380P014G000","8055261495036"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",761,"Coffee Bronze Brushed PVD",2490,"GPF753380E059G000","8055261570764"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",710,"Brass PVD",2194,"GPF753380P011G000","8055261495043"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",727,"Brass Brushed PVD",2341,"GPF753380P025G000","8055261495012"]
["BATHROOM","INCASTRI","INCASTRI","09268+75338",75338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 4 sorties indépendantes.","External part wall-mounted thermostatic mixer 4 indipendent exits.",845,"Dark Bronze",2341,"GPF753380V221G000","8055261494992"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340","09263","Inbouwdeel voor thermostatische mengkraan, 5 separate uitgangen","Partie encastrée du mitigeur thermostatique mural 5 sorties indépendantes","Built-in part for thermostatic mixer, FIVE separate exits","031","Chrome",1547,"GPF092630G001G000","8056603629980"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.","031","Chrome",1634,"GPF753400G001G000","8055261494978"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",149,"Finox Brushed Nickel",2206,"GPF753400G002G000","8055261494961"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",299,"Matte Black",2206,"GPF753400C072G000","8055261494985"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",706,"Black Metal PVD",2419,"GPF753400P001G000","8055261494947"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",707,"Black Metal Brushed PVD",2583,"GPF753400P004G000","8055261494930"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.","030","Copper PVD",2419,"GPF753400P000G000","8055261494954"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",708,"Copper Brushed PVD",2583,"GPF753400P006G000","8055261494923"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",735,"Warm Bronze PVD",2419,"GPF753400P037G000","8055261494879"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",726,"Warm Bronze Brushed PVD",2583,"GPF753400P024G000","8055261494893"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",720,"Nickel PVD",2419,"GPF753400P014G000","8055261494909"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",761,"Coffee Bronze Brushed PVD",2745,"GPF753400E059G000","8055261570740"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",710,"Brass PVD",2419,"GPF753400P011G000","8055261494916"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",727,"Brass Brushed PVD",2583,"GPF753400P025G000","8055261494886"]
["BATHROOM","INCASTRI","INCASTRI","09263+75340",75340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie apparente pour mitigeur thermostatique douche murale 5 sorties indépendantes.","External part wall-mounted thermostatic mixer 5 indipendent exits.",845,"Dark Bronze",2583,"GPF753400V221G000","8055261494862"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314","43103","Inbouwdeel Thermostatische mengkraan hoog debiet 2 onafhankelijke uitgangen","Partie encastrée mitigeur THERMOSTATIQUE douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","Built-in thermostatic high-capacity mixer with TWO SEPARATE EXITS. Vertical/Horizontal installation.","031","Chrome",1053,"GPF431033G001G000","8022692583069"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.","031","Chrome",1128,"GPF753140G001G000","8055261495883"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",149,"Finox Brushed Nickel",1524,"GPF753140G002G000","8055261495876"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",299,"Matte Black",1524,"GPF753140C072G000","8055261495890"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",706,"Black Metal PVD",1670,"GPF753140P001G000","8055261495852"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",707,"Black Metal Brushed PVD",1783,"GPF753140P004G000","8055261495845"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.","030","Copper PVD",1670,"GPF753140P000G000","8055261495869"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",708,"Copper Brushed PVD",1783,"GPF753140P006G000","8055261495838"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",735,"Warm Bronze PVD",1670,"GPF753140P037G000","8055261495784"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",726,"Warm Bronze Brushed PVD",1783,"GPF753140P024G000","8055261495807"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",720,"Nickel PVD",1670,"GPF753140P014G000","8055261495814"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",761,"Coffee Bronze Brushed PVD",1896,"GPF753140E059G000","8055261570887"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",710,"Brass PVD",1670,"GPF753140P011G000","8055261495821"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",727,"Brass Brushed PVD",1783,"GPF753140P025G000","8055261495791"]
["BATHROOM","INCASTRI","INCASTRI","43103+75314",75314,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",845,"Dark Bronze",1783,"GPF753140V221G000","8055261495777"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304","43103","Inbouwdeel Thermostatische mengkraan hoog debiet 2 onafhankelijke uitgangen","Partie encastrée mitigeur THERMOSTATIQUE douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","Built-in thermostatic high-capacity mixer with TWO SEPARATE EXITS. Vertical/Horizontal installation.","031","Chrome",1053,"GPF431033G001G000","8022692583069"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.","031","Chrome",1128,"GPF753040G001G000","8055261496408"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",149,"Finox Brushed Nickel",1524,"GPF753040G002G000","8055261496392"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",299,"Matte Black",1524,"GPF753040C072G000","8055261496415"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",706,"Black Metal PVD",1670,"GPF753040P001G000","8055261496378"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",707,"Black Metal Brushed PVD",1783,"GPF753040P004G000","8055261496361"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.","030","Copper PVD",1670,"GPF753040P000G000","8055261496385"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",708,"Copper Brushed PVD",1783,"GPF753040P006G000","8055261496354"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",735,"Warm Bronze PVD",1670,"GPF753040P037G000","8055261496309"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",726,"Warm Bronze Brushed PVD",1783,"GPF753040P024G000","8055261496323"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",720,"Nickel PVD",1670,"GPF753040P014G000","8055261496330"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",761,"Coffee Bronze Brushed PVD",1896,"GPF753040E059G000","8055261570962"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",710,"Brass PVD",1670,"GPF753040P011G000","8055261496347"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",727,"Brass Brushed PVD",1783,"GPF753040P025G000","8055261496316"]
["BATHROOM","INCASTRI","INCASTRI","43103+75304",75304,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, deux sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 2 separate exits. Vertical/Horizontal installation.",845,"Dark Bronze",1783,"GPF753040V221G000","8055261496293"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316","43105","Inbouwdeel Thermostatische mengkraan hoog debiet 3 onafhankelijke uitgangen","Partie encastrée mitigeur THERMOSTATIQUE douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","Built-in thermostatic high-capacity mixer with THREE SEPARATE EXITS. Vertical/Horizontal installation.","031","Chrome",1173,"GPF431053G001G000","8022692583199"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.","031","Chrome",1312,"GPF753160G001G000","8055261495753"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",149,"Finox Brushed Nickel",1771,"GPF753160G002G000","8055261495746"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",299,"Matte Black",1771,"GPF753160C072G000","8055261495760"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",706,"Black Metal PVD",1940,"GPF753160P001G000","8055261495722"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",707,"Black Metal Brushed PVD",2072,"GPF753160P004G000","8055261495715"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.","030","Copper PVD",1940,"GPF753160P000G000","8055261495739"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",708,"Copper Brushed PVD",2072,"GPF753160P006G000","8055261495708"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",735,"Warm Bronze PVD",1940,"GPF753160P037G000","8055261495654"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",726,"Warm Bronze Brushed PVD",2072,"GPF753160P024G000","8055261495678"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",720,"Nickel PVD",1940,"GPF753160P014G000","8055261495685"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",761,"Coffee Bronze Brushed PVD",2204,"GPF753160E059G000","8055261570863"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",710,"Brass PVD",1940,"GPF753160P011G000","8055261495692"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",727,"Brass Brushed PVD",2072,"GPF753160P025G000","8055261495661"]
["BATHROOM","INCASTRI","INCASTRI","43105+75316",75316,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",845,"Dark Bronze",2072,"GPF753160V221G000","8055261495647"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306","43105","Inbouwdeel Thermostatische mengkraan hoog debiet 3 onafhankelijke uitgangen","Partie encastrée mitigeur THERMOSTATIQUE douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","Built-in thermostatic high-capacity mixer with THREE SEPARATE EXITS. Vertical/Horizontal installation.","031","Chrome",1173,"GPF431053G001G000","8022692583199"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.","031","Chrome",1312,"GPF753060G001G000","8055261496279"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",149,"Finox Brushed Nickel",1771,"GPF753060G002G000","8055261496262"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",299,"Matte Black",1771,"GPF753060C072G000","8055261496286"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",706,"Black Metal PVD",1940,"GPF753060P001G000","8055261496248"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",707,"Black Metal Brushed PVD",2072,"GPF753060P004G000","8055261496231"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.","030","Copper PVD",1940,"GPF753060P000G000","8055261496255"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",708,"Copper Brushed PVD",2072,"GPF753060P006G000","8055261496224"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",735,"Warm Bronze PVD",1940,"GPF753060P037G000","8055261496170"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",726,"Warm Bronze Brushed PVD",2072,"GPF753060P024G000","8055261496194"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",720,"Nickel PVD",1940,"GPF753060P014G000","8055261496200"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",761,"Coffee Bronze Brushed PVD",2204,"GPF753060E059G000","8055261570948"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",710,"Brass PVD",1940,"GPF753060P011G000","8055261496217"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",727,"Brass Brushed PVD",2072,"GPF753060P025G000","8055261496187"]
["BATHROOM","INCASTRI","INCASTRI","43105+75306",75306,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 3 separate exits. Vertical/Horizontal installation.",845,"Dark Bronze",2072,"GPF753060V221G000","8055261496163"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318","43107","Inbouwdeel Thermostatische mengkraan hoog debiet 4 onafhankelijke uitgangen","Partie encastrée mitigeur THERMOSTATIQUE douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","Built-in thermostatic high-capacity mixer with FOUR SEPARATE EXITS. Vertical/Horizontal installation.","031","Chrome",1378,"GPF431073G001G000","8022692583304"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.","031","Chrome",1482,"GPF753180G001G000","8055261495623"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",149,"Finox Brushed Nickel",2002,"GPF753180G002G000","8055261495616"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",299,"Matte Black",2002,"GPF753180C072G000","8055261495630"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",706,"Black Metal PVD",2194,"GPF753180P001G000","8055261495593"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",707,"Black Metal Brushed PVD",2341,"GPF753180P004G000","8055261495586"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.","030","Copper PVD",2194,"GPF753180P000G000","8055261495609"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",708,"Copper Brushed PVD",2341,"GPF753180P006G000","8055261495579"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",735,"Warm Bronze PVD",2194,"GPF753180P037G000","8055261495524"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",726,"Warm Bronze Brushed PVD",2341,"GPF753180P024G000","8055261495548"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",720,"Nickel PVD",2194,"GPF753180P014G000","8055261495555"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",761,"Coffee Bronze Brushed PVD",2490,"GPF753180E059G000","8055261570849"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",710,"Brass PVD",2194,"GPF753180P011G000","8055261495562"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",727,"Brass Brushed PVD",2341,"GPF753180P025G000","8055261495531"]
["BATHROOM","INCASTRI","INCASTRI","43107+75318",75318,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",845,"Dark Bronze",2341,"GPF753180V221G000","8055261495517"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308","43107","Inbouwdeel Thermostatische mengkraan hoog debiet 4 onafhankelijke uitgangen","Partie encastrée mitigeur THERMOSTATIQUE douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","Built-in thermostatic high-capacity mixer with FOUR SEPARATE EXITS. Vertical/Horizontal installation.","031","Chrome",1378,"GPF431073G001G000","8022692583304"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.","031","Chrome",1482,"GPF753080G001G000","8055261496149"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",149,"Finox Brushed Nickel",2002,"GPF753080G002G000","8055261496132"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",299,"Matte Black",2002,"GPF753080C072G000","8055261496156"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",706,"Black Metal PVD",2194,"GPF753080P001G000","8055261496118"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",707,"Black Metal Brushed PVD",2341,"GPF753080P004G000","8055261496101"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.","030","Copper PVD",2194,"GPF753080P000G000","8055261496125"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",708,"Copper Brushed PVD",2341,"GPF753080P006G000","8055261496095"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",735,"Warm Bronze PVD",2194,"GPF753080P037G000","8055261496040"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",726,"Warm Bronze Brushed PVD",2341,"GPF753080P024G000","8055261496064"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",720,"Nickel PVD",2194,"GPF753080P014G000","8055261496071"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",761,"Coffee Bronze Brushed PVD",2490,"GPF753080E059G000","8055261570924"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",710,"Brass PVD",2194,"GPF753080P011G000","8055261496088"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",727,"Brass Brushed PVD",2341,"GPF753080P025G000","8055261496057"]
["BATHROOM","INCASTRI","INCASTRI","43107+75308",75308,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, quatre sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 4 separate exits. Vertical/Horizontal installation.",845,"Dark Bronze",2341,"GPF753080V221G000","8055261496033"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320","43109","Inbouwdeel Thermostatische mengkraan hoog debiet 5 onafhankelijke uitgangen","Partie encastrée mitigeur THERMOSTATIQUE douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","Built-in thermostatic high-capacity mixer with FIVE SEPARATE EXITS. Vertical/Horizontal installation.","031","Chrome",1547,"GPF431093G001G000","8022692583427"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.","031","Chrome",1634,"GPF753200G001G000","8055261495494"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",149,"Finox Brushed Nickel",2206,"GPF753200G002G000","8055261495487"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",299,"Matte Black",2206,"GPF753200C072G000","8055261495500"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",706,"Black Metal PVD",2419,"GPF753200P001G000","8055261495463"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",707,"Black Metal Brushed PVD",2583,"GPF753200P004G000","8055261495456"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.","030","Copper PVD",2419,"GPF753200P000G000","8055261495470"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",708,"Copper Brushed PVD",2583,"GPF753200P006G000","8055261495449"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",735,"Warm Bronze PVD",2419,"GPF753200P037G000","8055261495395"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",726,"Warm Bronze Brushed PVD",2583,"GPF753200P024G000","8055261495418"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",720,"Nickel PVD",2419,"GPF753200P014G000","8055261495425"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",761,"Coffee Bronze Brushed PVD",2745,"GPF753200E059G000","8055261570825"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",710,"Brass PVD",2419,"GPF753200P011G000","8055261495432"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",727,"Brass Brushed PVD",2583,"GPF753200P025G000","8055261495401"]
["BATHROOM","INCASTRI","INCASTRI","43109+75320",75320,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",845,"Dark Bronze",2583,"GPF753200V221G000","8055261495388"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310","43109","Inbouwdeel Thermostatische mengkraan hoog debiet 5 onafhankelijke uitgangen","Partie encastrée mitigeur THERMOSTATIQUE douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","Built-in thermostatic high-capacity mixer with FIVE SEPARATE EXITS. Vertical/Horizontal installation.","031","Chrome",1547,"GPF431093G001G000","8022692583427"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.","031","Chrome",1634,"GPF753100G001G000","8055261496019"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",149,"Finox Brushed Nickel",2206,"GPF753100G002G000","8055261496002"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",299,"Matte Black",2206,"GPF753100C072G000","8055261496026"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",706,"Black Metal PVD",2419,"GPF753100P001G000","8055261495982"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",707,"Black Metal Brushed PVD",2583,"GPF753100P004G000","8055261495975"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.","030","Copper PVD",2419,"GPF753100P000G000","8055261495999"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",708,"Copper Brushed PVD",2583,"GPF753100P006G000","8055261495968"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",735,"Warm Bronze PVD",2419,"GPF753100P037G000","8055261495913"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",726,"Warm Bronze Brushed PVD",2583,"GPF753100P024G000","8055261495937"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",720,"Nickel PVD",2419,"GPF753100P014G000","8055261495944"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",761,"Coffee Bronze Brushed PVD",2745,"GPF753100E059G000","8055261570900"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",710,"Brass PVD",2419,"GPF753100P011G000","8055261495951"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",727,"Brass Brushed PVD",2583,"GPF753100P025G000","8055261495920"]
["BATHROOM","INCASTRI","INCASTRI","43109+75310",75310,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur thermostatique douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","External part wall-mounted thermostatic high-capacity mixer, 5 separate exits. Vertical/Horizontal installation.",845,"Dark Bronze",2583,"GPF753100V221G000","8055261495906"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354","43281","Inbouwdeel Thermostatische mengkraan hoog debiet","Partie encastrée pour mitigeur THERMOSTATIQUE douche haut débit","Built-in thermostatic high-capacity mixer","031","Chrome",581,"GPF432812G001G000","8022692585445"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.","031","Chrome",550,"GPF753540G001G000","8055261494848"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",149,"Finox Brushed Nickel",742,"GPF753540G002G000","8055261494831"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",299,"Matte Black",742,"GPF753540C072G000","8055261494855"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",706,"Black Metal PVD",812,"GPF753540P001G000","8055261494817"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",707,"Black Metal Brushed PVD",868,"GPF753540P004G000","8055261494800"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.","030","Copper PVD",812,"GPF753540P000G000","8055261494824"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",708,"Copper Brushed PVD",868,"GPF753540P006G000","8055261494794"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",735,"Warm Bronze PVD",812,"GPF753540P037G000","8055261494749"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",726,"Warm Bronze Brushed PVD",868,"GPF753540P024G000","8055261494763"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",720,"Nickel PVD",812,"GPF753540P014G000","8055261494770"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",761,"Coffee Bronze Brushed PVD",924,"GPF753540E059G000","8055261570726"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",710,"Brass PVD",812,"GPF753540P011G000","8055261494787"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",727,"Brass Brushed PVD",868,"GPF753540P025G000","8055261494756"]
["BATHROOM","INCASTRI","INCASTRI","43281+75354",75354,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente pour mitigeur thermostatique douche haut débit","External part wall-mounted thermostatic high-capacity mixer.",845,"Dark Bronze",868,"GPF753540V221G000","8055261494732"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364","43283","Inbouwdeel Voor Stop Kraan Voor Thermostatische Hoog-Debiet Mengkraan","Partie encastrée robinet d’arrêt pour mitigeur douche haut débit","Built-in part for stop valve for thermostatic high-capacity mixer","031","Chrome",393,"GPF432833G001G000","8022692585469"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.","031","Chrome",330,"GPF753640G001G000","8055261494718"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",149,"Finox Brushed Nickel",446,"GPF753640G002G000","8055261494701"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",299,"Matte Black",446,"GPF753640C072G000","8055261494725"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",706,"Black Metal PVD",488,"GPF753640P001G000","8055261494688"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",707,"Black Metal Brushed PVD",522,"GPF753640P004G000","8055261494671"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.","030","Copper PVD",488,"GPF753640P000G000","8055261494695"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",708,"Copper Brushed PVD",522,"GPF753640P006G000","8055261494664"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",735,"Warm Bronze PVD",488,"GPF753640P037G000","8055261494619"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",726,"Warm Bronze Brushed PVD",522,"GPF753640P024G000","8055261494633"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",720,"Nickel PVD",488,"GPF753640P014G000","8055261494640"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",761,"Coffee Bronze Brushed PVD",555,"GPF753640E059G000","8055261570702"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",710,"Brass PVD",488,"GPF753640P011G000","8055261494657"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",727,"Brass Brushed PVD",522,"GPF753640P025G000","8055261494626"]
["BATHROOM","INCASTRI","INCASTRI","43283+75364",75364,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit","External part for stop valve for thermostatic high-capacity mixer.",845,"Dark Bronze",522,"GPF753640V221G000","8055261494602"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.","031","Chrome",1281,"GPF751480G001G000","8055261442030"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",149,"Finox Brushed Nickel",1729,"GPF751480G002G000","8055261442023"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",299,"Matte Black",1729,"GPF751480C072G000","8055261442047"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",706,"Black Metal PVD",1896,"GPF751480P001G000","8055261442009"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",707,"Black Metal Brushed PVD",2023,"GPF751480P004G000","8055261441996"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.","030","Copper PVD",1896,"GPF751480P000G000","8055261442016"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",708,"Copper Brushed PVD",2023,"GPF751480P006G000","8055261441989"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",735,"Warm Bronze PVD",1896,"GPF751480P037G000","8055261441934"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",726,"Warm Bronze Brushed PVD",2023,"GPF751480P024G000","8055261441958"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",720,"Nickel PVD",1896,"GPF751480P014G000","8055261441965"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",761,"Coffee Bronze Brushed PVD",2152,"GPF751480E059G000","8055261571181"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",710,"Brass PVD",1896,"GPF751480P011G000","8055261441972"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",727,"Brass Brushed PVD",2023,"GPF751480P025G000","8055261441941"]
["BATHROOM","INCASTRI","INCASTRI",75148,75148,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted headshower.",845,"Dark Bronze",2023,"GPF751480V221G000","8055261441927"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","031","Chrome",1159,"GPF630450G001G000","8055261729698"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",149,"Finox Brushed Nickel",1565,"GPF630450G002G000","8055261729681"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",299,"Matte Black",1565,"GPF630450C072G000","8055261729728"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",706,"Black Metal PVD",1715,"GPF630450P001G000","8055261729650"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",707,"Black Metal Brushed PVD",1831,"GPF630450P004G000","8055261729643"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","030","Copper PVD",1715,"GPF630450P000G000","8055261729667"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",708,"Copper Brushed PVD",1831,"GPF630450P006G000","8055261729636"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",735,"Warm Bronze PVD",1715,"GPF630450P037G000","8055261729582"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",726,"Warm Bronze Brushed PVD",1831,"GPF630450P024G000","8055261729605"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",720,"Nickel PVD",1715,"GPF630450P014G000","8055261729612"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",761,"Coffee Bronze Brushed PVD",1947,"GPF630450E059G000","8055261729704"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",710,"Brass PVD",1715,"GPF630450P011G000","8055261729629"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",727,"Brass Brushed PVD",1831,"GPF630450P025G000","8055261729599"]
["BATHROOM","INCASTRI","INCASTRI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",845,"Dark Bronze",1831,"GPF630450V221G000","8055261729568"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO","031","Chrome",1584,"GPF637450G001G000","8055261728677"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",149,"Finox Brushed Nickel",2140,"GPF637450G002G000","8055261728660"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",299,"Matte Black",2140,"GPF637450C072G000","8055261728707"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",706,"Black Metal PVD",2345,"GPF637450P001G000","8055261728639"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",707,"Black Metal Brushed PVD",2503,"GPF637450P004G000","8055261728622"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO","030","Copper PVD",2345,"GPF637450P000G000","8055261728646"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",708,"Copper Brushed PVD",2503,"GPF637450P006G000","8055261728615"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",735,"Warm Bronze PVD",2345,"GPF637450P037G000","8055261728561"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",726,"Warm Bronze Brushed PVD",2503,"GPF637450P024G000","8055261728585"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",720,"Nickel PVD",2345,"GPF637450P014G000","8055261728592"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",761,"Coffee Bronze Brushed PVD",2662,"GPF637450E059G000","8055261728684"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",710,"Brass PVD",2345,"GPF637450P011G000","8055261728608"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",727,"Brass Brushed PVD",2503,"GPF637450P025G000","8055261728578"]
["BATHROOM","INCASTRI","INCASTRI",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",845,"Dark Bronze",2503,"GPF637450V221G000","8055261728547"]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","031","Chrome",1488]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",149,"Finox Brushed Nickel",2009,"GPF630490G002G000","8055261497368"]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",299,"Matte Black",2009]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",706,"Black Metal PVD",2202]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",707,"Black Metal Brushed PVD",2352]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","030","Copper PVD",2202]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",708,"Copper Brushed PVD",2352]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",735,"Warm Bronze PVD",2202]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",726,"Warm Bronze Brushed PVD",2352]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",720,"Nickel PVD",2202]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",761,"Coffee Bronze Brushed PVD",2500,"GPF630490E059G000","8055261577336"]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",710,"Brass PVD",2202]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",727,"Brass Brushed PVD",2352]
["BATHROOM","INCASTRI","INCASTRI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",845,"Dark Bronze",2352]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","031","Chrome",2012,"GPF751490G001G000","8055261441903"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",149,"Finox Brushed Nickel",2717,"GPF751490G002G000","8055261441897"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",299,"Matte Black",2717,"GPF751490C072G000","8055261441910"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",706,"Black Metal PVD",2978,"GPF751490P001G000","8055261441873"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",707,"Black Metal Brushed PVD",3179,"GPF751490P004G000","8055261441866"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","030","Copper PVD",2978,"GPF751490P000G000","8055261441880"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",708,"Copper Brushed PVD",3179,"GPF751490P006G000","8055261441859"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",735,"Warm Bronze PVD",2978,"GPF751490P037G000","8055261441804"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",726,"Warm Bronze Brushed PVD",3179,"GPF751490P024G000","8055261441828"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",720,"Nickel PVD",2978,"GPF751490P014G000","8055261441835"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",761,"Coffee Bronze Brushed PVD",3381,"GPF751490E059G000","8055261571167"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",710,"Brass PVD",2978,"GPF751490P011G000","8055261441842"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",727,"Brass Brushed PVD",3179,"GPF751490P025G000","8055261441811"]
["BATHROOM","INCASTRI","INCASTRI",75149,75149,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",845,"Dark Bronze",3179,"GPF751490V221G000","8055261441798"]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","031","Chrome",1610]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",149,"Finox Brushed Nickel",2173]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",299,"Matte Black",2173]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",706,"Black Metal PVD",2383]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",707,"Black Metal Brushed PVD",2543]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","030","Copper PVD",2383]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",708,"Copper Brushed PVD",2543]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",735,"Warm Bronze PVD",2383]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",726,"Warm Bronze Brushed PVD",2543]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",720,"Nickel PVD",2383]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",761,"Coffee Bronze Brushed PVD",2705,"GPF630680E059G000","8055261577312"]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",710,"Brass PVD",2383]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",727,"Brass Brushed PVD",2543]
["BATHROOM","INCASTRI","INCASTRI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",845,"Dark Bronze",2543]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","031","Chrome",2134,"GPF751680G001G000","8055261441385"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",149,"Finox Brushed Nickel",2882,"GPF751680G002G000","8055261441378"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",299,"Matte Black",2882,"GPF751680C072G000","8055261441392"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",706,"Black Metal PVD",3158,"GPF751680P001G000","8055261441354"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",707,"Black Metal Brushed PVD",3371,"GPF751680P004G000","8055261441347"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","030","Copper PVD",3158,"GPF751680P000G000","8055261441361"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",708,"Copper Brushed PVD",3371,"GPF751680P006G000","8055261441330"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",735,"Warm Bronze PVD",3158,"GPF751680P037G000","8055261441286"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",726,"Warm Bronze Brushed PVD",3371,"GPF751680P024G000","8055261441309"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",720,"Nickel PVD",3158,"GPF751680P014G000","8055261441316"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",761,"Coffee Bronze Brushed PVD",3585,"GPF751680E059G000","8055261571143"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",710,"Brass PVD",3158,"GPF751680P011G000","8055261441323"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",727,"Brass Brushed PVD",3371,"GPF751680P025G000","8055261441293"]
["BATHROOM","INCASTRI","INCASTRI",75168,75168,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",845,"Dark Bronze",3371,"GPF751680V221G000","8055261441279"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.","031","Chrome",1092,"GPF630500G001G000","8055261729520"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",149,"Finox Brushed Nickel",1475,"GPF630500G002G000","8055261729513"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",299,"Matte Black",1475,"GPF630500C072G000","8055261729551"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",706,"Black Metal PVD",1616,"GPF630500P001G000","8055261729483"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",707,"Black Metal Brushed PVD",1726,"GPF630500P004G000","8055261729476"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.","030","Copper PVD",1616,"GPF630500P000G000","8055261729490"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",708,"Copper Brushed PVD",1726,"GPF630500P006G000","8055261729469"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",735,"Warm Bronze PVD",1616,"GPF630500P037G000","8055261729414"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",726,"Warm Bronze Brushed PVD",1726,"GPF630500P024G000","8055261729438"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",720,"Nickel PVD",1616,"GPF630500P014G000","8055261729445"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",761,"Coffee Bronze Brushed PVD",1834,"GPF630500E059G000","8055261729537"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",710,"Brass PVD",1616,"GPF630500P011G000","8055261729452"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",727,"Brass Brushed PVD",1726,"GPF630500P025G000","8055261729421"]
["BATHROOM","INCASTRI","INCASTRI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",845,"Dark Bronze",1726,"GPF630500V221G000","8055261729391"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO","031","Chrome",1580,"GPF637500G001G000","8055261728509"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",149,"Finox Brushed Nickel",2133,"GPF637500G002G000","8055261728493"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",299,"Matte Black",2133,"GPF637500C072G000","8055261728530"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",706,"Black Metal PVD",2338,"GPF637500P001G000","8055261728462"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",707,"Black Metal Brushed PVD",2497,"GPF637500P004G000","8055261728455"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO","030","Copper PVD",2338,"GPF637500P000G000","8055261728479"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",708,"Copper Brushed PVD",2497,"GPF637500P006G000","8055261728448"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",735,"Warm Bronze PVD",2338,"GPF637500P037G000","8055261728394"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",726,"Warm Bronze Brushed PVD",2497,"GPF637500P024G000","8055261728417"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",720,"Nickel PVD",2338,"GPF637500P014G000","8055261728424"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",761,"Coffee Bronze Brushed PVD",2654,"GPF637500E059G000","8055261728516"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",710,"Brass PVD",2338,"GPF637500P011G000","8055261728431"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",727,"Brass Brushed PVD",2497,"GPF637500P025G000","8055261728400"]
["BATHROOM","INCASTRI","INCASTRI",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",845,"Dark Bronze",2497,"GPF637500V221G000","8055261728370"]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.","031","Chrome",1488]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",149,"Finox Brushed Nickel",2009]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",299,"Matte Black",2009]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",706,"Black Metal PVD",2202]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",707,"Black Metal Brushed PVD",2352]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.","030","Copper PVD",2202]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",708,"Copper Brushed PVD",2352]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",735,"Warm Bronze PVD",2202]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",726,"Warm Bronze Brushed PVD",2352]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",720,"Nickel PVD",2202]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",761,"Coffee Bronze Brushed PVD",2500,"GPF630720E059G000","8055261577275"]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",710,"Brass PVD",2202]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",727,"Brass Brushed PVD",2352]
["BATHROOM","INCASTRI","INCASTRI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",845,"Dark Bronze",2352]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.","031","Chrome",2012,"GPF751720G001G000","8055261440999"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",149,"Finox Brushed Nickel",2717,"GPF751720G002G000","8055261440982"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",299,"Matte Black",2717,"GPF751720C072G000","8055261441002"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",706,"Black Metal PVD",2978,"GPF751720P001G000","8055261440968"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",707,"Black Metal Brushed PVD",3179,"GPF751720P004G000","8055261440951"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.","030","Copper PVD",2978,"GPF751720P000G000","8055261440975"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",708,"Copper Brushed PVD",3179,"GPF751720P006G000","8055261440944"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",735,"Warm Bronze PVD",2978,"GPF751720P037G000","8055261440890"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",726,"Warm Bronze Brushed PVD",3179,"GPF751720P024G000","8055261440913"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",720,"Nickel PVD",2978,"GPF751720P014G000","8055261440920"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",761,"Coffee Bronze Brushed PVD",3381,"GPF751720E059G000","8055261571105"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",710,"Brass PVD",2978,"GPF751720P011G000","8055261440937"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",727,"Brass Brushed PVD",3179,"GPF751720P025G000","8055261440906"]
["BATHROOM","INCASTRI","INCASTRI",75172,75172,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",845,"Dark Bronze",3179,"GPF751720V221G000","8055261440883"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.","031","Chrome",1420,"GPF630530G001G000","8055261729353"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",149,"Finox Brushed Nickel",1917,"GPF630530G002G000","8055261729346"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",299,"Matte Black",1917,"GPF630530C072G000","8055261729384"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",706,"Black Metal PVD",2101,"GPF630530P001G000","8055261729315"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",707,"Black Metal Brushed PVD",2243,"GPF630530P004G000","8055261729308"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.","030","Copper PVD",2101,"GPF630530P000G000","8055261729322"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",708,"Copper Brushed PVD",2243,"GPF630530P006G000","8055261729292"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",735,"Warm Bronze PVD",2101,"GPF630530P037G000","8055261729247"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",726,"Warm Bronze Brushed PVD",2243,"GPF630530P024G000","8055261729261"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",720,"Nickel PVD",2101,"GPF630530P014G000","8055261729278"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",761,"Coffee Bronze Brushed PVD",2385,"GPF630530E059G000","8055261729360"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",710,"Brass PVD",2101,"GPF630530P011G000","8055261729285"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",727,"Brass Brushed PVD",2243,"GPF630530P025G000","8055261729254"]
["BATHROOM","INCASTRI","INCASTRI",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",845,"Dark Bronze",2243,"GPF630530V221G000","8055261729223"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO","031","Chrome",2054,"GPF637530G001G000","8055261728332"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",149,"Finox Brushed Nickel",2773,"GPF637530G002G000","8055261728325"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",299,"Matte Black",2773,"GPF637530C072G000","8055261728363"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",706,"Black Metal PVD",3040,"GPF637530P001G000","8055261728295"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",707,"Black Metal Brushed PVD",3245,"GPF637530P004G000","8055261728288"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO","030","Copper PVD",3040,"GPF637530P000G000","8055261728301"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",708,"Copper Brushed PVD",3245,"GPF637530P006G000","8055261728271"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",735,"Warm Bronze PVD",3040,"GPF637530P037G000","8055261728226"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",726,"Warm Bronze Brushed PVD",3245,"GPF637530P024G000","8055261728240"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",720,"Nickel PVD",3040,"GPF637530P014G000","8055261728257"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",761,"Coffee Bronze Brushed PVD",3451,"GPF637530E059G000","8055261728349"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",710,"Brass PVD",3040,"GPF637530P011G000","8055261728264"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",727,"Brass Brushed PVD",3245,"GPF637530P025G000","8055261728233"]
["BATHROOM","INCASTRI","INCASTRI",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",845,"Dark Bronze",3245,"GPF637530V221G000","8055261728202"]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.","031","Chrome",2092]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",149,"Finox Brushed Nickel",2824]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",299,"Matte Black",2824]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",706,"Black Metal PVD",3096]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",707,"Black Metal Brushed PVD",3305]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.","030","Copper PVD",3096]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",708,"Copper Brushed PVD",3305]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",735,"Warm Bronze PVD",3096]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",726,"Warm Bronze Brushed PVD",3305]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",720,"Nickel PVD",3096]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",761,"Coffee Bronze Brushed PVD",3514,"GPF630700E059G000","8055261577299"]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",710,"Brass PVD",3096]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",727,"Brass Brushed PVD",3305]
["BATHROOM","INCASTRI","INCASTRI",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",845,"Dark Bronze",3305]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.","031","Chrome",2616,"GPF751700G001G000","8055261441125"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",149,"Finox Brushed Nickel",3531,"GPF751700G002G000","8055261441118"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",299,"Matte Black",3531,"GPF751700C072G000","8055261441132"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",706,"Black Metal PVD",3872,"GPF751700P001G000","8055261441095"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",707,"Black Metal Brushed PVD",4133,"GPF751700P004G000","8055261441088"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.","030","Copper PVD",3872,"GPF751700P000G000","8055261441101"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",708,"Copper Brushed PVD",4133,"GPF751700P006G000","8055261441071"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",735,"Warm Bronze PVD",3872,"GPF751700P037G000","8055261441026"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",726,"Warm Bronze Brushed PVD",4133,"GPF751700P024G000","8055261441040"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",720,"Nickel PVD",3872,"GPF751700P014G000","8055261441057"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",761,"Coffee Bronze Brushed PVD",4394,"GPF751700E059G000","8055261571129"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",710,"Brass PVD",3872,"GPF751700P011G000","8055261441064"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",727,"Brass Brushed PVD",4133,"GPF751700P025G000","8055261441033"]
["BATHROOM","INCASTRI","INCASTRI",75170,75170,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",845,"Dark Bronze",4133,"GPF751700V221G000","8055261441019"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.","031","Chrome",921,"GPF750400G001G000","8055261445413"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",149,"Finox Brushed Nickel",1242,"GPF750400G002G000","8055261445406"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",299,"Matte Black",1242,"GPF750400C072G000","8055261445420"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",706,"Black Metal PVD",1362,"GPF750400P001G000","8055261445383"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",707,"Black Metal Brushed PVD",1454,"GPF750400P004G000","8055261445376"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.","030","Copper PVD",1362,"GPF750400P000G000","8055261445390"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",708,"Copper Brushed PVD",1454,"GPF750400P006G000","8055261445369"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",735,"Warm Bronze PVD",1362,"GPF750400P037G000","8055261445314"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",726,"Warm Bronze Brushed PVD",1454,"GPF750400P024G000","8055261445338"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",720,"Nickel PVD",1362,"GPF750400P014G000","8055261445345"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",761,"Coffee Bronze Brushed PVD",1547,"GPF750400E059G000","8055261571563"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",710,"Brass PVD",1362,"GPF750400P011G000","8055261445352"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",727,"Brass Brushed PVD",1454,"GPF750400P025G000","8055261445321"]
["BATHROOM","INCASTRI","INCASTRI",75040,75040,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",845,"Dark Bronze",1454,"GPF750400V221G000","8055261445307"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.","031","Chrome",738,"GPF750420G001G000","8055261445284"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",149,"Finox Brushed Nickel",997,"GPF750420G002G000","8055261445277"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",299,"Matte Black",997,"GPF750420C072G000","8055261445291"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",706,"Black Metal PVD",1093,"GPF750420P001G000","8055261445253"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",707,"Black Metal Brushed PVD",1166,"GPF750420P004G000","8055261445246"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.","030","Copper PVD",1093,"GPF750420P000G000","8055261445260"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",708,"Copper Brushed PVD",1166,"GPF750420P006G000","8055261445239"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",735,"Warm Bronze PVD",1093,"GPF750420P037G000","8055261445185"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",726,"Warm Bronze Brushed PVD",1166,"GPF750420P024G000","8055261445208"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",720,"Nickel PVD",1093,"GPF750420P014G000","8055261445215"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",761,"Coffee Bronze Brushed PVD",1241,"GPF750420E059G000","8055261571549"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",710,"Brass PVD",1093,"GPF750420P011G000","8055261445222"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",727,"Brass Brushed PVD",1166,"GPF750420P025G000","8055261445192"]
["BATHROOM","INCASTRI","INCASTRI",75042,75042,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche avec flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet and 1,50 m flexible hose.",845,"Dark Bronze",1166,"GPF750420V221G000","8055261445178"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.","031","Chrome",604,"GPF750440G001G000","8055261445154"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",149,"Finox Brushed Nickel",815,"GPF750440G002G000","8055261445147"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",299,"Matte Black",815,"GPF750440C072G000","8055261445161"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",706,"Black Metal PVD",893,"GPF750440P001G000","8055261445123"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",707,"Black Metal Brushed PVD",953,"GPF750440P004G000","8055261445116"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.","030","Copper PVD",893,"GPF750440P000G000","8055261445130"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",708,"Copper Brushed PVD",953,"GPF750440P006G000","8055261445109"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",735,"Warm Bronze PVD",893,"GPF750440P037G000","8055261445055"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",726,"Warm Bronze Brushed PVD",953,"GPF750440P024G000","8055261445079"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",720,"Nickel PVD",893,"GPF750440P014G000","8055261445086"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",761,"Coffee Bronze Brushed PVD",1014,"GPF750440E059G000","8055261571525"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",710,"Brass PVD",893,"GPF750440P011G000","8055261445093"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",727,"Brass Brushed PVD",953,"GPF750440P025G000","8055261445062"]
["BATHROOM","INCASTRI","INCASTRI",75044,75044,"Glijstang","Barre de douche.","Sliding rail.",845,"Dark Bronze",953,"GPF750440V221G000","8055261445048"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.","031","Chrome",445,"GPF735230G001G000","8055261029217"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",149,"Finox Brushed Nickel",600,"GPF735230G002G000","8055261029200"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",299,"Matte Black",600,"GPF735230C072G000","8055261029224"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",706,"Black Metal PVD",658,"GPF735230P001G000","8055261029170"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",707,"Black Metal Brushed PVD",702,"GPF735230P004G000","8055261029163"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.","030","Copper PVD",658,"GPF735230P000G000","8055261029187"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",708,"Copper Brushed PVD",702,"GPF735230P006G000","8055261029156"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",735,"Warm Bronze PVD",658,"GPF735230P037G000","8055261029101"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",720,"Nickel PVD",686,"GPF735230P014G000","8055261029132"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",761,"Coffee Bronze Brushed PVD",747,"GPF735230E059G000","8055261577152"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",710,"Brass PVD",658,"GPF735230P011G000","8055261029149"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",727,"Brass Brushed PVD",702,"GPF735230P025G000","8055261029118"]
["BATHROOM","INCASTRI","INCASTRI",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",845,"Dark Bronze",732,"GPF735230V221G000","8055261029088"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower","031","Chrome",634,"GPF630990G001G000","8056329216082"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",149,"Finox Brushed Nickel",857,"GPF630990G002G000","8056329216068"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",299,"Matte Black",857,"GPF630990C072G000","8056329216105"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",706,"Black Metal PVD",940,"GPF630990P001G000","8056329216006"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",707,"Black Metal Brushed PVD",1003,"GPF630990P004G000","8056329215986"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower","030","Copper PVD",940,"GPF630990P000G000","8056329216020"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",708,"Copper Brushed PVD",1003,"GPF630990P006G000","8056329215962"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",735,"Warm Bronze PVD",940,"GPF630990P037G000","8056329558199"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",720,"Nickel PVD",940,"GPF630990P014G000","8056603463607"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",761,"Coffee Bronze Brushed PVD",1066,"GPF630990E059G000","8055261577251"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",710,"Brass PVD",940,"GPF630990P011G000","8056329592346"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",727,"Brass Brushed PVD",1003,"GPF630990P025G000","8056329215924"]
["BATHROOM","INCASTRI","INCASTRI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",845,"Dark Bronze",1003,"GPF630990V221G000","8056603633604"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet","031","Chrome",650,"GPF329751G001G000","8022692361360"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",149,"Finox Brushed Nickel",878,"GPF329751G002G000","8022692361384"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",299,"Matte Black",878,"GPF329751C072G000","8022692519228"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",706,"Black Metal PVD",962,"GPF329751P001G000","8022692642438"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",707,"Black Metal Brushed PVD",1029,"GPF329751P004G000","8022692832808"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet","030","Copper PVD",962,"GPF329751P000G000","8022692673715"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",708,"Copper Brushed PVD",1029,"GPF329751P006G000","8022692832815"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",735,"Warm Bronze PVD",962,"GPF329751P037G000","8056329609969"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",720,"Nickel PVD",962,"GPF329751P014G000","8056603607841"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",761,"Coffee Bronze Brushed PVD",1092,"GPF329751E059G000","8055261577596"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",710,"Brass PVD",962,"GPF329751P011G000","8056329609976"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",727,"Brass Brushed PVD",1029,"GPF329751P025G000","8056329529694"]
["BATHROOM","INCASTRI","INCASTRI",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",845,"Dark Bronze",1029,"GPF329751V221G000","8055261157569"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet","031","Chrome",299,"GPF329730G001G000","8022692066043"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",149,"Finox Brushed Nickel",404,"GPF329730G002G000","8022692794427"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",299,"Matte Black",404,"GPF329730C072G000","8022692361094"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",706,"Black Metal PVD",443,"GPF329730P001G000","8022692642193"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",707,"Black Metal Brushed PVD",474,"GPF329730P004G000","8022692361322"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet","030","Copper PVD",443,"GPF329730P000G000","8022692673685"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",708,"Copper Brushed PVD",474,"GPF329730P006G000","8022692361339"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",735,"Warm Bronze PVD",443,"GPF329730P037G000","8056329609983"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",720,"Nickel PVD",443,"GPF329730P014G000","8056603607858"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",761,"Coffee Bronze Brushed PVD",503,"GPF329730E059G000","8055261577619"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",710,"Brass PVD",443,"GPF329730P011G000","8056329609990"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",727,"Brass Brushed PVD",474,"GPF329730P025G000","8056329099401"]
["BATHROOM","INCASTRI","INCASTRI",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",845,"Dark Bronze",474,"GPF329730V221G000","8055261479074"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32987,"Inbouwdeel Laterale oriënteerbare hoofddouchekop","Partie encastrée pour douchette laterale orientable","Built-in part lateral and adjustable body jet","031","Chrome",202,"GPF329870G001G000","8022692519365"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet","031","Chrome",397,"GPF329840G001G000","8022692519334"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",149,"Finox Brushed Nickel",607,"GPF329840G002G000","8022692797480"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",299,"Matte Black",607,"GPF329840C072G000","8022692362046"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",706,"Black Metal PVD",685,"GPF329840P001G000","8022692673821"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",707,"Black Metal Brushed PVD",745,"GPF329840P004G000","8022692362343"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet","030","Copper PVD",685,"GPF329840P000G000","8022692832280"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",708,"Copper Brushed PVD",745,"GPF329840P006G000","8022692362350"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",735,"Warm Bronze PVD",685,"GPF329840P037G000","8056329609907"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",720,"Nickel PVD",685,"GPF329840P014G000","8056603607827"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",761,"Coffee Bronze Brushed PVD",804,"GPF329840E059G000","8055261577558"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",710,"Brass PVD",685,"GPF329840P011G000","8056329609914"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",727,"Brass Brushed PVD",745,"GPF329840P025G000","8056329529595"]
["BATHROOM","INCASTRI","INCASTRI","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",845,"Dark Bronze",745,"GPF329840V221G000","8055261058347"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer","031","Chrome",260,"GPF329791G001G000","8022692361872"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",149,"Finox Brushed Nickel",351,"GPF329791G002G000","8022692800623"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",299,"Matte Black",351,"GPF329791C072G000","8022692833201"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",706,"Black Metal PVD",381,"GPF329791P001G000","8022692673777"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",707,"Black Metal Brushed PVD",411,"GPF329791P004G000","8022692833188"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer","030","Copper PVD",381,"GPF329791P000G000","8056329529670"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",708,"Copper Brushed PVD",411,"GPF329791P006G000","8022692833195"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",735,"Warm Bronze PVD",381,"GPF329791P037G000","8056329609938"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",720,"Nickel PVD",381,"GPF329791P014G000","8056603607834"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",761,"Coffee Bronze Brushed PVD",437,"GPF329791E059G000","8055261577572"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",710,"Brass PVD",381,"GPF329791P011G000","8056329609945"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",727,"Brass Brushed PVD",411,"GPF329791P025G000","8056329529649"]
["BATHROOM","INCASTRI","INCASTRI",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",845,"Dark Bronze",411,"GPF329791V221G000","8055261479067"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet","031","Chrome",246,"GPF201720G001G000","8022692021431"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",149,"Finox Brushed Nickel",331,"GPF201720G002G000","8022692797626"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",299,"Matte Black",331,"GPF201720C072G000","8022692055245"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",706,"Black Metal PVD",362,"GPF201720P001G000","8022692223668"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",707,"Black Metal Brushed PVD",388,"GPF201720P004G000","8022692223781"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet","030","Copper PVD",362,"GPF201720P000G000","8022692223651"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",708,"Copper Brushed PVD",388,"GPF201720P006G000","8022692223798"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",735,"Warm Bronze PVD",362,"GPF201720P037G000","8056329613096"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",720,"Nickel PVD",362,"GPF201720P014G000","8022692223927"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",761,"Coffee Bronze Brushed PVD",414,"GPF201720E059G000","8055261577879"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",710,"Brass PVD",362,"GPF201720P011G000","8056329613102"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",727,"Brass Brushed PVD",388,"GPF201720P025G000","8056329529892"]
["BATHROOM","INCASTRI","INCASTRI",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",845,"Dark Bronze",388,"GPF201720V221G000","8055261479241"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",239,"Steel Brushed",1018,"GPF202950A000G000","8056329085749"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",238,"Mirror Steel",1018,"GPF202950A001G000","8056329085732"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",299,"Matte Black",1375,"GPF202950C072G000","8056329085725"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",706,"Black Metal PVD",1506,"GPF202950P001G000","8056329085695"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",707,"Black Metal Brushed PVD",1607,"GPF202950P004G000","8056329085756"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)","030","Copper PVD",1506,"GPF202950P000G000","8056329085701"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",708,"Copper Brushed PVD",1607,"GPF202950P006G000","8056329085671"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",735,"Warm Bronze PVD",1506,"GPF202950P037G000","8056329559073"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",720,"Nickel PVD",1506,"GPF202950P014G000","8056603457231"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",761,"Coffee Bronze Brushed PVD",1710,"GPF202950E059G000","8055261577855"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",710,"Brass PVD",1506,"GPF202950P011G000","8056329612891"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",727,"Brass Brushed PVD",1607,"GPF202950P025G000","8056329085657"]
["BATHROOM","INCASTRI","INCASTRI",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",845,"Dark Bronze",1607,"GPF202950V221G000","8056603634076"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.","031","Chrome",251,"GPF730610G001G000","8056603967839"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",149,"Finox Brushed Nickel",340,"GPF730610G002G000","8056603967822"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",299,"Matte Black",340,"GPF730610C072G000","8056603967846"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",706,"Black Metal PVD",371,"GPF730610P001G000","8056603967792"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",707,"Black Metal Brushed PVD",397,"GPF730610P004G000","8056603967785"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.","030","Copper PVD",371,"GPF730610P000G000","8056603967808"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",708,"Copper Brushed PVD",397,"GPF730610P006G000","8056603967778"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",735,"Warm Bronze PVD",371,"GPF730610P037G000","8056603967723"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",720,"Nickel PVD",387,"GPF730610P014G000","8056603967754"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",761,"Coffee Bronze Brushed PVD",421,"GPF730610E059G000","8055261577190"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",710,"Brass PVD",371,"GPF730610P011G000","8056603967761"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",727,"Brass Brushed PVD",397,"GPF730610P025G000","8056603967730"]
["BATHROOM","INCASTRI","INCASTRI",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",845,"Dark Bronze",414,"GPF730610V221G000","8056603967709"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.","031","Chrome",181,"GPF730690G001G000","8056603967686"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.",149,"Finox Brushed Nickel",243,"GPF730690G002G000","8056603967679"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.",299,"Matte Black",243,"GPF730690C072G000","8056603967693"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.",706,"Black Metal PVD",268,"GPF730690P001G000","8056603967648"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.",707,"Black Metal Brushed PVD",287,"GPF730690P004G000","8056603967631"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.","030","Copper PVD",268,"GPF730690P000G000","8056603967655"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.",708,"Copper Brushed PVD",287,"GPF730690P006G000","8056603967624"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.",735,"Warm Bronze PVD",268,"GPF730690P037G000","8056603967570"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.",720,"Nickel PVD",279,"GPF730690P014G000","8056603967600"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.",761,"Coffee Bronze Brushed PVD",304,"GPF730690E059G000","8055261577176"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.",710,"Brass PVD",268,"GPF730690P011G000","8056603967617"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.",727,"Brass Brushed PVD",287,"GPF730690P025G000","8056603967587"]
["BATHROOM","INCASTRI","INCASTRI",73069,73069,"water aansluitpunt.","Sortie coudée murale.","Water outlet.",845,"Dark Bronze",298,"GPF730690V221G000","8056603967556"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.","031","Chrome",145,"GPF730570G001G000","8056603968133"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",149,"Finox Brushed Nickel",196,"GPF730570G002G000","8056603968126"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",299,"Matte Black",196,"GPF730570C072G000","8056603968140"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",706,"Black Metal PVD",215,"GPF730570P001G000","8056603968096"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",707,"Black Metal Brushed PVD",227,"GPF730570P004G000","8056603968089"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.","030","Copper PVD",215,"GPF730570P000G000","8056603968102"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",708,"Copper Brushed PVD",227,"GPF730570P006G000","8056603968072"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",735,"Warm Bronze PVD",215,"GPF730570P037G000","8056603968027"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",720,"Nickel PVD",223,"GPF730570P014G000","8056603968058"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",761,"Coffee Bronze Brushed PVD",243,"GPF730570E059G000","8055261577237"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",710,"Brass PVD",215,"GPF730570P011G000","8056603968065"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",727,"Brass Brushed PVD",227,"GPF730570P025G000","8056603968034"]
["BATHROOM","INCASTRI","INCASTRI",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",845,"Dark Bronze",238,"GPF730570V221G000","8056603968003"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.","031","Chrome",313,"GPF730600G001G000","8056603967983"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.",149,"Finox Brushed Nickel",422,"GPF730600G002G000","8056603967976"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.",299,"Matte Black",422,"GPF730600C072G000","8056603967990"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.",706,"Black Metal PVD",462,"GPF730600P001G000","8056603967945"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.",707,"Black Metal Brushed PVD",493,"GPF730600P004G000","8056603967938"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.","030","Copper PVD",462,"GPF730600P000G000","8056603967952"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.",708,"Copper Brushed PVD",493,"GPF730600P006G000","8056603967921"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.",735,"Warm Bronze PVD",462,"GPF730600P037G000","8056603967877"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.",720,"Nickel PVD",482,"GPF730600P014G000","8056603967907"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.",761,"Coffee Bronze Brushed PVD",526,"GPF730600E059G000","8055261577213"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.",710,"Brass PVD",462,"GPF730600P011G000","8056603967914"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.",727,"Brass Brushed PVD",493,"GPF730600P025G000","8056603967884"]
["BATHROOM","INCASTRI","INCASTRI",73060,73060,"Verstelbare handdouche houder","Support orientable pour douchette.","Adjustable handshower hook.",845,"Dark Bronze",515,"GPF730600V221G000","8056603967853"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.","031","Chrome",278,"GPF329290G001G000","8055261227927"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",149,"Finox Brushed Nickel",376,"GPF329290G002G000","8055261227910"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",299,"Matte Black",376,"GPF329290C072G000","8055261227934"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",706,"Black Metal PVD",411,"GPF329290P001G000","8055261227880"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",707,"Black Metal Brushed PVD",438,"GPF329290P004G000","8055261227873"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.","030","Copper PVD",411,"GPF329290P000G000","8055261227897"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",708,"Copper Brushed PVD",438,"GPF329290P006G000","8055261227859"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",735,"Warm Bronze PVD",411,"GPF329290P037G000","8055261227798"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",720,"Nickel PVD",411,"GPF329290P014G000","8055261227828"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",761,"Coffee Bronze Brushed PVD",468,"GPF329290E059G000","8055261577657"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",710,"Brass PVD",411,"GPF329290P011G000","8055261227835"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",727,"Brass Brushed PVD",438,"GPF329290P025G000","8055261227804"]
["BATHROOM","INCASTRI","INCASTRI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",845,"Dark Bronze",438,"GPF329290V221G000","8055261479081"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.","031","Chrome",246,"GPF329300G001G000","8055261227767"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",149,"Finox Brushed Nickel",332,"GPF329300G002G000","8055261227750"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",299,"Matte Black",332,"GPF329300C072G000","8055261227774"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",706,"Black Metal PVD",364,"GPF329300P001G000","8055261227729"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",707,"Black Metal Brushed PVD",388,"GPF329300P004G000","8055261227712"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.","030","Copper PVD",364,"GPF329300P000G000","8055261227736"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",708,"Copper Brushed PVD",388,"GPF329300P006G000","8055261227699"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",735,"Warm Bronze PVD",364,"GPF329300P037G000","8055261227637"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",720,"Nickel PVD",364,"GPF329300P014G000","8055261227668"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",761,"Coffee Bronze Brushed PVD",414,"GPF329300E059G000","8055261577633"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",710,"Brass PVD",364,"GPF329300P011G000","8055261227675"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",727,"Brass Brushed PVD",388,"GPF329300P025G000","8055261227644"]
["BATHROOM","INCASTRI","INCASTRI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",845,"Dark Bronze",388,"GPF329300V221G000","8055261458079"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.","031","Chrome",69,"GPF143720G001G000","8022692017588"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",149,"Finox Brushed Nickel",116,"GPF143720G002G000","8022692787085"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",299,"Matte Black",114,"GPF143720C072G000","8022692435283"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",706,"Black Metal PVD",214,"GPF143720P001G000","8056329009271"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",707,"Black Metal Brushed PVD",235,"GPF143720P004G000","8056329037342"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.","030","Copper PVD",214,"GPF143720P000G000","8056329037366"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",708,"Copper Brushed PVD",235,"GPF143720P006G000","8056329037335"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",735,"Warm Bronze PVD",214,"GPF143720P037G000","8056329614444"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",720,"Nickel PVD",214,"GPF143720P014G000","8056603672054"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",761,"Coffee Bronze Brushed PVD",249,"GPF143720E059G000","8055261577893"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",710,"Brass PVD",214,"GPF143720P011G000","8056329614468"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",727,"Brass Brushed PVD",235,"GPF143720P025G000","8056329037311"]
["BATHROOM","INCASTRI","INCASTRI",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",845,"Dark Bronze",235,"GPF143720V221G000","8056603610254"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower","031","Chrome",97,"GPF143700G001G000","8022692028270"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",149,"Finox Brushed Nickel",193,"GPF143700G002G000","8022692788587"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",299,"Matte Black",193,"GPF143700C072G000","8022692435207"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",147,"Chome Brushed",193,"GPF143700G006G000","8022692842883"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",720,"Nickel PVD",223,"GPF143700P014G000","8056603631815"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",706,"Black Metal PVD",223,"GPF143700P001G000","8056329015135"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",707,"Black Metal Brushed PVD",239,"GPF143700P004G000","8056603463225"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower","030","Copper PVD",223,"GPF143700P000G000","8056603522588"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",708,"Copper Brushed PVD",239,"GPF143700P006G000","8056603145572"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",735,"Warm Bronze PVD",223,"GPF143700P037G000","8056603599139"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",726,"Warm Bronze Brushed PVD",239,"GPF143700P024G000","8056603445603"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",710,"Brass PVD",223,"GPF143700P011G000","8056603631822"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",727,"Brass Brushed PVD",239,"GPF143700P025G000","8056603469296"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",246,"Gold PVD",252,"GPF143700P007G000","8056603631839"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",716,"Gold Brushed PVD",252,"GPF143700P005G000","8055261231245"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",761,"Coffee Bronze Brushed PVD",252,"GPF143700E059G000","8055261609631"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",845,"Dark Bronze",239,"GPF143700V221G000","8056603631808"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",187,"Aged Bronze",239,"GPF143700G052G000","8056329707337"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",713,"Antique Brass",239,"GPF143700V204G000","8056329199644"]
["BATHROOM","INCASTRI","INCASTRI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",279,"Matte White",193,"GPF143700C071G000","8022692435191"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert","031","Chrome",206,"GPF143760G001G000","8022692028393"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",149,"Finox Brushed Nickel",278,"GPF143760G002G000","8022692788594"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",299,"Matte Black",278,"GPF143760C072G000","8022692435368"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",147,"Chome Brushed",278,"GPF143760G006G000","8022692153538"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",720,"Nickel PVD",325,"GPF143760P014G000","8056603631785"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",706,"Black Metal PVD",325,"GPF143760P001G000","8056603551748"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",707,"Black Metal Brushed PVD",346,"GPF143760P004G000","8056329700093"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert","030","Copper PVD",325,"GPF143760P000G000","8056603116497"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",708,"Copper Brushed PVD",346,"GPF143760P006G000","8056329701915"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",735,"Warm Bronze PVD",325,"GPF143760P037G000","8056603631778"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",726,"Warm Bronze Brushed PVD",346,"GPF143760P024G000","8056329652354"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",710,"Brass PVD",325,"GPF143760P011G000","8056603631792"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",727,"Brass Brushed PVD",346,"GPF143760P025G000","8056603111911"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",246,"Gold PVD",366,"GPF143760P007G000","8056603522571"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",716,"Gold Brushed PVD",366,"GPF143760P005G000","8055261231238"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",761,"Coffee Bronze Brushed PVD",367,"GPF143760E059G000","8055261609594"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",845,"Dark Bronze",346,"GPF143760V221G000","8056603631761"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",187,"Aged Bronze",346,"GPF143760G052G000","8056329070059"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",713,"Antique Brass",346,"GPF143760V204G000","8056329127364"]
["BATHROOM","INCASTRI","INCASTRI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",279,"Matte White",278,"GPF143760C071G000","8022692070149"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.","031","Chrome",206,"GPF143780G001G000","8056603633314"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",149,"Finox Brushed Nickel",278,"GPF143780G002G000","8056603633307"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",299,"Matte Black",278,"GPF143780C072G000","8056603633321"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",147,"Chome Brushed",278,"GPF143780G006G000","8056603633291"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",720,"Nickel PVD",325,"GPF143780P014G000","8056603633192"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",706,"Black Metal PVD",325,"GPF143780P001G000","8056603633246"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",707,"Black Metal Brushed PVD",346,"GPF143780P004G000","8056603633239"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.","030","Copper PVD",325,"GPF143780P000G000","8056603633253"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",708,"Copper Brushed PVD",346,"GPF143780P006G000","8056603633222"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",735,"Warm Bronze PVD",325,"GPF143780P037G000","8056603633161"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",726,"Warm Bronze Brushed PVD",346,"GPF143780P024G000","8056603633185"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",710,"Brass PVD",325,"GPF143780P011G000","8056603633208"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",727,"Brass Brushed PVD",346,"GPF143780P025G000","8056603633178"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",246,"Gold PVD",366,"GPF143780P007G000","8056603633215"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",716,"Gold Brushed PVD",366,"GPF143780P005G000","8055261231221"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",761,"Coffee Bronze Brushed PVD",367,"GPF143780E059G000","8055261609570"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",845,"Dark Bronze",346,"GPF143780V221G000","8056603633147"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",187,"Aged Bronze",346,"GPF143780G052G000","8056603633260"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",713,"Antique Brass",346,"GPF143780V204G000","8056603633154"]
["BATHROOM","INCASTRI","INCASTRI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",279,"Matte White",278,"GPF143780C071G000","8056603633338"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector","031","Chrome",161,"GPF473510G001G000","8056603535717"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",149,"Finox Brushed Nickel",217,"GPF473510G002G000","8056603535700"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",299,"Matte Black",217,"GPF473510C072G000","8056603535724"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",147,"Chome Brushed",217,"GPF473510G006G000","8056603631686"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",720,"Nickel PVD",252,"GPF473510P014G000","8056603631662"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",706,"Black Metal PVD",252,"GPF473510P001G000","8056603587068"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",707,"Black Metal Brushed PVD",269,"GPF473510P004G000","8056603587051"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector","030","Copper PVD",252,"GPF473510P000G000","8056603587075"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",708,"Copper Brushed PVD",269,"GPF473510P006G000","8056603587044"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",735,"Warm Bronze PVD",252,"GPF473510P037G000","8056603587006"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",726,"Warm Bronze Brushed PVD",269,"GPF473510P024G000","8056603587020"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",710,"Brass PVD",252,"GPF473510P011G000","8056603587037"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",727,"Brass Brushed PVD",269,"GPF473510P025G000","8056603587013"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",246,"Gold PVD",287,"GPF473510P007G000","8056603631679"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",716,"Gold Brushed PVD",287,"GPF473510P005G000","8056603723534"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",761,"Coffee Bronze Brushed PVD",284,"GPF473510E059G000","8055261602700"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",845,"Dark Bronze",269,"GPF473510V221G000","8056603631655"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",187,"Aged Bronze",269,"GPF473510G052G000","8056603587082"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",713,"Antique Brass",269,"GPF473510V204G000","8056603586993"]
["BATHROOM","INCASTRI","INCASTRI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",279,"Matte White",217,"GPF473510C071G000","8056603587099"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.","031","Chrome",161,"GPF473500G001G000","8056603535748"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",149,"Finox Brushed Nickel",217,"GPF473500G002G000","8056603535731"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",299,"Matte Black",217,"GPF473500C072G000","8056603535755"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",147,"Chome Brushed",217,"GPF473500G006G000","8056603631723"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",720,"Nickel PVD",252,"GPF473500P014G000","8056603631709"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",706,"Black Metal PVD",252,"GPF473500P001G000","8056603587174"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",707,"Black Metal Brushed PVD",269,"GPF473500P004G000","8056603587167"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.","030","Copper PVD",252,"GPF473500P000G000","8056603587181"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",708,"Copper Brushed PVD",269,"GPF473500P006G000","8056603587150"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",735,"Warm Bronze PVD",252,"GPF473500P037G000","8056603587112"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",726,"Warm Bronze Brushed PVD",269,"GPF473500P024G000","8056603587136"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",710,"Brass PVD",252,"GPF473500P011G000","8056603587143"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",727,"Brass Brushed PVD",269,"GPF473500P025G000","8056603587129"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",246,"Gold PVD",287,"GPF473500P007G000","8056603631716"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",716,"Gold Brushed PVD",287,"GPF473500P005G000","8055261230965"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",761,"Coffee Bronze Brushed PVD",284,"GPF473500E059G000","8055261602724"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",845,"Dark Bronze",269,"GPF473500V221G000","8056603631693"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",187,"Aged Bronze",269,"GPF473500G052G000","8056603587198"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",713,"Antique Brass",269,"GPF473500V204G000","8056603587105"]
["BATHROOM","INCASTRI","INCASTRI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",279,"Matte White",217,"GPF473500C071G000","8056603587204"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections","031","Chrome",72,"GPF016370G001G000","8022692026276"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",149,"Finox Brushed Nickel",81,"GPF016370G002G000","8022692785104"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",299,"Matte Black",134,"GPF016370C072G000","8022692845327"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",147,"Chome Brushed",81,"GPF016370G006G000","8056329136793"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",720,"Nickel PVD",102,"GPF016370P014G000","8056329725720"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",706,"Black Metal PVD",113,"GPF016370P001G000","8022692689037"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",707,"Black Metal Brushed PVD",120,"GPF016370P004G000","8022692655407"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections","030","Copper PVD",113,"GPF016370P000G000","8022692671254"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",708,"Copper Brushed PVD",120,"GPF016370P006G000","8022692092233"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",735,"Warm Bronze PVD",113,"GPF016370P037G000","8056329555662"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",726,"Warm Bronze Brushed PVD",120,"GPF016370P024G000","8056329555655"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",710,"Brass PVD",113,"GPF016370P011G000","8022692092493"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",727,"Brass Brushed PVD",120,"GPF016370P025G000","8056329037441"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",246,"Gold PVD",133,"GPF016370P007G000","8056329037458"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",716,"Gold Brushed PVD",128,"GPF016370P005G000","8022692092004"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",761,"Coffee Bronze Brushed PVD",128,"GPF016370E059G000","8055261609938"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",845,"Dark Bronze",120,"GPF016370V221G000","8056603623247"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",187,"Aged Bronze",133,"GPF016370G052G000","8056329008779"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",713,"Antique Brass",133,"GPF016370V204G000","8022692689044"]
["BATHROOM","INCASTRI","INCASTRI","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",279,"Matte White",134,"GPF016370C071G000","8022692891997"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections","031","Chrome",85,"GPF287460G001G000","8022692025996"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",149,"Finox Brushed Nickel",102,"GPF287460G002G000","8022692788600"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",299,"Matte Black",150,"GPF287460C072G000","8022692847376"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",720,"Nickel PVD",120,"GPF287460P014G000","8056603608053"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",706,"Black Metal PVD",134,"GPF287460P001G000","8056329105164"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",707,"Black Metal Brushed PVD",143,"GPF287460P004G000","8056329105171"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections","030","Copper PVD",134,"GPF287460P000G000","8056329105157"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",708,"Copper Brushed PVD",143,"GPF287460P006G000","8056329105188"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",735,"Warm Bronze PVD",134,"GPF287460P037G000","8056329610736"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",726,"Warm Bronze Brushed PVD",143,"GPF287460P024G000","8056329610743"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",710,"Brass PVD",134,"GPF287460P011G000","8056329610750"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",727,"Brass Brushed PVD",143,"GPF287460P025G000","8056329105201"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",246,"Gold PVD",150,"GPF287460P007G000","8056329105195"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",716,"Gold Brushed PVD",151,"GPF287460P005G000","8055261231160"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",761,"Coffee Bronze Brushed PVD",150,"GPF287460E059G000","8055261608771"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",845,"Dark Bronze",143,"GPF287460V221G000","8056603623186"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",187,"Aged Bronze",167,"GPF287460G052G000","8056329105218"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",713,"Antique Brass",167,"GPF287460V204G000","8056329048577"]
["BATHROOM","INCASTRI","INCASTRI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",279,"Matte White",150,"GPF287460C071G000","8056329049444"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish","031","Chrome",90,"GPF541370G001G000","8056329573116"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",239,"Steel Brushed",121,"GPF541370A000G000","8022692850154"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",299,"Matte Black",120,"GPF541370C072G000","8056329573130"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",720,"Nickel PVD",121,"GPF541370P014G000","8056603606868"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",706,"Black Metal PVD",143,"GPF541370P001G000","8056329573178"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",707,"Black Metal Brushed PVD",150,"GPF541370P004G000","8022692850161"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish","030","Copper PVD",143,"GPF541370P000G000","8056329573123"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",708,"Copper Brushed PVD",150,"GPF541370P006G000","8022692850178"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",735,"Warm Bronze PVD",143,"GPF541370P037G000","8056329573154"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",726,"Warm Bronze Brushed PVD",150,"GPF541370P024G000","8022692850185"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",710,"Brass PVD",143,"GPF541370P011G000","8056329600522"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",727,"Brass Brushed PVD",150,"GPF541370P025G000","8056329600515"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",761,"Coffee Bronze Brushed PVD",159,"GPF541370E059G000","8055261601420"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",845,"Dark Bronze",121,"GPF541370V221G000","8056603954174"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",187,"Aged Bronze",121,"GPF541370G052G000","8056329587823"]
["BATHROOM","INCASTRI","INCASTRI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",713,"Antique Brass",121,"GPF541370V204G000","8056329573147"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector","031","Chrome",96,"GPF017240G001G000","8055261240131"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",149,"Finox Brushed Nickel",130,"GPF017240G002G000","8055261240124"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",299,"Matte Black",130,"GPF017240C072G000","8055261240148"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",147,"Chome Brushed",130,"GPF017240G006G000","8055261240117"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",720,"Nickel PVD",152,"GPF017240P014G000","8055261240025"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",706,"Black Metal PVD",152,"GPF017240P001G000","8055261240087"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",707,"Black Metal Brushed PVD",162,"GPF017240P004G000","8055261240070"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector","030","Copper PVD",152,"GPF017240P000G000","8055261240094"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",708,"Copper Brushed PVD",162,"GPF017240P006G000","8055261240056"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",735,"Warm Bronze PVD",152,"GPF017240P037G000","8055261239999"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",726,"Warm Bronze Brushed PVD",162,"GPF017240P024G000","8055261240018"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",710,"Brass PVD",152,"GPF017240P011G000","8055261240032"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",727,"Brass Brushed PVD",162,"GPF017240P025G000","8055261240001"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",246,"Gold PVD",170,"GPF017240P007G000","8055261240049"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",716,"Gold Brushed PVD",170,"GPF017240P005G000","8055261240063"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",761,"Coffee Bronze Brushed PVD",170,"GPF017240E059G000","8055261609853"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",845,"Dark Bronze",162,"GPF017240V221G000","8055261239975"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",187,"Aged Bronze",162,"GPF017240G052G000","8055261240100"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",713,"Antique Brass",162,"GPF017240V204G000","8055261239982"]
["BATHROOM","INCASTRI","INCASTRI","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",279,"Matte White",130,"GPF017240C071G000","8055261240155"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.","031","Chrome",366,"GPF754010G001G000","8055261439696"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",149,"Finox Brushed Nickel",494,"GPF754010G002G000","8055261439689"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",299,"Matte Black",494,"GPF754010C072G000","8055261439702"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",706,"Black Metal PVD",542,"GPF754010P001G000","8055261439665"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",707,"Black Metal Brushed PVD",579,"GPF754010P004G000","8055261439658"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.","030","Copper PVD",542,"GPF754010P000G000","8055261439672"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",708,"Copper Brushed PVD",579,"GPF754010P006G000","8055261439641"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",735,"Warm Bronze PVD",542,"GPF754010P037G000","8055261439597"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",726,"Warm Bronze Brushed PVD",579,"GPF754010P024G000","8055261439610"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",720,"Nickel PVD",542,"GPF754010P014G000","8055261439627"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",761,"Coffee Bronze Brushed PVD",615,"GPF754010E059G000","8055261570689"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",710,"Brass PVD",542,"GPF754010P011G000","8055261439634"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",727,"Brass Brushed PVD",579,"GPF754010P025G000","8055261439603"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75401,75401,"Zeephouder voor aan de muur.","Porta savon mural.","Wall-mounted soap holder.",845,"Dark Bronze",579,"GPF754010V221G000","8055261439580"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.","031","Chrome",366,"GPF754070G001G000","8055261439436"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",149,"Finox Brushed Nickel",494,"GPF754070G002G000","8055261439429"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",299,"Matte Black",494,"GPF754070C072G000","8055261439443"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",706,"Black Metal PVD",542,"GPF754070P001G000","8055261439405"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",707,"Black Metal Brushed PVD",579,"GPF754070P004G000","8055261439399"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.","030","Copper PVD",542,"GPF754070P000G000","8055261439412"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",708,"Copper Brushed PVD",579,"GPF754070P006G000","8055261439382"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",735,"Warm Bronze PVD",542,"GPF754070P037G000","8055261439337"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",726,"Warm Bronze Brushed PVD",579,"GPF754070P024G000","8055261439351"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",720,"Nickel PVD",542,"GPF754070P014G000","8055261439368"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",761,"Coffee Bronze Brushed PVD",615,"GPF754070E059G000","8055261570641"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",710,"Brass PVD",542,"GPF754070P011G000","8055261439375"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",727,"Brass Brushed PVD",579,"GPF754070P025G000","8055261439344"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75407,75407,"Wandbeker voor aan de muur.","Porte verre mural.","Wall-mounted tumbler.",845,"Dark Bronze",579,"GPF754070V221G000","8055261439320"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.","031","Chrome",550,"GPF754130G001G000","8055261439177"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",149,"Finox Brushed Nickel",742,"GPF754130G002G000","8055261439160"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",299,"Matte Black",742,"GPF754130C072G000","8055261439184"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",706,"Black Metal PVD",812,"GPF754130P001G000","8055261439146"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",707,"Black Metal Brushed PVD",868,"GPF754130P004G000","8055261439139"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.","030","Copper PVD",812,"GPF754130P000G000","8055261439153"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",708,"Copper Brushed PVD",868,"GPF754130P006G000","8055261439122"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",735,"Warm Bronze PVD",812,"GPF754130P037G000","8055261439078"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",726,"Warm Bronze Brushed PVD",868,"GPF754130P024G000","8055261439092"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",720,"Nickel PVD",812,"GPF754130P014G000","8055261439108"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",761,"Coffee Bronze Brushed PVD",923,"GPF754130E059G000","8055261570603"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",710,"Brass PVD",812,"GPF754130P011G000","8055261439115"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",727,"Brass Brushed PVD",868,"GPF754130P025G000","8055261439085"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75413,75413,"Zeepdispenser voor aan de muur.","Distributeur de savon liquide mural.","Wall-mounted soap dispenser.",845,"Dark Bronze",868,"GPF754130V221G000","8055261439061"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.","031","Chrome",610,"GPF754210G001G000","8055261438910"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",149,"Finox Brushed Nickel",824,"GPF754210G002G000","8055261438903"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",299,"Matte Black",824,"GPF754210C072G000","8055261438927"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",706,"Black Metal PVD",903,"GPF754210P001G000","8055261438880"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",707,"Black Metal Brushed PVD",964,"GPF754210P004G000","8055261438873"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.","030","Copper PVD",903,"GPF754210P000G000","8055261438897"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",708,"Copper Brushed PVD",964,"GPF754210P006G000","8055261438866"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",735,"Warm Bronze PVD",903,"GPF754210P037G000","8055261438811"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",726,"Warm Bronze Brushed PVD",964,"GPF754210P024G000","8055261438835"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",720,"Nickel PVD",903,"GPF754210P014G000","8055261438842"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",761,"Coffee Bronze Brushed PVD",1024,"GPF754210E059G000","8055261570566"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",710,"Brass PVD",903,"GPF754210P011G000","8055261438859"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",727,"Brass Brushed PVD",964,"GPF754210P025G000","8055261438828"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75421,75421,"Toiletborstelhouder voor aan de muur.","Porta balayette mural.","Wall-mounted toilet brush holder.",845,"Dark Bronze",964,"GPF754210V221G000","8055261438804"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.","031","Chrome",366,"GPF754250G001G000","8055261438781"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",149,"Finox Brushed Nickel",494,"GPF754250G002G000","8055261438774"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",299,"Matte Black",494,"GPF754250C072G000","8055261438798"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",706,"Black Metal PVD",542,"GPF754250P001G000","8055261438750"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",707,"Black Metal Brushed PVD",579,"GPF754250P004G000","8055261438743"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.","030","Copper PVD",542,"GPF754250P000G000","8055261438767"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",708,"Copper Brushed PVD",579,"GPF754250P006G000","8055261438736"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",735,"Warm Bronze PVD",542,"GPF754250P037G000","8055261438682"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",726,"Warm Bronze Brushed PVD",579,"GPF754250P024G000","8055261438705"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",720,"Nickel PVD",542,"GPF754250P014G000","8055261438712"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",761,"Coffee Bronze Brushed PVD",615,"GPF754250E059G000","8055261570542"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",710,"Brass PVD",542,"GPF754250P011G000","8055261438729"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",727,"Brass Brushed PVD",579,"GPF754250P025G000","8055261438699"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75425,75425,"Staande zeephouder.","Porte savon à poser.","Standing soap holder.",845,"Dark Bronze",579,"GPF754250V221G000","8055261438675"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.","031","Chrome",366,"GPF754310G001G000","8055261438521"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",149,"Finox Brushed Nickel",494,"GPF754310G002G000","8055261438514"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",299,"Matte Black",494,"GPF754310C072G000","8055261438538"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",706,"Black Metal PVD",542,"GPF754310P001G000","8055261438491"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",707,"Black Metal Brushed PVD",579,"GPF754310P004G000","8055261438484"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.","030","Copper PVD",542,"GPF754310P000G000","8055261438507"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",708,"Copper Brushed PVD",579,"GPF754310P006G000","8055261438477"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",735,"Warm Bronze PVD",542,"GPF754310P037G000","8055261438422"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",726,"Warm Bronze Brushed PVD",579,"GPF754310P024G000","8055261438446"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",720,"Nickel PVD",542,"GPF754310P014G000","8055261438453"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",761,"Coffee Bronze Brushed PVD",615,"GPF754310E059G000","8055261570504"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",710,"Brass PVD",542,"GPF754310P011G000","8055261438460"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",727,"Brass Brushed PVD",579,"GPF754310P025G000","8055261438439"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75431,75431,"Staande beker.","Porte verre à poser.","Standing tumbler.",845,"Dark Bronze",579,"GPF754310V221G000","8055261438415"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.","031","Chrome",550,"GPF754370G001G000","8055261438262"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",149,"Finox Brushed Nickel",742,"GPF754370G002G000","8055261438255"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",299,"Matte Black",742,"GPF754370C072G000","8055261438279"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",706,"Black Metal PVD",812,"GPF754370P001G000","8055261438231"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",707,"Black Metal Brushed PVD",868,"GPF754370P004G000","8055261438224"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.","030","Copper PVD",812,"GPF754370P000G000","8055261438248"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",708,"Copper Brushed PVD",868,"GPF754370P006G000","8055261438217"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",735,"Warm Bronze PVD",812,"GPF754370P037G000","8055261438163"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",726,"Warm Bronze Brushed PVD",868,"GPF754370P024G000","8055261438187"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",720,"Nickel PVD",812,"GPF754370P014G000","8055261438194"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",761,"Coffee Bronze Brushed PVD",923,"GPF754370E059G000","8055261570467"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",710,"Brass PVD",812,"GPF754370P011G000","8055261438200"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",727,"Brass Brushed PVD",868,"GPF754370P025G000","8055261438170"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75437,75437,"Staande zeepdispenser.","Distributeur de savon liquide à poser.","Standing soap dispenser.",845,"Dark Bronze",868,"GPF754370V221G000","8055261438156"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75570,75570,"Staand dienblad.","Plateau à poser.","Standing tray.",561,"Yakisugi",332,"GPF755700B061G000","8055261646469"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.","031","Chrome",610,"GPF754450G001G000","8055261438002"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",149,"Finox Brushed Nickel",824,"GPF754450G002G000","8055261437999"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",299,"Matte Black",824,"GPF754450C072G000","8055261438019"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",706,"Black Metal PVD",903,"GPF754450P001G000","8055261437975"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",707,"Black Metal Brushed PVD",964,"GPF754450P004G000","8055261437968"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.","030","Copper PVD",903,"GPF754450P000G000","8055261437982"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",708,"Copper Brushed PVD",964,"GPF754450P006G000","8055261437951"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",735,"Warm Bronze PVD",903,"GPF754450P037G000","8055261437906"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",726,"Warm Bronze Brushed PVD",964,"GPF754450P024G000","8055261437920"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",720,"Nickel PVD",903,"GPF754450P014G000","8055261437937"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",761,"Coffee Bronze Brushed PVD",1024,"GPF754450E059G000","8055261570429"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",710,"Brass PVD",903,"GPF754450P011G000","8055261437944"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",727,"Brass Brushed PVD",964,"GPF754450P025G000","8055261437913"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75445,75445,"Staande toiletborstelhouder","Porte balayette à poser.","Standing toilet brush holder.",845,"Dark Bronze",964,"GPF754450V221G000","8055261437890"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.","031","Chrome",306,"GPF754550G001G000","8055261437876"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",149,"Finox Brushed Nickel",413,"GPF754550G002G000","8055261437869"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",299,"Matte Black",413,"GPF754550C072G000","8055261437883"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",706,"Black Metal PVD",452,"GPF754550P001G000","8055261437845"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",707,"Black Metal Brushed PVD",483,"GPF754550P004G000","8055261437838"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.","030","Copper PVD",452,"GPF754550P000G000","8055261437852"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",708,"Copper Brushed PVD",483,"GPF754550P006G000","8055261437821"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",735,"Warm Bronze PVD",452,"GPF754550P037G000","8055261437777"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",726,"Warm Bronze Brushed PVD",483,"GPF754550P024G000","8055261437791"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",720,"Nickel PVD",452,"GPF754550P014G000","8055261437807"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",761,"Coffee Bronze Brushed PVD",514,"GPF754550E059G000","8055261570405"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",710,"Brass PVD",452,"GPF754550P011G000","8055261437814"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",727,"Brass Brushed PVD",483,"GPF754550P025G000","8055261437784"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75455,75455,"Wand-toiletrolhouder","Porte papier mural.","Wall-mounted paper roll holder.",845,"Dark Bronze",483,"GPF754550V221G000","8055261437760"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.","031","Chrome",428,"GPF754970G001G000","8055261437746"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",149,"Finox Brushed Nickel",577,"GPF754970G002G000","8055261437739"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",299,"Matte Black",577,"GPF754970C072G000","8055261437753"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",706,"Black Metal PVD",632,"GPF754970P001G000","8055261437715"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",707,"Black Metal Brushed PVD",675,"GPF754970P004G000","8055261437708"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.","030","Copper PVD",632,"GPF754970P000G000","8055261437722"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",708,"Copper Brushed PVD",675,"GPF754970P006G000","8055261437692"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",735,"Warm Bronze PVD",632,"GPF754970P037G000","8055261437647"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",726,"Warm Bronze Brushed PVD",675,"GPF754970P024G000","8055261437661"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",720,"Nickel PVD",632,"GPF754970P014G000","8055261437678"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",761,"Coffee Bronze Brushed PVD",719,"GPF754970E059G000","8055261570382"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",710,"Brass PVD",632,"GPF754970P011G000","8055261437685"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",727,"Brass Brushed PVD",675,"GPF754970P025G000","8055261437654"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75497,75497,"Handdoekhouder 30 cm","Porte serviette 30 cm.","Wall-mounted towel rail, 30 cm.",845,"Dark Bronze",675,"GPF754970V221G000","8055261437630"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.","031","Chrome",458,"GPF755000G001G000","8055261437616"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",149,"Finox Brushed Nickel",620,"GPF755000G002G000","8055261437609"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",299,"Matte Black",620,"GPF755000C072G000","8055261437623"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",706,"Black Metal PVD",678,"GPF755000P001G000","8055261437586"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",707,"Black Metal Brushed PVD",723,"GPF755000P004G000","8055261437579"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.","030","Copper PVD",678,"GPF755000P000G000","8055261437593"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",708,"Copper Brushed PVD",723,"GPF755000P006G000","8055261437562"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",735,"Warm Bronze PVD",678,"GPF755000P037G000","8055261437517"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",726,"Warm Bronze Brushed PVD",723,"GPF755000P024G000","8055261437531"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",720,"Nickel PVD",678,"GPF755000P014G000","8055261437548"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",761,"Coffee Bronze Brushed PVD",770,"GPF755000E059G000","8055261570368"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",710,"Brass PVD",678,"GPF755000P011G000","8055261437555"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",727,"Brass Brushed PVD",723,"GPF755000P025G000","8055261437524"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75500,75500,"Handdoekhouder 45 cm","Porte serviette 45 cm.","Wall-mounted towel rail, 45 cm.",845,"Dark Bronze",723,"GPF755000V221G000","8055261437500"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.","031","Chrome",488,"GPF755030G001G000","8055261437487"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",149,"Finox Brushed Nickel",659,"GPF755030G002G000","8055261437470"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",299,"Matte Black",659,"GPF755030C072G000","8055261437494"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",706,"Black Metal PVD",722,"GPF755030P001G000","8055261437456"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",707,"Black Metal Brushed PVD",771,"GPF755030P004G000","8055261437449"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.","030","Copper PVD",722,"GPF755030P000G000","8055261437463"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",708,"Copper Brushed PVD",771,"GPF755030P006G000","8055261437432"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",735,"Warm Bronze PVD",722,"GPF755030P037G000","8055261437388"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",726,"Warm Bronze Brushed PVD",771,"GPF755030P024G000","8055261437401"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",720,"Nickel PVD",722,"GPF755030P014G000","8055261437418"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",761,"Coffee Bronze Brushed PVD",820,"GPF755030E059G000","8055261570344"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",710,"Brass PVD",722,"GPF755030P011G000","8055261437425"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",727,"Brass Brushed PVD",771,"GPF755030P025G000","8055261437395"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75503,75503,"Handdoekhouder 60 cm","Porte serviette 60 cm.","Wall-mounted towel rail, 60 cm.",845,"Dark Bronze",771,"GPF755030V221G000","8055261437371"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.","031","Chrome",184,"GPF755210G001G000","8055261436961"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",149,"Finox Brushed Nickel",249,"GPF755210G002G000","8055261436954"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",299,"Matte Black",249,"GPF755210C072G000","8055261436978"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",706,"Black Metal PVD",272,"GPF755210P001G000","8055261436930"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",707,"Black Metal Brushed PVD",290,"GPF755210P004G000","8055261436923"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.","030","Copper PVD",272,"GPF755210P000G000","8055261436947"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",708,"Copper Brushed PVD",290,"GPF755210P006G000","8055261436916"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",735,"Warm Bronze PVD",272,"GPF755210P037G000","8055261436862"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",726,"Warm Bronze Brushed PVD",290,"GPF755210P024G000","8055261436886"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",720,"Nickel PVD",272,"GPF755210P014G000","8055261436893"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",761,"Coffee Bronze Brushed PVD",309,"GPF755210E059G000","8055261570269"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",710,"Brass PVD",272,"GPF755210P011G000","8055261436909"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",727,"Brass Brushed PVD",290,"GPF755210P025G000","8055261436879"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75521,75521,"Wand-kledinghaak","Pàtere.","Wall-mounted robe hook.",845,"Dark Bronze",290,"GPF755210V221G000","8055261436855"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.","031","Chrome",550,"GPF755110G001G000","8055261437357"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",149,"Finox Brushed Nickel",742,"GPF755110G002G000","8055261437340"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",299,"Matte Black",742,"GPF755110C072G000","8055261437364"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",706,"Black Metal PVD",812,"GPF755110P001G000","8055261437326"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",707,"Black Metal Brushed PVD",868,"GPF755110P004G000","8055261437319"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.","030","Copper PVD",812,"GPF755110P000G000","8055261437333"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",708,"Copper Brushed PVD",868,"GPF755110P006G000","8055261437302"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",735,"Warm Bronze PVD",812,"GPF755110P037G000","8055261437258"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",726,"Warm Bronze Brushed PVD",868,"GPF755110P024G000","8055261437272"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",720,"Nickel PVD",812,"GPF755110P014G000","8055261437289"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",761,"Coffee Bronze Brushed PVD",924,"GPF755110E059G000","8055261570320"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",710,"Brass PVD",812,"GPF755110P011G000","8055261437296"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",727,"Brass Brushed PVD",868,"GPF755110P025G000","8055261437265"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75511,75511,"Handdoekhouder 30 cm","Porte serviette pour verre 30 cm.","Towel rail for glass fixing, 30 cm.",845,"Dark Bronze",868,"GPF755110V221G000","8055261437241"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.","031","Chrome",580,"GPF755130G001G000","8055261437227"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",149,"Finox Brushed Nickel",784,"GPF755130G002G000","8055261437210"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",299,"Matte Black",784,"GPF755130C072G000","8055261437234"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",706,"Black Metal PVD",858,"GPF755130P001G000","8055261437197"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",707,"Black Metal Brushed PVD",916,"GPF755130P004G000","8055261437180"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.","030","Copper PVD",858,"GPF755130P000G000","8055261437203"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",708,"Copper Brushed PVD",916,"GPF755130P006G000","8055261437173"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",735,"Warm Bronze PVD",858,"GPF755130P037G000","8055261437128"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",726,"Warm Bronze Brushed PVD",916,"GPF755130P024G000","8055261437142"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",720,"Nickel PVD",858,"GPF755130P014G000","8055261437159"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",761,"Coffee Bronze Brushed PVD",975,"GPF755130E059G000","8055261570306"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",710,"Brass PVD",858,"GPF755130P011G000","8055261437166"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",727,"Brass Brushed PVD",916,"GPF755130P025G000","8055261437135"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75513,75513,"Handdoekhouder 45 cm","Porte serviette pour verre 45 cm.","Towel rail for glass fixing, 45 cm.",845,"Dark Bronze",916,"GPF755130V221G000","8055261437111"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.","031","Chrome",610,"GPF755150G001G000","8055261437098"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",149,"Finox Brushed Nickel",824,"GPF755150G002G000","8055261437081"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",299,"Matte Black",824,"GPF755150C072G000","8055261437104"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",706,"Black Metal PVD",903,"GPF755150P001G000","8055261437067"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",707,"Black Metal Brushed PVD",964,"GPF755150P004G000","8055261437050"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.","030","Copper PVD",903,"GPF755150P000G000","8055261437074"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",708,"Copper Brushed PVD",964,"GPF755150P006G000","8055261437043"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",735,"Warm Bronze PVD",903,"GPF755150P037G000","8055261436992"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",726,"Warm Bronze Brushed PVD",964,"GPF755150P024G000","8055261437012"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",720,"Nickel PVD",903,"GPF755150P014G000","8055261437029"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",761,"Coffee Bronze Brushed PVD",1024,"GPF755150E059G000","8055261570283"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",710,"Brass PVD",903,"GPF755150P011G000","8055261437036"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",727,"Brass Brushed PVD",964,"GPF755150P025G000","8055261437005"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75515,75515,"Handdoekhouder 60 cm","Porte serviette pour verre 60 cm.","Towel rail for glass fixing, 60 cm.",845,"Dark Bronze",964,"GPF755150V221G000","8055261436985"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf","031","Chrome",435,"GPF208610G001G000","8022692021448"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",149,"Finox Brushed Nickel",588,"GPF208610G002G000","8022692786149"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",299,"Matte Black",588,"GPF208610C072G000","8022692054507"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",720,"Nickel PVD",644,"GPF208610P014G000","8056603479868"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",706,"Black Metal PVD",644,"GPF208610P001G000","8022692257557"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",707,"Black Metal Brushed PVD",686,"GPF208610P004G000","8022692257717"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf","030","Copper PVD",644,"GPF208610P000G000","8022692257533"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",708,"Copper Brushed PVD",686,"GPF208610P006G000","8022692257724"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",735,"Warm Bronze PVD",644,"GPF208610P037G000","8056329611825"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",726,"Warm Bronze Brushed PVD",686,"GPF208610P024G000","8056329058286"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",761,"Coffee Bronze Brushed PVD",731,"GPF208610E059G000","8055261577831"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",710,"Brass PVD",644,"GPF208610P011G000","8056329611832"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",727,"Brass Brushed PVD",686,"GPF208610P025G000","8056329143708"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",187,"Aged Bronze",686,"GPF208610G052G000","8056329142015"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",713,"Antique Brass",686,"GPF208610V204G000","8056329119673"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",845,"Dark Bronze",686,"GPF208610V221G000","8055261479210"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.","031","Chrome",417,"GPF209470G001G000","8022692021127"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",149,"Finox Brushed Nickel",561,"GPF209470G002G000","8022692782981"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",299,"Matte Black",561,"GPF209470C072G000","8022692065565"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",720,"Nickel PVD",614,"GPF209470P014G000","8056603608152"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",706,"Black Metal PVD",614,"GPF209470P001G000","8022692272741"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",707,"Black Metal Brushed PVD",658,"GPF209470P004G000","8022692273052"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.","030","Copper PVD",614,"GPF209470P000G000","8022692272703"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",708,"Copper Brushed PVD",658,"GPF209470P006G000","8022692273090"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",735,"Warm Bronze PVD",614,"GPF209470P037G000","8056329611269"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",726,"Warm Bronze Brushed PVD",658,"GPF209470P024G000","8056329186194"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",761,"Coffee Bronze Brushed PVD",701,"GPF209470E059G000","8055261577794"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",710,"Brass PVD",614,"GPF209470P011G000","8056329611276"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",727,"Brass Brushed PVD",658,"GPF209470P025G000","8056329163232"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",187,"Aged Bronze",658,"GPF209470G052G000","8056329545991"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",713,"Antique Brass",658,"GPF209470V204G000","8022692847697"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",845,"Dark Bronze",658,"GPF209470V221G000","8055261265738"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm","031","Chrome",549,"GPF209490G001G000","8022692025521"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",149,"Finox Brushed Nickel",739,"GPF209490G002G000","8022692788075"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",299,"Matte Black",739,"GPF209490C072G000","8022692056433"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",720,"Nickel PVD",810,"GPF209490P014G000","8056603479806"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",706,"Black Metal PVD",810,"GPF209490P001G000","8022692273410"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",707,"Black Metal Brushed PVD",865,"GPF209490P004G000","8022692273748"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm","030","Copper PVD",810,"GPF209490P000G000","8022692273380"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",708,"Copper Brushed PVD",865,"GPF209490P006G000","8022692273779"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",735,"Warm Bronze PVD",810,"GPF209490P037G000","8056329611245"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",726,"Warm Bronze Brushed PVD",865,"GPF209490P024G000","8056329086098"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",761,"Coffee Bronze Brushed PVD",922,"GPF209490E059G000","8055261577770"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",710,"Brass PVD",810,"GPF209490P011G000","8056329611252"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",727,"Brass Brushed PVD",865,"GPF209490P025G000","8056329080386"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",187,"Aged Bronze",865,"GPF209490G052G000","8056603628266"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",713,"Antique Brass",865,"GPF209490V204G000","8022692847703"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20949,20949,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",845,"Dark Bronze",867,"GPF209490V221G000","8055261458154"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm","031","Chrome",762,"GPF209500G001G000","8022692046717"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",149,"Finox Brushed Nickel",1029,"GPF209500G002G000","8022692789317"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",299,"Matte Black",1029,"GPF209500C072G000","8022692474695"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",720,"Nickel PVD",1125,"GPF209500P014G000","8056603608145"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",706,"Black Metal PVD",1125,"GPF209500P001G000","8022692274035"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",707,"Black Metal Brushed PVD",1203,"GPF209500P004G000","8022692274042"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm","030","Copper PVD",1125,"GPF209500P000G000","8022692274011"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",708,"Copper Brushed PVD",1203,"GPF209500P006G000","8022692274073"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",735,"Warm Bronze PVD",1125,"GPF209500P037G000","8056329611214"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",726,"Warm Bronze Brushed PVD",1203,"GPF209500P024G000","8056329020566"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",761,"Coffee Bronze Brushed PVD",1280,"GPF209500E059G000","8055261577756"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",710,"Brass PVD",1125,"GPF209500P011G000","8056329611238"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",727,"Brass Brushed PVD",1203,"GPF209500P025G000","8056329611221"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",187,"Aged Bronze",1203,"GPF209500G052G000","8056603628242"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",713,"Antique Brass",1203,"GPF209500V204G000","8056329224254"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20950,20950,"Wandrekje 60 cm","Console murale 60 cm.","Shelf 60 cm",845,"Dark Bronze",1203,"GPF209500V221G000","8055261429611"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm","031","Chrome",579,"GPF209450G001G000","8022692026955"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",149,"Finox Brushed Nickel",781,"GPF209450G002G000","8022692788068"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",299,"Matte Black",781,"GPF209450C072G000","8022692474541"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",720,"Nickel PVD",856,"GPF209450P014G000","8056603608169"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",706,"Black Metal PVD",856,"GPF209450P001G000","8022692272420"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",707,"Black Metal Brushed PVD",914,"GPF209450P004G000","8022692272437"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm","030","Copper PVD",856,"GPF209450P000G000","8022692272413"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",708,"Copper Brushed PVD",914,"GPF209450P006G000","8022692272444"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",735,"Warm Bronze PVD",856,"GPF209450P037G000","8056329611283"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",726,"Warm Bronze Brushed PVD",914,"GPF209450P024G000","8056329611306"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",761,"Coffee Bronze Brushed PVD",974,"GPF209450E059G000","8055261577817"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",710,"Brass PVD",856,"GPF209450P011G000","8056329611313"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",727,"Brass Brushed PVD",914,"GPF209450P025G000","8056329611290"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",187,"Aged Bronze",914,"GPF209450G052G000","8056603628297"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",713,"Antique Brass",914,"GPF209450V204G000","8056329147744"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",845,"Dark Bronze",914,"GPF209450V221G000","8055261479142"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.","031","Chrome",549,"GPF209880G001G000","8022692019643"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",149,"Finox Brushed Nickel",739,"GPF209880G002G000","8022692788754"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",299,"Matte Black",739,"GPF209880C072G000","8022692065237"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",720,"Nickel PVD",810,"GPF209880P014G000","8056603479790"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",706,"Black Metal PVD",810,"GPF209880P001G000","8022692275230"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",707,"Black Metal Brushed PVD",865,"GPF209880P004G000","8022692275339"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.","030","Copper PVD",810,"GPF209880P000G000","8022692275155"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",708,"Copper Brushed PVD",865,"GPF209880P006G000","8022692275346"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",735,"Warm Bronze PVD",810,"GPF209880P037G000","8056329610972"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",726,"Warm Bronze Brushed PVD",865,"GPF209880P024G000","8056329610996"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",761,"Coffee Bronze Brushed PVD",922,"GPF209880E059G000","8055261577732"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",710,"Brass PVD",810,"GPF209880P011G000","8056329611009"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",727,"Brass Brushed PVD",865,"GPF209880P025G000","8056329610989"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",187,"Aged Bronze",865,"GPF209880G052G000","8056329181267"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",713,"Antique Brass",865,"GPF209880V204G000","8056329224247"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",20988,20988,"Staande oriënteerbare spiegel","Miroir grossissant orientable à poser.","Adjustable standing mirror.",845,"Dark Bronze",865,"GPF209880V221G000","8055261479104"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",75990,75990,"Papierbak.","Poubelle.","Waste-paper basket.",561,"Yakisugi",589,"GPF759900B061G000","8055261667853"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.","031","Chrome",989,"GPF584241G001G000","8056329545564"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",149,"Finox Brushed Nickel",1337,"GPF584241G002G000","8056329523388"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",299,"Matte Black",1337,"GPF584241C072G000","8056329523401"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",720,"Nickel PVD",1465,"GPF584241P014G000","8056603501231"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",706,"Black Metal PVD",1465,"GPF584241P001G000","8056329545502"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",707,"Black Metal Brushed PVD",1565,"GPF584241P004G000","8056329545519"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.","030","Copper PVD",1465,"GPF584241P000G000","8056329545496"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",708,"Copper Brushed PVD",1565,"GPF584241P006G000","8056329545526"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",735,"Warm Bronze PVD",1465,"GPF584241P037G000","8056329556461"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",726,"Warm Bronze Brushed PVD",1565,"GPF584241P024G000","8056329545557"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",761,"Coffee Bronze Brushed PVD",1663,"GPF584241E059G000","8055261574359"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",710,"Brass PVD",1465,"GPF584241P011G000","8056329595057"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",727,"Brass Brushed PVD",1565,"GPF584241P025G000","8056329545533"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",246,"Gold PVD",1663,"GPF584241P007G000","8056329545540"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",716,"Gold Brushed PVD",1663,"GPF584241P005G000","8055261042711"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",845,"Dark Bronze",1565,"GPF584241V221G000","8056603637466"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",187,"Aged Bronze",1565,"GPF584241G052G000","8056329545472"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",713,"Antique Brass",1565,"GPF584241V204G000","8056329545489"]
["BATHROOM","INCASTRI","INCASTRI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",279,"Matte White",1337,"GPF584241C071G000","8055261185050"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39118,39118,"Wandtoilet van Keramiek (6 liter) met geïntegreerde sifon. Scharnieren met vertraagde sluiting en laterale gatafdekkingen opgenomen in afwerking 031","Cuvette suspendue en Céramique (6 litres) avec abattant muni de système “SOFT CLOSE” ou assisté. Charnière et enjoliveurs latéraux en finition 031","Wall hung WC (6 litres) in Ceramic, integrated siphon. Soft-closing hardware and lateral holes plugs included in 031 finishing.",518,"White Ceramic",1201,"GPF391180C083G000","8056603448529"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39118,39118,"Wandtoilet van Keramiek (6 liter) met geïntegreerde sifon. Scharnieren met vertraagde sluiting en laterale gatafdekkingen opgenomen in afwerking 031","Cuvette suspendue en Céramique (6 litres) avec abattant muni de système “SOFT CLOSE” ou assisté. Charnière et enjoliveurs latéraux en finition 031","Wall hung WC (6 litres) in Ceramic, integrated siphon. Soft-closing hardware and lateral holes plugs included in 031 finishing.",531,"Matte White Ceramic",1711,"GPF391180C288G000","8056603448536"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39118,39118,"Wandtoilet van Keramiek (6 liter) met geïntegreerde sifon. Scharnieren met vertraagde sluiting en laterale gatafdekkingen opgenomen in afwerking 031","Cuvette suspendue en Céramique (6 litres) avec abattant muni de système “SOFT CLOSE” ou assisté. Charnière et enjoliveurs latéraux en finition 031","Wall hung WC (6 litres) in Ceramic, integrated siphon. Soft-closing hardware and lateral holes plugs included in 031 finishing.",532,"Matte Black Ceramic",1711,"GPF391180C289G000","8056603448543"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39113,39113,"Wandtoilet van Keramiek (6 liter) met geïntegreerde sifon. Scharnieren met vertraagde sluiting en laterale gatafdekkingen opgenomen in afwerking 031","Cuvette suspendue en Céramique (6 litres) avec abattant muni de système “SOFT CLOSE” ou assisté. Charnière et enjoliveurs latéraux en finition 031","Wall hung WC (6 litres) in Ceramic, integrated siphon. Soft-closing hardware and lateral holes plugs included in 031 finishing.",518,"White Ceramic",1140,"GPF391133C083G000","8022692511543"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39113,39113,"Wandtoilet van Keramiek (6 liter) met geïntegreerde sifon. Scharnieren met vertraagde sluiting en laterale gatafdekkingen opgenomen in afwerking 031","Cuvette suspendue en Céramique (6 litres) avec abattant muni de système “SOFT CLOSE” ou assisté. Charnière et enjoliveurs latéraux en finition 031","Wall hung WC (6 litres) in Ceramic, integrated siphon. Soft-closing hardware and lateral holes plugs included in 031 finishing.",531,"Matte White Ceramic",1706,"GPF391133C288G000","8056329052512"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39113,39113,"Wandtoilet van Keramiek (6 liter) met geïntegreerde sifon. Scharnieren met vertraagde sluiting en laterale gatafdekkingen opgenomen in afwerking 031","Cuvette suspendue en Céramique (6 litres) avec abattant muni de système “SOFT CLOSE” ou assisté. Charnière et enjoliveurs latéraux en finition 031","Wall hung WC (6 litres) in Ceramic, integrated siphon. Soft-closing hardware and lateral holes plugs included in 031 finishing.",532,"Matte Black Ceramic",1706,"GPF391133C289G000","8056329052505"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39114,39114,"wand gemonteerde WC (6 liters) in keramiek, geïntegreerde sifon. Hardware en pluggen voor laterale gaten niet inbegrepen.","Cuvette murale en céramique (6 litres) avec siphon intégré. Charnières et sièges non inclus.","Wall hung WC (6 litres) in Ceramic, integrated siphon. Hardware and lateral holes plugs not included.",518,"White Ceramic",834,"GPF391140C083G000","8056603626675"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39114,39114,"wand gemonteerde WC (6 liters) in keramiek, geïntegreerde sifon. Hardware en pluggen voor laterale gaten niet inbegrepen.","Cuvette murale en céramique (6 litres) avec siphon intégré. Charnières et sièges non inclus.","Wall hung WC (6 litres) in Ceramic, integrated siphon. Hardware and lateral holes plugs not included.",531,"Matte White Ceramic",1249,"GPF391140C288G000","8056603626682"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39114,39114,"wand gemonteerde WC (6 liters) in keramiek, geïntegreerde sifon. Hardware en pluggen voor laterale gaten niet inbegrepen.","Cuvette murale en céramique (6 litres) avec siphon intégré. Charnières et sièges non inclus.","Wall hung WC (6 litres) in Ceramic, integrated siphon. Hardware and lateral holes plugs not included.",532,"Matte Black Ceramic",1249,"GPF391140C289G000","8056603626699"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39168,39168,"Toiletzitting van antibacteriële hars voor artikel 39114. Te completeren met zachtsluitend beslag 39184 (niet inbegrepen).","Siège en résine antibactérienne pour cuvette 39114. À combiner avec les charnières 39184 (non inclues).","Anti-bacterical resin WC seat for item 39114. To be completed with soft-closing hardware 39184 (not included).","031","Chrome",291,"GPF391680G001G000","8056603452380"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39168,39168,"Toiletzitting van antibacteriële hars voor artikel 39114. Te completeren met zachtsluitend beslag 39184 (niet inbegrepen).","Siège en résine antibactérienne pour cuvette 39114. À combiner avec les charnières 39184 (non inclues).","Anti-bacterical resin WC seat for item 39114. To be completed with soft-closing hardware 39184 (not included).",279,"Matte White",394,"GPF391680C071G000","8056603462334"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39168,39168,"Toiletzitting van antibacteriële hars voor artikel 39114. Te completeren met zachtsluitend beslag 39184 (niet inbegrepen).","Siège en résine antibactérienne pour cuvette 39114. À combiner avec les charnières 39184 (non inclues).","Anti-bacterical resin WC seat for item 39114. To be completed with soft-closing hardware 39184 (not included).",299,"Matte Black",394,"GPF391680C072G000","8056603462310"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.","031","Chrome",154,"GPF391840G001G000","8056603452038"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",239,"Steel Brushed",209,"GPF391840A000G000","8056603452069"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",149,"Finox Brushed Nickel",209,"GPF391840G002G000","8056603452021"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",299,"Matte Black",209,"GPF391840C072G000","8056603452045"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",720,"Nickel PVD",246,"GPF391840P014G000","8056603467148"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",706,"Black Metal PVD",246,"GPF391840P001G000","8056603451932"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",707,"Black Metal Brushed PVD",260,"GPF391840P004G000","8056603451925"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.","030","Copper PVD",246,"GPF391840P000G000","8056603451949"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",708,"Copper Brushed PVD",260,"GPF391840P006G000","8056603451901"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",735,"Warm Bronze PVD",246,"GPF391840P037G000","8056603451857"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",726,"Warm Bronze Brushed PVD",260,"GPF391840P024G000","8056603451871"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",761,"Coffee Bronze Brushed PVD",275,"GPF391840E059G000","8055261577497"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",710,"Brass PVD",246,"GPF391840P011G000","8056603451888"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",727,"Brass Brushed PVD",260,"GPF391840P025G000","8056603451864"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",246,"Gold PVD",275,"GPF391840P007G000","8056603451895"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",716,"Gold Brushed PVD",275,"GPF391840P005G000","8056603451918"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",187,"Aged Bronze",260,"GPF391840G052G000","8056603451987"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",713,"Antique Brass",260,"GPF391840V204G000","8056603451840"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",279,"Matte White",209,"GPF391840C071G000","8056603452052"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",29463,29463,"Toiletzitting van antibacteriële hars voor artikel 39114. Te completeren met zachtsluitend beslag 37584 (niet inbegrepen).","Siège en résine antibactérienne pour cuvette 39114. À combiner avec les charnières 37584 (non inclues).","Anti-bacterical resin WC seat for item 39114. To be completed with soft-closing hardware 37584 (not included).","031","Chrome",275,"GPF294630G001G000","8022692786163"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",29463,29463,"Toiletzitting van antibacteriële hars voor artikel 39114. Te completeren met zachtsluitend beslag 37584 (niet inbegrepen).","Siège en résine antibactérienne pour cuvette 39114. À combiner avec les charnières 37584 (non inclues).","Anti-bacterical resin WC seat for item 39114. To be completed with soft-closing hardware 37584 (not included).",299,"Matte Black",411,"GPF294630C072G000","8056329097667"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",29463,29463,"Toiletzitting van antibacteriële hars voor artikel 39114. Te completeren met zachtsluitend beslag 37584 (niet inbegrepen).","Siège en résine antibactérienne pour cuvette 39114. À combiner avec les charnières 37584 (non inclues).","Anti-bacterical resin WC seat for item 39114. To be completed with soft-closing hardware 37584 (not included).",279,"Matte White",411,"GPF294630C071G000","8056329097674"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.","031","Chrome",163,"GPF375842G001G000","8022692429954"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",149,"Finox Brushed Nickel",220,"GPF375842G002G000","8022692430172"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",299,"Matte Black",220,"GPF375842C072G000","8056329006386"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",147,"Chome Brushed",220,"GPF375842G006G000","8022692429961"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",720,"Nickel PVD",257,"GPF375842P014G000","8056603457033"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",706,"Black Metal PVD",257,"GPF375842P001G000","8022692674286"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",707,"Black Metal Brushed PVD",273,"GPF375842P004G000","8022692430424"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.","030","Copper PVD",257,"GPF375842P000G000","8022692674279"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",708,"Copper Brushed PVD",273,"GPF375842P006G000","8022692430080"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",735,"Warm Bronze PVD",257,"GPF375842P037G000","8056329558748"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",726,"Warm Bronze Brushed PVD",273,"GPF375842P024G000","8056329006379"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",761,"Coffee Bronze Brushed PVD",290,"GPF375842E059G000","8055261577534"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",710,"Brass PVD",257,"GPF375842P011G000","8056329609228"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",727,"Brass Brushed PVD",273,"GPF375842P025G000","8056329080393"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",246,"Gold PVD",290,"GPF375842P007G000","8056329097582"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",716,"Gold Brushed PVD",290,"GPF375842P005G000","8056329025462"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",187,"Aged Bronze",273,"GPF375842G052G000","8056329008762"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",713,"Antique Brass",273,"GPF375842V204G000","8022692430332"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",279,"Matte White",220,"GPF375842C071G000","8056329006393"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530","09276","Inbouwdeel voor afsluitbare douche met mengkraan.","Partie encastrée pour douchette shut-off avec mitigeur.","Built-in part for shut-off douchette with mixer.","031","Chrome",324,"GPF092760G001G000","8055261237261"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI","031","Chrome",624,"GPF755300G001G000","8055261645387"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",149,"Finox Brushed Nickel",842,"GPF755300G002G000","8055261645370"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",299,"Matte Black",842,"GPF755300C072G000","8055261645417"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",720,"Nickel PVD",924,"GPF755300P014G000","8055261645318"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",706,"Black Metal PVD",924,"GPF755300P001G000","8055261645356"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",707,"Black Metal Brushed PVD",986,"GPF755300P004G000","8055261645349"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI","030","Copper PVD",924,"GPF755300P000G000","8055261645363"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",708,"Copper Brushed PVD",986,"GPF755300P006G000","8055261645332"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",735,"Warm Bronze PVD",924,"GPF755300P037G000","8055261645288"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",726,"Warm Bronze Brushed PVD",986,"GPF755300P024G000","8055261645301"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",761,"Coffee Bronze Brushed PVD",1048,"GPF755300E059G000","8055261645394"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",710,"Brass PVD",924,"GPF755300P011G000","8055261645325"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",727,"Brass Brushed PVD",986,"GPF755300P025G000","8055261645295"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+75530",75530,"Shut-off douchette met mengkraan. INCASTRI","Douchette shut-off avec mitigeur. INCASTRI","Shut-off douchette with mixer. INCASTRI",845,"Dark Bronze",986,"GPF755300V221G000","8055261645271"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230","09276","Inbouwdeel voor afsluitbare douche met mengkraan.","Partie encastrée pour douchette shut-off avec mitigeur.","Built-in part for shut-off douchette with mixer.","031","Chrome",324,"GPF092760G001G000","8055261237261"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","031","Chrome",528,"GPF452300G001G000","8055261645684"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",149,"Finox Brushed Nickel",714,"GPF452300G002G000","8055261645677"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",299,"Matte Black",714,"GPF452300C072G000","8055261645714"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",720,"Nickel PVD",783,"GPF452300P014G000","8055261645615"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",706,"Black Metal PVD",783,"GPF452300P001G000","8055261645653"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",707,"Black Metal Brushed PVD",836,"GPF452300P004G000","8055261645646"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","030","Copper PVD",783,"GPF452300P000G000","8055261645660"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",708,"Copper Brushed PVD",836,"GPF452300P006G000","8055261645639"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",735,"Warm Bronze PVD",783,"GPF452300P037G000","8055261645585"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",726,"Warm Bronze Brushed PVD",836,"GPF452300P024G000","8055261645608"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",761,"Coffee Bronze Brushed PVD",889,"GPF452300E059G000","8055261645691"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",710,"Brass PVD",783,"GPF452300P011G000","8055261645622"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",727,"Brass Brushed PVD",836,"GPF452300P025G000","8055261645592"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",845,"Dark Bronze",836,"GPF452300V221G000","8055261645578"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130","09276","Inbouwdeel voor afsluitbare douche met mengkraan.","Partie encastrée pour douchette shut-off avec mitigeur.","Built-in part for shut-off douchette with mixer.","031","Chrome",324,"GPF092760G001G000","8055261237261"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","031","Chrome",480,"GPF451300G001G000","8055261227606"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",149,"Finox Brushed Nickel",648,"GPF451300G002G000","8055261227590"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",299,"Matte Black",648,"GPF451300C072G000","8055261227613"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",147,"Chome Brushed",648,"GPF451300G006G000","8055261227583"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",720,"Nickel PVD",711,"GPF451300P014G000","8055261227491"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",706,"Black Metal PVD",711,"GPF451300P001G000","8055261227552"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",707,"Black Metal Brushed PVD",758,"GPF451300P004G000","8055261227545"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","030","Copper PVD",711,"GPF451300P000G000","8055261227569"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",708,"Copper Brushed PVD",758,"GPF451300P006G000","8055261227521"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",735,"Warm Bronze PVD",711,"GPF451300P037G000","8055261227460"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",726,"Warm Bronze Brushed PVD",758,"GPF451300P024G000","8055261227484"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",761,"Coffee Bronze Brushed PVD",806,"GPF451300E059G000","8055261577411"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",710,"Brass PVD",711,"GPF451300P011G000","8055261227507"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",727,"Brass Brushed PVD",758,"GPF451300P025G000","8055261227477"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",246,"Gold PVD",807,"GPF451300P007G000","8055261227514"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",716,"Gold Brushed PVD",807,"GPF451300P005G000","8055261227538"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",187,"Aged Bronze",758,"GPF451300G052G000","8055261227576"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",713,"Antique Brass",758,"GPF451300V204G000","8055261227453"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",279,"Matte White",648,"GPF451300C071G000","8055261236233"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131","09276","Inbouwdeel voor afsluitbare douche met mengkraan.","Partie encastrée pour douchette shut-off avec mitigeur.","Built-in part for shut-off douchette with mixer.","031","Chrome",324,"GPF092760G001G000","8055261237261"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","031","Chrome",480,"GPF451310G001G000","8055261227422"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",149,"Finox Brushed Nickel",648,"GPF451310G002G000","8055261227415"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",299,"Matte Black",648,"GPF451310C072G000","8055261227439"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",147,"Chome Brushed",648,"GPF451310G006G000","8055261227408"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",720,"Nickel PVD",711,"GPF451310P014G000","8055261227316"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",706,"Black Metal PVD",711,"GPF451310P001G000","8055261227378"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",707,"Black Metal Brushed PVD",758,"GPF451310P004G000","8055261227361"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","030","Copper PVD",711,"GPF451310P000G000","8055261227385"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",708,"Copper Brushed PVD",758,"GPF451310P006G000","8055261227347"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",735,"Warm Bronze PVD",711,"GPF451310P037G000","8055261227286"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",726,"Warm Bronze Brushed PVD",758,"GPF451310P024G000","8055261227309"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",761,"Coffee Bronze Brushed PVD",806,"GPF451310E059G000","8055261577398"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",710,"Brass PVD",711,"GPF451310P011G000","8055261227323"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",727,"Brass Brushed PVD",758,"GPF451310P025G000","8055261227293"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",246,"Gold PVD",807,"GPF451310P007G000","8055261227330"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",716,"Gold Brushed PVD",807,"GPF451310P005G000","8055261227354"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",187,"Aged Bronze",758,"GPF451310G052G000","8055261227392"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",713,"Antique Brass",758,"GPF451310V204G000","8055261227279"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",279,"Matte White",648,"GPF451310C071G000","8055261236226"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.","031","Chrome",940,"GPF451220G001G000","8056603616072"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1268,"GPF451220G002G000","8056603616065"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",299,"Matte Black",1268,"GPF451220C072G000","8056603616089"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",720,"Nickel PVD",1390,"GPF451220P014G000","8056603615976"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1390,"GPF451220P001G000","8056603616027"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1482,"GPF451220P004G000","8056603616010"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.","030","Copper PVD",1390,"GPF451220P000G000","8056603616034"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1482,"GPF451220P006G000","8056603616003"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1390,"GPF451220P037G000","8056603615945"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1482,"GPF451220P024G000","8056603615969"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1579,"GPF451220E059G000","8055261577473"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1390,"GPF451220P011G000","8056603615983"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1482,"GPF451220P025G000","8056603615952"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",246,"Gold PVD",1579,"GPF451220P007G000","8056603615990"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",716,"Gold Brushed PVD",1579,"GPF451220P005G000","8055261186811"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",187,"Aged Bronze",1482,"GPF451220G052G000","8056603616041"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",713,"Antique Brass",1482,"GPF451220V204G000","8056603615938"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",279,"Matte White",1268,"GPF451220C071G000","8056603616096"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI","031","Chrome",880,"GPF755270G001G000","8055261645530"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",149,"Finox Brushed Nickel",1189,"GPF755270G002G000","8055261645523"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",299,"Matte Black",1189,"GPF755270C072G000","8055261645561"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",720,"Nickel PVD",1303,"GPF755270P014G000","8055261645462"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",706,"Black Metal PVD",1303,"GPF755270P001G000","8055261645509"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",707,"Black Metal Brushed PVD",1390,"GPF755270P004G000","8055261645493"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI","030","Copper PVD",1303,"GPF755270P000G000","8055261645516"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",708,"Copper Brushed PVD",1390,"GPF755270P006G000","8055261645486"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",735,"Warm Bronze PVD",1303,"GPF755270P037G000","8055261645431"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",726,"Warm Bronze Brushed PVD",1390,"GPF755270P024G000","8055261645455"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",761,"Coffee Bronze Brushed PVD",1478,"GPF755270E059G000","8055261645547"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",710,"Brass PVD",1303,"GPF755270P011G000","8055261645479"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",727,"Brass Brushed PVD",1390,"GPF755270P025G000","8055261645448"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",845,"Dark Bronze",1390,"GPF755270V221G000","8055261645424"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","031","Chrome",785,"GPF452270G001G000","8055261645837"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1060,"GPF452270G002G000","8055261645820"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",299,"Matte Black",1060,"GPF452270C072G000","8055261645868"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",720,"Nickel PVD",1161,"GPF452270P014G000","8055261645769"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1161,"GPF452270P001G000","8055261645806"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1240,"GPF452270P004G000","8055261645790"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","030","Copper PVD",1161,"GPF452270P000G000","8055261645813"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1240,"GPF452270P006G000","8055261645783"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1161,"GPF452270P037G000","8055261645738"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1240,"GPF452270P024G000","8055261645752"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1319,"GPF452270E059G000","8055261645844"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1161,"GPF452270P011G000","8055261645776"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1240,"GPF452270P025G000","8055261645745"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",845,"Dark Bronze",1240,"GPF452270V221G000","8055261645721"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","031","Chrome",779,"GPF451240G001G000","8056603615907"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1051,"GPF451240G002G000","8056603615891"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",299,"Matte Black",1051,"GPF451240C072G000","8056603615914"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",720,"Nickel PVD",1152,"GPF451240P014G000","8056603615785"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1152,"GPF451240P001G000","8056603615839"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1230,"GPF451240P004G000","8056603615822"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","030","Copper PVD",1152,"GPF451240P000G000","8056603615846"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1230,"GPF451240P006G000","8056603615815"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1152,"GPF451240P037G000","8056603615754"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1230,"GPF451240P024G000","8056603615778"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1309,"GPF451240E059G000","8055261577459"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1152,"GPF451240P011G000","8056603615792"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1230,"GPF451240P025G000","8056603615761"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",246,"Gold PVD",1307,"GPF451240P007G000","8056603615808"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",716,"Gold Brushed PVD",1307,"GPF451240P005G000","8055261230972"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",187,"Aged Bronze",1230,"GPF451240G052G000","8056603615853"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",713,"Antique Brass",1230,"GPF451240V204G000","8056603615747"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",279,"Matte White",1051,"GPF451240C071G000","8056603615921"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","031","Chrome",857,"GPF452260G001G000","8055261645981"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1157,"GPF452260G002G000","8055261645974"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",299,"Matte Black",1157,"GPF452260C072G000","8055261646018"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",720,"Nickel PVD",1267,"GPF452260P014G000","8055261645912"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1267,"GPF452260P001G000","8055261645950"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1354,"GPF452260P004G000","8055261645943"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","030","Copper PVD",1267,"GPF452260P000G000","8055261645967"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1354,"GPF452260P006G000","8055261645936"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1267,"GPF452260P037G000","8055261645882"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1354,"GPF452260P024G000","8055261645905"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1439,"GPF452260E059G000","8055261645998"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1267,"GPF452260P011G000","8055261645929"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1354,"GPF452260P025G000","8055261645899"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",845,"Dark Bronze",1354,"GPF452260V221G000","8055261645875"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","031","Chrome",779,"GPF451260G001G000","8056603633000"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1051,"GPF451260G002G000","8056603632997"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",299,"Matte Black",1051,"GPF451260C072G000","8056603633017"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",720,"Nickel PVD",1152,"GPF451260P014G000","8056603632881"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1152,"GPF451260P001G000","8056603632935"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1230,"GPF451260P004G000","8056603632928"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","030","Copper PVD",1152,"GPF451260P000G000","8056603632942"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1230,"GPF451260P006G000","8056603632911"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1152,"GPF451260P037G000","8056603632850"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1230,"GPF451260P024G000","8056603632874"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1309,"GPF451260E059G000","8055261577435"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1152,"GPF451260P011G000","8056603632898"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1230,"GPF451260P025G000","8056603632867"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",246,"Gold PVD",1307,"GPF451260P007G000","8056603632904"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",716,"Gold Brushed PVD",1307,"GPF451260P005G000","8056603695046"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",187,"Aged Bronze",1230,"GPF451260G052G000","8056603632959"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",713,"Antique Brass",1230,"GPF451260V204G000","8056603632843"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",279,"Matte White",1051,"GPF451260C071G000","8056603633024"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.","031","Chrome",891,"GPF591511G001G000","8056329057715"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",149,"Finox Brushed Nickel",1201,"GPF591511G002G000","8056329057708"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",299,"Matte Black",1201,"GPF591511C072G000","8056329057722"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",720,"Nickel PVD",1317,"GPF591511P014G000","8056603605656"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",706,"Black Metal PVD",1317,"GPF591511P001G000","8056329057647"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",707,"Black Metal Brushed PVD",1406,"GPF591511P004G000","8056329057623"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.","030","Copper PVD",1317,"GPF591511P000G000","8056329057654"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",708,"Copper Brushed PVD",1406,"GPF591511P006G000","8056329057609"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",735,"Warm Bronze PVD",1317,"GPF591511P037G000","8056329593497"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1406,"GPF591511P024G000","8056329057586"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1497,"GPF591511E059G000","8055261577374"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",710,"Brass PVD",1317,"GPF591511P011G000","8056329593503"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",727,"Brass Brushed PVD",1406,"GPF591511P025G000","8056329057579"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",279,"Matte White",1201,"GPF591511C071G000","8056329057739"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",717,"GPF591531G001G000","8056329057548"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",966,"GPF591531G002G000","8056329057531"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",299,"Matte Black",966,"GPF591531C072G000","8056329057555"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",720,"Nickel PVD",1059,"GPF591531P014G000","8056603605632"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",706,"Black Metal PVD",1059,"GPF591531P001G000","8056329057470"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",707,"Black Metal Brushed PVD",1127,"GPF591531P004G000","8056329057456"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","030","Copper PVD",1059,"GPF591531P000G000","8056329057487"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",708,"Copper Brushed PVD",1127,"GPF591531P006G000","8056329057432"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",735,"Warm Bronze PVD",1059,"GPF591531P037G000","8056329593459"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",726,"Warm Bronze Brushed PVD",1127,"GPF591531P024G000","8056329057418"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1205,"GPF591531E059G000","8055261577350"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",710,"Brass PVD",1059,"GPF591531P011G000","8056329593466"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",727,"Brass Brushed PVD",1127,"GPF591531P025G000","8056329057401"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",279,"Matte White",966,"GPF591531C071G000","8056329057562"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",717,"GPF144310G001G000","8055261646131"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",967,"GPF144310G002G000","8055261646124"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",299,"Matte Black",967,"GPF144310C072G000","8055261646162"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",720,"Nickel PVD",1060,"GPF144310P014G000","8055261646063"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",706,"Black Metal PVD",1060,"GPF144310P001G000","8055261646100"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",707,"Black Metal Brushed PVD",1133,"GPF144310P004G000","8055261646094"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","030","Copper PVD",1060,"GPF144310P000G000","8055261646117"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",708,"Copper Brushed PVD",1133,"GPF144310P006G000","8055261646087"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",735,"Warm Bronze PVD",1060,"GPF144310P037G000","8055261646032"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",726,"Warm Bronze Brushed PVD",1133,"GPF144310P024G000","8055261646056"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1205,"GPF144310E059G000","8055261646148"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",710,"Brass PVD",1060,"GPF144310P011G000","8055261646070"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",727,"Brass Brushed PVD",1133,"GPF144310P025G000","8055261646049"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",845,"Dark Bronze",1133,"GPF144310V221G000","8055261646025"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",650,"GPF143313G001G000","8022692049831"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",878,"GPF143313G002G000","8022692792669"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",299,"Matte Black",878,"GPF143313C072G000","8056329225343"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",147,"Chome Brushed",878,"GPF143313G006G000","8056329082557"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",720,"Nickel PVD",963,"GPF143313P014G000","8056603635639"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",706,"Black Metal PVD",963,"GPF143313P001G000","8056603447171"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",707,"Black Metal Brushed PVD",1029,"GPF143313P004G000","8056329192676"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","030","Copper PVD",963,"GPF143313P000G000","8056329545854"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",708,"Copper Brushed PVD",1029,"GPF143313P006G000","8056329183179"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",735,"Warm Bronze PVD",963,"GPF143313P037G000","8056603635646"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",726,"Warm Bronze Brushed PVD",1029,"GPF143313P024G000","8056329723795"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1092,"GPF143313E059G000","8055261577916"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",710,"Brass PVD",963,"GPF143313P011G000","8056329542099"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",727,"Brass Brushed PVD",1029,"GPF143313P025G000","8056329191044"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",246,"Gold PVD",1092,"GPF143313P007G000","8056329223974"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",716,"Gold Brushed PVD",1092,"GPF143313P005G000","8056329625204"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",187,"Aged Bronze",1029,"GPF143313G052G000","8056603507691"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",713,"Antique Brass",1029,"GPF143313V204G000","8056603507707"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12","031","Chrome",659,"GPF756110G001G000","8055261447370"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",149,"Finox Brushed Nickel",890,"GPF756110G002G000","8055261447363"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",299,"Matte Black",890,"GPF756110C072G000","8055261447387"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",706,"Black Metal PVD",976,"GPF756110P001G000","8055261447332"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",707,"Black Metal Brushed PVD",1042,"GPF756110P004G000","8055261447325"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12","030","Copper PVD",976,"GPF756110P000G000","8055261447349"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",708,"Copper Brushed PVD",1042,"GPF756110P006G000","8055261447301"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",735,"Warm Bronze PVD",976,"GPF756110P037G000","8055261447240"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",726,"Warm Bronze Brushed PVD",1042,"GPF756110P024G000","8055261447264"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",720,"Nickel PVD",976,"GPF756110P014G000","8055261447271"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",761,"Coffee Bronze Brushed PVD",1107,"GPF756110E059G000","8055261570108"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",710,"Brass PVD",976,"GPF756110P011G000","8055261447288"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",727,"Brass Brushed PVD",1042,"GPF756110P025G000","8055261447257"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75611,75611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",845,"Dark Bronze",1042,"GPF756110V221G000","8055261447226"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.","031","Chrome",1031,"GPF756130G001G000","8055261447202"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",149,"Finox Brushed Nickel",1392,"GPF756130G002G000","8055261447196"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",299,"Matte Black",1392,"GPF756130C072G000","8055261447219"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",706,"Black Metal PVD",1526,"GPF756130P001G000","8055261447165"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",707,"Black Metal Brushed PVD",1630,"GPF756130P004G000","8055261447158"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.","030","Copper PVD",1526,"GPF756130P000G000","8055261447172"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",708,"Copper Brushed PVD",1630,"GPF756130P006G000","8055261447134"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",735,"Warm Bronze PVD",1526,"GPF756130P037G000","8055261447073"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",726,"Warm Bronze Brushed PVD",1630,"GPF756130P024G000","8055261447097"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",720,"Nickel PVD",1526,"GPF756130P014G000","8055261447103"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",761,"Coffee Bronze Brushed PVD",1731,"GPF756130E059G000","8055261570085"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",710,"Brass PVD",1526,"GPF756130P011G000","8055261447110"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",727,"Brass Brushed PVD",1630,"GPF756130P025G000","8055261447080"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75613,75613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",845,"Dark Bronze",1630,"GPF756130V221G000","8055261447059"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.","031","Chrome",629,"GPF756150G001G000","8055261447035"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",149,"Finox Brushed Nickel",850,"GPF756150G002G000","8055261447028"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",299,"Matte Black",850,"GPF756150C072G000","8055261447042"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",706,"Black Metal PVD",931,"GPF756150P001G000","8055261446991"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",707,"Black Metal Brushed PVD",994,"GPF756150P004G000","8055261446984"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.","030","Copper PVD",931,"GPF756150P000G000","8055261447004"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",708,"Copper Brushed PVD",994,"GPF756150P006G000","8055261446960"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",735,"Warm Bronze PVD",931,"GPF756150P037G000","8055261446908"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",726,"Warm Bronze Brushed PVD",994,"GPF756150P024G000","8055261446922"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",720,"Nickel PVD",931,"GPF756150P014G000","8055261446939"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",761,"Coffee Bronze Brushed PVD",1057,"GPF756150E059G000","8055261570061"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",710,"Brass PVD",931,"GPF756150P011G000","8055261446946"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",727,"Brass Brushed PVD",994,"GPF756150P025G000","8055261446915"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75615,75615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",845,"Dark Bronze",994,"GPF756150V221G000","8055261446885"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE","031","Chrome",702,"GPF756170G001G000","8055261446861"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",149,"Finox Brushed Nickel",948,"GPF756170G002G000","8055261446854"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",299,"Matte Black",948,"GPF756170C072G000","8055261446878"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",706,"Black Metal PVD",1038,"GPF756170P001G000","8055261446823"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",707,"Black Metal Brushed PVD",1109,"GPF756170P004G000","8055261446816"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE","030","Copper PVD",1038,"GPF756170P000G000","8055261446830"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",708,"Copper Brushed PVD",1109,"GPF756170P006G000","8055261446793"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",735,"Warm Bronze PVD",1038,"GPF756170P037G000","8055261446731"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",726,"Warm Bronze Brushed PVD",1109,"GPF756170P024G000","8055261446755"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",720,"Nickel PVD",1038,"GPF756170P014G000","8055261446762"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",761,"Coffee Bronze Brushed PVD",1180,"GPF756170E059G000","8055261570047"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",710,"Brass PVD",1038,"GPF756170P011G000","8055261446779"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",727,"Brass Brushed PVD",1109,"GPF756170P025G000","8055261446748"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75617,75617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",845,"Dark Bronze",1109,"GPF756170V221G000","8055261446717"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","031","Chrome",915,"GPF756190G001G000","8055261446694"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",149,"Finox Brushed Nickel",1235,"GPF756190G002G000","8055261446687"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",299,"Matte Black",1235,"GPF756190C072G000","8055261446700"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",706,"Black Metal PVD",1354,"GPF756190P001G000","8055261446656"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",707,"Black Metal Brushed PVD",1445,"GPF756190P004G000","8055261446649"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","030","Copper PVD",1354,"GPF756190P000G000","8055261446663"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",708,"Copper Brushed PVD",1445,"GPF756190P006G000","8055261446625"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",735,"Warm Bronze PVD",1354,"GPF756190P037G000","8055261446564"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",726,"Warm Bronze Brushed PVD",1445,"GPF756190P024G000","8055261446588"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",720,"Nickel PVD",1354,"GPF756190P014G000","8055261446595"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",761,"Coffee Bronze Brushed PVD",1537,"GPF756190E059G000","8055261570023"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",710,"Brass PVD",1354,"GPF756190P011G000","8055261446601"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",727,"Brass Brushed PVD",1445,"GPF756190P025G000","8055261446571"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75619,75619,"Bedieningsplaat SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",845,"Dark Bronze",1445,"GPF756190V221G000","8055261446540"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.","031","Chrome",1159,"GPF756210G001G000","8055261446526"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",149,"Finox Brushed Nickel",1565,"GPF756210G002G000","8055261446519"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",299,"Matte Black",1565,"GPF756210C072G000","8055261446533"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",706,"Black Metal PVD",1715,"GPF756210P001G000","8055261446489"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",707,"Black Metal Brushed PVD",1831,"GPF756210P004G000","8055261446472"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.","030","Copper PVD",1715,"GPF756210P000G000","8055261446496"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",708,"Copper Brushed PVD",1831,"GPF756210P006G000","8055261446458"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",735,"Warm Bronze PVD",1715,"GPF756210P037G000","8055261446397"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",726,"Warm Bronze Brushed PVD",1831,"GPF756210P024G000","8055261446410"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",720,"Nickel PVD",1715,"GPF756210P014G000","8055261446427"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",761,"Coffee Bronze Brushed PVD",1948,"GPF756210E059G000","8055261570009"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",710,"Brass PVD",1715,"GPF756210P011G000","8055261446434"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",727,"Brass Brushed PVD",1831,"GPF756210P025G000","8055261446403"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",75621,75621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",845,"Dark Bronze",1831,"GPF756210V221G000","8055261446373"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39115,39115,"Wandbidet van Keramiek met overloop. Met centraal gat voor kraanwerk. Dop overloop en laterale gatafdekkingen opgenomen in afwerking 031.","Bidet suspendu en Céramique Blanc Europe avec vidage et trop plein, percé monotrou pour la robinetterie, fourni avec cache de trop plein et enjoliveurs latéraux en finition 031.","Wall hung bidet in in White Europe Ceramic with overflow waste, with central hole for taps and fittings. Overflow cap and side covering caps included in 031 finishing",518,"White Ceramic",769,"GPF391150C083G000","8022692785302"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39115,39115,"Wandbidet van Keramiek met overloop. Met centraal gat voor kraanwerk. Dop overloop en laterale gatafdekkingen opgenomen in afwerking 031.","Bidet suspendu en Céramique Blanc Europe avec vidage et trop plein, percé monotrou pour la robinetterie, fourni avec cache de trop plein et enjoliveurs latéraux en finition 031.","Wall hung bidet in in White Europe Ceramic with overflow waste, with central hole for taps and fittings. Overflow cap and side covering caps included in 031 finishing",531,"Matte White Ceramic",1152,"GPF391150C288G000","8056329052529"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",39115,39115,"Wandbidet van Keramiek met overloop. Met centraal gat voor kraanwerk. Dop overloop en laterale gatafdekkingen opgenomen in afwerking 031.","Bidet suspendu en Céramique Blanc Europe avec vidage et trop plein, percé monotrou pour la robinetterie, fourni avec cache de trop plein et enjoliveurs latéraux en finition 031.","Wall hung bidet in in White Europe Ceramic with overflow waste, with central hole for taps and fittings. Overflow cap and side covering caps included in 031 finishing",532,"Matte Black Ceramic",1152,"GPF391150C289G000","8056329052536"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs","031","Chrome",93,"GPF375870G001G000","8022692536119"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",149,"Finox Brushed Nickel",125,"GPF375870G002G000","8022692796995"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",299,"Matte Black",125,"GPF375870C072G000","8056329006317"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",147,"Chome Brushed",125,"GPF375870G006G000","8022692536164"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",720,"Nickel PVD",146,"GPF375870P014G000","8056603457026"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",706,"Black Metal PVD",146,"GPF375870P001G000","8022692674347"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",707,"Black Metal Brushed PVD",154,"GPF375870P004G000","8022692430561"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs","030","Copper PVD",146,"GPF375870P000G000","8022692654813"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",708,"Copper Brushed PVD",154,"GPF375870P006G000","8022692430578"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",735,"Warm Bronze PVD",146,"GPF375870P037G000","8056329558731"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",726,"Warm Bronze Brushed PVD",154,"GPF375870P024G000","8056329006300"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",761,"Coffee Bronze Brushed PVD",165,"GPF375870E059G000","8055261577510"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",710,"Brass PVD",146,"GPF375870P011G000","8056329609174"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",727,"Brass Brushed PVD",154,"GPF375870P025G000","8056329081987"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",246,"Gold PVD",165,"GPF375870P007G000","8056329097599"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",716,"Gold Brushed PVD",165,"GPF375870P005G000","8022692833676"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",187,"Aged Bronze",154,"GPF375870G052G000","8056329008755"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",713,"Antique Brass",154,"GPF375870V204G000","8056329055544"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01375","01375","Sifon Bidet","Siphon Bidet","Syphon Bidet","031","Chrome",194,"GPF013750G001G000","8022692018905"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01375","01375","Sifon Bidet","Siphon Bidet","Syphon Bidet",149,"Finox Brushed Nickel",381,"GPF013750G002G000","8022692786293"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01375","01375","Sifon Bidet","Siphon Bidet","Syphon Bidet",299,"Matte Black",381,"GPF013750C072G000","8022692120851"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01375","01375","Sifon Bidet","Siphon Bidet","Syphon Bidet",147,"Chome Brushed",381,"GPF013750G006G000","8022692120820"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01375","01375","Sifon Bidet","Siphon Bidet","Syphon Bidet",720,"Nickel PVD",420,"GPF013750P014G000","8056603569828"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01375","01375","Sifon Bidet","Siphon Bidet","Syphon Bidet",706,"Black Metal PVD",420,"GPF013750P001G000","8056329039872"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01375","01375","Sifon Bidet","Siphon Bidet","Syphon Bidet",707,"Black Metal Brushed PVD",455,"GPF013750P004G000","8056329008113"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",28767,28767,"Verlengstuk buis voor sifon, lengte 40 cm","Tubelure prolongée pour siphone, longueur 40 cm","Syphon pipe extension, 40 cm length",707,"Black Metal Brushed PVD",88,"GPF287670P004G000","8056329104259"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK",54605,54605,"Opzetwastafel in roestvrij staal zonder overloop 400x400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 400x400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 400x400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",707,"Black Metal Brushed PVD",3957,"GPF546050P004G000","8056329224971"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.","031","Chrome",60,"GPF014210G001G000","8056603964326"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",727,"Brass Brushed PVD",169,"GPF014210P025G000","8056603964173"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01410","01410","Sifon van 1 1/4\"","Siphon 1 1/4”.","1 1/4\" syphon",720,"Nickel PVD",556,"GPF014100P014G000","8022692656169"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01377","01377","1 1/4\" sifon","Siphon 1 1/4”.","1 1/4\" syphon",761,"Coffee Bronze Brushed PVD",482,"GPF013771E059G000","8055261577992"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01412","01412","Hoekstopkraan onder wastafel met filter en aansluiting van 1/2\"","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection",761,"Coffee Bronze Brushed PVD",397,"GPF014120E059G000","8055261577930"]
["BATHROOM","INCASTRI","INCASTRI TOTAL LOOK","01411","01411","Onderbouwmengkraan met filter en 1/2\" aansluiting","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection","031","Chrome",103,"GPF014110G001G000","8022692037494"]
["BATHROOM","INCASTRI","INCASTRI HANDLES AREA",75540,75540,"Set van 2 bennendeurkrukken met terugstelveer en patentrozet. Met vierkante stift, compatibel met 7/8/9 mm vierkante stiftsloten.","Jeu de 2 poignées de porte intérieur avec ressort de rappel et rosace de type Patent. Avec fer carré, compatible avec les serrures carrées 7/8/9 mm.","Set of 2 internal door handles with return spring and Patent-type escutcheon. With square spindle, compatible with 7/8/9 mm square spindle locks.",726,"Warm Bronze Brushed PVD",771,"GPF755400P024G000","8055261436756"]
["BATHROOM","INCASTRI","INCASTRI HANDLES AREA",75542,75542,"Set van 2 binnendeurklinken met terugstelveer. Met vierkante stift, compatibel met 7/8/9 mm vierkante stiftsloten.","Jeu de 2 poignées de porte intérieur avec ressort de rappel. Avec fer carré, compatible avec les serrures carrées 7/8/9 mm.","Set of 2 internal door handles with return spring. With square spindle, compatible with 7/8/9 mm square spindle locks.",727,"Brass Brushed PVD",675,"GPF755420P025G000","8055261436480"]
["BATHROOM","INCASTRI","INCASTRI HANDLES AREA",75630,75630,"Dubbele handgreep 20 cm voor glas/hout. Verticale/Horizontale montage.","Double poignée pour verre/bois 20 cm. Installation verticale/horizontale.","Double handle 20 cm for glass/wood. Vertical/Horizontal installation.",707,"Black Metal Brushed PVD",1302,"GPF756300P004G000","8055261494022"]
["BATHROOM","INCASTRI","INCASTRI HANDLES AREA",75631,75631,"Dubbele handgreep 30 cm voor glas/hout. Verticale/Horizontale montage.","Double poignée pour verre/bois 30 cm. Installation verticale/horizontale.","Double handle 30 cm for glass/wood. Vertical/Horizontal installation.",720,"Nickel PVD",1444,"GPF756310P014G000","8055261493865"]
["BATHROOM","INCASTRI","INCASTRI HANDLES AREA",75632,75632,"Dubbele handgreep 45 cm voor glas/hout. Verticale/Horizontale montage.","Double poignée pour verre/bois 45 cm. Installation verticale/horizontale.","Double handle 45 cm for glass/wood. Vertical/Horizontal installation.",720,"Nickel PVD",1760,"GPF756320P014G000","8055261493735"]
["BATHROOM","INCASTRI","INCASTRI HANDLES AREA",75633,75633,"Dubbele handgreep 60 cm voor glas/hout. Verticale/Horizontale montage.","Double poignée pour verre/bois 60 cm. Installation verticale/horizontale.","Double handle 60 cm for glass/wood. Vertical/Horizontal installation.",727,"Brass Brushed PVD",2023,"GPF756330P025G000","8055261493582"]
["BATHROOM","INCASTRI","INCASTRI HANDLES AREA",75635,75635,"Stanggreep 30 cm voor hout. Verticale/Horizontale montage.","Poignée à barre pour bois 30 cm. Installation verticale/horizontale.","Bar handle 30 cm for wood. Vertical/Horizontal installation.",707,"Black Metal Brushed PVD",1013,"GPF756350P004G000","8055261493377"]
["BATHROOM","INCASTRI","INCASTRI HANDLES AREA",75637,75637,"Stanggreep 60 cm voor hout. Verticale/Horizontale montage.","Poignée à barre pour bois 60 cm. Installation verticale/horizontale.","Bar handle 60 cm for wood. Vertical/Horizontal installation.",727,"Brass Brushed PVD",1234,"GPF756370P025G000","8055261493063"]
["BATHROOM","INVERSO","INVERSO RIGATO",73502,73502,"Wastafelmengkraan, zonder plug, met flexibele slangen. RIGATO.","Mitigeur lavabo, sans vidage, avec flexibles de raccordement. RIGATO.","Basin mixer without waste, with connecting flexibles. RIGATO.",710,"Brass PVD",781,"GPF735020P011G000","8056603948647"]
["BATHROOM","INVERSO","INVERSO RIGATO",73555,73555,"Medium versie Wastafelmengkraan, met vaste plug, met flexibele slangen. RIGATO.","Mitigeur lavabo moyen, avec bonde \"Stop&Go\" et flexibles de raccordement. RIGATO.","Medium version basin mixer with Stop&Go waste and connecting flexibles. RIGATO.",710,"Brass PVD",948,"GPF735550P011G000","8056603962803"]
["BATHROOM","INVERSO","INVERSO RIGATO",73553,73553,"Hoge versie Wastafelmengkraan, met vaste plug, met flexibele slangen. RIGATO.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement. RIGATO.","High version basin mixer with Stop&Go waste and connecting flexibles. RIGATO.","031","Chrome",687,"GPF735530G001G000","8056603963022"]
["BATHROOM","INVERSO","INVERSO RIGATO","63397+73588",73588,"Afbouwdeel wandgemonteerde wastafelmengkraan. RIGATO.","Partie apparente mitigeur lavabo mural. RIGATO.","External part wall-mounted basin mixer. RIGATO.",149,"Finox Brushed Nickel",808,"GPF735880G002G000","8056603946759"]
["BATHROOM","INVERSO","INVERSO RIGATO",73104,73104,"Wandgemonteerde wastafelmengkraan, lengte op aanvraag.","Bec lavabo mural avec longueur à la demande.","Wall-mounted basin spout, length on request.",735,"Warm Bronze PVD",1127,"GPF731040P037G000","8056603948906"]
["BATHROOM","INVERSO","INVERSO RIGATO",20099,20099,"Plafonduitloop. Aan te vullen met afstandsbediening","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout to be completed with separate control",299,"Matte Black",1304,"GPF200990C072G000","8022692047929"]
["BATHROOM","INVERSO","INVERSO RIGATO","63412+73509",73509,"Wandgemonteerde 1-weg wastafelmengkraan. RIGATO.","Partie apparente mitigeur lavabo mural une sortie. RIGATO.","Wall-mounted one-way basin mixer. RIGATO.",706,"Black Metal PVD",380,"GPF735090P001G000","8056603948074"]
["BATHROOM","INVERSO","INVERSO RIGATO","46189+73595",73595,"Afbouwdeel vrijstaande wastafelmengkraan. RIGATO.","Partie apparente mitigeur lavabo au sol. RIGATO.","External part freestanding basin mixer. RIGATO.","030","Copper PVD",2512,"GPF735950P000G000","8056603946582"]
["BATHROOM","INVERSO","INVERSO RIGATO",73103,73103,"Wandgemonteerde bad uitloop.","Bec de baignoire mural.","Wall-mounted bath spout.","031","Chrome",362,"GPF731030G001G000","8056603949163"]
["BATHROOM","INVERSO","INVERSO RIGATO","54139+73536",73536,"Afbouwdeel wandgemonteerde 2-weg douche mengkraan met omstel en anti-kalk handdouche. RIGATO.","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire. RIGATO.","External part wall-mounted two-ways shower mixer with diverter and antilimestone handshower. RIGATO.",761,"Coffee Bronze Brushed PVD",1542,"GPF735360E059G000","8055261582309"]
["BATHROOM","INVERSO","INVERSO RIGATO","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",708,"Copper Brushed PVD",388,"GPF540580P006G000","8056329025714"]
["BATHROOM","INVERSO","INVERSO RIGATO","54073+73538",73538,"Afbouwdeel wandgemonteerde 2-weg douche mengkraan. RIGATO.","Partie apparente pour mitigeur douche murale 2 sorties. RIGATO.","External part wall-mounted two-ways shower mixer. RIGATO.",149,"Finox Brushed Nickel",858,"GPF735380G002G000","8056603947053"]
["BATHROOM","INVERSO","INVERSO RIGATO","54169+73032",73032,"Afbouwdeel wandgemonteerde 1-weg thermostatisch douche mengkraan.","Partie apparente pour mitigeur thermostatique douche mural 1 sortie.","External part wall-mounted one-way thermostatic shower mixer.",735,"Warm Bronze PVD",1176,"GPF730320P037G000","8056603968478"]
["BATHROOM","INVERSO","INVERSO RIGATO","54169+73036",73036,"Afbouwdeel wandgemonteerde 3-weg thermostatisch douche mengkraan.","Partie apparente pour mitigeur thermostatique douche mural 3 sorties.","External part wall-mounted three-ways thermostatic shower mixer.",707,"Black Metal Brushed PVD",1256,"GPF730360P004G000","8056603968232"]
["BATHROOM","INVERSO","INVERSO RIGATO","09269+73533",73533,"afbouwdeel voor 1-uitgang thermostatische mengkraan.","Partie apparente pour mitigeur thermostatique mural 1 sortie.","External part for 1-outlet thermostatic mixer.",708,"Copper Brushed PVD",1392,"GPF735330P006G000","8055261232198"]
["BATHROOM","INVERSO","INVERSO RIGATO","09269+73535",73535,"afbouwdeel voor 2-uitgang thermostatische mengkraan.","Partie apparente pour mitigeur thermostatique mural 2 sortie.","External part for 2-outlet thermostatic mixer.",726,"Warm Bronze Brushed PVD",1392,"GPF735350P024G000","8055261232020"]
["BATHROOM","INVERSO","INVERSO RIGATO",73541,73541,"Glijstang met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang. RIGATO.","Barre de douche complète avec sortie coudée murale, douchette anticalcaire et flexible 1,50 m. RIGATO.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose. RIGATO.",706,"Black Metal PVD",1363,"GPF735410P001G000","8056603967495"]
["BATHROOM","INVERSO","INVERSO RIGATO",63584,63584,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m. RIGATO.","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m. RIGATO.","Sliding rail with antilimestone handshower, 1,50 m flexible hose. RIGATO.",726,"Warm Bronze Brushed PVD",1166,"GPF635840P024G000","8056329569713"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO",73602,73602,"Wastafelmengkraan, zonder plug, met flexibele slangen. DIAMANTATO.","Mitigeur lavabo, sans vidage, avec flexibles de raccordement. DIAMANTATO.","Basin mixer without waste, with connecting flexibles. DIAMANTATO.",735,"Warm Bronze PVD",781,"GPF736020P037G000","8056603946209"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO",73606,73606,"Medium versie Wastafelmengkraan, zonder plug, met flexibele slangen. DIAMANTATO.","Mitigeur lavabo moyen, sans vidage, avec flexibles de raccordement. DIAMANTATO.","Medium version basin mixer without waste, with connecting flexibles. DIAMANTATO.",299,"Matte Black",834,"GPF736060C072G000","8056603958714"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO",73653,73653,"Hoge versie Wastafelmengkraan, met vaste plug, met flexibele slangen. DIAMANTATO.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement. DIAMANTATO.","High version basin mixer with Stop&Go waste and connecting flexibles. DIAMANTATO.",761,"Coffee Bronze Brushed PVD",1154,"GPF736530E059G000","8055261581807"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO","63397+73688",73688,"Afbouwdeel wandgemonteerde wastafelmengkraan. DIAMANTATO.","Partie apparente mitigeur lavabo mural. DIAMANTATO.","External part wall-mounted basin mixer. DIAMANTATO.","031","Chrome",598,"GPF736880G001G000","8056603944519"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO",73102,73102,"Wandgemonteerde wastafel uitloop.","Bec lavabo mural.","Wall-mounted basin spout.",761,"Coffee Bronze Brushed PVD",641,"GPF731020E059G000","8055261582569"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO",20199,20199,"Plafonduitloop aanpasbare hoogte. Aan te vullen met afstandsbediening","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout, length on request with separate control (not included)",720,"Nickel PVD",1855,"GPF201990P014G000","8056603608343"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO","63412+73609",73609,"Wandgemonteerde 1-weg wastafelmengkraan. DIAMANTATO.","Partie apparente mitigeur lavabo mural une sortie. DIAMANTATO.","Wall-mounted one-way basin mixer. DIAMANTATO.",726,"Warm Bronze Brushed PVD",405,"GPF736090P024G000","8056603945622"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO",73607,73607,"Bidet mengkraan met vaste plug, met flexibele slangen. DIAMANTATO.","Mitigeur bidet avec vidage et flexibles de raccordement. DIAMANTATO.","Bidet mixer with waste and connecting flexibles. DIAMANTATO.",727,"Brass Brushed PVD",872,"GPF736070P025G000","8056603945769"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO","46189+73628",73628,"afbouwdeel vrijstaande badmengkraan met omstel en antikalk handdouche. DIAMANTATO.","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire. DIAMANTATO.","External part freestanding bath mixer with automatic diverter and antilimestone handshower. DIAMANTATO.","030","Copper PVD",3391,"GPF736280P000G000","8056603945387"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO","54139+73636",73636,"Afbouwdeel wandgemonteerde 2-weg douche mengkraan met omstel en anti-kalk handdouche. DIAMANTATO.","Partie apparente pour mitigeur douche mural 2 sorties avec inverseur et douchette anticalcaire. DIAMANTATO.","External part wall-mounted two-ways shower mixer with diverter and antilimestone handshower. DIAMANTATO.",710,"Brass PVD",1357,"GPF736360P011G000","8056603944892"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO","54055+73619",73619,"Afbouwdeel wandgemonteerde 1-weg douche mengkraan. DIAMANTATO.","Partie apparente pour mitigeur douche murale 1 sortie. DIAMANTATO.","External part wall-mounted one-way shower mixer. DIAMANTATO.","031","Chrome",282,"GPF736190G001G000","8056603945561"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO","54073+73638",73638,"Afbouwdeel wandgemonteerde 2-weg douche mengkraan. DIAMANTATO.","Partie apparente pour mitigeur douche murale 2 sorties. DIAMANTATO.","External part wall-mounted two-ways shower mixer. DIAMANTATO.",149,"Finox Brushed Nickel",858,"GPF736380G002G000","8056603944809"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO","44673+73679",73679,"Afbouwdeel wandgemonteerde 2-weg mixer with automatic bath/shower diverter. DIAMANTATO.","Partie apparente pour mitigeur murale 2 sorties avec inverseur bain-douche. DIAMANTATO.","External part wall-mounted two-ways mixer with automatic bath/shower diverter. DIAMANTATO.",710,"Brass PVD",807,"GPF736790P011G000","8056603944595"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO","54169+73036",73036,"Afbouwdeel wandgemonteerde 3-weg thermostatisch douche mengkraan.","Partie apparente pour mitigeur thermostatique douche mural 3 sorties.","External part wall-mounted three-ways thermostatic shower mixer.","030","Copper PVD",1176,"GPF730360P000G000","8056603968256"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO","09269+73633",73633,"afbouwdeel voor 1-uitgang thermostatische mengkraan.","Partie apparente pour mitigeur thermostatique mural 1 sortie.","External part for 1-outlet thermostatic mixer.",727,"Brass Brushed PVD",1392,"GPF736330P025G000","8055261231733"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO","09269+73637",73637,"afbouwdeel voor 3-uitgang thermostatische mengkraan.","Partie apparente pour mitigeur thermostatique mural 3 sortie.","External part for 3-outlet thermostatic mixer.",149,"Finox Brushed Nickel",1190,"GPF736370G002G000","8055261231542"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO",73641,73641,"Glijstang met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang. DIAMANTATO.","Barre de douche complète avec sortie coudée murale, douchette anticalcaire et flexible 1,50 m. DIAMANTATO.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose. DIAMANTATO.",710,"Brass PVD",1363,"GPF736410P011G000","8056603967310"]
["BATHROOM","INVERSO","INVERSO DIAMANTATO",63485,63485,"Glijstang. DIAMANTATO.","Barre de douche. DIAMANTATO.","Sliding rail. DIAMANTATO.","031","Chrome",604,"GPF634850G001G000","8056329565012"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","09266+44336",44336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie externe mitigeur thermostatique mural à 3 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with three separate exits.",726,"Warm Bronze Brushed PVD",2069,"GPF443360P024G000","8056603620505"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","09263+44340",44340,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie externe mitigeur thermostatique mural à 5 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with five separate exits.",707,"Black Metal Brushed PVD",2574,"GPF443400P004G000","8056603630955"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","43103+43024",43024,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",299,"Matte Black",1889,"GPF430241C072G000","8022692628791"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","43105+43026",43026,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS","031","Chrome",1311,"GPF430261G001G000","8022692581010"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","43105+43026",43026,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",726,"Warm Bronze Brushed PVD",2750,"GPF430261P024G000","8056329608825"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","43107+43028",43028,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",707,"Black Metal Brushed PVD",3144,"GPF430281P004G000","8022692840285"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","43109+43030",43030,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",726,"Warm Bronze Brushed PVD",3472,"GPF430301P024G000","8056329046146"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","43109+43220",43220,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",710,"Brass PVD",3153,"GPF432201P011G000","8056329608337"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","43281+43252",43252,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente mitigeur THERMOSTATIQUE douche haut débit","External parts wall-mounted thermostatic high-capacity mixer",710,"Brass PVD",1020,"GPF432521P011G000","8056329608214"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","43283+43264",43264,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur haut débit.","External parts for stop valve for thermostatic high-capacity mixer.",720,"Nickel PVD",639,"GPF432640P014G000","8056603607605"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",33095,33095,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted shower head",238,"Mirror Steel",2499,"GPF330951A001G000","8022692365436"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63548,63548,"Oriënteerbare wand-hoofddouchekop RIGATO","Pomme de douche latérale orientable. RIGATO","Wall-mounted adjustable showerhead RIGATO",735,"Warm Bronze PVD",1932,"GPF635480P037G000","8056329563056"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63448,63448,"Oriënteerbare wand-hoofddouchekop DIAMANTATO","Pomme de douche latérale orientable. DIAMANTATO","Wall-mounted adjustable showerhead DIAMANTATO",735,"Warm Bronze PVD",1932,"GPF634480P037G000","8056329563384"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63452,63452,"Oriënteerbare plafond-hoofddouchekop DIAMANTATO","Pomme de douche au plafond orientable. DIAMANTATO","Ceiling-mounted adjustable showerhead DIAMANTATO",187,"Aged Bronze",1957,"GPF634520G052G000","8056329563223"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63450,63450,"Plafond-hoofddouchekop arm aanpasbare hoogte DIAMANTATO","Pomme de douche au plafond avec bras orientable, longueur à la DEMANDE. DIAMANTATO","Ceiling-mounted showerhead, length on request DIAMANTATO",706,"Black Metal PVD",2566,"GPF634500P001G000","8056329563315"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",707,"Black Metal Brushed PVD",1831,"GPF630450P004G000","8055261729643"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO",708,"Copper Brushed PVD",2503,"GPF637450P006G000","8055261728615"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63645,63645,"Verstelbare hoofddouche voor wandmontage. DIAMANTATO","Pomme de douche murale orientable. DIAMANTATO","Wall-mounted adjustable headshower. DIAMANTATO",845,"Dark Bronze",2503,"GPF636450V221G000","8055261729056"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",845,"Dark Bronze",1726,"GPF630500V221G000","8055261729391"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",710,"Brass PVD",2101,"GPF630530P011G000","8055261729285"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63653,63653,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. DIAMANTATO","Pomme de douche au plafond orientable, longueur à la demande. DIAMANTATO","Ceiling-mounted adjustable headshower, length on request. DIAMANTATO",707,"Black Metal Brushed PVD",3245,"GPF636530P004G000","8055261728790"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","031","Chrome",1488]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63549,63549,"Verstelbare hoofddouche aan de muur. RIGATO.","Pomme de douche latérale orientable. RIGATO.","Wall-mounted adjustable headshower. RIGATO.",187,"Aged Bronze",3179,"GPF635490G052G000","8055261241671"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",761,"Coffee Bronze Brushed PVD",2705,"GPF630680E059G000","8055261577312"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63568,63568,"Verstelbare hoofddouche aan de muur. RIGATO.","Pomme de douche latérale orientable. RIGATO.","Wall-mounted adjustable headshower. RIGATO.",761,"Coffee Bronze Brushed PVD",3584,"GPF635680E059G000","8055261591905"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63468,63468,"Verstelbare hoofddouche aan de muur. DIAMANTATO.","Pomme de douche latérale orientable. DIAMANTATO.","Wall-mounted adjustable headshower. DIAMANTATO.",706,"Black Metal PVD",3158,"GPF634680P001G000","8055261242104"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63572,63572,"Verstelbare plafonddouche. RIGATO.","Pomme de douche au plafond orientable. RIGATO.","Ceiling-mounted adjustable headshower. RIGATO.","031","Chrome",2012,"GPF635720G001G000","8055261241244"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",149,"Finox Brushed Nickel",2824]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63570,63570,"Verstelbare plafonddouche. lengte op aanvraag. RIGATO.","Pomme de douche au plafond avec bras orientable, longueur à la demande. RIGATO.","Ceiling-mounted adjustable headshower. Length on request. RIGATO.",710,"Brass PVD",3872,"GPF635700P011G000","8055261241329"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63470,63470,"Verstelbare plafonddouche. lengte op aanvraag. DIAMANTATO.","Pomme de douche au plafond avec bras orientable, longueur à la demande. DIAMANTATO.","Ceiling-mounted adjustable headshower. Length on request. DIAMANTATO.",726,"Warm Bronze Brushed PVD",4133,"GPF634700P024G000","8055261241909"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",59158,59158,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-fixing antilimestone and adjustable headshower",735,"Warm Bronze PVD",961,"GPF591580P037G000","8056329593398"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",59155,59155,"Antikalk-hoofddouchekop Plafonddouche oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead",726,"Warm Bronze Brushed PVD",918,"GPF591550P024G000","8056329029934"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",59159,59159,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",708,"Copper Brushed PVD",1378,"GPF591590P006G000","8056329037755"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",15186,15186,"Antikalk-hoofddouchekop plafond oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead",735,"Warm Bronze PVD",2340,"GPF151860P037G000","8056329614406"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",15199,15199,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",707,"Black Metal Brushed PVD",3315,"GPF151990P004G000","8022692157161"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",707,"Black Metal Brushed PVD",1029,"GPF329751P004G000","8022692832808"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",707,"Black Metal Brushed PVD",474,"GPF329730P004G000","8022692361322"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",735,"Warm Bronze PVD",685,"GPF329840P037G000","8056329609907"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",238,"Mirror Steel",1018,"GPF202950A001G000","8056329085732"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",73523,73523,"Douche set met water aansluitpunt, Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang.","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexible 1,50 m.","Shower set with water outlet, antilimestone handshower and 1,50 m flexible hose.",707,"Black Metal Brushed PVD",702,"GPF735230P004G000","8055261029163"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",707,"Black Metal Brushed PVD",1003,"GPF630990P004G000","8056329215986"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",73061,73061,"water aansluitpunt met houder voor handdouche.","Sortie coudée murale avec support fixe pour douchette.","Water outlet with handshower hook.",299,"Matte Black",340,"GPF730610C072G000","8056603967846"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",73057,73057,"vaste handdouche houder","Support fixe pour douchette.","Fixing handshower hook.",706,"Black Metal PVD",215,"GPF730570P001G000","8056603968096"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",726,"Warm Bronze Brushed PVD",438,"GPF329290P024G000","8055261227811"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",713,"Antique Brass",438,"GPF329290V204G000","8055261227781"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",708,"Copper Brushed PVD",235,"GPF143720P006G000","8056329037335"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",279,"Matte White",193,"GPF143700C071G000","8022692435191"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.","031","Chrome",206,"GPF143780G001G000","8056603633314"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",761,"Coffee Bronze Brushed PVD",367,"GPF143780E059G000","8055261609570"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",710,"Brass PVD",252,"GPF473510P011G000","8056603587037"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",726,"Warm Bronze Brushed PVD",269,"GPF473500P024G000","8056603587136"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",708,"Copper Brushed PVD",120,"GPF016370P006G000","8022692092233"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",708,"Copper Brushed PVD",150,"GPF541370P006G000","8022692850178"]
["BATHROOM","INVERSO","INVERSO BATH-SHOWER","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",726,"Warm Bronze Brushed PVD",162,"GPF017240P024G000","8055261240018"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20801,20801,"Wand-zeepbakje wit","Porte-savon mural blanc.","Wall-mounted soap dish, white",735,"Warm Bronze PVD",491,"GPF208011P037G000","8056329612563"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20802,20802,"Wand-zeepbakje zwart","Porte-savon mural noir.","Wall-mounted soap dish, black","030","Copper PVD",491,"GPF208020P000G000","8022692243536"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20808,20808,"Wand-glashouder zwart","Porte-verre mural noir.","Wall-mounted holder, black","031","Chrome",331,"GPF208080G001G000","8022692025620"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20814,20814,"Wand-dispenserhouder zwart","Distributeur de savon liquide mural noir.","Wall-mounted liquid soap dispenser - black",706,"Black Metal PVD",741,"GPF208141P001G000","8022692245875"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20820,20820,"Wand-toiletborstelhouder zwart","Porte-balayette mural noir.","Black wall-mounted brush holder",149,"Finox Brushed Nickel",738,"GPF208202G002G000","8022692247701"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20820,20820,"Wand-toiletborstelhouder zwart","Porte-balayette mural noir.","Black wall-mounted brush holder",726,"Warm Bronze Brushed PVD",864,"GPF208202P024G000","8056329612235"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20825,20825,"Staand zeepbakje wit","Porte-savon à poser blanc.","White standing soap holder",726,"Warm Bronze Brushed PVD",332,"GPF208251P024G000","8056329612198"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20831,20831,"Staande glashouder wit","Porte-verre à poser blanc.","Standing tumbler holder white",726,"Warm Bronze Brushed PVD",332,"GPF208311P024G000","8056329612129"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20837,20837,"Staande dispenserhouder wit","Distributeur de savon liquide à poser blanc.","Standing Soap dispenser white",707,"Black Metal Brushed PVD",574,"GPF208372P004G000","8022692833072"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20837,20837,"Staande dispenserhouder wit","Distributeur de savon liquide à poser blanc.","Standing Soap dispenser white",187,"Aged Bronze",574,"GPF208372G052G000","8056603553278"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20843,20843,"Staande toiletborstelhouder wit","Porte-balayette à poser blanche.","White standing brush holder",710,"Brass PVD",557,"GPF208433P011G000","8056329611924"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20844,20844,"Staande toiletborstelhouder zwart","Porte-balayette a poser noir","Black standing brush holder",710,"Brass PVD",557,"GPF208442P011G000","8056329611894"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20867,20867,"Wandkolom met toiletrolhouder en toiletborstelhouder wit","Serviteur mural avec porte-papier et porte-balayette blanc.","Wall-mounted column with paper roll holder and white brush holder",149,"Finox Brushed Nickel",997,"GPF208673G002G000","8022692258486"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20868,20868,"Wandkolom met toiletrolhouder en toiletborstelhouder zwart","Serviteur mural avec porte-papier et porte-balayette noir.","Wall-mounted column with paper roll holder and black brush holder",735,"Warm Bronze PVD",1093,"GPF208682P037G000","8056329611740"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20933,20933,"Vloerstandaard met toiletrolhouder en toiletborstelhouder wit","Serviteur sur pied avec porte-papier et porte-balayette blanc.","Standing set with paper roll holder and white brush holder",735,"Warm Bronze PVD",1121,"GPF209333P037G000","8056329611429"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20939,20939,"Vloerstandaard handdoekhouder","Serviteur sur pied porte-serviette.","Freestanding towel rail","031","Chrome",1020,"GPF209390G001G000","8022692021189"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20897,20897,"Wand-handdoekhouder 30 cm","Porte-serviette 30 cm.","30 cm centre distance towel rail",735,"Warm Bronze PVD",510,"GPF208970P037G000","8056329611603"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20900,20900,"Wand-handdoekhouder 45 cm","Porte-serviette 45 cm.","45 cm centre distance towel rail",710,"Brass PVD",526,"GPF209000P011G000","8056329611597"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20903,20903,"Wand-handdoekhouder 60 cm","Porte-serviette 60 cm.","60 cm centre distance towel rail",713,"Antique Brass",586,"GPF209030V204G000","8056329200227"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",73521,73521,"wandgemonteerde badjas haak. RIGATO.","Patère. RIGATO.","Wall-mounted robe hook. RIGATO.",299,"Matte Black",227,"GPF735210C072G000","8056603947824"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",73621,73621,"wandgemonteerde badjas haak. DIAMANTATO.","Patère. DIAMANTATO.","Wall-mounted robe hook. DIAMANTATO.",708,"Copper Brushed PVD",267,"GPF736210P006G000","8056603971874"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20963,20963,"Handdoekhouder 45 cm","Porte-serviette 45 cm à fixer sur le verre.","45 cm towel rail for glass fixing","031","Chrome",698,"GPF209630G001G000","8056329539457"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20861,20861,"Wandrekje voor bad/douche","Console d'angle pour baignoire ou douche.","Wall-mounted bath/shower shelf",149,"Finox Brushed Nickel",588,"GPF208610G002G000","8022692786149"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",707,"Black Metal Brushed PVD",658,"GPF209470P004G000","8022692273052"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm","031","Chrome",579,"GPF209450G001G000","8022692026955"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",710,"Brass PVD",856,"GPF209450P011G000","8056329611313"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20990,20990,"Papierbak wit","Poubelle blanche.","White waste-paper basket.",708,"Copper Brushed PVD",903,"GPF209901P006G000","8022692275469"]
["BATHROOM","INVERSO","INVERSO ACCESSORIES",20893,20893,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip-handle for bathtub and shower enclosure, 45 cm length",299,"Matte Black",655,"GPF208930C072G000","8056329025882"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",39114,39114,"wand gemonteerde WC (6 liters) in keramiek, geïntegreerde sifon. Hardware en pluggen voor laterale gaten niet inbegrepen.","Cuvette murale en céramique (6 litres) avec siphon intégré. Charnières et sièges non inclus.","Wall hung WC (6 litres) in Ceramic, integrated siphon. Hardware and lateral holes plugs not included.",518,"White Ceramic",834,"GPF391140C083G000","8056603626675"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",299,"Matte Black",220,"GPF375842C072G000","8056329006386"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",149,"Finox Brushed Nickel",125,"GPF375870G002G000","8022692796995"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",279,"Matte White",125,"GPF375870C071G000","8056329006324"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",149,"Finox Brushed Nickel",648,"GPF451300G002G000","8055261227590"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK","09276+45131","09276","Inbouwdeel voor afsluitbare douche met mengkraan.","Partie encastrée pour douchette shut-off avec mitigeur.","Built-in part for shut-off douchette with mixer.","031","Chrome",324,"GPF092760G001G000","8055261237261"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",713,"Antique Brass",758,"GPF451310V204G000","8055261227279"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1051,"GPF451240G002G000","8056603615891"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1354,"GPF452260P004G000","8055261645943"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1152,"GPF451260P001G000","8056603632935"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",710,"Brass PVD",1317,"GPF591511P011G000","8056329593503"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",708,"Copper Brushed PVD",1127,"GPF591531P006G000","8056329057432"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",187,"Aged Bronze",1029,"GPF143313G052G000","8056603507691"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",54611,54611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",273,"Matte Greige",848,"GPF546110T208G000","8056603588218"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",54613,54613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",720,"Nickel PVD",1495,"GPF546130P014G000","8056603456906"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",707,"Black Metal Brushed PVD",883,"GPF546150P004G000","8056329070264"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",845,"Dark Bronze",883,"GPF546150V221G000","8056603637688"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",54617,54617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",761,"Coffee Bronze Brushed PVD",1057,"GPF546170E059G000","8055261574373"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",54621,54621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",273,"Matte Greige",1497,"GPF546211T208G000","8056603587969"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",54621,54621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",716,"Gold Brushed PVD",1865,"GPF546211P005G000","8056603550789"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",54681,54681,"bedieningspaneel DIAMANTATO voor GEBERIT SIGMA 8 & 12","Plaque de finissage DIAMANTATO pour GEBRIT SIGMA 8 et 12","Cover plate DIAMANTATO for GEBERIT SIGMA 8 & 12",727,"Brass Brushed PVD",2092,"GPF546810P025G000","8056603458177"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",54681,54681,"bedieningspaneel DIAMANTATO voor GEBERIT SIGMA 8 & 12","Plaque de finissage DIAMANTATO pour GEBRIT SIGMA 8 et 12","Cover plate DIAMANTATO for GEBERIT SIGMA 8 & 12",761,"Coffee Bronze Brushed PVD",2225]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",273,"Matte Greige",168,"GPF014210T208G000","8056603964159"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",713,"Antique Brass",194,"GPF014210V204G000","8056603964104"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK",28767,28767,"Verlengstuk buis voor sifon, lengte 40 cm","Tubelure prolongée pour siphone, longueur 40 cm","Syphon pipe extension, 40 cm length",279,"Matte White",68,"GPF287670C071G000","8022692624267"]
["BATHROOM","INVERSO","INVERSO TOTAL LOOK","01410","01410","Sifon van 1 1/4\"","Siphon 1 1/4”.","1 1/4\" syphon",716,"Gold Brushed PVD",670,"GPF014100P005G000","8022692622331"]
["BATHROOM","VENTAGLIO","VENTAGLIO",72002,72002,"Wastafelmengkraan, zonder plug, met flexibele slangen.","Mitigeur lavabo, sans vidage, avec flexibles de raccordement.","Basin mixer without waste, with connecting flexibles.",299,"Matte Black",617,"GPF720020C072G000","8056603936279"]
["BATHROOM","VENTAGLIO","VENTAGLIO",72053,72053,"Hoge versie wastafelmengkraan, met vaste plug, met flexibele slangen.","Mitigeur lavabo réhaussé, avec bonde \"Stop&Go\" et flexibles de raccordement.","High version basin mixer with Stop&Go waste and connecting flexibles.",708,"Copper Brushed PVD",1091,"GPF720530P006G000","8056603963442"]
["BATHROOM","VENTAGLIO","VENTAGLIO",72004,72004,"Hoge versie wastafelmengkraan, zonder plug, met flexibele slangen.","Mitigeur lavabo réhaussé, sans vidage, avec flexibles de raccordement.","High version basin mixer without waste, with connecting flexibles.",707,"Black Metal Brushed PVD",1053,"GPF720040P004G000","8056603935876"]
["BATHROOM","VENTAGLIO","VENTAGLIO","63397+72088",72088,"Afbouwdeel wandgemonteerde wastafelmengkraan.","Partie apparente mitigeur lavabo mural.","External part wall-mounted basin mixer.",726,"Warm Bronze Brushed PVD",979,"GPF720880P024G000","8056603934961"]
["BATHROOM","VENTAGLIO","VENTAGLIO",63399,63399,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond à compléter par un mitigeur à commande séparée","Ceiling-mounted spout. To be completed with separate control.",277,"Glossy Ocra",1474,"GPF633990T211G000","8056603609470"]
["BATHROOM","VENTAGLIO","VENTAGLIO",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.",726,"Warm Bronze Brushed PVD",2061,"GPF634990P024G000","8056329555457"]
["BATHROOM","VENTAGLIO","VENTAGLIO",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.",246,"Gold PVD",2193,"GPF634990P007G000","8055261233782"]
["BATHROOM","VENTAGLIO","VENTAGLIO","46189+72095",72095,"Afbouwdeel vrijstaande wastafelmengkraan.","Partie apparente mitigeur lavabo au sol.","External part freestanding basin mixer.","030","Copper PVD",2985,"GPF720950P000G000","8056603934879"]
["BATHROOM","VENTAGLIO","VENTAGLIO","46189+72028",72028,"Afbouwdeel vrijstaande badmengkraan met omstel en antikalk handdouche.","Partie apparente pour mitigeur baignoire sur pied avec inverseur et douchette anticalcaire.","External part freestanding bath mixer with automatic diverter and antilimestone handshower.",735,"Warm Bronze PVD",3718,"GPF720280P037G000","8056603935456"]
["BATHROOM","VENTAGLIO","VENTAGLIO","54139+72036",72036,"Afbouwdeel wandgemonteerde 2-weg douche mengkraan met handdouche en omstel.","Partie apparente pour mitigeur douche murale 2 sorties avec douchette et inverseur.","External part wall-mounted two-ways shower mixer with handshower and diverter.",706,"Black Metal PVD",1448,"GPF720360P001G000","8056603935371"]
["BATHROOM","VENTAGLIO","VENTAGLIO","54157+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",706,"Black Metal PVD",388,"GPF540580P001G000","8056603627962"]
["BATHROOM","VENTAGLIO","VENTAGLIO","54157+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",761,"Coffee Bronze Brushed PVD",396,"GPF540580E059G000","8055261602076"]
["BATHROOM","VENTAGLIO","VENTAGLIO","54073+72038",72038,"Afbouwdeel wandgemonteerde 2-weg douche mengkraan.","Partie apparente pour mitigeur douche murale 2 sorties.","External part wall-mounted two-ways shower mixer.",707,"Black Metal Brushed PVD",900,"GPF720380P004G000","8056603971621"]
["BATHROOM","VENTAGLIO","VENTAGLIO","44673+72079",72079,"Afbouwdeel wandgemonteerde 2-weg mixer with met bad/douche omstel.","Partie apparente pour mitigeur murale 2 sorties avec inverseur bain-douche.","External part wall-mounted two-ways shower mixer with diverter.",707,"Black Metal Brushed PVD",771,"GPF720790P004G000","8056603935197"]
["BATHROOM","VENTAGLIO","VENTAGLIO","54169+63332",63332,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche mural 1 sortie.","External parts for thermostatic mixer, one-way diverter",187,"Aged Bronze",1346,"GPF633320G052G000","8056329561526"]
["BATHROOM","VENTAGLIO","VENTAGLIO","54169+63333",63333,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche mural 2 sorties.","External parts for thermostatic mixer, two-ways diverter",727,"Brass Brushed PVD",1216,"GPF633330P025G000","8056329591998"]
["BATHROOM","VENTAGLIO","VENTAGLIO","54169+63334",63334,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche mural 2 sorties.","External parts for thermostatic mixer, two-ways diverter",187,"Aged Bronze",1346,"GPF633340G052G000","8056329561489"]
["BATHROOM","VENTAGLIO","VENTAGLIO","54169+63335",63335,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche mural 3 sorties.","External parts for thermostatic mixer, three-ways diverter",845,"Dark Bronze",1216,"GPF633350V221G000","8055261040861"]
["BATHROOM","VENTAGLIO","VENTAGLIO","54169+63336",63336,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche mural 3 sorties.","External parts for thermostatic mixer, three-ways diverter",845,"Dark Bronze",1346,"GPF633360V221G000","8055261058606"]
["BATHROOM","VENTAGLIO","VENTAGLIO","09268+63438",63438,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie externe mitigeur thermostatique mural à 4 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with four separate exits.","031","Chrome",1484,"GPF634380G001G000","8056603618809"]
["BATHROOM","VENTAGLIO","VENTAGLIO","09263+63440",63440,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie externe mitigeur thermostatique mural à 5 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with five separate exits.",720,"Nickel PVD",2412,"GPF634400P014G000","8056603630344"]
["BATHROOM","VENTAGLIO","VENTAGLIO","43103+43064",43064,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",149,"Finox Brushed Nickel",1889,"GPF430642G002G000","8022692582222"]
["BATHROOM","VENTAGLIO","VENTAGLIO","43103+43064",43064,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",279,"Matte White",1889,"GPF430642C071G000","8022692855784"]
["BATHROOM","VENTAGLIO","VENTAGLIO","43105+43066",43066,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",149,"Finox Brushed Nickel",2180,"GPF430662G002G000","8022692582352"]
["BATHROOM","VENTAGLIO","VENTAGLIO","43105+43236",43236,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",713,"Antique Brass",2750,"GPF432361V204G000","8056329562073"]
["BATHROOM","VENTAGLIO","VENTAGLIO","43107+43068",43068,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS","031","Chrome",1484,"GPF430682G001G000","8022692582512"]
["BATHROOM","VENTAGLIO","VENTAGLIO","43107+43238",43238,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",727,"Brass Brushed PVD",3144,"GPF432381P025G000","8056329608245"]
["BATHROOM","VENTAGLIO","VENTAGLIO","43109+43070",43070,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",708,"Copper Brushed PVD",3472,"GPF430702P006G000","8056329131521"]
["BATHROOM","VENTAGLIO","VENTAGLIO","43111+43072",43111,"Inbouw deel Thermostatische mengkraan hoog debiet 5 uitgangen met enkele selectie","Partie encastrée mitigeur thermostatique douche haut débit, cinq sorties avec manette selective.","Built-in thermostatic high-capacity mixer with FIVE SEPARATE EXITS with single selection","031","Chrome",1428,"GPF431113G001G000","8022692583496"]
["BATHROOM","VENTAGLIO","VENTAGLIO","43281+43256",43256,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente mitigeur THERMOSTATIQUE douche haut débit","External parts wall-mounted thermostatic high-capacity mixer","030","Copper PVD",1020,"GPF432561P000G000","8056329131231"]
["BATHROOM","VENTAGLIO","VENTAGLIO","43281+43256",43256,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente mitigeur THERMOSTATIQUE douche haut débit","External parts wall-mounted thermostatic high-capacity mixer",761,"Coffee Bronze Brushed PVD",1235,"GPF432561E059G000","8055261603080"]
["BATHROOM","VENTAGLIO","VENTAGLIO",45163,45163,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted shower head",238,"Mirror Steel",1828,"GPF451630A001G000","8022692812374"]
["BATHROOM","VENTAGLIO","VENTAGLIO",33095,33095,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted shower head",238,"Mirror Steel",2499,"GPF330951A001G000","8022692365436"]
["BATHROOM","VENTAGLIO","VENTAGLIO",63352,63352,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable shower head",720,"Nickel PVD",751,"GPF633520P014G000","8056603605168"]
["BATHROOM","VENTAGLIO","VENTAGLIO",63350,63350,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted showerhead, length on request",707,"Black Metal Brushed PVD",1122,"GPF633500P004G000","8056329555570"]
["BATHROOM","VENTAGLIO","VENTAGLIO",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",299,"Matte Black",1565,"GPF630450C072G000","8055261729728"]
["BATHROOM","VENTAGLIO","VENTAGLIO",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",706,"Black Metal PVD",1616,"GPF630500P001G000","8055261729483"]
["BATHROOM","VENTAGLIO","VENTAGLIO",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",710,"Brass PVD",2101,"GPF630530P011G000","8055261729285"]
["BATHROOM","VENTAGLIO","VENTAGLIO",66068,66068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",149,"Finox Brushed Nickel",2173]
["BATHROOM","VENTAGLIO","VENTAGLIO",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",707,"Black Metal Brushed PVD",2543]
["BATHROOM","VENTAGLIO","VENTAGLIO",66072,66072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",845,"Dark Bronze",2352]
["BATHROOM","VENTAGLIO","VENTAGLIO",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.","030","Copper PVD",2202]
["BATHROOM","VENTAGLIO","VENTAGLIO",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",706,"Black Metal PVD",3096]
["BATHROOM","VENTAGLIO","VENTAGLIO",70045,70045,"Glijrail met antikalk handdouche, 1,50 m flexibele slang.","Barre de douche complète avec douchette anticalcaire et flexibles 1,50 m.","Sliding rail with antilimestone handshower, 1,50 m flexible hose.",149,"Finox Brushed Nickel",939,"GPF700450G002G000","8056603685078"]
["BATHROOM","VENTAGLIO","VENTAGLIO",70044,70044,"Sliding rail.","Barre de douche.","Sliding rail.","031","Chrome",568,"GPF700440G001G000","8056603667609"]
["BATHROOM","VENTAGLIO","VENTAGLIO",32971,32971,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",187,"Aged Bronze",474,"GPF329710G052G000","8056329037281"]
["BATHROOM","VENTAGLIO","VENTAGLIO",32971,32971,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",761,"Coffee Bronze Brushed PVD",503,"GPF329710E059G000","8055261608634"]
["BATHROOM","VENTAGLIO","VENTAGLIO","32985+32982",32982,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour douchette laterale orientable","External parts for adjustable lateral body jet",727,"Brass Brushed PVD",745,"GPF329820P025G000","8056329037182"]
["BATHROOM","VENTAGLIO","VENTAGLIO",13375,13375,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","Adjustable lateral body jet",716,"Gold Brushed PVD",358,"GPF133750P005G000","8056329637184"]
["BATHROOM","VENTAGLIO","VENTAGLIO",65295,65295,"Afbouwdeel Voor Waterval Douche Uitloop Nog Compleet Te Maken Met Separate Bediening (Niet Inclusief)","Partie apparente pour bec cascade de douche murale. À compléter par commande séparée.","Waterfall shower spout to be completed with separate control (not included)",707,"Black Metal Brushed PVD",1607,"GPF652950P004G000","8056603003933"]
["BATHROOM","VENTAGLIO","VENTAGLIO",63329,63329,"Doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m.","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",710,"Brass PVD",658,"GPF633290P011G000","8056329592063"]
["BATHROOM","VENTAGLIO","VENTAGLIO",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",726,"Warm Bronze Brushed PVD",1003,"GPF630990P024G000","8056329215948"]
["BATHROOM","VENTAGLIO","VENTAGLIO",63469,63469,"Wateraansluitpunt","Sortie murale coudée.","Water outlet",727,"Brass Brushed PVD",249,"GPF634690P025G000","8056329591332"]
["BATHROOM","VENTAGLIO","VENTAGLIO",58157,58157,"Vaste houder voor handdouche","Support fixe pour douchette.","Fixed handshower hook",761,"Coffee Bronze Brushed PVD",205,"GPF581570E059G000","8055261595590"]
["BATHROOM","VENTAGLIO","VENTAGLIO",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",149,"Finox Brushed Nickel",376,"GPF329290G002G000","8055261227910"]
["BATHROOM","VENTAGLIO","VENTAGLIO",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.","031","Chrome",246,"GPF329300G001G000","8055261227767"]
["BATHROOM","VENTAGLIO","VENTAGLIO",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",279,"Matte White",120,"GPF143720C071G000","8022692435276"]
["BATHROOM","VENTAGLIO","VENTAGLIO",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",761,"Coffee Bronze Brushed PVD",252,"GPF143700E059G000","8055261609631"]
["BATHROOM","VENTAGLIO","VENTAGLIO",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",246,"Gold PVD",366,"GPF143760P007G000","8056603522571"]
["BATHROOM","VENTAGLIO","VENTAGLIO",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",187,"Aged Bronze",346,"GPF143780G052G000","8056603633260"]
["BATHROOM","VENTAGLIO","VENTAGLIO",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",708,"Copper Brushed PVD",269,"GPF473510P006G000","8056603587044"]
["BATHROOM","VENTAGLIO","VENTAGLIO",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",246,"Gold PVD",287,"GPF473500P007G000","8056603631716"]
["BATHROOM","VENTAGLIO","VENTAGLIO",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections","031","Chrome",85,"GPF287460G001G000","8022692025996"]
["BATHROOM","VENTAGLIO","VENTAGLIO",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish","031","Chrome",90,"GPF541370G001G000","8056329573116"]
["BATHROOM","VENTAGLIO","VENTAGLIO","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",246,"Gold PVD",170,"GPF017240P007G000","8055261240049"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63601,63601,"witte wandgemonteerde soap houder","Porte-savon mural blanc","Wall-mounted white soap holder",713,"Antique Brass",312,"GPF636010V204G000","8056329560437"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63602,63602,"zwarte wandgemonteerde soap houder","Porte-savon mural noir","Wall-mounted black soap holder",727,"Brass Brushed PVD",312,"GPF636020P025G000","8056329590595"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63607,63607,"witte wandgemonteerde beker houder","Porte-verre mural blanc","Wall-mounted white tumbler holder",716,"Gold Brushed PVD",362,"GPF636070P005G000","8055261230019"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63608,63608,"zwarte wandgemonteerde beker houder","Porte-verre mural noir","Wall-mounted black tumbler holder",716,"Gold Brushed PVD",362,"GPF636080P005G000","8055261230002"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63613,63613,"witte wandgemonteerde soap","Distributeur de savon liquide mural blanc","Wall-mounted white dispenser",708,"Copper Brushed PVD",557,"GPF636130P006G000","8056329547681"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63619,63619,"witte wandgemonteerde borstel houder","Porte-balayette mural blanche","Wall-mounted white toilet brush holder",735,"Warm Bronze PVD",499,"GPF636190P037G000","8056603452878"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63620,63620,"zwarte wandgemonteerde borstel houder","Porte-balayette mural noir","Wall-mounted black toilet brush holder",726,"Warm Bronze Brushed PVD",532,"GPF636200P024G000","8056603452748"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",58525,58525,"Witte Staande Zeephouder","Porte-savon à poser blanc","Standing soap holder, white",707,"Black Metal Brushed PVD",381,"GPF585250P004G000","8022692874082"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",58526,58526,"Zwarte Witte Staande Zeephouder","Porte-savon à poser noir","Standing soap holder, black",149,"Finox Brushed Nickel",327,"GPF585260G002G000","8056329062320"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",58531,58531,"Witte Staande Bekerhouder","Porte-verre à poser blanc.","Standing tumbler holder, white",707,"Black Metal Brushed PVD",417,"GPF585310P004G000","8022692874105"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",66437,66437,"staande witte zeep dispenser","Distributeur de savon liquide à poser blanc","Standing soap dispenser holder, white","031","Chrome",373,"GPF664370G001G000","8056603573047"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",66437,66437,"staande witte zeep dispenser","Distributeur de savon liquide à poser blanc","Standing soap dispenser holder, white",706,"Black Metal PVD",552,"GPF664370P001G000","8056603573023"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",66438,66438,"staande zwarte zeep dispenser","Distributeur de savon liquide à poser noir","Standing soap dispenser holder, black",713,"Antique Brass",589,"GPF664380V204G000","8056603609227"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63744,63744,"Staande toiletborstelhouder zwart","Porte-balayette a poser noir","Standing brush holder, black",299,"Matte Black",421,"GPF637440C072G000","8056329575202"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63744,63744,"Staande toiletborstelhouder zwart","Porte-balayette a poser noir","Standing brush holder, black",716,"Gold Brushed PVD",526,"GPF637440P005G000","8056603531207"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63697,63697,"30 cm Handdoekhouder","Porte-serviette 30 cm","30 cm Towel rail",727,"Brass Brushed PVD",262,"GPF636971P025G000","8056329590359"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63700,63700,"45 cm Handdoekhouder","Porte-serviette 45 cm","45 cm Towel rail",299,"Matte Black",271,"GPF637001C072G000","8056329546950"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63703,63703,"60 cm Handdoekhouder","Porte-serviette 60 cm","60 cm Towel rail",735,"Warm Bronze PVD",324,"GPF637031P037G000","8056329546769"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",72521,72521,"Wandgemonteerde badjas haak.","Patère.","Wall-mounted robe hook.","031","Chrome",85,"GPF725210G001G000","8056603934398"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",72521,72521,"Wandgemonteerde badjas haak.","Patère.","Wall-mounted robe hook.",707,"Black Metal Brushed PVD",134,"GPF725210P004G000","8056603934343"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63726,63726,"45 cm Handdoekhouder voor glasmontage","Poignée et porte-serviette pour verre 45 cm","45 cm Towel rail for glass fixing",735,"Warm Bronze PVD",576,"GPF637261P037G000","8056329546561"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",63728,63728,"60 cm Handdoekhouder voor glasmontage","Poignée et porte-serviette pour verre 60 cm","60 cm Towel rail for glass fixing",149,"Finox Brushed Nickel",550,"GPF637281G002G000","8056329546530"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",45590,45590,"Papierbak wit","Poubelle blanche.","White waste-paper basket",707,"Black Metal Brushed PVD",854,"GPF455900P004G000","8022692815177"]
["BATHROOM","VENTAGLIO","VENTAGLIO ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.","031","Chrome",989,"GPF584241G001G000","8056329545564"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",39118,39118,"Wandtoilet van Keramiek (6 liter) met geïntegreerde sifon. Scharnieren met vertraagde sluiting en laterale gatafdekkingen opgenomen in afwerking 031","Cuvette suspendue en Céramique (6 litres) avec abattant muni de système “SOFT CLOSE” ou assisté. Charnière et enjoliveurs latéraux en finition 031","Wall hung WC (6 litres) in Ceramic, integrated siphon. Soft-closing hardware and lateral holes plugs included in 031 finishing.",532,"Matte Black Ceramic",1711,"GPF391180C289G000","8056603448543"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",706,"Black Metal PVD",257,"GPF375842P001G000","8022692674286"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",39115,39115,"Wandbidet van Keramiek met overloop. Met centraal gat voor kraanwerk. Dop overloop en laterale gatafdekkingen opgenomen in afwerking 031.","Bidet suspendu en Céramique Blanc Europe avec vidage et trop plein, percé monotrou pour la robinetterie, fourni avec cache de trop plein et enjoliveurs latéraux en finition 031.","Wall hung bidet in in White Europe Ceramic with overflow waste, with central hole for taps and fittings. Overflow cap and side covering caps included in 031 finishing",518,"White Ceramic",769,"GPF391150C083G000","8022692785302"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",187,"Aged Bronze",154,"GPF375870G052G000","8056329008755"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","031","Chrome",480,"GPF451300G001G000","8055261227606"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",713,"Antique Brass",758,"GPF451310V204G000","8055261227279"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",279,"Matte White",648,"GPF451310C071G000","8055261236226"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",187,"Aged Bronze",1230,"GPF451240G052G000","8056603615853"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",713,"Antique Brass",1029,"GPF451231V204G000","8056329561953"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1230,"GPF451260P024G000","8056603632874"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",147,"Chome Brushed",878,"GPF143313G006G000","8056329082557"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",716,"Gold Brushed PVD",1092,"GPF143313P005G000","8056329625204"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",299,"Matte Black",1095,"GPF451211C072G000","8022692811643"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",54611,54611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",845,"Dark Bronze",930,"GPF546110V221G000","8056603637664"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",54613,54613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",727,"Brass Brushed PVD",1495,"GPF546130P025G000","8056329070363"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",299,"Matte Black",807,"GPF546150C072G000","8056329070332"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",54617,54617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE","031","Chrome",669,"GPF546170G001G000","8056329098848"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",54617,54617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",716,"Gold Brushed PVD",1121,"GPF546170P005G000","8056329098770"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",54619,54619,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaque de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",706,"Black Metal PVD",1298,"GPF546190P001G000","8056329540934"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",54605,54605,"Opzetwastafel in roestvrij staal zonder overloop 400x400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 400x400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 400x400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",707,"Black Metal Brushed PVD",3957,"GPF546050P004G000","8056329224971"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",708,"Copper Brushed PVD",3783,"GPF546010P006G000","8022692851540"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",278,"Glossy Coral",161,"GPF013910T212G000","8056603635141"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",710,"Brass PVD",150,"GPF013910P011G000","8022692833010"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",735,"Warm Bronze PVD",169,"GPF014210P037G000","8056603964166"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",299,"Matte Black",262,"GPF014200C072G000","8056329039803"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",713,"Antique Brass",236,"GPF014200V204G000","8022692089646"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",735,"Warm Bronze PVD",80,"GPF013460P037G000","8056329559233"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",187,"Aged Bronze",80,"GPF013460G052G000","8056329184244"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","01377","01377","1 1/4\" sifon","Siphon 1 1/4”.","1 1/4\" syphon",720,"Nickel PVD",429,"GPF013771P014G000","8056603560665"]
["BATHROOM","VENTAGLIO","VENTAGLIO TOTAL LOOK","01411","01411","Onderbouwmengkraan met filter en 1/2\" aansluiting","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection",716,"Gold Brushed PVD",264,"GPF014110P005G000","8056603978088"]
["BATHROOM","ORIGINI","ORIGINI",66600,66600,"inleg","Insert","Insert",277,"Glossy Ocra",102,"GPF666000T211G000","8056603572736"]
["BATHROOM","ORIGINI","ORIGINI",66604,66604,"Kit 5 inleg","Kit 5 inserts","Kit 5 Insert",277,"Glossy Ocra",436,"GPF666040T211G000","8056603626798"]
["BATHROOM","ORIGINI","ORIGINI",66605,66605,"Kit 5 Inleg ART","Kit 5 inserts ART","Kit 5 Insert ART",286,"Neutral",450,"GPF666050T215G000","8056603626743"]
["BATHROOM","ORIGINI","ORIGINI",66005,66005,"Medium versie Wastafel mengkraan, Flexibele slangen, met vaste plug. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Mitigeur lavabo moyen avec vidage et flexibles de raccordement. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","Medium version basin mixer with waste and connecting flexibles. Can be combined with inserts with different finishes: art. 66600and art. 66602.",273,"Matte Greige",803,"GPF660050T208G000","8056603569910"]
["BATHROOM","ORIGINI","ORIGINI",66006,66006,"Medium versie Wastafel mengkraan, flexible connection, zonder waste. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602.","Mitigeur lavabo moyen sans vidage, avec flexibles de raccordement. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","Medium version basin mixer without waste and connecting flexibles. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",707,"Black Metal Brushed PVD",868,"GPF660060P004G000","8056603568029"]
["BATHROOM","ORIGINI","ORIGINI",66003,66003,"Verhoogde versie Wastafel mengkraan, Flexibele slangen, met vaste plug. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Mitigeur lavabo réhaussé avec vidage et flexibles de raccordement. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","High version basin mixer with waste and connecting flexibles. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",706,"Black Metal PVD",953,"GPF660030P001G000","8056603568227"]
["BATHROOM","ORIGINI","ORIGINI",66004,66004,"Verhoogde versie Wastafel mengkraan, Flexibele slangen, zonder plug. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Mitigeur lavabo réhaussé sans vidage avec flexibles de raccordement. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","High version basin mixer without waste and connecting flexibles. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",708,"Copper Brushed PVD",946,"GPF660040P006G000","8056603568111"]
["BATHROOM","ORIGINI","ORIGINI",66016,66016,"3-gats Verhoogde versie Wastafel mengkraan, Flexibele slangen, zonder plug. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Group lavabo trois trous réhaussé sans vidage et flexibles de raccordement. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","Three-holes high version basin mixer without waste and connecting flexibles. Can be combined with inserts with different finishes: art. 66600 and art. 66602.","031","Chrome",930,"GPF660160G001G000","8056603575935"]
["BATHROOM","ORIGINI","ORIGINI","66236+66090",66090,"afbouwdelen 3-gats wastafelkraan, zonder plug. Kan gecombineerd worden met inleg in verschillende afwerkingen: art. 66600 and art. 66602","Partie apparente mélangeur lavabo mural trois sorties avec bec moyen sans vidage. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","External parts three-holes basin mixer, without waste. Can be combined with inserts with different finishes: art. 66600 and art.66602.",299,"Matte Black",880,"GPF660900C072G000","8056603618212"]
["BATHROOM","ORIGINI","ORIGINI",66021,66021,"Medium uitloop wastafel","Bec de lavabo moyen","Medium spout basin",706,"Black Metal PVD",549,"GPF660210P001G000","8056603567640"]
["BATHROOM","ORIGINI","ORIGINI",66025,66025,"Verhoogde uitloop wastafel","Bec de lavabo réhaussé","High spout basin",845,"Dark Bronze",696,"GPF660250V221G000","8056603575652"]
["BATHROOM","ORIGINI","ORIGINI",66102,66102,"wand-gemonteerde uitloop wastafel, medium uitloop","Bec de lavabo mural moyen","Wall-mounted medium spout basin",707,"Black Metal Brushed PVD",325,"GPF661020P004G000","8056603566643"]
["BATHROOM","ORIGINI","ORIGINI",63399,63399,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond à compléter par un mitigeur à commande séparée","Ceiling-mounted spout. To be completed with separate control.",278,"Glossy Coral",1474,"GPF633990T212G000","8056603609463"]
["BATHROOM","ORIGINI","ORIGINI",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.","030","Copper PVD",1932,"GPF634990P000G000","8056329555495"]
["BATHROOM","ORIGINI","ORIGINI",66100,66100,"separate bediening. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Commande séparée. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","Separate control. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",277,"Glossy Ocra",549,"GPF661000T211G000","8056603568548"]
["BATHROOM","ORIGINI","ORIGINI","46189+66095","66095","Externe delen voor vrijstaene Wastafel mengkraan zonder waste. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Parties apparentes mitigeur lavabo au sol sans vidage. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","External part for freestanding basin mixer without waste. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",275,"Matte Cipria",2151,"GPF660950T209G000","8056603568616"]
["BATHROOM","ORIGINI","ORIGINI","46189+66095","66095","Externe delen voor vrijstaene Wastafel mengkraan zonder waste. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Parties apparentes mitigeur lavabo au sol sans vidage. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","External part for freestanding basin mixer without waste. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",149,"Finox Brushed Nickel",2151,"GPF660950G002G000","8056603566865"]
["BATHROOM","ORIGINI","ORIGINI",66037,66037,"4-gats badkraan met omstel, bad uitloop, 1,50 m flexibele slang en antikalk handdouche. kan gecombineerd worden met inleg met verschillende afwerkingen: art. 66600 en art. 66602.","Ensemble de baignoire 4 trous avec inverseur, bec, flexible de 1,50 m et douchette anticalcaire. Il peut être combiné avec des inserts dans des finitions différentes : réf. 66600 et réf. 66602.","Four-holes bath mixer with diverter, tub-filler spout, 1,50 m flexible hose and antilimestone hand shower. Can be combined withinserts with different finishes: art. 66600 and art. 66602.",727,"Brass Brushed PVD",2482,"GPF660370P025G000","8056603567190"]
["BATHROOM","ORIGINI","ORIGINI","01663","01663","Drie-gats afwerkplaat voor montagebox","Plaque de finition 3 trous pour la boîte de sécurité","Three-holes finishing plate for mounting box",710,"Brass PVD",736,"GPF016631P011G000","8056329615182"]
["BATHROOM","ORIGINI","ORIGINI","01664","01664","Four-holes finishing plaatje voor montage box","Plaque de finition 4 trous pour la boîte de sécurité","Four-holes finishing plate for mounting box",707,"Black Metal Brushed PVD",841,"GPF016641P004G000","8056329060715"]
["BATHROOM","ORIGINI","ORIGINI","01785","01785","Uittrekbare handdouche afvoerset, tegelwandinstallatie. Niet passend op artikelen 01669, 01658, 01663 en 01664.","Système de récupération d'eau pour douchette flexible de bord de baignoire, installation murale. Ne peut être combiné avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, tile wall installation. Not fitting items 01669, 01658, 01663 and 01664.","031","Chrome",1081,"GPF017850G001G000","8056329562653"]
["BATHROOM","ORIGINI","ORIGINI","01786","01786","Uittrekbare handdouche afvoerset, randinstallatie. Niet passend op artikelen 01669, 01658, 01663 en 01664.","Système de récupération d'eau pour flexible de douchette, installation sur le bord de la baignoire. Ne peut être combiné avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, rim installation. Not fitting items 01669, 01658, 01663 and 01664.","030","Copper PVD",1302,"GPF017860P000G000","8056329562523"]
["BATHROOM","ORIGINI","ORIGINI",20191,20191,"Cascade-uitloop Badrand Aan te vullen met afstandsbediening","Bec cascade pour baignoire à compléter par un mitigeur à commande séparée.","Bath group waterfall spout to be completed with separate control",707,"Black Metal Brushed PVD",2673,"GPF201910P004G000","8022692224917"]
["BATHROOM","ORIGINI","ORIGINI",66103,66103,"wandfixing baduitloop","Bec de bagnoire mural","Wall-fixing bath spout","031","Chrome",267,"GPF661030G001G000","8056603566575"]
["BATHROOM","ORIGINI","ORIGINI","54139+66036","66036","Externe delen wandgemonteerde douche mixer, 2-weg, met omstel kraan, water uitgang en handdouche haak. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Parties apparentes mitigeur de douche mural 2 sorties avec inverseur, sortie coudée et support douchette. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","External parts wall-mounted two-ways shower mixer, with diverter, water outlet and hand shower hook. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",720,"Nickel PVD",1248,"GPF660360P014G000","8056603567312"]
["BATHROOM","ORIGINI","ORIGINI","54057+54058","54058","Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",246,"Gold PVD",388,"GPF540580P007G000","8056603627955"]
["BATHROOM","ORIGINI","ORIGINI","54055+66109","66109","Externe delen wandgemonteerde wastafel/douche separate bediening, 1-weg. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Parties apparentes commande séparée lavabo/douche mural, 1 sortie. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","External parts mixer one-way diverter. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",845,"Dark Bronze",393,"GPF661090V221G000","8056603566391"]
["BATHROOM","ORIGINI","ORIGINI","54169+66136","66136","Externe delen wandgemonteerde thermostatic douche mixer, 3-weg. Inleg met afwerking inbegrepen. Combineerbaar met verschillendeafwerkingen met inleg 66600 of inleg ART 66602","Parties apparentes mitigeur thermostatique douche mural 3 sorties. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","External part wall-mounted thermostatic three-ways shower mixer. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",707,"Black Metal Brushed PVD",1215,"GPF661360P004G000","8056603566049"]
["BATHROOM","ORIGINI","ORIGINI","63013+66224","63013","Inbouwdeel Voor Thermostatische Mengkraan Voor Drie Gelijktijdige Functies, Met 3/4\" Aansluitingen","Partie encastrée pour mitigeur thermostatique trois fonctions avecraccordements 3/4”","Built-in part for thermostatic mixer for three simultaneous functions, with 3/4\" connections","031","Chrome",951,"GPF630130G001G000","8056329219168"]
["BATHROOM","ORIGINI","ORIGINI","63015+66226","66226","Afbouwdeel Voor Thermostatische Mengkraan Vier Gelijktijdige Functies, Met Druk Knop Aan/Uit Bediening. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg art 66602","Partie apparente pour mitiguer thermostatique quatre fonctions avectouche on/off. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","External parts for thermostatic mixer for four separate functions, with push-button on/off controls. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",845,"Dark Bronze",3384,"GPF662260V221G000","8056603580953"]
["BATHROOM","ORIGINI","ORIGINI","09266+66336","66336","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen. kan gecombineerd worden met inleg met verschillende afwerkingen: art. 66600 en art. 66602.","Partie externe mitigeur thermostatique mural à 3 sorties indépendantes. Installation verticale/horizontale. Il peut être combinéavec des inserts en plusieurs finitions : art. 66600 et art. 66602.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with three separate exits. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",149,"Finox Brushed Nickel",1768,"GPF663360G002G000","8056603617932"]
["BATHROOM","ORIGINI","ORIGINI","63215+63209","63209","Externe delen voor doucheset met 1 uitgang, compleet te maken met 66211 kit en douche in gewenste afwerking.","Parties apparentes pour colonne de douche pour l'extérieure 1 sortie, à compléter avec le kit 66211 et spotwater dans la finition souhaitée","External part for one exit outdoor shower column, to complete with 66211 kit and shower head in the desired finishing.",281,"Matte Coral",5879,"GPF632090T214G000","8056603626569"]
["BATHROOM","ORIGINI","ORIGINI","63215+63209","63209","Externe delen voor doucheset met 1 uitgang, compleet te maken met 66211 kit en douche in gewenste afwerking.","Parties apparentes pour colonne de douche pour l'extérieure 1 sortie, à compléter avec le kit 66211 et spotwater dans la finition souhaitée","External part for one exit outdoor shower column, to complete with 66211 kit and shower head in the desired finishing.",856,"Corten",5879,"GPF632090T091G000","8056603626613"]
["BATHROOM","ORIGINI","ORIGINI",66150,66150,"wandgemonteerde antikalk en verstelbare hoofddouche","Pomme de douche murale orientable.","Wall-mounted anti limestone and adjustable head shower",706,"Black Metal PVD",2181,"GPF661500P001G000","8056603578677"]
["BATHROOM","ORIGINI","ORIGINI",66148,66148,"wandgemonteerde antikalk en verstelbare hoofddouche","Pomme de douche murale orientable.","Wall-mounted anti limestone and adjustable head shower","031","Chrome",599,"GPF661480G001G000","8056603572637"]
["BATHROOM","ORIGINI","ORIGINI",66148,66148,"wandgemonteerde antikalk en verstelbare hoofddouche","Pomme de douche murale orientable.","Wall-mounted anti limestone and adjustable head shower",706,"Black Metal PVD",888,"GPF661480P001G000","8056603573450"]
["BATHROOM","ORIGINI","ORIGINI",63352,63352,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable shower head",727,"Brass Brushed PVD",802,"GPF633520P025G000","8056329591752"]
["BATHROOM","ORIGINI","ORIGINI",63350,63350,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted showerhead, length on request",149,"Finox Brushed Nickel",959,"GPF633500G002G000","8056329555617"]
["BATHROOM","ORIGINI","ORIGINI",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",726,"Warm Bronze Brushed PVD",1831,"GPF630450P024G000","8055261729605"]
["BATHROOM","ORIGINI","ORIGINI",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.","030","Copper PVD",1616,"GPF630500P000G000","8055261729490"]
["BATHROOM","ORIGINI","ORIGINI",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",299,"Matte Black",2009]
["BATHROOM","ORIGINI","ORIGINI",66068,66068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","030","Copper PVD",2383]
["BATHROOM","ORIGINI","ORIGINI",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",735,"Warm Bronze PVD",2383]
["BATHROOM","ORIGINI","ORIGINI",66072,66072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",735,"Warm Bronze PVD",2202]
["BATHROOM","ORIGINI","ORIGINI",63072,63072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",845,"Dark Bronze",2352]
["BATHROOM","ORIGINI","ORIGINI",66142,66142,"glijstang met water uitgang, antikalk handdouche en 1,50 flexibele slang. Inleg met afwerking inbegrepen.Combineerbaar met verschillende afwerkingen met inleg 66600 en inleg ART 66602","Barre de douche complète avec sortie murale coudée, douchette anticalcaire et flexibles 1,50 m. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 et insert ART 66602","Sliding rail with water outlet, anti limestone hand shower and 1,50 flexible hose. Finishing insert included. It can be combiedto different finishes with insert 66600 and insert ART 66602",706,"Black Metal PVD",1821,"GPF661420P001G000","8056603575614"]
["BATHROOM","ORIGINI","ORIGINI",66142,66142,"glijstang met water uitgang, antikalk handdouche en 1,50 flexibele slang. Inleg met afwerking inbegrepen.Combineerbaar met verschillende afwerkingen met inleg 66600 en inleg ART 66602","Barre de douche complète avec sortie murale coudée, douchette anticalcaire et flexibles 1,50 m. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 et insert ART 66602","Sliding rail with water outlet, anti limestone hand shower and 1,50 flexible hose. Finishing insert included. It can be combiedto different finishes with insert 66600 and insert ART 66602",708,"Copper Brushed PVD",1942,"GPF661420P006G000","8056603575591"]
["BATHROOM","ORIGINI","ORIGINI",32971,32971,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",735,"Warm Bronze PVD",444,"GPF329710P037G000","8056329555907"]
["BATHROOM","ORIGINI","ORIGINI",32977,32977,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",720,"Nickel PVD",385,"GPF329771P014G000","8056603455978"]
["BATHROOM","ORIGINI","ORIGINI","32985+32982",32982,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour douchette laterale orientable","External parts for adjustable lateral body jet",726,"Warm Bronze Brushed PVD",745,"GPF329820P024G000","8056329006881"]
["BATHROOM","ORIGINI","ORIGINI",66123,66123,"douche set met water uitgang, 1,50 m flexibele slang en antikalk handdouche. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m. Insert en finition inclus. Combiner avecfinitions differentes avec insert 66600 ou insert ART 66602","Shower set with water outlet, anti limestone hand shower and 1,50 m flexible hose. Can be combined with inserts with different finishes: art. 66600 and art. 66602.","031","Chrome",459,"GPF661230G001G000","8056603566377"]
["BATHROOM","ORIGINI","ORIGINI",66123,66123,"douche set met water uitgang, 1,50 m flexibele slang en antikalk handdouche. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m. Insert en finition inclus. Combiner avecfinitions differentes avec insert 66600 ou insert ART 66602","Shower set with water outlet, anti limestone hand shower and 1,50 m flexible hose. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",727,"Brass Brushed PVD",727,"GPF661230P025G000","8056603566308"]
["BATHROOM","ORIGINI","ORIGINI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",735,"Warm Bronze PVD",940,"GPF630990P037G000","8056329558199"]
["BATHROOM","ORIGINI","ORIGINI",66169,66169,"Wateraansluitpunt. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART 66602","Sortie murale coudée. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","Water outlet. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",727,"Brass Brushed PVD",457,"GPF661690P025G000","8056603603492"]
["BATHROOM","ORIGINI","ORIGINI",66157,66157,"Vaste handdouche haak. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg ART66602","Support fixe pour douchette. Insert en fi nition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","Fixed hand shower hook. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",707,"Black Metal Brushed PVD",421,"GPF661570P004G000","8056603587884"]
["BATHROOM","ORIGINI","ORIGINI",58157,58157,"Vaste houder voor handdouche","Support fixe pour douchette.","Fixed handshower hook","031","Chrome",121,"GPF581570G001G000","8022692870725"]
["BATHROOM","ORIGINI","ORIGINI",58157,58157,"Vaste houder voor handdouche","Support fixe pour douchette.","Fixed handshower hook",710,"Brass PVD",179,"GPF581570P011G000","8056329596047"]
["BATHROOM","ORIGINI","ORIGINI",58160,58160,"Oriënteerbare duplex houder voor handdouche","Support mural orientable pour douchette.","Adjustable handshower hook",761,"Coffee Bronze Brushed PVD",360,"GPF581600E059G000","8055261595576"]
["BATHROOM","ORIGINI","ORIGINI",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",710,"Brass PVD",411,"GPF329290P011G000","8055261227835"]
["BATHROOM","ORIGINI","ORIGINI",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",187,"Aged Bronze",388,"GPF329300G052G000","8055261227743"]
["BATHROOM","ORIGINI","ORIGINI",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",246,"Gold PVD",252,"GPF143700P007G000","8056603631839"]
["BATHROOM","ORIGINI","ORIGINI",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",735,"Warm Bronze PVD",325,"GPF143760P037G000","8056603631778"]
["BATHROOM","ORIGINI","ORIGINI",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",708,"Copper Brushed PVD",346,"GPF143780P006G000","8056603633222"]
["BATHROOM","ORIGINI","ORIGINI",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",707,"Black Metal Brushed PVD",269,"GPF473510P004G000","8056603587051"]
["BATHROOM","ORIGINI","ORIGINI",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",147,"Chome Brushed",217,"GPF473500G006G000","8056603631723"]
["BATHROOM","ORIGINI","ORIGINI",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish","030","Copper PVD",143,"GPF541370P000G000","8056329573123"]
["BATHROOM","ORIGINI","ORIGINI",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections","031","Chrome",85,"GPF287460G001G000","8022692025996"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66401,66401,"wandgemonteerde witte zeep dispenser","Porte-savon mural blanc","Wall-mounted soap dish, white","031","Chrome",225,"GPF664010G001G000","8056603565974"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66402,66402,"wandgemonteerde zwarte zeep dispenser","Porte-savon mural noir","Wall-mounted soap dish, black",707,"Black Metal Brushed PVD",356,"GPF664020P004G000","8056603565844"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66407,66407,"wandgemonteerde witte beker houder","Porte-verre mural blanc","Wall-mounted holder, white",845,"Dark Bronze",415,"GPF664070V221G000","8056603565691"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66408,66408,"wandgemonteerde zwarte beker houder","Porte-verre mural noir","Wall-mounted holder, black",706,"Black Metal PVD",388,"GPF664080P001G000","8056603565653"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66413,66413,"wandgemonteerde witte zeep houder","Distributeur de savon liquide mural blanc","Wall-mounted liquid soap dispenser , white",727,"Brass Brushed PVD",663,"GPF664130P025G000","8056603565509"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66414,66414,"wandgemonteerde zwarte zeep houder","Distributeur de savon liquide mural noir","Wall-mounted liquid soap dispenser - black",727,"Brass Brushed PVD",663,"GPF664140P025G000","8056603565400"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66420,66420,"wandgemonteerde zwarte borstel houder","Porte-balayette mural noir","Wall-mounted brush holder, black",720,"Nickel PVD",658,"GPF664200P014G000","8056603565226"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",58525,58525,"Witte Staande Zeephouder","Porte-savon à poser blanc","Standing soap holder, white","030","Copper PVD",357,"GPF585250P000G000","8022692861389"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",58526,58526,"Zwarte Witte Staande Zeephouder","Porte-savon à poser noir","Standing soap holder, black",299,"Matte Black",327,"GPF585260C072G000","8056329062344"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",58531,58531,"Witte Staande Bekerhouder","Porte-verre à poser blanc.","Standing tumbler holder, white",720,"Nickel PVD",391,"GPF585310P014G000","8056603455916"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",58531,58531,"Witte Staande Bekerhouder","Porte-verre à poser blanc.","Standing tumbler holder, white",761,"Coffee Bronze Brushed PVD",444,"GPF585310E059G000","8055261594296"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66438,66438,"staande zwarte zeep dispenser","Distributeur de savon liquide à poser noir","Standing soap dispenser holder, black",149,"Finox Brushed Nickel",503,"GPF664380G002G000","8056603572934"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66438,66438,"staande zwarte zeep dispenser","Distributeur de savon liquide à poser noir","Standing soap dispenser holder, black",279,"Matte White",503,"GPF664380C071G000","8056603609272"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",58544,58544,"Zwarte Staande Borstelhouder","Porte-balayette à poser noir.","Standing brush holder, black","031","Chrome",467,"GPF585441G001G000","8056329062009"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",58544,58544,"Zwarte Staande Borstelhouder","Porte-balayette à poser noir.","Standing brush holder, black",845,"Dark Bronze",734,"GPF585441V221G000","8056603621960"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66455,66455,"toiletrol houder voor horizontaal/verticaal installatie","Porte-papier mural horizontal ou vertical","Horizontal/Vertical paper-roll holder",845,"Dark Bronze",325,"GPF664550V221G000","8056603565097"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66502,66502,"45 cm Handdoekhouder","Porte-serviette 45 cm","45 cm Towel rail",716,"Gold Brushed PVD",482,"GPF665020P005G000","8055261229174"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66504,66504,"60 cm Handdoekhouder","Porte-serviette 60 cm","60 cm Towel rail",726,"Warm Bronze Brushed PVD",479,"GPF665040P024G000","8056603564816"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66521,66521,"wandgemonteerde robe haak. Inleg met afwerking inbegrepen. Combineerbaar met verschillende afwerkingen met inleg 66600 of inlegART 66602","Patère mural. Insert en finition inclus. Combiner avec finitions differentes avec insert 66600 ou insert ART 66602","Wall-mounted robe hook. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",279,"Matte White",257,"GPF665210C071G000","8056603636346"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66523,66523,"wand gemonteerde badjas haak.","Patère murale","Wall-mounted robe hook.",708,"Copper Brushed PVD",217,"GPF665230P006G000","8056603632782"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66511,66511,"30 cm Handdoekhouder voor glasmontage","Porte-serviette 30 cm à fixer sur le verre","30 cm Towel rail for glass fixing",716,"Gold Brushed PVD",1148,"GPF665110P005G000","8055261229150"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",66515,66515,"60 cm Handdoekhouder voor glasmontage","Porte-serviette 60 cm à fixer sur le verre","60 cm Towel rail for glass fixing","030","Copper PVD",1227,"GPF665150P000G000","8056603636391"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",299,"Matte Black",1337,"GPF584241C072G000","8056329523401"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",45590,45590,"Papierbak wit","Poubelle blanche.","White waste-paper basket",246,"Gold PVD",913,"GPF455900P007G000","8056603597333"]
["BATHROOM","ORIGINI","ORIGINI ACCESSORIES",45590,45590,"Papierbak wit","Poubelle blanche.","White waste-paper basket",761,"Coffee Bronze Brushed PVD",913,"GPF455900E059G000","8055261602762"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",39114,39114,"wand gemonteerde WC (6 liters) in keramiek, geïntegreerde sifon. Hardware en pluggen voor laterale gaten niet inbegrepen.","Cuvette murale en céramique (6 litres) avec siphon intégré. Charnières et sièges non inclus.","Wall hung WC (6 litres) in Ceramic, integrated siphon. Hardware and lateral holes plugs not included.",531,"Matte White Ceramic",1249,"GPF391140C288G000","8056603626682"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",29463,29463,"Toiletzitting van antibacteriële hars voor artikel 39114. Te completeren met zachtsluitend beslag 37584 (niet inbegrepen).","Siège en résine antibactérienne pour cuvette 39114. À combiner avec les charnières 37584 (non inclues).","Anti-bacterical resin WC seat for item 39114. To be completed with soft-closing hardware 37584 (not included).","031","Chrome",275,"GPF294630G001G000","8022692786163"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",735,"Warm Bronze PVD",257,"GPF375842P037G000","8056329558748"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",707,"Black Metal Brushed PVD",154,"GPF375870P004G000","8022692430561"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",707,"Black Metal Brushed PVD",836,"GPF452300P004G000","8055261645646"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","030","Copper PVD",711,"GPF451310P000G000","8055261227385"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1240,"GPF452270P006G000","8055261645783"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1230,"GPF451240P025G000","8056603615761"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","030","Copper PVD",962,"GPF451231P000G000","8022692811674"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1354,"GPF452260P006G000","8055261645936"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",187,"Aged Bronze",1230,"GPF451260G052G000","8056603632959"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",246,"Gold PVD",1092,"GPF143313P007G000","8056329223974"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",707,"Black Metal Brushed PVD",1281,"GPF451211P004G000","8022692822861"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",246,"Gold PVD",1364,"GPF451211P007G000","8056603462327"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",54611,54611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",735,"Warm Bronze PVD",930,"GPF546110P037G000","8056329558724"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",54613,54613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",727,"Brass Brushed PVD",1495,"GPF546130P025G000","8056329070363"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",246,"Gold PVD",1003,"GPF546150P007G000","8056329070233"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",54617,54617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",281,"Matte Coral",903,"GPF546170T214G000","8056603609647"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",54619,54619,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaque de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",280,"Matte Ocra",1183,"GPF546190T213G000","8056603609630"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",54621,54621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",708,"Copper Brushed PVD",1749,"GPF546211P006G000","8056329540781"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",66603,66603,"vrijstaene waskom in Cristalplant®, zonder overflow waste","Vasque au sol en Cristalplant®, sans trop plein","Freestanding washbasin in Cristalplant®, without overflow waste. Grille-plug and syphon included.",507,"Cristalplant Matte Cipria",6346,"GPF666030B037G000","8056603587532"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",727,"Brass Brushed PVD",84,"GPF013460P025G000","8056329184220"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK",28767,28767,"Verlengstuk buis voor sifon, lengte 40 cm","Tubelure prolongée pour siphone, longueur 40 cm","Syphon pipe extension, 40 cm length",727,"Brass Brushed PVD",88,"GPF287670P025G000","8056329198999"]
["BATHROOM","ORIGINI","ORIGINI TOTAL LOOK","01377","01377","1 1/4\" sifon","Siphon 1 1/4”.","1 1/4\" syphon",726,"Warm Bronze Brushed PVD",455,"GPF013771P024G000","8022692878592"]
["BATHROOM","GESSI316","GESSI316 FLESSA",54002,54002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo, sans vidage, avec flexibles de raccordement.","Basin mixer, flexible connections, without waste",708,"Copper Brushed PVD",761,"GPF540020P006G000","8022692829853"]
["BATHROOM","GESSI316","GESSI316 FLESSA",54003,54003,"Mengkraan Wastafel hoog, lange uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec long. Avec vidage et flexibles de raccordement.","High version basin mixer , long spout, flexible connections, with waste",239,"Steel Brushed",726,"GPF540030A000G000","8022692829082"]
["BATHROOM","GESSI316","GESSI316 FLESSA",54012,54012,"3-gats wastafelmengkraan middelhoog zonder waste met buigzame aansluitslangen","Mélangeur moyen sans vidage avec flexibles de raccordement.","Medium version three-hole basin mixer, with flexible hoses. Without waste",299,"Matte Black",1278,"GPF540120C072G000","8056329601147"]
["BATHROOM","GESSI316","GESSI316 FLESSA","54198+54084",54084,"Extern deel Wand-Mengkraan Wastafel, uitloop aanpasbare lengte zonder waste","Partie apparente pour mitigeur lavabo mural, longueur à la demande, sans vidage.","External parts basin mixer, spout,length on request, without waste",299,"Matte Black",1469,"GPF540840C072G000","8056329600850"]
["BATHROOM","GESSI316","GESSI316 FLESSA","54198+54083",54083,"Extern deel Wand-Mengkraan Wastafel, middelgrote uitloop zonder waste","Partie apparente pour mitigeur lavabo mural sans vidage.","External parts basin mixer, medium spout, without waste",726,"Warm Bronze Brushed PVD",705,"GPF540830P024G000","8022692837797"]
["BATHROOM","GESSI316","GESSI316 FLESSA","45089+54094",54094,"Extern deel Wand 3-gats wastafelmengkraan lange uitloop zonder waste","Partie apparente pour mélangeur mural avec bec long sans vidage.","External parts three-holes basin mixer with long spout, without waste.",707,"Black Metal Brushed PVD",1144,"GPF540940P004G000","8022692849882"]
["BATHROOM","GESSI316","GESSI316 FLESSA",54210,54210,"Wanduitloop Wastafel uitloop aanpasbare lengte","Bec de lavabo mural, longueur à la demande","Wall-mounted spout basin, spout with length on request",299,"Matte Black",664,"GPF542100C072G000","8056329600119"]
["BATHROOM","GESSI316","GESSI316 FLESSA",54005,54005,"Mengkraan bladmontage","Commande séparée pour bec de lavabo","Basin counter separate control",727,"Brass Brushed PVD",579,"GPF540050P025G000","8056329184947"]
["BATHROOM","GESSI316","GESSI316 FLESSA","54055+54019",54019,"Extern deel Wandafstandsbediening Wastafel/Douche 1-weg","Partie apparente pour commande séparée lavabo/douche mural une sortie","External parts mixer one-way diverter",708,"Copper Brushed PVD",377,"GPF540190P006G000","8022692836158"]
["BATHROOM","GESSI316","GESSI316 TRAME",54309,54309,"Mengkraan Wastafel hoog, korte uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec court. Sans vidage, avec flexibles de raccordement.","High version basin mixer , short spout, flexible connections, without waste",726,"Warm Bronze Brushed PVD",1137,"GPF543090P024G000","8022692830491"]
["BATHROOM","GESSI316","GESSI316 TRAME",54303,54303,"Mengkraan Wastafel hoog, lange uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec long. Avec vidage et flexibles de raccordement.","High version basin mixer , long spout, flexible connections, with waste",727,"Brass Brushed PVD",1287,"GPF543030P025G000","8056329599703"]
["BATHROOM","GESSI316","GESSI316 TRAME","54198+54384",54198,"Inbouwdeel voor eengreeps inbouw wastafelmengkraan voor wandmontage.","Partie encastrée pour mitigeur lavabo mural.","Built-in part for mixer with spout.",239,"Steel Brushed",447,"GPF541980A000G000","8056329052345"]
["BATHROOM","GESSI316","GESSI316 TRAME","54198+54383",54383,"Extern deel Wand-Mengkraan Wastafel, middelgrote uitloop zonder waste","Partie apparente pour mitigeur lavabo mural sans vidage.","External parts basin mixer, medium spout, without waste",707,"Black Metal Brushed PVD",845,"GPF543830P004G000","8022692837964"]
["BATHROOM","GESSI316","GESSI316 TRAME","45089+54394",54394,"Extern deel Wand 3-gats wastafelmengkraan lange uitloop zonder waste","Partie apparente pour mélangeur mural avec bec long sans vidage.","External parts three-holes basin mixer with long spout, without waste.",708,"Copper Brushed PVD",1286,"GPF543940P006G000","8022692850970"]
["BATHROOM","GESSI316","GESSI316 TRAME",54399,54399,"Plafonduitloop. Aan te vullen met afstandsbediening TRAME","Bec au plafond TRAME. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout to be completed with separate control TRAME",707,"Black Metal Brushed PVD",2037,"GPF543990P004G000","8022692837155"]
["BATHROOM","GESSI316","GESSI316 TRAME",54305,54305,"Mengkraan bladmontage","Commande séparée.","Separate control",708,"Copper Brushed PVD",696,"GPF543050P006G000","8022692850772"]
["BATHROOM","GESSI316","GESSI316 INTRECCIO",54101,54101,"Mengkraan Wastafel met waste met buigzame aansluitslangen","Mitigeur lavabo, avec vidage et flexibles de raccordement.","Basin mixer, flexible connections, with waste",299,"Matte Black",950,"GPF541010C072G000","8056329600775"]
["BATHROOM","GESSI316","GESSI316 INTRECCIO",54104,54104,"Mengkraan Wastafel hoog, korte uitloop met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec court. Avec vidage et flexibles de raccordement","Basin mixer high , short spout, flexible connections, with waste",761,"Coffee Bronze Brushed PVD",1348,"GPF541040E059G000","8055261601673"]
["BATHROOM","GESSI316","GESSI316 INTRECCIO","54198+54190",54198,"Inbouwdeel voor eengreeps inbouw wastafelmengkraan voor wandmontage.","Partie encastrée pour mitigeur lavabo mural.","Built-in part for mixer with spout.",239,"Steel Brushed",447,"GPF541980A000G000","8056329052345"]
["BATHROOM","GESSI316","GESSI316 INTRECCIO","54198+54183",54183,"Extern deel Wand-Mengkraan Wastafel, middelgrote uitloop zonder waste","Partie apparente pour mitigeur lavabo mural sans vidage.","External parts basin mixer, medium spout, without waste",727,"Brass Brushed PVD",845,"GPF541830P025G000","8056329544895"]
["BATHROOM","GESSI316","GESSI316 INTRECCIO","54198+54189",54189,"Extern deel Wand-Mengkraan Wastafel, uitloop aanpasbare lengte zonder waste","Partie apparente pour mitigeur lavabo mural, longueur à la demande, sans vidage.","External parts basin mixer, spout,length on request, without waste",707,"Black Metal Brushed PVD",1688,"GPF541890P004G000","8022692836547"]
["BATHROOM","GESSI316","GESSI316 INTRECCIO",54091,54091,"Middelgrote wastafeluitloop","Bec de lavabo longueur moyenne","Medium spout basin",707,"Black Metal Brushed PVD",498,"GPF540910P004G000","8022692841176"]
["BATHROOM","GESSI316","GESSI316 INTRECCIO",54110,54110,"Wanduitloop Wastafel lange uitloop","Bec de lavabo mural long","Wall-mounted spout basin, long spout",761,"Coffee Bronze Brushed PVD",414,"GPF541100E059G000","8055261601574"]
["BATHROOM","GESSI316","GESSI316 INTRECCIO","54055+54119",54119,"Extern deel Wand-mengkraan 1-weg","Partie apparente pour mitigeur mural, 1 sortie.","External parts mixer one-way diverter",299,"Matte Black",413,"GPF541190C072G000","8056329600607"]
["BATHROOM","GESSI316","GESSI316 INTRECCIO",54107,54107,"Mengkraan Bidet met waste met buigzame aansluitslangen","Mitigeur bidet, avec flexibles de raccordement et vidage.","Bidet mixer, flexible connections, with waste",239,"Steel Brushed",704,"GPF541070A000G000","8022692829297"]
["BATHROOM","GESSI316","GESSI316 MECCANICA",54209,54209,"Mengkraan Wastafel hoog, korte uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec court. Sans vidage, avec flexibles de raccordement.","High version basin mixer , short spout, flexible connections, without waste",299,"Matte Black",1036,"GPF542090C072G000","8056329600133"]
["BATHROOM","GESSI316","GESSI316 MECCANICA",54206,54206,"Mengkraan Wastafel hoog, lange uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec long. Sans vidage, avec flexibles de raccordement.","High version basin mixer , long spout, flexible connections, without waste",707,"Black Metal Brushed PVD",1158,"GPF542060P004G000","8022692829617"]
["BATHROOM","GESSI316","GESSI316 MECCANICA","54198+54284",54284,"Extern deel Wand-Mengkraan Wastafel, uitloop aanpasbare lengte zonder waste","Partie apparente pour mitigeur lavabo mural, longueur à la demande, sans vidage.","External parts basin mixer, spout,length on request, without waste",707,"Black Metal Brushed PVD",1936,"GPF542840P004G000","8022692836745"]
["BATHROOM","GESSI316","GESSI316 MECCANICA","54198+54289",54289,"Extern deel Wand-Mengkraan Wastafel, uitloop aanpasbare lengte zonder waste","Partie apparente pour mitigeur lavabo mural, longueur à la demande, sans vidage.","External parts basin mixer, spout,length on request, without waste",708,"Copper Brushed PVD",1688,"GPF542890P006G000","8022692836837"]
["BATHROOM","GESSI316","GESSI316 MECCANICA","45089+54294",54294,"Extern deel Wand 3-gats wastafelmengkraan lange uitloop zonder waste","Partie apparente pour mélangeur mural avec bec long sans vidage.","External parts three-holes basin mixer with long spout, without waste.",708,"Copper Brushed PVD",1286,"GPF542940P006G000","8022692850697"]
["BATHROOM","GESSI316","GESSI316 MECCANICA",54110,54110,"Wanduitloop Wastafel lange uitloop","Bec de lavabo mural long","Wall-mounted spout basin, long spout",707,"Black Metal Brushed PVD",385,"GPF541100P004G000","8022692850000"]
["BATHROOM","GESSI316","GESSI316 MECCANICA",54299,54299,"Plafonduitloop. Aan te vullen met afstandsbediening MECCANICA","Bec au plafond MECCANICA. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout to be completed with separate control MECCANICA",708,"Copper Brushed PVD",2037,"GPF542990P006G000","8022692836912"]
["BATHROOM","GESSI316","GESSI316 CESELLO",54401,54401,"Mengkraan Wastafel met waste met buigzame aansluitslangen","Mitigeur lavabo, avec vidage et flexibles de raccordement.","Basin mixer, flexible connections, with waste",726,"Warm Bronze Brushed PVD",1042,"GPF544010P024G000","8022692830255"]
["BATHROOM","GESSI316","GESSI316 CESELLO",54409,54409,"Mengkraan Wastafel hoog, korte uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec court. Sans vidage, avec flexibles de raccordement.","High version basin mixer , short spout, flexible connections, without waste",707,"Black Metal Brushed PVD",1137,"GPF544090P004G000","8022692829686"]
["BATHROOM","GESSI316","GESSI316 CESELLO",54406,54406,"Mengkraan Wastafel hoog, lange uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec long. Sans vidage, avec flexibles de raccordement.","High version basin mixer , long spout, flexible connections, without waste",707,"Black Metal Brushed PVD",1158,"GPF544060P004G000","8022692829631"]
["BATHROOM","GESSI316","GESSI316 CESELLO","54198+54490",54490,"Extern deel Wand-Mengkraan Wastafel lange uitloop zonder waste","Partie apparente mitigeur lavabo mural avec bec long sans vidage","External parts wall-mounted basin mixer, long spout, without waste",239,"Steel Brushed",669,"GPF544900A000G000","8022692837353"]
["BATHROOM","GESSI316","GESSI316 CESELLO","54198+54483",54483,"Extern deel Wand-Mengkraan Wastafel, middelgrote uitloop zonder waste","Partie apparente pour mitigeur lavabo mural sans vidage.","External parts basin mixer, medium spout, without waste",239,"Steel Brushed",574,"GPF544830A000G000","8022692837995"]
["BATHROOM","GESSI316","GESSI316 CESELLO","54198+54489",54489,"Extern deel Wand-Mengkraan Wastafel, uitloop aanpasbare lengte zonder waste","Partie apparente pour mitigeur lavabo mural, longueur à la demande, sans vidage.","External parts basin mixer, spout,length on request, without waste",708,"Copper Brushed PVD",1688,"GPF544890P006G000","8022692837339"]
["BATHROOM","GESSI316","GESSI316 CESELLO",54110,54110,"Wanduitloop Wastafel lange uitloop","Bec de lavabo mural long","Wall-mounted spout basin, long spout",708,"Copper Brushed PVD",385,"GPF541100P006G000","8022692850017"]
["BATHROOM","GESSI316","GESSI316 CESELLO",54496,54496,"Plafonduitloop aanpasbare hoogte. Aan te vullen met afstandsbediening CESELLO","Bec au plafond CESELLO, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout, length on request, to be completed with separate control CESELLO",707,"Black Metal Brushed PVD",2688,"GPF544960P004G000","8022692851298"]
["BATHROOM","GESSI316","GESSI316 CESELLO","54055+54419",54419,"Extern deel Wand-mengkraan 1-weg","Partie apparente pour mitigeur mural, 1 sortie.","External parts mixer one-way diverter",707,"Black Metal Brushed PVD",451,"GPF544190P004G000","8022692837193"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",54037,54037,"Groep Badrand 4 gaten met wateruitloop, omstelknop, buigzame slang 1,50 m en antikalk-handdouche","Mélangeur bain-douche avec bec, inverseur, flexibles de raccordement 1,50m et douchette anticalcaire.","Four-holes bath mixer with diverter, tub-filler spout and 1,50 m flexible hose and antilimestone handshower",708,"Copper Brushed PVD",2222,"GPF540370P006G000","8022692849592"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",54592,54592,"Uittrekbare handdouchekit. Niet geschikt voor artikels 01669, 01658, 01663, 01664.","Système de récupération eau pour flexible de douchette bain-douche. Non compatible avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit. Not fitting items 01669, 01658, 01663 and 01664.",726,"Warm Bronze Brushed PVD",1124,"GPF545920P024G000","8056329077263"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","01080","01080","Polyethyleen badafvoer met overloopdopvuller. Lengte van de aanvoer leiding 80 cm","Vidage en polyéthylène baignoire avec trop-plein. Longueur 80 cm","Polyethylene column bath waste with overflow cap filler. Length of control cable 80 cm",735,"Warm Bronze PVD",639,"GPF010802P037G000","8056329559240"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",20191,20191,"Cascade-uitloop Badrand Aan te vullen met afstandsbediening","Bec cascade pour baignoire à compléter par un mitigeur à commande séparée.","Bath group waterfall spout to be completed with separate control",761,"Coffee Bronze Brushed PVD",2840,"GPF201910E059G000","8055261609471"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",54195,54195,"Extern deel vrijstaande wastafel mengkraan.","Bec de baignoire au sol. À compléter par commande séparée","Freestanding bath spout. To be completed with separate control",239,"Steel Brushed",1306,"GPF541950A000G000","8056329224636"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",54008,54008,"Wanduitloop Bad","Bec de bagnoire mural latéral","Wall-fixing bath spout",707,"Black Metal Brushed PVD",366,"GPF540080P004G000","8022692841329"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",299,"Matte Black",356,"GPF540580C072G000","8056329536968"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",713,"Antique Brass",388,"GPF540580V204G000","8056603509398"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","54073+54077",54077,"Extern deel Wandmengkraan Douche 2-weg","Partie apparentepour mitigeur douche mura deux sorties","External parts wall-mounted for shower mixer, two-way with diverter",707,"Black Metal Brushed PVD",877,"GPF540770P004G000","8056329535893"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","54169+54232","54232","Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche mural 1 sortie.","External parts for thermostatic mixer, one-way diverter",299,"Matte Black",1144,"GPF542320C072G000","8056329599970"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","09264+54334","09264","Inbouwdeel voor thermostatische mengkraan, 2 separate uitgangen","Partie encastrée du mitigeur thermostatique mural 2 sorties indépendantes","Built-in part for thermostatic mixer, TWO separate exits","031","Chrome",1053,"GPF092640G001G000","8056603620796"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","09268+54338","54338","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie externe mitigeur thermostatique mural à 4 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with four separate exits.",299,"Matte Black",1707,"GPF543380C072G000","8056603620185"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","43103+54514","54514","Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",726,"Warm Bronze Brushed PVD",1287,"GPF545140P024G000","8022692851359"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","43105+54516","54516","Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",726,"Warm Bronze Brushed PVD",1579,"GPF545160P024G000","8022692851397"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","43107+54518","54518","Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",708,"Copper Brushed PVD",1874,"GPF545180P006G000","8022692851427"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","43109+54510","54510","Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",299,"Matte Black",1972,"GPF545100C072G000","8056329598997"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",45163,45163,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted shower head",246,"Gold PVD",3070,"GPF451630P007G000","8056603637480"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",54148,54148,"Oriënteerbare wand-hoofddouchekop","Pomme de douche orientable anticalcaire avec bras mural.","Wall-mounted adjustable showerhead",726,"Warm Bronze Brushed PVD",2746,"GPF541481P024G000","8022692850260"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",54146,54146,"Verstelbare plafonddouche.","Pomme de douche au plafond orientable","Ceiling-mounted adjustable headshower.",239,"Steel Brushed",1355,"GPF541460A000G000","8055261227187"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",54147,54147,"Verstelbare plafonddouche. lengte op aanvraag.","Pomme de douche au plafond orientable. Longueur personnalisable.","Ceiling-mounted adjustable headshower. Length on request.",707,"Black Metal Brushed PVD",2697,"GPF541470P004G000","8055261227095"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",54023,54023,"Doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m.","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",239,"Steel Brushed",523,"GPF540230A000G000","8022692841350"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",735,"Warm Bronze PVD",940,"GPF630990P037G000","8056329558199"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",63199,63199,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en Darkflex buigzame slang 1,50 m","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et Darkflex flexibles 1,50 m.","Magnetic shower set with water outlet, 1,50 m Darkflex flexible hose and antilimestone handshower",761,"Coffee Bronze Brushed PVD",1067,"GPF631990E059G000","8055261593633"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",32971,32971,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet","030","Copper PVD",444,"GPF329710P000G000","8022692623192"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",32977,32977,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",187,"Aged Bronze",411,"GPF329771G052G000","8056329037243"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",13375,13375,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","Adjustable lateral body jet",299,"Matte Black",288,"GPF133750C072G000","8056329037434"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",13375,13375,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","Adjustable lateral body jet",713,"Antique Brass",337,"GPF133750V204G000","8056329037397"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",735,"Warm Bronze PVD",1506,"GPF202950P037G000","8056329559073"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",65295,65295,"Afbouwdeel Voor Waterval Douche Uitloop Nog Compleet Te Maken Met Separate Bediening (Niet Inclusief)","Partie apparente pour bec cascade de douche murale. À compléter par commande séparée.","Waterfall shower spout to be completed with separate control (not included)",716,"Gold Brushed PVD",1710,"GPF652950P005G000","8056603711364"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",54054,54054,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",299,"Matte Black",291,"GPF540540C072G000","8056329225220"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",706,"Black Metal PVD",143,"GPF541370P001G000","8056329573178"]
["BATHROOM","GESSI316","GESSI316 BATH-SHOWER","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections","030","Copper PVD",113,"GPF016370P000G000","8022692671254"]
["BATHROOM","GESSI316","GESSI316 ACCESSORIES",54701,54701,"Wand-zeepbakje wit","Porte-savon mural blanc.","Wall-mounted soap dish, white",726,"Warm Bronze Brushed PVD",930,"GPF547010P024G000","8022692851595"]
["BATHROOM","GESSI316","GESSI316 ACCESSORIES",54708,54708,"Glashouder wit voor wandmontage.","Porte-verre mural noir.","Wall-mounted holder, black",299,"Matte Black",663,"GPF547080C072G000","8056329598386"]
["BATHROOM","GESSI316","GESSI316 ACCESSORIES",54714,54714,"Zeepdispenser zwart voor wandmontage.","Distributeur de savon liquide mural noir.","Wall-mounted liquid soap dispenser - black",761,"Coffee Bronze Brushed PVD",1331,"GPF547141E059G000","8055261598294"]
["BATHROOM","GESSI316","GESSI316 ACCESSORIES",54726,54726,"Zeephouder wit staand.","Porte-savon à poser noir.","Standing soap holder, black",726,"Warm Bronze Brushed PVD",585,"GPF547260P024G000","8056329063013"]
["BATHROOM","GESSI316","GESSI316 ACCESSORIES",54738,54738,"Zeepdispenser wit staand.","Distributeur de savon liquide à poser noir.","Standing soap dispenser holder, black",707,"Black Metal Brushed PVD",899,"GPF547381P004G000","8056329062955"]
["BATHROOM","GESSI316","GESSI316 ACCESSORIES",54743,54743,"Staande toiletborstelhouder wit","Porte-balayette à poser blanche.","Standing brush holder, white",726,"Warm Bronze Brushed PVD",673,"GPF547431P024G000","8022692851878"]
["BATHROOM","GESSI316","GESSI316 ACCESSORIES",54749,54749,"Wand-toiletrolhouder","Porte-papier mural.","Wall-mounted paper roll holder. Vertical/horizontal installation",707,"Black Metal Brushed PVD",848,"GPF547491P004G000","8055261432659"]
["BATHROOM","GESSI316","GESSI316 ACCESSORIES",54803,54803,"Handdoekhouder 60 cm","Porte-serviette 60 cm.","60 cm towel rail",761,"Coffee Bronze Brushed PVD",1011,"GPF548030E059G000","8055261597976"]
["BATHROOM","GESSI316","GESSI316 ACCESSORIES",54925,54925,"Handdoekhouder 60 cm","Porte-serviette 60 cm à fixer sur le verre.","60 cm towel rail for glass fixing",727,"Brass Brushed PVD",1208,"GPF549250P025G000","8056329598188"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",39114,39114,"wand gemonteerde WC (6 liters) in keramiek, geïntegreerde sifon. Hardware en pluggen voor laterale gaten niet inbegrepen.","Cuvette murale en céramique (6 litres) avec siphon intégré. Charnières et sièges non inclus.","Wall hung WC (6 litres) in Ceramic, integrated siphon. Hardware and lateral holes plugs not included.",532,"Matte Black Ceramic",1249,"GPF391140C289G000","8056603626699"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",29463,29463,"Toiletzitting van antibacteriële hars voor artikel 39114. Te completeren met zachtsluitend beslag 37584 (niet inbegrepen).","Siège en résine antibactérienne pour cuvette 39114. À combiner avec les charnières 37584 (non inclues).","Anti-bacterical resin WC seat for item 39114. To be completed with soft-closing hardware 37584 (not included).",299,"Matte Black",411,"GPF294630C072G000","8056329097667"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",727,"Brass Brushed PVD",154,"GPF375870P025G000","8056329081987"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","030","Copper PVD",783,"GPF452300P000G000","8055261645660"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",727,"Brass Brushed PVD",758,"GPF451300P025G000","8055261227477"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",708,"Copper Brushed PVD",758,"GPF451310P006G000","8055261227347"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1161,"GPF452270P037G000","8055261645738"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1354,"GPF452260P025G000","8055261645899"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",717,"GPF144310G001G000","8055261646131"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",878,"GPF143313G002G000","8022692792669"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1482,"GPF451220P004G000","8056603616010"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",54611,54611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12","031","Chrome",630,"GPF546110G001G000","8056329070622"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",54611,54611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",187,"Aged Bronze",930,"GPF546110G052G000","8056329070615"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",720,"Nickel PVD",883,"GPF546150P014G000","8056603456890"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",761,"Coffee Bronze Brushed PVD",947,"GPF546150E059G000","8055261598850"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",54617,54617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",761,"Coffee Bronze Brushed PVD",1057,"GPF546170E059G000","8055261574373"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",54619,54619,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaque de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",707,"Black Metal Brushed PVD",1386,"GPF546190P004G000","8056329540927"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",54621,54621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",708,"Copper Brushed PVD",1749,"GPF546211P006G000","8056329540781"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",54681,54681,"bedieningspaneel DIAMANTATO voor GEBERIT SIGMA 8 & 12","Plaque de finissage DIAMANTATO pour GEBRIT SIGMA 8 et 12","Cover plate DIAMANTATO for GEBERIT SIGMA 8 & 12",720,"Nickel PVD",1960,"GPF546810P014G000","8056603458191"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",708,"Copper Brushed PVD",3783,"GPF546010P006G000","8022692851540"]
["BATHROOM","GESSI316","GESSI316 TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",727,"Brass Brushed PVD",3783,"GPF546010P025G000","8056329085220"]
["BATHROOM","INCISO","INCISO -",58012,58012,"3-gats wastafelmengkraan zonder waste met buigzame aansluitslangen","Mélangeur trois trous sans vidage avec flexibles de raccordement","three-holes basin mixer, with flexible hoses. Without waste",706,"Black Metal PVD",1686,"GPF580120P001G000","8022692861563"]
["BATHROOM","INCISO","INCISO -",58012,58012,"3-gats wastafelmengkraan zonder waste met buigzame aansluitslangen","Mélangeur trois trous sans vidage avec flexibles de raccordement","three-holes basin mixer, with flexible hoses. Without waste",713,"Antique Brass",1799,"GPF580120V204G000","8022692872217"]
["BATHROOM","INCISO","INCISO -",58013,58013,"3-gats wastafelmengkraan middelhoog met waste met buigzame aansluitslangen","Mélangeur trois trous hauteur moyenne avec vidage et flexibles de raccordement","Medium version three-holes basin mixer, with flexible hoses with waste",761,"Coffee Bronze Brushed PVD",1955,"GPF580130E059G000","8055261596498"]
["BATHROOM","INCISO","INCISO -",58014,58014,"3-gats wastafelmengkraan middelhoog zonder waste met buigzame aansluitslangen","Mélangeur trois trous hauteur moyenne sans vidage avec flexibles de raccordement","Medium version three-hole basin mixer, with flexible hoses. Without waste",845,"Dark Bronze",1799,"GPF580140V221G000","8056603623025"]
["BATHROOM","INCISO","INCISO -","45089+58090",58090,"Extern deel Wand 3-gats wastafelmengkraan middelgrote uitloop zonder waste","Partie apparente mélangeur lavabo mural trois sorties avec bec moyen sans vidage","External parts three-holes basin mixer with medium spout, without waste.",713,"Antique Brass",1181,"GPF580900V204G000","8022692872279"]
["BATHROOM","INCISO","INCISO -",58002,58002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo, sans vidage, avec flexibles de raccordement.","Basin mixer, flexible connections, without waste","031","Chrome",652,"GPF580020G001G000","8022692870411"]
["BATHROOM","INCISO","INCISO -",58002,58002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo, sans vidage, avec flexibles de raccordement.","Basin mixer, flexible connections, without waste",761,"Coffee Bronze Brushed PVD",1095,"GPF580020E059G000","8055261596658"]
["BATHROOM","INCISO","INCISO -",58003,58003,"Mengkraan Wastafel hoog, met waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, avec vidage et flexibles de raccordement.","High basin mixer, flexible connections, with waste",716,"Gold Brushed PVD",1247,"GPF580030P005G000","8056329538207"]
["BATHROOM","INCISO","INCISO -",58009,58009,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo, sans vidage, avec flexibles de raccordement.","Basin mixer, flexible connections, without waste","031","Chrome",721,"GPF580090G001G000","8056329626768"]
["BATHROOM","INCISO","INCISO -",58006,58006,"Mengkraan Wastafel hoog, zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, sans vidage, avec flexibles de raccordement.","High basin mixer, flexible connections, without waste",713,"Antique Brass",1241,"GPF580060V204G000","8056329626928"]
["BATHROOM","INCISO","INCISO -","54198+58088",58088,"Extern deel Wand-Mengkraan Wastafel wand korte uitloop zonder waste","Partie apparente mitigeur lavabo muralavec bec court sans vidage","External parts for wall-mounted basin mixer, short spout, without waste",713,"Antique Brass",939,"GPF580880V204G000","8022692872316"]
["BATHROOM","INCISO","INCISO -",58100,58100,"Wanduitloop Wastafel middelgrote uitloop","Bec de lavabo mural moyen","Wall-mounted spout basin, medium spout",149,"Finox Brushed Nickel",381,"GPF581000G002G000","8022692871012"]
["BATHROOM","INCISO","INCISO -",58100,58100,"Wanduitloop Wastafel middelgrote uitloop","Bec de lavabo mural moyen","Wall-mounted spout basin, medium spout",726,"Warm Bronze Brushed PVD",446,"GPF581000P024G000","8056329596788"]
["BATHROOM","INCISO","INCISO -","54055+58109",58109,"Extern deel Wandafstandsbediening Wastafel/Douche 1-weg","Partie apparente pour commande séparée lavabo/douche mural une sortie","External parts mixer one-way diverter",149,"Finox Brushed Nickel",331,"GPF581090G002G000","8022692871050"]
["BATHROOM","INCISO","INCISO -",58199,58199,"Plafonduitloop. Aan te vullen met afstandsbediening","Bec au plafond à compléter par un mitigeur à commande séparée.","Ceiling-mounted spout to be completed with separate control",710,"Brass PVD",1807,"GPF581990P011G000","8056329595811"]
["BATHROOM","INCISO","INCISO -",58199,58199,"Plafonduitloop. Aan te vullen met afstandsbediening","Bec au plafond à compléter par un mitigeur à commande séparée.","Ceiling-mounted spout to be completed with separate control",845,"Dark Bronze",1929,"GPF581990V221G000","8056603622530"]
["BATHROOM","INCISO","INCISO -",58093,58093,"Middelgrote wastafeluitloop","Bec de lavabo longueur moyenne","Medium spout basin",726,"Warm Bronze Brushed PVD",933,"GPF580930P024G000","8056329564053"]
["BATHROOM","INCISO","INCISO -",58200,58200,"Mengkraan bladmontage","Commande séparée.","Separate control","030","Copper PVD",543,"GPF582000P000G000","8056329019683"]
["BATHROOM","INCISO","INCISO -",58103,58103,"Vloeruitloop Bad","Bec de bagnoire mural latéral","Wall-fixing bath spout",707,"Black Metal Brushed PVD",479,"GPF581030P004G000","8022692873689"]
["BATHROOM","INCISO","INCISO -","65099+58029",58029,"Extern deel voor externe standaard bad met handdouche","Partie apparente pour mélangeur bain-douche sur pied avec douchette et flexible.","External parts for freestanding external bath mixer with automatic diverter.",708,"Copper Brushed PVD",4139,"GPF580290P006G000","8056329537682"]
["BATHROOM","INCISO","INCISO -",58040,58040,"Badrandgroep 5 gaten met wateruitloop, omstelknop, buigzame slang 1,50 m en antikalk-handdouche","Mélangeur de baignoire avec bec, inverseur, flexibles de raccordement 1,50m et douchette anticalcaire","Five-holes bath mixer with diverter, tub-filler spout and 1,50 m flexible hose, antilimestone handshower",149,"Finox Brushed Nickel",2692,"GPF580400G002G000","8022692871159"]
["BATHROOM","INCISO","INCISO -",58043,58043,"Badrandgroep 4 gaten met omstelknop, buigzame slang 1,50 m en antikalk-handdouche. Afgifte naar de badkolom","Mélangeur bain-douche avec inverseur, flexibles de raccordement 1,50m et douchette anticalcaire.","Four-holes bath mixer, diverter, 1,50 mflexible hose and pull-out handshower. To be used withoverflow filler","030","Copper PVD",2390,"GPF580430P000G000","8022692861020"]
["BATHROOM","INCISO","INCISO -","01664","01664","Four-holes finishing plaatje voor montage box","Plaque de finition 4 trous pour la boîte de sécurité","Four-holes finishing plate for mounting box",299,"Matte Black",586,"GPF016641C072G000","8022692888591"]
["BATHROOM","INCISO","INCISO -","01758","01758","Afwerkplaat 5 gaten voor secur box","Plaque de finition pour Secu Box robinetterie 5 trous","Five-holes finishing plate for mounting box",149,"Finox Brushed Nickel",612,"GPF017580G002G000","8022692882995"]
["BATHROOM","INCISO","INCISO -","01814","01814","Uittrekbare handdouchekit, zijrand installatie. Niet geschikt voor artikels 01669, 01658, 01663, 01664.","Système de récupération eau pour flexible de douchette bain-douche, installation sur plan de bagnoire. Non compatible avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, rim installation. Not fitting items 01669, 01658, 01663 and 01664.","031","Chrome",867,"GPF018140G001G000","8056329058095"]
["BATHROOM","INCISO","INCISO -","01080","01080","Polyethyleen badafvoer met overloopdopvuller. Lengte van de aanvoer leiding 80 cm","Vidage en polyéthylène baignoire avec trop-plein. Longueur 80 cm","Polyethylene column bath waste with overflow cap filler. Length of control cable 80 cm","031","Chrome",404,"GPF010802G001G000","8022692013580"]
["BATHROOM","INCISO","INCISO -","01080","01080","Polyethyleen badafvoer met overloopdopvuller. Lengte van de aanvoer leiding 80 cm","Vidage en polyéthylène baignoire avec trop-plein. Longueur 80 cm","Polyethylene column bath waste with overflow cap filler. Length of control cable 80 cm",845,"Dark Bronze",680,"GPF010802V221G000","8056603623254"]
["BATHROOM","INCISO","INCISO +",58111,58111,"3-gats wastafelmengkraan met waste met buigzame aansluitslangen","Mélangeur avec vidage et flexibles de raccordement.","Three-holes basin mixer , with flexible hoses with waste",149,"Finox Brushed Nickel",1653,"GPF581110G002G000","8022692858211"]
["BATHROOM","INCISO","INCISO +",58112,58112,"3-gats wastafelmengkraan zonder waste met buigzame aansluitslangen","Mélangeur sans vidage avec flexibles de raccordement.","three-holes basin mixer, with flexible hoses. Without waste",187,"Aged Bronze",1896,"GPF581120G052G000","8022692858594"]
["BATHROOM","INCISO","INCISO +",58113,58113,"3-gats wastafelmengkraan middelhoog met waste met buigzame aansluitslangen","Mélangeur moyen avec vidage et flexibles de raccordement.","Medium version three-holes basin mixer, with flexible hoses with waste",713,"Antique Brass",1932,"GPF581130V204G000","8022692858495"]
["BATHROOM","INCISO","INCISO +","45089+58190",58190,"Extern deel Wand 3-gats wastafelmengkraan middelgrote uitloop zonder waste","Partie apparente pour mélangeur mural avec bec moyen sans vidage","External parts three-holes basin mixer with medium spout, without waste.",720,"Nickel PVD",1199,"GPF581900P014G000","8056603606165"]
["BATHROOM","INCISO","INCISO +","45089+58190",58190,"Extern deel Wand 3-gats wastafelmengkraan middelgrote uitloop zonder waste","Partie apparente pour mélangeur mural avec bec moyen sans vidage","External parts three-holes basin mixer with medium spout, without waste.",845,"Dark Bronze",1281,"GPF581900V221G000","8056603622554"]
["BATHROOM","INCISO","INCISO +","65099+58129",58129,"Extern deel voor externe standaard bad met handdouche","Partie apparente pour mélangeur bain-douche sur pied avec douchette et flexible.","External parts for freestanding external bath mixer with handshower and automatic diverter",299,"Matte Black",3623,"GPF581290C072G000","8056329544161"]
["BATHROOM","INCISO","INCISO +",58140,58140,"Badrandgroep 5 gaten met wateruitloop, omstelknop, buigzame slang 1,50 m en antikalk-handdouche","Mélangeur de baignoire avec bec, inverseur, flexibles de raccordement 1,50m et douchette anticalcaire","Five-holes bath mixer with diverter, tub-filler spout and 1,50 m flexible hose, antilimestone handshower",710,"Brass PVD",3042,"GPF581400P011G000","8056329596269"]
["BATHROOM","INCISO","INCISO +",58143,58143,"Badrandgroep 4 gaten met omstelknop, buigzame slang 1,50 m en antikalk-handdouche. Afgifte naar de badkolom","Mélangeur bain-douche avec inverseur, flexibles de raccordement 1,50m et douchette anticalcaire.","Four-holes bath mixer, diverter, 1,50 mflexible hose and pull-out handshower. To be used withoverflow filler",727,"Brass Brushed PVD",2652,"GPF581430P025G000","8022692858457"]
["BATHROOM","INCISO","INCISO +","01664","01664","Four-holes finishing plaatje voor montage box","Plaque de finition 4 trous pour la boîte de sécurité","Four-holes finishing plate for mounting box","031","Chrome",491,"GPF016641G001G000","8022692037623"]
["BATHROOM","INCISO","INCISO +","01758","01758","Afwerkplaat 5 gaten voor secur box","Plaque de finition pour Secu Box robinetterie 5 trous","Five-holes finishing plate for mounting box",147,"Chome Brushed",612,"GPF017580G006G000","8056329184114"]
["BATHROOM","INCISO","INCISO +","01814","01814","Uittrekbare handdouchekit, zijrand installatie. Niet geschikt voor artikels 01669, 01658, 01663, 01664.","Système de récupération eau pour flexible de douchette bain-douche, installation sur plan de bagnoire. Non compatible avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, rim installation. Not fitting items 01669, 01658, 01663 and 01664.",149,"Finox Brushed Nickel",1038,"GPF018140G002G000","8056329058088"]
["BATHROOM","INCISO","INCISO +","01080","01080","Polyethyleen badafvoer met overloopdopvuller. Lengte van de aanvoer leiding 80 cm","Vidage en polyéthylène baignoire avec trop-plein. Longueur 80 cm","Polyethylene column bath waste with overflow cap filler. Length of control cable 80 cm",147,"Chome Brushed",504,"GPF010802G006G000","8022692115079"]
["BATHROOM","INCISO","INCISO +",20191,20191,"Cascade-uitloop Badrand Aan te vullen met afstandsbediening","Bec cascade pour baignoire à compléter par un mitigeur à commande séparée.","Bath group waterfall spout to be completed with separate control","031","Chrome",1690,"GPF201910G001G000","8022692028911"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","54139+58345","58345","afbouwdelen wandgemonteerd for douche kraan, 2-weg omstel, water uitgang, handdouche haak.","Parties apparentes mitigeur de baignoire mural deux sorties, avec inverseur, prise d'eau et support pour douchette","External parts wall-mounted for shower mixer, two way with diverter, water outlet, handshower hook.",149,"Finox Brushed Nickel",1199,"GPF583450G002G000","8056603629249"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","54139+58345","58345","afbouwdelen wandgemonteerd for douche kraan, 2-weg omstel, water uitgang, handdouche haak.","Parties apparentes mitigeur de baignoire mural deux sorties, avec inverseur, prise d'eau et support pour douchette","External parts wall-mounted for shower mixer, two way with diverter, water outlet, handshower hook.",761,"Coffee Bronze Brushed PVD",1493,"GPF583450E059G000","8055261594838"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","54055+58109","54055","Inbouwdeel Voor Wandgemonteerde Douche/Wastafelmengkraan, 1-Weg","Partie encastrée pour mitigeur lavabo/douche mural une sortie","Built-in part for wall-mounted shower/basin mixer, one way",239,"Steel Brushed",296,"GPF540550A000G000","8022692835960"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","54073+58077","58077","Afbouwdeel wand gemonteerd 2-weg douche mengkraan.","Partie apparente mitigeur douche mural 2 voies avec inverseur bain/douche.","External part wall-mounted two ways shower mixer.",713,"Antique Brass",1060,"GPF580770V204G000","8055261194632"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","44673+58079","58079","Extern deel Wand-Mengkraan 2-weg met automatische omstelknop bad/douche","Partie apparente mitigeur mural avec inverseur automatique bain-douche deux sorties","External parts for wall-mounted mixer two-way, automatic bath/ shower diverter",149,"Finox Brushed Nickel",908,"GPF580790G002G000","8022692871180"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","44673+58079","58079","Extern deel Wand-Mengkraan 2-weg met automatische omstelknop bad/douche","Partie apparente mitigeur mural avec inverseur automatique bain-douche deux sorties","External parts for wall-mounted mixer two-way, automatic bath/ shower diverter",716,"Gold Brushed PVD",1129,"GPF580790P005G000","8056603119375"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","54169+58131","58131","Afbouwdeel wand gemonteerd 1-weg thermostatische mengkraan.","Partie apparente mitigeur thermostatique mural 1 voie.","External part wall-mounted one way thermostatic mixer.",735,"Warm Bronze PVD",1267,"GPF581310P037G000","8055261194496"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","54169+58133","58133","Afbouwdeel wand gemonteerd 2-weg thermostatische mengkraan.","Partie apparente mitigeur thermostatique mural 2 voies.","External part wall-mounted two ways thermostatic mixer.",187,"Aged Bronze",1354,"GPF581330G052G000","8055261194434"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09269+58132","58132","Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche mural 1 sortie.","External parts for thermostatic mixer, one-way diverter",708,"Copper Brushed PVD",1433,"GPF581320P006G000","8022692884241"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09269+58232","58232","Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche mural 1 sortie.","External parts for thermostatic mixer, one-way diverter",716,"Gold Brushed PVD",1525,"GPF582320P005G000","8056603915366"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09269+58134","58134","Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche mural 2 sorties.","External parts for thermostatic mixer, two-way diverter",706,"Black Metal PVD",1341,"GPF581340P001G000","8022692861839"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09269+58234","58234","Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche mural 2 sorties.","External parts for thermostatic mixer, two-way diverter","031","Chrome",908,"GPF582340G001G000","8056329066830"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09269+58136","58136","Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche mural 3 sorties.","External parts for thermostatic mixer, three-way diverter",716,"Gold Brushed PVD",1525,"GPF581360P005G000","8055261230675"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09264+58334","09264","Inbouwdeel voor thermostatische mengkraan, 2 separate uitgangen","Partie encastrée du mitigeur thermostatique mural 2 sorties indépendantes","Built-in part for thermostatic mixer, TWO separate exits","031","Chrome",1053,"GPF092640G001G000","8056603620796"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09264+58334","58334","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie externe mitigeur thermostatique mural à 2 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with two separate exits.",735,"Warm Bronze PVD",1668,"GPF583340P037G000","8056603619981"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09264+58434","58434","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie externe mitigeur thermostatique mural à 2 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with two separate exits.",187,"Aged Bronze",1779,"GPF584340G052G000","8056603619578"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09266+58436","58436","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie externe mitigeur thermostatique mural à 3 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with three separate exits.",710,"Brass PVD",1938,"GPF584360P011G000","8056603619349"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09268+58338",58338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie externe mitigeur thermostatique mural à 4 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with four separate exits.",710,"Brass PVD",2198,"GPF583380P011G000","8056603619684"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09268+58438","58438","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie externe mitigeur thermostatique mural à 4 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with four separate exits.",710,"Brass PVD",2198,"GPF584380P011G000","8056603619172"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09263+58340","58340","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie externe mitigeur thermostatique mural à 5 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with five separate exits.","030","Copper PVD",2412,"GPF583400P000G000","8056603630757"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","09263+58440","58440","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie externe mitigeur thermostatique mural à 5 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with five separate exits.",708,"Copper Brushed PVD",2574,"GPF584400P006G000","8056603630542"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43103+58204","58204","Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douchel haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",707,"Black Metal Brushed PVD",2389,"GPF582040P004G000","8022692873788"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43103+58224","58224","Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",299,"Matte Black",1889,"GPF582240C072G000","8056329067394"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43103+58344","58344","Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",299,"Matte Black",1889,"GPF583440C072G000","8056329066403"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43105+58206","58206","Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",706,"Black Metal PVD",2327,"GPF582060P001G000","8022692861860"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43105+58216","43105","Inbouwdeel Thermostatische mengkraan hoog debiet 3 onafhankelijke uitgangen","Partie encastrée mitigeur THERMOSTATIQUE douche haut débit, trois sorties indépendantes. Installation verticale/horizontale.","Built-in thermostatic high-capacity mixer with THREE SEPARATE EXITS. Vertical/Horizontal installation.","031","Chrome",1173,"GPF431053G001G000","8022692583199"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43105+58226","58226","Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",720,"Nickel PVD",2327,"GPF582260P014G000","8056603552141"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43105+58346","58346","Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",716,"Gold Brushed PVD",2799,"GPF583460P005G000","8055261230330"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43107+58218","58218","Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",707,"Black Metal Brushed PVD",3144,"GPF582180P004G000","8022692873849"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43107+58218","58218","Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",710,"Brass PVD",2858,"GPF582180P011G000","8056329595613"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43107+58348","58348","Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",735,"Warm Bronze PVD",2858,"GPF583480P037G000","8056329595156"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43109+58210","58210","Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",149,"Finox Brushed Nickel",2742,"GPF582100G002G000","8022692871258"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43109+58220","58220","Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",707,"Black Metal Brushed PVD",3472,"GPF582200P004G000","8022692873856"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43109+58230","58230","Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS","031","Chrome",1630,"GPF582300G001G000","8056329067059"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43109+58350","58350","Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",299,"Matte Black",2742,"GPF583500C072G000","8056329066076"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43283+58263","58263","Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit.","External parts for stop valve for thermostatic high-capacity mixer.","031","Chrome",305,"GPF582630G001G000","8022692870671"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43283+58363","43283","Inbouwdeel Voor Stop Kraan Voor Thermostatische Hoog-Debiet Mengkraan","Partie encastrée robinet d’arrêt pour mitigeur douche haut débit","Built-in part for stop valve for thermostatic high-capacity mixer","031","Chrome",393,"GPF432833G001G000","8022692585469"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","43283+58363","58363","Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur douche haut débit.","External parts for stop valve for thermostatic high-capacity mixer.",713,"Antique Brass",708,"GPF583630V204G000","8056329065901"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58186,58186,"Antikalk-hoofddouchekop Plafonddouche oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead","031","Chrome",1300,"GPF581860G001G000","8056329020122"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58186,58186,"Antikalk-hoofddouchekop Plafonddouche oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead",187,"Aged Bronze",2056,"GPF581860G052G000","8056329020108"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58189,58189,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche anticalcaire laterale orientable.","Wall-fixing antilimestone and adjustable headshower",187,"Aged Bronze",1493,"GPF581890G052G000","8056329077010"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58252,58252,"Antikalk-hoofddouchekop Plafonddouche oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead",720,"Nickel PVD",1554,"GPF582520P014G000","8056603606073"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58252,58252,"Antikalk-hoofddouchekop Plafonddouche oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead",845,"Dark Bronze",1658,"GPF582520V221G000","8056603622349"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58148,58148,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-fixing antilimestone and adjustable headshower","031","Chrome",874,"GPF581480G001G000","8022692870688"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58148,58148,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-fixing antilimestone and adjustable headshower",716,"Gold Brushed PVD",1468,"GPF581480P005G000","8055261230620"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58150,58150,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",149,"Finox Brushed Nickel",1574,"GPF581500G002G000","8056329020894"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",149,"Finox Brushed Nickel",1475,"GPF630500G002G000","8055261729513"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",299,"Matte Black",1917,"GPF630530C072G000","8055261729384"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",299,"Matte Black",2173]
["BATHROOM","INCISO","INCISO BATH-SHOWER",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",720,"Nickel PVD",2383]
["BATHROOM","INCISO","INCISO BATH-SHOWER",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",710,"Brass PVD",3096]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58145,58145,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m","Sliding rail with antilimestone handshower, 1,50 m flexible hose",149,"Finox Brushed Nickel",1101,"GPF581451G002G000","8022692871401"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58144,58144,"Glijstang","Barre de douche.","Sliding rail",299,"Matte Black",1022,"GPF581441C072G000","8022692874617"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",32971,32971,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",279,"Matte White",404,"GPF329710C071G000","8022692625813"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","32985+32982",32985,"Inbouwdeel Laterale oriënteerbare hoofddouchekop","Partie encastrée pour douchette laterale orientable","Built-in part lateral and adjustable body jet","031","Chrome",202,"GPF329850G001G000","8022692519358"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","32985+32982",32982,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour douchette laterale orientable","External parts for adjustable lateral body jet",716,"Gold Brushed PVD",804,"GPF329820P005G000","8056603933162"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",13375,13375,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","Adjustable lateral body jet",726,"Warm Bronze Brushed PVD",337,"GPF133750P024G000","8056329007642"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58123,58123,"Doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m.","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",727,"Brass Brushed PVD",777,"GPF581230P025G000","8022692871982"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",708,"Copper Brushed PVD",1003,"GPF630990P006G000","8056329215962"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58169,58169,"Wateraansluitpunt","Sortie murale coudée.","water outlet",727,"Brass Brushed PVD",332,"GPF581690P025G000","8022692872026"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58157,58157,"Vaste houder voor handdouche","Support fixe pour douchette.","Fixed handshower hook",845,"Dark Bronze",192,"GPF581570V221G000","8056603622639"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",58160,58160,"Oriënteerbare duplex houder voor handdouche","Support mural orientable pour douchette.","Adjustable handshower hook","030","Copper PVD",316,"GPF581600P000G000","8022692861235"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",713,"Antique Brass",438,"GPF329290V204G000","8055261227781"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",735,"Warm Bronze PVD",214,"GPF143720P037G000","8056329614444"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",14371,14371,"Antikalk handdouche","Douchette anticalcaire.","Antilimestone handshower",720,"Nickel PVD",208,"GPF143710P014G000","8055261239807"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",14371,14371,"Antikalk handdouche","Douchette anticalcaire.","Antilimestone handshower",246,"Gold PVD",234,"GPF143710P007G000","8055261239821"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert","031","Chrome",206,"GPF143760G001G000","8022692028393"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",246,"Gold PVD",366,"GPF143780P007G000","8056603633215"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",187,"Aged Bronze",269,"GPF473510G052G000","8056603587082"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",707,"Black Metal Brushed PVD",269,"GPF473500P004G000","8056603587167"]
["BATHROOM","INCISO","INCISO BATH-SHOWER","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",710,"Brass PVD",113,"GPF016370P011G000","8022692092493"]
["BATHROOM","INCISO","INCISO BATH-SHOWER",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections","030","Copper PVD",134,"GPF287460P000G000","8056329105157"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58501,"58501","Wand-zeepbakje wit","Porte-savon mural blanc.","Wall-mounted soap dish, white",299,"Matte Black",480,"GPF585010C072G000","8022692874716"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58502,"58502","Wand-zeepbakje zwart","Porte-savon mural noir.","Wall-mounted soap dish, black",707,"Black Metal Brushed PVD",561,"GPF585020P004G000","8056329062719"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58507,"58507","Wand-glashouder wit","Porte-verre mural blanc.","Wall-mounted holder, white",720,"Nickel PVD",571,"GPF585070P014G000","8056603478120"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58508,"58508","Wand-glashouder zwart","Porte-verre mural noir.","Wall-mounted holder, black",706,"Black Metal PVD",571,"GPF585080P001G000","8056329062627"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58513,"58513","Wand-dispenserhouder wit","Distributeur de savon liquide mural blanc.","Wall-mounted liquid soap dispenser , white",149,"Finox Brushed Nickel",892,"GPF585131G002G000","8022692871494"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58514,"58514","Wand-dispenserhouder zwart","Distributeur de savon liquide mural noir.","Wall-mounted liquid soap dispenser - black",299,"Matte Black",892,"GPF585141C072G000","8056329062566"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58520,"58520","Wand-toiletborstelhouder zwart","Porte-balayette mural noir.","Wall-mounted brush holder, black",720,"Nickel PVD",845,"GPF585201P014G000","8056603478069"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58525,"58525","Witte Staande Zeephouder","Porte-savon à poser blanc","Standing soap holder, white",708,"Copper Brushed PVD",381,"GPF585250P006G000","8022692884579"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58526,"58526","Zwarte Witte Staande Zeephouder","Porte-savon à poser noir","Standing soap holder, black",149,"Finox Brushed Nickel",327,"GPF585260G002G000","8056329062320"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58526,"58526","Zwarte Witte Staande Zeephouder","Porte-savon à poser noir","Standing soap holder, black",713,"Antique Brass",381,"GPF585260V204G000","8056329062283"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58532,"58532","Zwarte Staande Bekerhouder","Porte-verre à poser noir","Standing tumbler holder, black",720,"Nickel PVD",391,"GPF585320P014G000","8056603455909"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58537,"58537","Staande dispenserhouder wit","Distributeur de savon liquide à poser blanc.","Standing soap dispenser holder, white",187,"Aged Bronze",907,"GPF585371G052G000","8022692873429"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58538,"58538","Staande dispenserhouder zwart","Distributeur de savon liquide à poser noir.","Standing soap dispenser holder, black",720,"Nickel PVD",850,"GPF585381P014G000","8056603478038"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58543,"58543","Witte Staande Borstelhouder","Porte-balayette à poser blanche","Standing brush holder, white",710,"Brass PVD",688,"GPF585431P011G000","8056329594524"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58455,"58455","Horizontale of verticale wand-toiletrolhouder","Porte-papier mural horizontal ou vertical.","Paper-roll holder for horizontal/vertical installation","030","Copper PVD",466,"GPF584551P000G000","8022692861280"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58497,"58497","Wand-handdoekhouder 30 cm","Porte-serviette 30 cm.","30 cm centre distance towel rail",710,"Brass PVD",655,"GPF584971P011G000","8056329595033"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58500,"58500","Wand-handdoekhouder 45 cm","Porte-serviette 45 cm.","45 cm centre distance towel rail",727,"Brass Brushed PVD",732,"GPF585001P025G000","8022692872088"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58503,"58503","Wand-handdoekhouder 60 cm","Porte-serviette 60 cm.","60 cm centre distance towel rail",707,"Black Metal Brushed PVD",781,"GPF585030P004G000","8022692874013"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58505,"58505","Wand-handdoekhouder 80 cm","Porte-serviette 80 cm.","80 cm centre distance towel rail","030","Copper PVD",810,"GPF585051P000G000","8022692861327"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58509,"58509","Wand-handdoekhouder ringvorm","Anneau porte-serviette.","Towel ring","030","Copper PVD",384,"GPF585090P000G000","8022692861334"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58613,"58613","Handdoekhouder 30 cm","Porte-serviette 30 cm à fixer sur le verre.","30 cm towel rail for glass fixing",735,"Warm Bronze PVD",858,"GPF586131P037G000","8056329594463"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58615,"58615","Handdoekhouder 45 cm","Porte-serviette 45 cm à fixer sur le verre.","45 cm towel rail for glass fixing",726,"Warm Bronze Brushed PVD",1016,"GPF586151P024G000","8056329594449"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58617,"58617","Handdoekhouder 60 cm","Porte-serviette 60 cm à fixer sur le verre.","60 cm towel rail for glass fixing",726,"Warm Bronze Brushed PVD",1065,"GPF586171P024G000","8056329201170"]
["BATHROOM","INCISO","INCISO ACCESSORIES",58423,"58423","Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip-handle for bathtub and shower enclosure, 45 cm length",706,"Black Metal PVD",1543,"GPF584231P001G000","8056329523470"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",39168,39168,"Toiletzitting van antibacteriële hars voor artikel 39114. Te completeren met zachtsluitend beslag 39184 (niet inbegrepen).","Siège en résine antibactérienne pour cuvette 39114. À combiner avec les charnières 39184 (non inclues).","Anti-bacterical resin WC seat for item 39114. To be completed with soft-closing hardware 39184 (not included).",299,"Matte Black",394,"GPF391680C072G000","8056603462310"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.","030","Copper PVD",257,"GPF375842P000G000","8022692674279"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",708,"Copper Brushed PVD",154,"GPF375870P006G000","8022692430578"]
["BATHROOM","INCISO","INCISO TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","031","Chrome",528,"GPF452300G001G000","8055261645684"]
["BATHROOM","INCISO","INCISO TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","031","Chrome",480,"GPF451300G001G000","8055261227606"]
["BATHROOM","INCISO","INCISO TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",726,"Warm Bronze Brushed PVD",758,"GPF451310P024G000","8055261227309"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",720,"Nickel PVD",1152,"GPF451240P014G000","8056603615785"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1152,"GPF451240P011G000","8056603615792"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","030","Copper PVD",1152,"GPF451260P000G000","8056603632942"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",720,"Nickel PVD",1059,"GPF581531P014G000","8056603606226"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",147,"Chome Brushed",878,"GPF143313G006G000","8056329082557"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1482,"GPF451220P024G000","8056603615969"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",706,"Black Metal PVD",1317,"GPF581511P001G000","8056329020412"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",54611,54611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",720,"Nickel PVD",930,"GPF546110P014G000","8056603456913"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",54613,54613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",713,"Antique Brass",1495,"GPF546130V204G000","8056329070424"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",708,"Copper Brushed PVD",883,"GPF546150P006G000","8056329070240"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",54617,54617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",299,"Matte Black",903,"GPF546170C072G000","8056329098855"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",54619,54619,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaque de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",275,"Matte Cipria",1183,"GPF546190T209G000","8056603588003"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",54619,54619,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaque de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",716,"Gold Brushed PVD",1474,"GPF546190P005G000","8055261230941"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",54621,54621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",710,"Brass PVD",1641,"GPF546211P011G000","8056329598799"]
["BATHROOM","INCISO","INCISO TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",276,"Matte Agave",168,"GPF014210T210G000","8056603964135"]
["BATHROOM","INCISO","INCISO TOTAL LOOK",28767,28767,"Verlengstuk buis voor sifon, lengte 40 cm","Tubelure prolongée pour siphone, longueur 40 cm","Syphon pipe extension, 40 cm length",299,"Matte Black",68,"GPF287670C072G000","8022692655629"]
["BATHROOM","INCISO","INCISO TOTAL LOOK","01377","01377","1 1/4\" sifon","Siphon 1 1/4”.","1 1/4\" syphon",708,"Copper Brushed PVD",455,"GPF013771P006G000","8022692088663"]
["BATHROOM","INCISO","INCISO TOTAL LOOK","01411","01411","Onderbouwmengkraan met filter en 1/2\" aansluiting","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection",713,"Antique Brass",240,"GPF014110V204G000","8056329068810"]
["BATHROOM","VENTI20","VENTI20",65001,65001,"Wastafelmengkraan, Flexibele Aansluitingen, Met Plug","Mitigeur lavabo, avec vidage et flexibles de raccordement","Basin mixer, flexible connections, with waste",708,"Copper Brushed PVD",1166,"GPF650010P006G000","8056603011860"]
["BATHROOM","VENTI20","VENTI20",65002,65002,"Wastafelmengkraan, Flexibele Aansluitingen, Zonder Plug","Mitigeur lavabo, sans vidage, avec flexibles de raccordement","Basin mixer, flexible connections, without waste",713,"Antique Brass",1056,"GPF650020V204G000","8056603011679"]
["BATHROOM","VENTI20","VENTI20",65004,65004,"Verhoogde Wastafelmengkraan, Flexibele Aansluitingen, Zonder Plug","Mitigeur lavabo réhaussé, sans vidage, avec flexibles deraccordement","High basin mixer, flexible connections, without waste","031","Chrome",819,"GPF650040G001G000","8056603011532"]
["BATHROOM","VENTI20","VENTI20",65011,65011,"Drie-Gats Wastafelmengkraan , Met Flexible Slangen Met Plug","Mélangeur avec vidage et flexibles de raccordement","Three-holes basin mixer, with flexible hoses, with waste",187,"Aged Bronze",2322,"GPF650110G052G000","8056603011259"]
["BATHROOM","VENTI20","VENTI20",65012,65012,"Medium Drie-Gats Wastafelmengkraan, Met Flexible Slangen, Met Plug","Mélangeur moyen avec vidage et flexibles de raccordement.","Medium three-hole basin mixer, with flexible hoses, with waste",149,"Finox Brushed Nickel",2075,"GPF650120G002G000","8056603011136"]
["BATHROOM","VENTI20","VENTI20",65014,65014,"Medium Drie-Gats Wastafelmengkraan, Met Flexible Slangen. Zonder Plug","Mélangeur moyen sans vidage avec flexibles de raccordement","Medium three-hole basin mixer, with flexible hoses. Without waste","031","Chrome",1470,"GPF650140G001G000","8056603010887"]
["BATHROOM","VENTI20","VENTI20",65015,65015,"Drie-Gats Wastafelmengkraan Met Umbrella Uitloop, Met Flexible Slangen. Met Plug","Mélangeur moyen avec vidage et flexibles de raccordement","Three-hole basin mixer with umbrella spout, with flexible hoses. With waste",299,"Matte Black",2075,"GPF650150C072G000","8056603475211"]
["BATHROOM","VENTI20","VENTI20",65016,65016,"Drie-Gats Wastafelmengkraan Met Umbrella Uitloop,, Met Flexible Slangen. Zonder Plug","Mélangeur moyen sans vidage avec flexibles de raccordement","Three-hole basin mixer with umbrella spout, with flexible hoses. Without waste",720,"Nickel PVD",2175,"GPF650160P014G000","8056603010542"]
["BATHROOM","VENTI20","VENTI20","63397+65089","65089","Afbouwdelen Voor Wandgemonteerde Wastafelmengkraan, Medium Uitloop, Zonder Plug","Partie apparente mitigeur lavabo mural avec sans vidage","External parts for wall-mounted basin mixer, medium spout, without waste",299,"Matte Black",950,"GPF650890C072G000","8056603475075"]
["BATHROOM","VENTI20","VENTI20","45089+65091","65091","Afbouwdelen 3-Gats Wastafelmengkraan Met Medium Uitloop, Zonder Plug","Partie apparente pour mélangeur mural avec bec moyen sans vidage.","External parts three-hole basin mixer with medium spout, withoutwaste",299,"Matte Black",1445,"GPF650910C072G000","8056603475051"]
["BATHROOM","VENTI20","VENTI20","45089+65090","65090","Afbouwdelen Wastafelmengkraan Met Lange Uitloop, Zonder Plug","Partie apparente pour mélangeur mural avec bec long sans vidage.","External parts basin mixer with long spout, without waste","030","Copper PVD",1668,"GPF650900P000G000","8056603008778"]
["BATHROOM","VENTI20","VENTI20",65021,65021,"Lage Wastafel Uitloop","Bec de lavabo","Small basin spout",299,"Matte Black",759,"GPF650210C072G000","8056603475198"]
["BATHROOM","VENTI20","VENTI20",65023,65023,"Medium Wastafel Uitloop","Bec de lavabo longueur moyenne","Medium basin spout",707,"Black Metal Brushed PVD",994,"GPF650230P004G000","8056603010313"]
["BATHROOM","VENTI20","VENTI20",65025,65025,"Medium Wastafel Uitloop","Bec de lavabo moyen.","Medium basin spout",720,"Nickel PVD",932,"GPF650250P014G000","8056603010153"]
["BATHROOM","VENTI20","VENTI20",65101,65101,"Wandgemonteerde Wastafel Uitloop, Lange Uitloop","Bec de lavabo mural long","Wall-mounted basin spout, long spout",707,"Black Metal Brushed PVD",602,"GPF651010P004G000","8056603008228"]
["BATHROOM","VENTI20","VENTI20",65101,65101,"Wandgemonteerde Wastafel Uitloop, Lange Uitloop","Bec de lavabo mural long","Wall-mounted basin spout, long spout",727,"Brass Brushed PVD",602,"GPF651010P025G000","8056603008174"]
["BATHROOM","VENTI20","VENTI20",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.","031","Chrome",1305,"GPF634990G001G000","8056329555525"]
["BATHROOM","VENTI20","VENTI20",65100,65100,"Separate Bediening","Commande séparée","Separate control",720,"Nickel PVD",652,"GPF651000P014G000","8056603008327"]
["BATHROOM","VENTI20","VENTI20",65100,65100,"Separate Bediening","Commande séparée","Separate control",246,"Gold PVD",741,"GPF651000P007G000","8055261233652"]
["BATHROOM","VENTI20","VENTI20","46189+65095","65095","Afbouwdelen Voor Vrijstaande Wastafelmengkraan Zonder Plug","Partie apparente mitigeur de lavabo au sol sans vidage","External parts for freestanding basin mixer without waste",706,"Black Metal PVD",2703,"GPF650950P001G000","8056603008501"]
["BATHROOM","VENTI20","VENTI20",65007,65007,"Bidet Mengkraan Met Flexibele Aansluitingen","Mitigeur bidet avec vidage et flexibles de raccordement","Bidet mixer with flexible connections",727,"Brass Brushed PVD",1166,"GPF650070P025G000","8056603011303"]
["BATHROOM","VENTI20","VENTI20",65113,65113,"Afbouwdelen Voor Wandgemonteerde Badkraan, Bad/Douche Omstel, 1,50 M Flexibele Slang And Antikalk Handdouche Met Vaste Haak","Mélangeur baignoire murale avec inverseur, flexibles de raccordement 1,50m et douchette anticalcaire, avec support fixe.","External parts for wall-mounted bath mixer, bath/shower diverter, 1,50 m flexible hose and antilimestone handshower with fixed hook",716,"Gold Brushed PVD",3219,"GPF651130P005G000","8055261065215"]
["BATHROOM","VENTI20","VENTI20","65099+65128","65128","Afbouwdeel Voor Vrijstaande Badkraan","Partie apparente pour mélangeur bain-douche sur pied avec douchetteet flexible.","External part for freestanding bath mixer with automatic diverter",710,"Brass PVD",5683,"GPF651280P011G000","8056603007160"]
["BATHROOM","VENTI20","VENTI20","65099+65128","65128","Afbouwdeel Voor Vrijstaande Badkraan","Partie apparente pour mélangeur bain-douche sur pied avec douchetteet flexible.","External part for freestanding bath mixer with automatic diverter",716,"Gold Brushed PVD",6451,"GPF651280P005G000","8056603865357"]
["BATHROOM","VENTI20","VENTI20",65037,65037,"Drie-Gats Wastafelmengkraan Met Omstel, Uitloop, 1,50 M Flexibele Slang And Uittrekbare Antikalk Handdouche","Mitigeur bain-douche trois trous sur plan avec bec, inverseur, flexible1,50m et douchette extractible anticalcaire","Three-hole bath mixer with diverter, spout, 1,50 m flexible hose and pull-out antilimestone handshower",716,"Gold Brushed PVD",3219,"GPF650370P005G000","8055261229822"]
["BATHROOM","VENTI20","VENTI20",65045,65045,"4-gats badkraan met omstel, bad uitloop, 1,50 m flexibele slang, antikalk handdouche","Ensemble de baignoire 4 trous avec inverseur, bec, flexible de 1,50 m et douchette anticalcaire","Four-holes bath mixer with diverter, tub-filler spout, 1,50 m flexible hose, antilimestone handshower",187,"Aged Bronze",3872,"GPF650450G052G000","8056603614559"]
["BATHROOM","VENTI20","VENTI20",65127,65127,"Conische Douche Haak Met Antikalk Handdouche And 1,5 M Flexibele Slang","Support douchette avec douchette anticacaire et flexibles 1,5m","Conical shower hook with antilimestone handshower and 1,5 m flexible hose",761,"Coffee Bronze Brushed PVD",1084,"GPF651270E059G000","8055261589827"]
["BATHROOM","VENTI20","VENTI20","01664","01664","Four-holes finishing plaatje voor montage box","Plaque de finition 4 trous pour la boîte de sécurité","Four-holes finishing plate for mounting box",716,"Gold Brushed PVD",874,"GPF016641P005G000","8055261231283"]
["BATHROOM","VENTI20","VENTI20",65050,65050,"Uittrekbare handdouchekit, zijrand installatie","Système de récupération eau pour flexible de douchette bain-douche,installation sur plan de bagnoire","Pull-out handshower drain kit, rim installation",187,"Aged Bronze",1547,"GPF650500G052G000","8056603009171"]
["BATHROOM","VENTI20","VENTI20",65049,65049,"Uittrekbare handdouchekit, installatie op zijplan in de badkuip.","Système de récupération eau pour flexible de douchette bain-douche,installation sur plan latéral à la bagnoire","Pull-out handshower drain kit, tile wall installation",761,"Coffee Bronze Brushed PVD",2119,"GPF650490E059G000","8055261590168"]
["BATHROOM","VENTI20","VENTI20","01080","01080","Polyethyleen badafvoer met overloopdopvuller. Lengte van de aanvoer leiding 80 cm","Vidage en polyéthylène baignoire avec trop-plein. Longueur 80 cm","Polyethylene column bath waste with overflow cap filler. Length of control cable 80 cm",710,"Brass PVD",639,"GPF010802P011G000","8056329615328"]
["BATHROOM","VENTI20","VENTI20",65103,65103,"Wandgemonteerde Bad Uitloop","Bec de baignoire mural latéral","Wall-mounted bath spout","031","Chrome",479,"GPF651030G001G000","8056603008013"]
["BATHROOM","VENTI20","VENTI20",65103,65103,"Wandgemonteerde Bad Uitloop","Bec de baignoire mural latéral","Wall-mounted bath spout",710,"Brass PVD",710,"GPF651030P011G000","8056603007948"]
["BATHROOM","VENTI20","VENTI20","54057+54058","54058","Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",710,"Brass PVD",388,"GPF540580P011G000","8056603627948"]
["BATHROOM","VENTI20","VENTI20","54057+54058","54058","Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",761,"Coffee Bronze Brushed PVD",396,"GPF540580E059G000","8055261602076"]
["BATHROOM","VENTI20","VENTI20","54073+65038","65038","Afbouwdeel Voor Mengkraan, 2-Weg Omstel","Partie apparente mitigeur mural avec inverseur automatiquebain-douche deux sorties","External part for mixer, two-way diverter",735,"Warm Bronze PVD",1104,"GPF650380P037G000","8056603009737"]
["BATHROOM","VENTI20","VENTI20","44673+65079","65079","Afbouwdeel Wandgemonteerde Mengkraan, 2-Weg","Partie apparente mitigeur mural avec inverseur automatiquebain-douche deux sorties","External part wall-mounted mixer, two-way automatic diverter",720,"Nickel PVD",1095,"GPF650790P014G000","8056603028622"]
["BATHROOM","VENTI20","VENTI20","54169+65233","65233","Afbouwdeel wand gemonteerd 1-wegthermostatische mengkraan.","Partie apparente mitigeur thermostatique 1 voie.","External part wall-mounted one way thermostatic mixer.",726,"Warm Bronze Brushed PVD",1558,"GPF652330P024G000","8055261192973"]
["BATHROOM","VENTI20","VENTI20","54169+65235","65235","Afbouwdeel wand gemonteerd 2-weg thermostatische mengkraan.","Partie apparente mitigeur thermostatique 2 voies.","External part wall-mounted two ways thermostatic mixer.","030","Copper PVD",1459,"GPF652350P000G000","8055261192898"]
["BATHROOM","VENTI20","VENTI20","54169+65237","65237","Afbouwdeel wand gemonteerd 3-weg thermostatische mengkraan.","Partie apparente mitigeur thermostatique 3 voies.","External part wall-mounted three ways thermostatic mixer.",149,"Finox Brushed Nickel",1331,"GPF652370G002G000","8055261192775"]
["BATHROOM","VENTI20","VENTI20","09269+65133","65133","Afbouwdeel Voor Thermostatische Mengkraan, 1-Weg Omstel","Partie apparente pour mitigeur thermostatique douche mural 1 sortie","External part for thermostatic mixer, one-way diverter",707,"Black Metal Brushed PVD",1832,"GPF651330P004G000","8056603028516"]
["BATHROOM","VENTI20","VENTI20","09269+65137","65137","Afbouwdeel Voor Thermostatische Mengkraan, 3-Weg Omstel","Partie apparente pour mitigeur thermostatique douche mural 3 sorties","External part for thermostatic mixer, three-way diverter",299,"Matte Black",1566,"GPF651370C072G000","8056603099776"]
["BATHROOM","VENTI20","VENTI20","09264+65334","65334","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie externe mitigeur thermostatique mural à 2 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with two separate exits.",708,"Copper Brushed PVD",1779,"GPF653340P006G000","8056603618595"]
["BATHROOM","VENTI20","VENTI20","09266+65336","65336","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie externe mitigeur thermostatique mural à 3 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with three separate exits.",706,"Black Metal PVD",1938,"GPF653360P001G000","8056603618465"]
["BATHROOM","VENTI20","VENTI20","09268+65338","65338","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie externe mitigeur thermostatique mural à 4 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with four separate exits.",707,"Black Metal Brushed PVD",2346,"GPF653380P004G000","8056603618304"]
["BATHROOM","VENTI20","VENTI20","09263+65340","65340","afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie externe mitigeur thermostatique mural à 5 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with five separate exits.",720,"Nickel PVD",2412,"GPF653400P014G000","8056603630191"]
["BATHROOM","VENTI20","VENTI20","43103+65200","65200","afbouwdeel voor wand-gemonteerd thermostatic high-capacity mixer. Vertical/horizontal setting up met TWO separate uitgangen","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. 2 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",299,"Matte Black",1522,"GPF652000C072G000","8055261236219"]
["BATHROOM","VENTI20","VENTI20","43105+65204","65204","afbouwdeel voor wand-gemonteerd thermostatic high-capacity mixer. Vertical/horizontal setting up met THREE separate uitgangen","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. 3 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",707,"Black Metal Brushed PVD",2069,"GPF652040P004G000","8055261233157"]
["BATHROOM","VENTI20","VENTI20","43105+65206","65206","afbouwdeel voor wand-gemonteerd thermostatic high-capacity mixer. Vertical/horizontal setting up met THREE separate uitgangen","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. 3 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",708,"Copper Brushed PVD",2069,"GPF652060P006G000","8055261233010"]
["BATHROOM","VENTI20","VENTI20","43107+65208","65208","afbouwdeel voor wand-gemonteerd thermostatic high-capacity mixer. Vertical/horizontal setting up met FOUR separate uitgangen","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. 4 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",706,"Black Metal PVD",2198,"GPF652080P001G000","8055261232907"]
["BATHROOM","VENTI20","VENTI20","43107+65210","65210","afbouwdeel voor wand-gemonteerd thermostatic high-capacity mixer. Vertical/horizontal setting up met FOUR separate uitgangen","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. 4 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",149,"Finox Brushed Nickel",2004,"GPF652100G002G000","8055261232808"]
["BATHROOM","VENTI20","VENTI20","43281+65316","65316","Afbouwdeel wand-gemonteerd thermostatic high-capacity mixer","Partie apparente mitigeur THERMOSTATIQUE douche haut débit","External parts wall-mounted thermostatic high-capacity mixer","030","Copper PVD",741,"GPF653160P000G000","8055261228788"]
["BATHROOM","VENTI20","VENTI20",65156,65156,"Wandgemonteerde verstelbare hoofddouche","Pomme de douche murale orientable","Wall-fixing adjustable headshower",706,"Black Metal PVD",1400,"GPF651560P001G000","8056603585972"]
["BATHROOM","VENTI20","VENTI20",65156,65156,"Wandgemonteerde verstelbare hoofddouche","Pomme de douche murale orientable","Wall-fixing adjustable headshower",735,"Warm Bronze PVD",1400,"GPF651560P037G000","8056603585903"]
["BATHROOM","VENTI20","VENTI20",65148,65148,"Wandgemonteerde Verstelbare Hoofddouche","Douchette anticalcaire laterale orientable","Wall-mounted adjustable showerhead",149,"Finox Brushed Nickel",1799,"GPF651480G002G000","8056603006187"]
["BATHROOM","VENTI20","VENTI20",65149,65149,"Wandgemonteerde Verstelbare Hoofddouche","Douchette anticalcaire laterale orientable","Wall-mounted adjustable showerhead",720,"Nickel PVD",2956,"GPF651490P014G000","8056603005982"]
["BATHROOM","VENTI20","VENTI20",65152,65152,"Plafond Gemonteerd Verstelbare Hoofddouche","Pomme de douche orientable anticalcaire avec bras au plafond.","Ceiling-mounted adjustable showerhead",713,"Antique Brass",2000,"GPF651520V204G000","8056603005814"]
["BATHROOM","VENTI20","VENTI20",65150,65150,"Plafond Gemonteerd Hoofddouche, Lengte Op Aanvraag","Pomme de douche anticalcaire orientable avec bras au plafond, longueur à la demande.","Ceiling-mounted showerhead, length on request",735,"Warm Bronze PVD",2621,"GPF651500P037G000","8056603456395"]
["BATHROOM","VENTI20","VENTI20",65155,65155,"Plafond Gemonteerd Hoofddouche, Lengte Op Aanvraag","Pomme de douche anticalcaire orientable avec bras au plafond, longueur à la demande.","Ceiling-mounted showerhead, length on request",149,"Finox Brushed Nickel",3583,"GPF651550G002G000","8056603456357"]
["BATHROOM","VENTI20","VENTI20",65142,65142,"Glijstang Met Antikalk Handdouche, 1,50 M Flexibele Slang And Water Uitgang","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée","Sliding rail with antilimestone handshower, 1,50 m flexible hose and water outlet",707,"Black Metal Brushed PVD",2521,"GPF651420P004G000","8056603006538"]
["BATHROOM","VENTI20","VENTI20",65145,65145,"Glijstang","Barre de douche","Sliding rail",726,"Warm Bronze Brushed PVD",1663,"GPF651450P024G000","8056603006231"]
["BATHROOM","VENTI20","VENTI20",65141,65141,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with antilimestone handshower, 1,50 m flexible hose and water outlet",710,"Brass PVD",1388,"GPF651410P011G000","8056603466523"]
["BATHROOM","VENTI20","VENTI20",65143,65143,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m","Sliding rail with antilimestone handshower, 1,50 m flexible hose",246,"Gold PVD",1300,"GPF651430P007G000","8055261233591"]
["BATHROOM","VENTI20","VENTI20",65123,65123,"Douche Set Met Water Uitgang, 1,50 M Flexibele Slang And Antikalk Handdouche","Ensemble comprenant: sortie coudée murale, douchette anticalcaire etflexibles 1,50 m","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",727,"Brass Brushed PVD",1118,"GPF651230P025G000","8056603007399"]
["BATHROOM","VENTI20","VENTI20",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",726,"Warm Bronze Brushed PVD",1003,"GPF630990P024G000","8056329215948"]
["BATHROOM","VENTI20","VENTI20",32971,32971,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",246,"Gold PVD",503,"GPF329710P007G000","8056329037267"]
["BATHROOM","VENTI20","VENTI20","32985+32982","32982","Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour douchette laterale orientable","External parts for adjustable lateral body jet",707,"Black Metal Brushed PVD",745,"GPF329820P004G000","8022692889321"]
["BATHROOM","VENTI20","VENTI20",13375,13375,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","Adjustable lateral body jet",149,"Finox Brushed Nickel",288,"GPF133750G002G000","8056329007673"]
["BATHROOM","VENTI20","VENTI20",65295,65295,"Afbouwdeel Voor Waterval Douche Uitloop Nog Compleet Te Maken Met Separate Bediening (Niet Inclusief)","Partie apparente pour bec cascade de douche murale. À compléter par commande séparée.","Waterfall shower spout to be completed with separate control (not included)",708,"Copper Brushed PVD",1607,"GPF652950P006G000","8056603003926"]
["BATHROOM","VENTI20","VENTI20",65295,65295,"Afbouwdeel Voor Waterval Douche Uitloop Nog Compleet Te Maken Met Separate Bediening (Niet Inclusief)","Partie apparente pour bec cascade de douche murale. À compléter par commande séparée.","Waterfall shower spout to be completed with separate control (not included)",713,"Antique Brass",1607,"GPF652950V204G000","8056603003865"]
["BATHROOM","VENTI20","VENTI20",65161,65161,"Water Uitgang En Handdouche Haak","Sortie murale coudée avec support fixe pour douchette","Water outlet and handshower hook",735,"Warm Bronze PVD",411,"GPF651610P037G000","8056603005173"]
["BATHROOM","VENTI20","VENTI20",65160,65160,"Verstelbare Handdouche Haak","Support mural orientable pour douchette","Adjustable handshower hook",299,"Matte Black",490,"GPF651600C072G000","8056603474856"]
["BATHROOM","VENTI20","VENTI20",65154,65154,"Antikalk Handdouche","Douchette anticalcaire","Antilimestone handshower","031","Chrome",430,"GPF651540G001G000","8056603005678"]
["BATHROOM","VENTI20","VENTI20",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",187,"Aged Bronze",438,"GPF329290G052G000","8055261227903"]
["BATHROOM","VENTI20","VENTI20",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",761,"Coffee Bronze Brushed PVD",468,"GPF329290E059G000","8055261577657"]
["BATHROOM","VENTI20","VENTI20","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",726,"Warm Bronze Brushed PVD",120,"GPF016370P024G000","8056329555655"]
["BATHROOM","VENTI20","VENTI20",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",713,"Antique Brass",167,"GPF287460V204G000","8056329048577"]
["BATHROOM","VENTI20","VENTI20","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",708,"Copper Brushed PVD",162,"GPF017240P006G000","8055261240056"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65401,65401,"Wandgemonteerde Zeep Houder Wit","Porte-savon mural blanc","Wall-mounted soap dish, white",246,"Gold PVD",597,"GPF654010P007G000","8056603698580"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65402,65402,"Wandgemonteerde Zeep Houder Zwart","Porte-savon mural noir","Wall-mounted soap dish, black",710,"Brass PVD",526,"GPF654020P011G000","8056603003650"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65408,65408,"Wandgemonteerde Bekerhouder Zwart","Porte-verre mural noir","Wall-mounted holder, black",246,"Gold PVD",645,"GPF654080P007G000","8055261188396"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65413,65413,"Wandgemonteerde Wit Zeep Dispenser","Distributeur de savon liquide mural blanc.","Wall-mounted liquid soap dispenser , white",713,"Antique Brass",1040,"GPF654130V204G000","8056603003216"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65414,65414,"Wandgemonteerde Zwart Zeep Dispenser","Distributeur de savon liquide mural noir","Wall-mounted liquid soap dispenser - black",713,"Antique Brass",1040,"GPF654140V204G000","8056603003087"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65419,65419,"Wit Wandgemonteerde Toilet Brush","Porte-balayette mural blanche","Wall-mounted brush holder, white",761,"Coffee Bronze Brushed PVD",958,"GPF654190E059G000","8055261588806"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",58525,58525,"Witte Staande Zeephouder","Porte-savon à poser blanc","Standing soap holder, white",761,"Coffee Bronze Brushed PVD",406,"GPF585250E059G000","8055261594333"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",58531,58531,"Witte Staande Bekerhouder","Porte-verre à poser blanc.","Standing tumbler holder, white",149,"Finox Brushed Nickel",356,"GPF585310G002G000","8022692871548"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",58531,58531,"Witte Staande Bekerhouder","Porte-verre à poser blanc.","Standing tumbler holder, white",187,"Aged Bronze",417,"GPF585310G052G000","8022692873467"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65437,65437,"Witte Vrijstaande Zeep Dispenser","Distributeur de savon liquide à poser blanc","Standing soap dispenser holder, white","031","Chrome",573,"GPF654370G001G000","8056603002813"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65437,65437,"Witte Vrijstaande Zeep Dispenser","Distributeur de savon liquide à poser blanc","Standing soap dispenser holder, white",735,"Warm Bronze PVD",845,"GPF654370P037G000","8056603002707"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65523,65523,"Scheermes Houder","Support de rasoir","Razor holder",720,"Nickel PVD",365,"GPF655230P014G000","8056603001045"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",58543,58543,"Witte Staande Borstelhouder","Porte-balayette à poser blanche","Standing brush holder, white",716,"Gold Brushed PVD",784,"GPF585431P005G000","8056603563604"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",58544,58544,"Zwarte Staande Borstelhouder","Porte-balayette à poser noir.","Standing brush holder, black",716,"Gold Brushed PVD",784,"GPF585441P005G000","8055261230149"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65449,65449,"Wandgemonteerde Papier Rol Houder Met Cover","Porte-papier mural à couvercle.","Wall-mounted paper roll holder with cover","030","Copper PVD",604,"GPF654490P000G000","8056603002523"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65497,65497,"30 Cm Handdoek Houder","Porte-serviette 30 cm","30 cm towel rail",246,"Gold PVD",744,"GPF654970P007G000","8056603560535"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65500,65500,"45 Cm Handdoek Houder","Porte-serviette 45 cm","45 cm towel rail",726,"Warm Bronze Brushed PVD",730,"GPF655000P024G000","8056603002073"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65503,65503,"60 Cm Handdoek Houder","Porte-serviette 60 cm","60 cm towel rail",716,"Gold Brushed PVD",828,"GPF655030P005G000","8055261229334"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65509,65509,"Handdoek Ring","Anneau porte-serviette.","Towel ring",713,"Antique Brass",547,"GPF655090V204G000","8056603001786"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",59549,59549,"Plank 30 Cm","Console murale 30 cm","Shelf 30 cm",727,"Brass Brushed PVD",641,"GPF595491P025G000","8056329026209"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65521,65521,"Wandgemonteerde Robe Haak","Patère.","Wall-mounted robe hook",187,"Aged Bronze",327,"GPF655210G052G000","8056603001236"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65513,65513,"45 Cm Handdoek Houder Voor Glas Montage","Porte-serviette 45 cm à fixer sur le verre","45 cm towel rail for glass fixing","031","Chrome",644,"GPF655130G001G000","8056603001649"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65513,65513,"45 Cm Handdoek Houder Voor Glas Montage","Porte-serviette 45 cm à fixer sur le verre","45 cm towel rail for glass fixing",713,"Antique Brass",1015,"GPF655130V204G000","8056603001526"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65515,65515,"60 Cm Handdoek Houder Voor Glas Montage","Porte-serviette 60 cm à fixer sur le verre","60 cm towel rail for glass fixing",761,"Coffee Bronze Brushed PVD",1133,"GPF655150E059G000","8055261588561"]
["BATHROOM","VENTI20","VENTI20 ACCESSORIES",65517,65517,"Veiligheidsgreep Voor Bad- And Douche Toepassingen, 45 Cm Lengte","Poignée de soutien pour baignoire/douche 45 cm","Safety grip-handle for bathtub and shower enclosure, 45 cm length",761,"Coffee Bronze Brushed PVD",1756,"GPF655170E059G000","8055261588547"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",29463,29463,"Toiletzitting van antibacteriële hars voor artikel 39114. Te completeren met zachtsluitend beslag 37584 (niet inbegrepen).","Siège en résine antibactérienne pour cuvette 39114. À combiner avec les charnières 37584 (non inclues).","Anti-bacterical resin WC seat for item 39114. To be completed with soft-closing hardware 37584 (not included).","031","Chrome",275,"GPF294630G001G000","8022692786163"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.","031","Chrome",163,"GPF375842G001G000","8022692429954"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",735,"Warm Bronze PVD",146,"GPF375870P037G000","8056329558731"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",299,"Matte Black",714,"GPF452300C072G000","8055261645714"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",845,"Dark Bronze",836,"GPF452300V221G000","8055261645578"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",716,"Gold Brushed PVD",807,"GPF451310P005G000","8055261227354"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1060,"GPF452270G002G000","8055261645820"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",279,"Matte White",1051,"GPF451240C071G000","8056603615921"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",187,"Aged Bronze",1230,"GPF451260G052G000","8056603632959"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",967,"GPF581531G002G000","8056329020337"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",706,"Black Metal PVD",963,"GPF143313P001G000","8056603447171"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1092,"GPF143313E059G000","8055261577916"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",706,"Black Metal PVD",1317,"GPF581511P001G000","8056329020412"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",54651,54651,"Bedieningsplaat Geberit Sigma 8 & 12","Plaques de déclenchement pour Geberit SIgma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12","031","Chrome",816,"GPF546510G001G000","8056603012706"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",54653,54653,"Bedieningsplaat Viega 1H, 2H, 2L","Plaques de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA 1H, 2H, 2L",706,"Black Metal PVD",1689,"GPF546530P001G000","8056603012539"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",54657,54657,"Bedieningsplaat Tece","Plaques de déclenchement pour TECE","Cover plate TECE",735,"Warm Bronze PVD",1386,"GPF546570P037G000","8056603012201"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",54659,54659,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600.","Plaques de déclenchement pour SANIT","Cover plate SANIT",707,"Black Metal Brushed PVD",1381,"GPF546590P004G000","8056603012133"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",54661,54661,"Bedieningsplaat Viega Prevista 12.","Plaques de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",708,"Copper Brushed PVD",1746,"GPF546611P006G000","8056603011990"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",726,"Warm Bronze Brushed PVD",3783,"GPF546010P024G000","8022692851557"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",187,"Aged Bronze",194,"GPF014210G052G000","8056603964272"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK",28767,28767,"Verlengstuk buis voor sifon, lengte 40 cm","Tubelure prolongée pour siphone, longueur 40 cm","Syphon pipe extension, 40 cm length",299,"Matte Black",68,"GPF287670C072G000","8022692655629"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK","01377","01377","1 1/4\" sifon","Siphon 1 1/4”.","1 1/4\" syphon",246,"Gold PVD",484,"GPF013771P007G000","8056329068896"]
["BATHROOM","VENTI20","VENTI20 TOTAL LOOK","01411","01411","Onderbouwmengkraan met filter en 1/2\" aansluiting","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection",246,"Gold PVD",264,"GPF014110P007G000","8056329068803"]
["BATHROOM","ANELLO","ANELLO",63302,63302,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo, sans vidage, avec flexibles de raccordement.","Basin mixer, flexible connections, without waste",707,"Black Metal Brushed PVD",708,"GPF633020P004G000","8056329555013"]
["BATHROOM","ANELLO","ANELLO",63304,63304,"Mengkraan Wastafel hoog, korte uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec court, sans vidage, avec flexibles de raccordement.","High version basin mixer , short spout, flexible connections, without waste",149,"Finox Brushed Nickel",785,"GPF633040G002G000","8056329554856"]
["BATHROOM","ANELLO","ANELLO",63304,63304,"Mengkraan Wastafel hoog, korte uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec court, sans vidage, avec flexibles de raccordement.","High version basin mixer , short spout, flexible connections, without waste",187,"Aged Bronze",917,"GPF633040G052G000","8056329561762"]
["BATHROOM","ANELLO","ANELLO",63306,63306,"Mengkraan Wastafel hoog, lange uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec long, sans vidage, avec flexibles de raccordement.","High version basin mixer , long spout, flexible connections, without waste","030","Copper PVD",883,"GPF633060P000G000","8056329554634"]
["BATHROOM","ANELLO","ANELLO",63321,63321,"Middelgrote wastafeluitloop","Bec de lavabo longueur moyenne","Medium spout basin",708,"Copper Brushed PVD",441,"GPF633210P006G000","8056329554207"]
["BATHROOM","ANELLO","ANELLO",63400,63400,"Afstandsbediening","Commande séparée.","Separate control",299,"Matte Black",519,"GPF634000C072G000","8056329551466"]
["BATHROOM","ANELLO","ANELLO","63397+63388","63388","Extern deel Wand-Mengkraan Wastafel wand korte uitloop zonder waste","Partie apparente mitigeur lavabo muralavec bec court sans vidage","External parts for wall-mounted basin mixer, short spout, without waste",149,"Finox Brushed Nickel",703,"GPF633880G002G000","8056329551756"]
["BATHROOM","ANELLO","ANELLO","63397+63389","63389","Extern deel Wand-Mengkraan Wastafel lange uitloop zonder waste","Partie apparente mitigeur lavabo mural avec bec long sans vidage","External parts wall-mounted basin mixer, long spout, without waste",299,"Matte Black",703,"GPF633890C072G000","8056329551671"]
["BATHROOM","ANELLO","ANELLO","63397+63381","63381","Extern deel Wand-Mengkraan Wastafel wand korte uitloop zonder waste","Partie apparente mitigeur lavabo muralavec bec court sans vidage","External parts for wall-mounted basin mixer, short spout, without waste",706,"Black Metal PVD",665,"GPF633810P001G000","8056329551923"]
["BATHROOM","ANELLO","ANELLO","63397+63383","63383","Extern deel Wand-Mengkraan Wastafel lange uitloop zonder waste","Partie apparente mitigeur lavabo mural avec bec long sans vidage","External parts wall-mounted basin mixer, long spout, without waste",720,"Nickel PVD",665,"GPF633830P014G000","8056603605106"]
["BATHROOM","ANELLO","ANELLO",63403,63403,"Wanduitloop Wastafel middelgrote uitloop","Bec de lavabo mural moyen","Wall-mounted spout basin, medium spout",713,"Antique Brass",338,"GPF634030V204G000","8056329561076"]
["BATHROOM","ANELLO","ANELLO",63404,63404,"Wanduitloop Wastafel lange uitloop","Bec de lavabo mural long","Wall-mounted spout basin, long spout",713,"Antique Brass",345,"GPF634040V204G000","8056329561052"]
["BATHROOM","ANELLO","ANELLO",63399,63399,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond à compléter par un mitigeur à commande séparée","Ceiling-mounted spout. To be completed with separate control.",713,"Antique Brass",1474,"GPF633990V204G000","8056329561113"]
["BATHROOM","ANELLO","ANELLO",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.",707,"Black Metal Brushed PVD",2061,"GPF634990P004G000","8056329555471"]
["BATHROOM","ANELLO","ANELLO","46189+63393",63393,"Afbouwdelen voor vrijstaande wastafelmengkraan zonder afvoer","Partie externe mitigeur de lavabo au sol sans vidage","External parts for freestanding basin mixer without waste",708,"Copper Brushed PVD",2581,"GPF633930P006G000","8056603617277"]
["BATHROOM","ANELLO","ANELLO","46189+63328",63328,"Extern deel Vloer-Mengkraan Bad","Parties apparentes pour mitigeur bain-douche sur pied","External parts freestanding bath mixer with automatic diverter",727,"Brass Brushed PVD",3367,"GPF633280P025G000","8056329592070"]
["BATHROOM","ANELLO","ANELLO",63337,63337,"Groep Badrand 4 gaten met wateruitloop, omstelknop, buigzame slang 1,50 m en antikalk-handdouche","Mitigeur bain-douche quatre trous sur plan avec bec, inverseur, flexible 1,50m et douchette extractible anticalcaire.","Four-holes bath mixer with diverter, tub-filler spout and 1,50 m flexible hose and antilimestone handshower",707,"Black Metal Brushed PVD",2607,"GPF633370P004G000","8056329553118"]
["BATHROOM","ANELLO","ANELLO",63337,63337,"Groep Badrand 4 gaten met wateruitloop, omstelknop, buigzame slang 1,50 m en antikalk-handdouche","Mitigeur bain-douche quatre trous sur plan avec bec, inverseur, flexible 1,50m et douchette extractible anticalcaire.","Four-holes bath mixer with diverter, tub-filler spout and 1,50 m flexible hose and antilimestone handshower",187,"Aged Bronze",2607,"GPF633370G052G000","8056329561427"]
["BATHROOM","ANELLO","ANELLO","01663","01663","Drie-gats afwerkplaat voor montagebox","Plaque de finition 3 trous pour la boîte de sécurité","Three-holes finishing plate for mounting box",149,"Finox Brushed Nickel",612,"GPF016631G002G000","8022692785098"]
["BATHROOM","ANELLO","ANELLO","01664","01664","Four-holes finishing plaatje voor montage box","Plaque de finition 4 trous pour la boîte de sécurité","Four-holes finishing plate for mounting box",708,"Copper Brushed PVD",841,"GPF016641P006G000","8056329060708"]
["BATHROOM","ANELLO","ANELLO","01786","01786","Uittrekbare handdouche afvoerset, randinstallatie. Niet passend op artikelen 01669, 01658, 01663 en 01664.","Système de récupération d'eau pour flexible de douchette, installation sur le bord de la baignoire. Ne peut être combiné avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, rim installation. Not fitting items 01669, 01658, 01663 and 01664.",299,"Matte Black",988,"GPF017860C072G000","8056329562561"]
["BATHROOM","ANELLO","ANELLO","01786","01786","Uittrekbare handdouche afvoerset, randinstallatie. Niet passend op artikelen 01669, 01658, 01663 en 01664.","Système de récupération d'eau pour flexible de douchette, installation sur le bord de la baignoire. Ne peut être combiné avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, rim installation. Not fitting items 01669, 01658, 01663 and 01664.",710,"Brass PVD",1302,"GPF017860P011G000","8056329614789"]
["BATHROOM","ANELLO","ANELLO","01080","01080","Polyethyleen badafvoer met overloopdopvuller. Lengte van de aanvoer leiding 80 cm","Vidage en polyéthylène baignoire avec trop-plein. Longueur 80 cm","Polyethylene column bath waste with overflow cap filler. Length of control cable 80 cm",279,"Matte White",504,"GPF010802C071G000","8056329074811"]
["BATHROOM","ANELLO","ANELLO",63603,63603,"Wanduitloop Bad","Bec de bagnoire mural.","Wall-fixing bath spout",149,"Finox Brushed Nickel",332,"GPF636030G002G000","8056329548138"]
["BATHROOM","ANELLO","ANELLO","54139+63345","63345","Extern deel Wand-mengkraan Douche 2 -wegs met omstelknop, wateraansluitpunt en houder handdouche","Partie apparente mitigeur de baignoire mural deux sorties, avec inverseur, prise d'eau et support pour douchette","External parts wall-mounted for shower mixer, two-way, diverter, water outlet, handshower hook",299,"Matte Black",1292,"GPF633450C072G000","8056329552678"]
["BATHROOM","ANELLO","ANELLO","54057+54058","54058","Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",726,"Warm Bronze Brushed PVD",388,"GPF540580P024G000","8056329025707"]
["BATHROOM","ANELLO","ANELLO","54055+63361","63361","Extern deel Wand-mengkraan 1-weg","Partie apparente pour mitigeur mural, 1 sortie.","External parts mixer one-way diverter",706,"Black Metal PVD",393,"GPF633610P001G000","8056329552227"]
["BATHROOM","ANELLO","ANELLO","54073+63379","63379","Extern deel Wand-Mengkraan 2-weg met automatische omstelknop bad/douche","Partie apparente mitigeur mural avec inverseur automatique bain-douche deux sorties","External parts for wall-mounted mixer two-way, bath/ shower diverter",707,"Black Metal Brushed PVD",1127,"GPF633790P004G000","8056329552111"]
["BATHROOM","ANELLO","ANELLO","54073+63380","63380","Parte esterna Miscelatore a parete 2 vie con deviatore bagno/doccia","Partie apparente mitigeur mural avec inverseur bain-douche deux sorties","External parts for wall-mounted mixer two-way, bath/ shower diverter",735,"Warm Bronze PVD",894,"GPF633800P037G000","8056329551985"]
["BATHROOM","ANELLO","ANELLO","54169+63332",54169,"Inbouwdeel Thermostatische Mengkraan Wanddouche","Partie encastrée pour mitigeur thermostatique douche mural","Built-in part for wall-mounted thermostatic shower mixer.",239,"Steel Brushed",438,"GPF541690A000G000","8022692841398"]
["BATHROOM","ANELLO","ANELLO","54169+63332",63332,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche mural 1 sortie.","External parts for thermostatic mixer, one-way diverter",187,"Aged Bronze",1346,"GPF633320G052G000","8056329561526"]
["BATHROOM","ANELLO","ANELLO","54169+63334",63334,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche mural 2 sorties.","External parts for thermostatic mixer, two-ways diverter",706,"Black Metal PVD",1260,"GPF633340P001G000","8056329553422"]
["BATHROOM","ANELLO","ANELLO","54169+63335",54169,"Inbouwdeel Thermostatische Mengkraan Wanddouche","Partie encastrée pour mitigeur thermostatique douche mural","Built-in part for wall-mounted thermostatic shower mixer.",239,"Steel Brushed",438,"GPF541690A000G000","8022692841398"]
["BATHROOM","ANELLO","ANELLO","54169+63336",63336,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche mural 3 sorties.","External parts for thermostatic mixer, three-ways diverter",726,"Warm Bronze Brushed PVD",1346,"GPF633360P024G000","8056329553194"]
["BATHROOM","ANELLO","ANELLO","09269+63135",63135,"afbouwdeel voor 2-uitgang thermostatische mengkraan","Partie apparente mitigeur thermostatique 2 voies.","External part for 2-outlet thermostat mixer",708,"Copper Brushed PVD",1392,"GPF631350P006G000","8056603879286"]
["BATHROOM","ANELLO","ANELLO","09269+63137",63137,"afbouwdeel voor 3-uitgang thermostatische mengkraan","Partie apparente mitigeur thermostatique 3 voies.","External part for 3-outlet thermostat mixer","030","Copper PVD",1304,"GPF631370P000G000","8056603879040"]
["BATHROOM","ANELLO","ANELLO","09266+63436",63436,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie externe mitigeur thermostatique mural à 3 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with three separate exits.",706,"Black Metal PVD",1938,"GPF634360P001G000","8056603618908"]
["BATHROOM","ANELLO","ANELLO","09266+63436",63436,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie externe mitigeur thermostatique mural à 3 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with three separate exits.",726,"Warm Bronze Brushed PVD",2069,"GPF634360P024G000","8056603618854"]
["BATHROOM","ANELLO","ANELLO","09263+63440",63440,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie externe mitigeur thermostatique mural à 5 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with five separate exits.",707,"Black Metal Brushed PVD",2574,"GPF634400P004G000","8056603630375"]
["BATHROOM","ANELLO","ANELLO","43103+43234",43234,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",149,"Finox Brushed Nickel",1889,"GPF432341G002G000","8022692624106"]
["BATHROOM","ANELLO","ANELLO","43105+43066",43066,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS","031","Chrome",1311,"GPF430662G001G000","8022692582345"]
["BATHROOM","ANELLO","ANELLO","43105+43066",43066,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",761,"Coffee Bronze Brushed PVD",2997,"GPF430662E059G000","8055261603349"]
["BATHROOM","ANELLO","ANELLO","43107+43068",43068,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",720,"Nickel PVD",2858,"GPF430682P014G000","8056603456999"]
["BATHROOM","ANELLO","ANELLO","43109+43070",43070,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",707,"Black Metal Brushed PVD",3472,"GPF430702P004G000","8056329131538"]
["BATHROOM","ANELLO","ANELLO","43109+43240",43240,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",727,"Brass Brushed PVD",3472,"GPF432401P025G000","8056329608221"]
["BATHROOM","ANELLO","ANELLO","43111+43072",43072,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 uitgangen met enkele selectie. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties avec manette selective. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS with single selection",710,"Brass PVD",2353,"GPF430722P011G000","8056329608610"]
["BATHROOM","ANELLO","ANELLO","43281+43256",43256,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente mitigeur THERMOSTATIQUE douche haut débit","External parts wall-mounted thermostatic high-capacity mixer",761,"Coffee Bronze Brushed PVD",1235,"GPF432561E059G000","8055261603080"]
["BATHROOM","ANELLO","ANELLO","43283+43268",43268,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur haut débit.","External parts for stop valve for thermostatic high-capacity mixer.",713,"Antique Brass",708,"GPF432680V204G000","8056329561991"]
["BATHROOM","ANELLO","ANELLO",63356,63356,"Multifunctionele verstelbare wandgemonteerde anti-kalk douche head","Pomme de douche anticalcaire latérale orientable. MULTI-FONCTION","Multifunctional adjustable wall-mounted anti-limescale shower head",706,"Black Metal PVD",1400,"GPF633560P001G000","8056603586399"]
["BATHROOM","ANELLO","ANELLO",63348,63348,"Oriënteerbare wand-hoofddouchekop","Pomme de douche latérale orientable.","Wall-mounted adjustable showerhead",707,"Black Metal Brushed PVD",900,"GPF633480P004G000","8056329552418"]
["BATHROOM","ANELLO","ANELLO",63352,63352,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable shower head",708,"Copper Brushed PVD",802,"GPF633520P006G000","8056329552302"]
["BATHROOM","ANELLO","ANELLO",63352,63352,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable shower head",279,"Matte White",686,"GPF633520C071G000","8056603637343"]
["BATHROOM","ANELLO","ANELLO",63450,63450,"Plafond-hoofddouchekop arm aanpasbare hoogte DIAMANTATO","Pomme de douche au plafond avec bras orientable, longueur à la DEMANDE. DIAMANTATO","Ceiling-mounted showerhead, length on request DIAMANTATO",706,"Black Metal PVD",2566,"GPF634500P001G000","8056329563315"]
["BATHROOM","ANELLO","ANELLO",63450,63450,"Plafond-hoofddouchekop arm aanpasbare hoogte DIAMANTATO","Pomme de douche au plafond avec bras orientable, longueur à la DEMANDE. DIAMANTATO","Ceiling-mounted showerhead, length on request DIAMANTATO",708,"Copper Brushed PVD",2737,"GPF634500P006G000","8056329563292"]
["BATHROOM","ANELLO","ANELLO",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",720,"Nickel PVD",1715,"GPF630450P014G000","8055261729612"]
["BATHROOM","ANELLO","ANELLO",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",726,"Warm Bronze Brushed PVD",1726,"GPF630500P024G000","8055261729438"]
["BATHROOM","ANELLO","ANELLO",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",727,"Brass Brushed PVD",1726,"GPF630500P025G000","8055261729421"]
["BATHROOM","ANELLO","ANELLO",63653,63653,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. DIAMANTATO","Pomme de douche au plafond orientable, longueur à la demande. DIAMANTATO","Ceiling-mounted adjustable headshower, length on request. DIAMANTATO",706,"Black Metal PVD",3040,"GPF636530P001G000","8055261728806"]
["BATHROOM","ANELLO","ANELLO",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",727,"Brass Brushed PVD",2352]
["BATHROOM","ANELLO","ANELLO",63449,63449,"Verstelbare hoofddouche aan de muur. DIAMANTATO.","Pomme de douche latérale orientable. DIAMANTATO.","Wall-mounted adjustable headshower. DIAMANTATO.",187,"Aged Bronze",3179,"GPF634490G052G000","8055261242272"]
["BATHROOM","ANELLO","ANELLO",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",727,"Brass Brushed PVD",2543]
["BATHROOM","ANELLO","ANELLO",63472,63472,"Verstelbare plafonddouche. DIAMANTATO.","Pomme de douche au plafond orientable. DIAMANTATO.","Ceiling-mounted adjustable headshower. DIAMANTATO.",726,"Warm Bronze Brushed PVD",3179,"GPF634720P024G000","8055261241756"]
["BATHROOM","ANELLO","ANELLO",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",710,"Brass PVD",3096]
["BATHROOM","ANELLO","ANELLO",63470,63470,"Verstelbare plafonddouche. lengte op aanvraag. DIAMANTATO.","Pomme de douche au plafond avec bras orientable, longueur à la demande. DIAMANTATO.","Ceiling-mounted adjustable headshower. Length on request. DIAMANTATO.",713,"Antique Brass",4133,"GPF634700V204G000","8055261241879"]
["BATHROOM","ANELLO","ANELLO",63482,63482,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m. DIAMANTATO.","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée. DIAMANTATO.","Sliding rail with antilimestone handshower, 1,50 m flexible hose and water outlet. DIAMANTATO.",713,"Antique Brass",1372,"GPF634820V204G000","8056329565159"]
["BATHROOM","ANELLO","ANELLO",63485,63485,"Glijstang. DIAMANTATO.","Barre de douche. DIAMANTATO.","Sliding rail. DIAMANTATO.",706,"Black Metal PVD",891,"GPF634850P001G000","8056329564961"]
["BATHROOM","ANELLO","ANELLO",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",726,"Warm Bronze Brushed PVD",1003,"GPF630990P024G000","8056329215948"]
["BATHROOM","ANELLO","ANELLO",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",727,"Brass Brushed PVD",1003,"GPF630990P025G000","8056329215924"]
["BATHROOM","ANELLO","ANELLO",32977,32977,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",707,"Black Metal Brushed PVD",411,"GPF329771P004G000","8022692889314"]
["BATHROOM","ANELLO","ANELLO","32985+32982",32982,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour douchette laterale orientable","External parts for adjustable lateral body jet","031","Chrome",397,"GPF329820G001G000","8022692519297"]
["BATHROOM","ANELLO","ANELLO",13375,13375,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","Adjustable lateral body jet","030","Copper PVD",315,"GPF133750P000G000","8056329037410"]
["BATHROOM","ANELLO","ANELLO",65295,65295,"Afbouwdeel Voor Waterval Douche Uitloop Nog Compleet Te Maken Met Separate Bediening (Niet Inclusief)","Partie apparente pour bec cascade de douche murale. À compléter par commande séparée.","Waterfall shower spout to be completed with separate control (not included)",713,"Antique Brass",1607,"GPF652950V204G000","8056603003865"]
["BATHROOM","ANELLO","ANELLO",20293,20293,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",238,"Mirror Steel",1550,"GPF202930A001G000","8022692642421"]
["BATHROOM","ANELLO","ANELLO",63461,63461,"Wateraansluitpunt met houder handdouche","Sortie murale coudée avec support fixe pour douchette.","Water outlet and handshower hook",713,"Antique Brass",381,"GPF634610V204G000","8056329560956"]
["BATHROOM","ANELLO","ANELLO",58157,58157,"Vaste houder voor handdouche","Support fixe pour douchette.","Fixed handshower hook",727,"Brass Brushed PVD",192,"GPF581570P025G000","8022692872002"]
["BATHROOM","ANELLO","ANELLO",58160,58160,"Oriënteerbare duplex houder voor handdouche","Support mural orientable pour douchette.","Adjustable handshower hook","031","Chrome",215,"GPF581600G001G000","8022692870732"]
["BATHROOM","ANELLO","ANELLO",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",761,"Coffee Bronze Brushed PVD",468,"GPF329290E059G000","8055261577657"]
["BATHROOM","ANELLO","ANELLO",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",735,"Warm Bronze PVD",364,"GPF329300P037G000","8055261227637"]
["BATHROOM","ANELLO","ANELLO",14371,14371,"Antikalk handdouche","Douchette anticalcaire.","Antilimestone handshower",845,"Dark Bronze",220,"GPF143710V221G000","8055261239753"]
["BATHROOM","ANELLO","ANELLO",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",708,"Copper Brushed PVD",239,"GPF143700P006G000","8056603145572"]
["BATHROOM","ANELLO","ANELLO",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",710,"Brass PVD",325,"GPF143760P011G000","8056603631792"]
["BATHROOM","ANELLO","ANELLO",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector","030","Copper PVD",252,"GPF473510P000G000","8056603587075"]
["BATHROOM","ANELLO","ANELLO",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",147,"Chome Brushed",217,"GPF473500G006G000","8056603631723"]
["BATHROOM","ANELLO","ANELLO","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",299,"Matte Black",134,"GPF016370C072G000","8022692845327"]
["BATHROOM","ANELLO","ANELLO",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish","031","Chrome",90,"GPF541370G001G000","8056329573116"]
["BATHROOM","ANELLO","ANELLO",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",761,"Coffee Bronze Brushed PVD",150,"GPF287460E059G000","8055261608771"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63701,63701,"Wand-zeepbakje wit","Porte-savon mural blanc.","White wall-mounted soap holder",706,"Black Metal PVD",419,"GPF637010P001G000","8056329587779"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63701,63701,"Wand-zeepbakje wit","Porte-savon mural blanc.","White wall-mounted soap holder",761,"Coffee Bronze Brushed PVD",475,"GPF637010E059G000","8055261591349"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63707,63707,"Wand-glashouder wit","Porte-verre mural blanc.","Wall-mounted tumbler holder white",720,"Nickel PVD",471,"GPF637070P014G000","8056603494731"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63708,63708,"Wand-glashouder zwart","Porte-verre mural noir.","Wall-mounted tumbler holder black",187,"Aged Bronze",502,"GPF637080G052G000","8056329587496"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63714,63714,"Wand-dispenserhouder zwart","Distributeur de savon liquide mural noir.","Black wall-mounted soap dispenser holder",710,"Brass PVD",650,"GPF637140P011G000","8056329590205"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63719,63719,"Wand-toiletborstelhouder wit","Porte-balayette mural blanche.","White wall-mounted brush holder",706,"Black Metal PVD",640,"GPF637190P001G000","8056329587175"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",58525,58525,"Witte Staande Zeephouder","Porte-savon à poser blanc","Standing soap holder, white","031","Chrome",242,"GPF585250G001G000","8022692870886"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",58525,58525,"Witte Staande Zeephouder","Porte-savon à poser blanc","Standing soap holder, white",187,"Aged Bronze",381,"GPF585250G052G000","8022692873443"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",58531,58531,"Witte Staande Bekerhouder","Porte-verre à poser blanc.","Standing tumbler holder, white",727,"Brass Brushed PVD",417,"GPF585310P025G000","8022692872187"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",58532,58532,"Zwarte Staande Bekerhouder","Porte-verre à poser noir","Standing tumbler holder, black",845,"Dark Bronze",417,"GPF585320V221G000","8056603622004"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",66437,66437,"staande witte zeep dispenser","Distributeur de savon liquide à poser blanc","Standing soap dispenser holder, white",710,"Brass PVD",552,"GPF664370P011G000","8056603609302"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",66438,66438,"staande zwarte zeep dispenser","Distributeur de savon liquide à poser noir","Standing soap dispenser holder, black",727,"Brass Brushed PVD",589,"GPF664380P025G000","8056603572873"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63744,63744,"Staande toiletborstelhouder zwart","Porte-balayette a poser noir","Standing brush holder, black",735,"Warm Bronze PVD",464,"GPF637440P037G000","8056329566774"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63755,63755,"Horizontale of verticale wand-toiletrolhouder","Porte-papier mural horizontal ou vertical.","Paper-roll holder for horizontal/vertical installation",710,"Brass PVD",290,"GPF637550P011G000","8056329590021"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63797,63797,"Wand-handdoekhouder 30 cm","Porte-serviette 30 cm.","30 cm centre distance towel rail",710,"Brass PVD",485,"GPF637971P011G000","8056329590007"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63803,63803,"Wand-handdoekhouder 60 cm","Porte-serviette 60 cm.","60 cm centre distance towel rail",149,"Finox Brushed Nickel",468,"GPF638031G002G000","8056329586406"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63809,63809,"Wand-handdoekhouder ringvorm","Anneau porte-serviette.","Towel ring","031","Chrome",300,"GPF638090G001G000","8056329567931"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63721,63721,"Wand-kledinghaak","Patère.","Wall-mounted robe hook",706,"Black Metal PVD",185,"GPF637210P001G000","8056329586970"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63826,63826,"Handdoekhouder 45 cm","Poignée et porte-serviette pour verre 45 cm","45 cm towel rail for glass fixing",727,"Brass Brushed PVD",875,"GPF638261P025G000","8056329589711"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",63828,63828,"Handdoekhouder 60 cm","Poignée et porte-serviette pour verre 60 cm","60 cm towel rail for glass fixing",727,"Brass Brushed PVD",886,"GPF638281P025G000","8056329589698"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",45590,45590,"Papierbak wit","Poubelle blanche.","White waste-paper basket","031","Chrome",543,"GPF455900G001G000","8022692815122"]
["BATHROOM","ANELLO","ANELLO ACCESSORIES",45590,45590,"Papierbak wit","Poubelle blanche.","White waste-paper basket",246,"Gold PVD",913,"GPF455900P007G000","8056603597333"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",706,"Black Metal PVD",246,"GPF391840P001G000","8056603451932"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",716,"Gold Brushed PVD",290,"GPF375842P005G000","8056329025462"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs","030","Copper PVD",146,"GPF375870P000G000","8022692654813"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",149,"Finox Brushed Nickel",648,"GPF451300G002G000","8055261227590"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","030","Copper PVD",711,"GPF451300P000G000","8055261227569"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",761,"Coffee Bronze Brushed PVD",806,"GPF451310E059G000","8055261577398"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1152,"GPF451240P011G000","8056603615792"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",706,"Black Metal PVD",962,"GPF451231P001G000","8022692811728"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1354,"GPF452260P004G000","8055261645943"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1152,"GPF451260P011G000","8056603632898"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",187,"Aged Bronze",1029,"GPF143313G052G000","8056603507691"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",246,"Gold PVD",1579,"GPF451220P007G000","8056603615990"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",279,"Matte White",1095,"GPF451211C071G000","8022692811636"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",54623,54623,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12. DIAMANTATO","Plaques de déclenchement pour Geberit SIgma 8 e Sigma 12. DIAMANTATO","Cover plate GEBERIT SIGMA 8 & 12. DIAMANTATO",727,"Brass Brushed PVD",1039,"GPF546230P025G000","8056329598768"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",54627,54627,"Bedieningspaneel voor Geberit OMEGA 12. DIAMANTATO","Plaques de déclenchement pour GEBERIT OMEGA 12. DIAMANTATO","Cover plate GEBERIT OMEGA 12. DIAMANTATO","031","Chrome",628,"GPF546270G001G000","8056329566422"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",54629,54629,"Bedieningspaneel voor TECE. DIAMANTATO","Plaques de déclenchement pour TECE. DIAMANTATO","Cover plate TECE. DIAMANTATO","030","Copper PVD",1036,"GPF546290P000G000","8056329566279"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",54633,54633,"Bedieningspaneel voor VIEGA PREVISTA 12. DIAMANTATO","Plaques de déclenchement pour VIEGA PREVISTA 12. DIAMANTATO","Cover plate VIEGA PREVISTA 12. DIAMANTATO",708,"Copper Brushed PVD",1836,"GPF546331P006G000","8056329566026"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",761,"Coffee Bronze Brushed PVD",4037,"GPF546010E059G000","8055261598959"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",54599,54599,"Afvoerplug \"Stop&Go\"","Bonde de lavabo “Stop & Go” 2 en 1 : un mécanisme d'ouverture et de fermeture dévissable et remplaçable avec un mécanisme toujours ouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",726,"Warm Bronze Brushed PVD",194,"GPF545990P024G000","8022692841817"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK",28767,28767,"Verlengstuk buis voor sifon, lengte 40 cm","Tubelure prolongée pour siphone, longueur 40 cm","Syphon pipe extension, 40 cm length","031","Chrome",52,"GPF287670G001G000","8022692497403"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK","01377","01377","1 1/4\" sifon","Siphon 1 1/4”.","1 1/4\" syphon",710,"Brass PVD",429,"GPF013771P011G000","8056329615274"]
["BATHROOM","ANELLO","ANELLO TOTAL LOOK","01411","01411","Onderbouwmengkraan met filter en 1/2\" aansluiting","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection","030","Copper PVD",225,"GPF014110P000G000","8022692633597"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63501,63501,"Mengkraan Wastafel met waste met buigzame aansluitslangen","Mitigeur lavabo, avec vidage et flexibles de raccordement.","Basin mixer, flexible connections, with waste","031","Chrome",499,"GPF635010G001G000","8056329550742"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63502,63502,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo, sans vidage, avec flexibles de raccordement.","Basin mixer, flexible connections, without waste",735,"Warm Bronze PVD",663,"GPF635020P037G000","8056329550568"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63504,63504,"Mengkraan Wastafel hoog, korte uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec court, sans vidage, avec flexibles de raccordement.","High version basin mixer , short spout, flexible connections, without waste",710,"Brass PVD",859,"GPF635040P011G000","8056329591189"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63506,63506,"Mengkraan Wastafel hoog, lange uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec long, sans vidage, avec flexibles de raccordement.","High version basin mixer , long spout, flexible connections, without waste",706,"Black Metal PVD",883,"GPF635060P001G000","8056329550209"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63515,63515,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo, sans vidage, avec flexibles de raccordement.","Basin mixer, flexible connections, without waste",706,"Black Metal PVD",1015,"GPF635150P001G000","8056329550001"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63321,63321,"Middelgrote wastafeluitloop","Bec de lavabo longueur moyenne","Medium spout basin",708,"Copper Brushed PVD",441,"GPF633210P006G000","8056329554207"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63323,63323,"Hoge wastafeluitloop","Bec de lavabo long","High spout basin",726,"Warm Bronze Brushed PVD",493,"GPF633230P024G000","8056329554092"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","63397+63589",63589,"Extern deel Wand-Mengkraan Wastafel lange uitloop zonder waste","Partie apparente mitigeur lavabo mural avec bec long sans vidage","External parts wall-mounted basin mixer, long spout, without waste","031","Chrome",522,"GPF635890G001G000","8056329548541"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","63397+63581",63581,"Extern deel Wand-Mengkraan Wastafel wand korte uitloop zonder waste","Partie apparente mitigeur lavabo muralavec bec court sans vidage","External parts for wall-mounted basin mixer, short spout, without waste",299,"Matte Black",607,"GPF635810C072G000","8056329548855"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","63397+63583",63583,"Extern deel Wand-Mengkraan Wastafel lange uitloop zonder waste","Partie apparente mitigeur lavabo mural avec bec long sans vidage","External parts wall-mounted basin mixer, long spout, without waste",149,"Finox Brushed Nickel",607,"GPF635830G002G000","8056329548732"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","63412+63609",63609,"Extern deel Wandafstandsbediening Wastafel 1-weg","Partie apparente pour commande séparée lavabo mural une sortie","External parts wall-mounted basin separate control, one-way",707,"Black Metal Brushed PVD",271,"GPF636090P004G000","8056329547797"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63403,63403,"Wanduitloop Wastafel middelgrote uitloop","Bec de lavabo mural moyen","Wall-mounted spout basin, medium spout",707,"Black Metal Brushed PVD",338,"GPF634030P004G000","8056329551305"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63404,63404,"Wanduitloop Wastafel lange uitloop","Bec de lavabo mural long","Wall-mounted spout basin, long spout",187,"Aged Bronze",345,"GPF634040G052G000","8056329561069"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.",720,"Nickel PVD",1932,"GPF634990P014G000","8056603455817"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","46189+63593",63593,"Afbouwdelen voor vrijstaande wastafelmengkraan zonder afvoer","Partie externe mitigeur de lavabo au sol sans vidage","External parts for freestanding basin mixer without waste",726,"Warm Bronze Brushed PVD",2581,"GPF635930P024G000","8056603617093"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63507,63507,"Mengkraan Bidet met buigzame aansluitslangen","Mitigeur bidet avec vidage et flexibles de raccordement","Bidet mixer with flexible connections","031","Chrome",499,"GPF635070G001G000","8056329550148"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63547,63547,"Badrandgroep 3 gaten met omstelknop, buigzame slang 1,50 m en antikalk-handdouche. Afgifte naar de badkolom","Mélangeur bain-douche trois trous avec inverseur, flexibles de raccordement 1,50m et douchette anticalcaire, sortie coudée.","Three-holes bath mixer with diverter, 1,50 m flexible hose and antilimestone handshower. To be used with overflow filler",726,"Warm Bronze Brushed PVD",2200,"GPF635470P024G000","8056329549173"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63537,63537,"Groep Badrand 4 gaten met wateruitloop, omstelknop, buigzame slang 1,50 m en antikalk-handdouche","Mélangeur bain-douche quatre trous avec bec, inverseur, flexibles de raccordement 1,50m et douchette anticalcaire","Four-holes bath mixer with diverter, tub-filler spout and 1,50 m flexible hose and antilimestone handshower",149,"Finox Brushed Nickel",2226,"GPF635370G002G000","8056329549739"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63327,63327,"Conus handdouchehouder met antikalk-handdouche en buigzame slang 1,50 m","Support douchette avec douchette anticacaire et flexibles 1,5m","Conical shower hook with antilimestone handshower and 1,5 m flexible",710,"Brass PVD",525,"GPF633270P011G000","8056329592100"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","01663","01663","Drie-gats afwerkplaat voor montagebox","Plaque de finition 3 trous pour la boîte de sécurité","Three-holes finishing plate for mounting box","030","Copper PVD",736,"GPF016631P000G000","8022692877946"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","01664","01664","Four-holes finishing plaatje voor montage box","Plaque de finition 4 trous pour la boîte de sécurité","Four-holes finishing plate for mounting box",735,"Warm Bronze PVD",788,"GPF016641P037G000","8056329559080"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","01786","01786","Uittrekbare handdouche afvoerset, randinstallatie. Niet passend op artikelen 01669, 01658, 01663 en 01664.","Système de récupération d'eau pour flexible de douchette, installation sur le bord de la baignoire. Ne peut être combiné avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, rim installation. Not fitting items 01669, 01658, 01663 and 01664.",761,"Coffee Bronze Brushed PVD",1469,"GPF017860E059G000","8055261609754"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","01080","01080","Polyethyleen badafvoer met overloopdopvuller. Lengte van de aanvoer leiding 80 cm","Vidage en polyéthylène baignoire avec trop-plein. Longueur 80 cm","Polyethylene column bath waste with overflow cap filler. Length of control cable 80 cm",727,"Brass Brushed PVD",680,"GPF010802P025G000","8056329076006"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",20191,20191,"Cascade-uitloop Badrand Aan te vullen met afstandsbediening","Bec cascade pour baignoire à compléter par un mitigeur à commande séparée.","Bath group waterfall spout to be completed with separate control",710,"Brass PVD",2503,"GPF201910P011G000","8056329612952"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63603,63603,"Wanduitloop Bad","Bec de bagnoire mural.","Wall-fixing bath spout",713,"Antique Brass",390,"GPF636030V204G000","8056329560390"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",299,"Matte Black",356,"GPF540580C072G000","8056329536968"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","54055+63561",63561,"Extern deel Wand-mengkraan 1-weg","Partie apparente pour mitigeur mural, 1 sortie.","External parts mixer one-way diverter",707,"Black Metal Brushed PVD",418,"GPF635610P004G000","8056329549098"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","54073+63579",63579,"Extern deel Wand-Mengkraan 2-weg met automatische omstelknop bad/douche","Partie apparente mitigeur mural avec inverseur automatique bain-douche deux sorties","External parts for wall-mounted mixer two-way, bath/ shower diverter",299,"Matte Black",965,"GPF635790C072G000","8056329549050"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","54073+63580",63580,"Extern deel Wand-Mengkraan 2-weg met automatische omstelknop bad/douche","Partie apparente mitigeur mural avec inverseur automatique bain-douche deux sorties","External parts for wall-mounted mixer two-way, bath/ shower diverter",149,"Finox Brushed Nickel",817,"GPF635800G002G000","8056329548930"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","44673+63577",63577,"Extern deel Wand-Mengkraan 2-weg met automatische omstelknop bad/douche","Partie apparente mitigeur mural avec inverseur automatique bain-douche deux sorties","External parts for wall-mounted mixer two-way, automatic bath/ shower diverter",710,"Brass PVD",679,"GPF635770P011G000","8056329590847"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","54169+63332",63332,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche mural 1 sortie.","External parts for thermostatic mixer, one-way diverter",735,"Warm Bronze PVD",1260,"GPF633320P037G000","8056329553583"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","54169+63332",63332,"Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche mural 1 sortie.","External parts for thermostatic mixer, one-way diverter",710,"Brass PVD",1260,"GPF633320P011G000","8056329592025"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","54169+63334",63334,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche mural 2 sorties.","External parts for thermostatic mixer, two-ways diverter",726,"Warm Bronze Brushed PVD",1346,"GPF633340P024G000","8056329553392"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","54169+63335",63335,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche mural 3 sorties.","External parts for thermostatic mixer, three-ways diverter",708,"Copper Brushed PVD",1216,"GPF633350P006G000","8056329553309"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","09269+63139",63139,"afbouwdeel voor 1-uitgang thermostatische mengkraan","Partie apparente mitigeur thermostatique 1 voie.","External part for 1-outlet thermostat mixer",706,"Black Metal PVD",1304,"GPF631390P001G000","8056603878722"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","09269+63141",63141,"afbouwdeel voor 2-uitgang thermostatische mengkraan","Partie apparente mitigeur thermostatique 2 voies.","External part for 2-outlet thermostat mixer",713,"Antique Brass",1392,"GPF631410V204G000","8056603878265"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","09269+63143",63143,"afbouwdeel voor 3-uitgang thermostatische mengkraan","Partie apparente mitigeur thermostatique 3 voies.","External part for 3-outlet thermostat mixer",707,"Black Metal Brushed PVD",1392,"GPF631430P004G000","8056603878104"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","09266+63436","09266","Inbouwdeel voor thermostatische mengkraan, 3 separate uitgangen","Partie encastrée du mitigeur thermostatique mural 3 sorties indépendantes","Built-in part for thermostatic mixer, THREE separate exits","031","Chrome",1173,"GPF092660G001G000","8056603620789"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","09268+63438",63438,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie externe mitigeur thermostatique mural à 4 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with four separate exits.",845,"Dark Bronze",2346,"GPF634380V221G000","8056603993210"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","09263+63440",63440,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie externe mitigeur thermostatique mural à 5 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with five separate exits.","031","Chrome",1630,"GPF634400G001G000","8056603630443"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","43103+43234",43234,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS","031","Chrome",1126,"GPF432341G001G000","8022692584912"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","43103+43234",43234,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",713,"Antique Brass",2389,"GPF432341V204G000","8056329562097"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","43105+43066",43066,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",279,"Matte White",2180,"GPF430662C071G000","8022692623956"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","43105+43236",43236,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",187,"Aged Bronze",2750,"GPF432361G052G000","8056329562080"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","43107+43238",43238,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",710,"Brass PVD",2858,"GPF432381P011G000","8056329608252"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","43109+43070",43070,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",710,"Brass PVD",3153,"GPF430702P011G000","8056329608634"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","43109+43240",43240,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",727,"Brass Brushed PVD",3472,"GPF432401P025G000","8056329608221"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","43111+43072",43072,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 uitgangen met enkele selectie. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties avec manette selective. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS with single selection",708,"Copper Brushed PVD",2607,"GPF430722P006G000","8056329131453"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","43281+43256",43256,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente mitigeur THERMOSTATIQUE douche haut débit","External parts wall-mounted thermostatic high-capacity mixer",710,"Brass PVD",1020,"GPF432561P011G000","8056329565289"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",45163,45163,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted shower head",706,"Black Metal PVD",2706,"GPF451630P001G000","8022692889734"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63554,63554,"wandgemonteerde antikalk en verstelbare hoofddouche","Pomme de douche anticalcaire latérale orientable.","Wall-mounted anti-limestone showerhead",706,"Black Metal PVD",1400,"GPF635540P001G000","8056603586252"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63348,63348,"Oriënteerbare wand-hoofddouchekop","Pomme de douche latérale orientable.","Wall-mounted adjustable showerhead","031","Chrome",572,"GPF633480G001G000","8056329552463"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63348,63348,"Oriënteerbare wand-hoofddouchekop","Pomme de douche latérale orientable.","Wall-mounted adjustable showerhead",707,"Black Metal Brushed PVD",900,"GPF633480P004G000","8056329552418"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63352,63352,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable shower head",761,"Coffee Bronze Brushed PVD",852,"GPF633520E059G000","8055261592988"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63548,63548,"Oriënteerbare wand-hoofddouchekop RIGATO","Pomme de douche latérale orientable. RIGATO","Wall-mounted adjustable showerhead RIGATO",706,"Black Metal PVD",1932,"GPF635480P001G000","8056329563094"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63550,63550,"Plafond-hoofddouchekop arm aanpasbare hoogte RIGATO","Pomme de douche au plafond avec bras orientable, longueur à la DEMANDE. RIGATO","Ceiling-mounted showerhead, length on request RIGATO",299,"Matte Black",2340,"GPF635500C072G000","8056329563032"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63552,63552,"Oriënteerbare plafond-hoofddouchekop RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable showerhead RIGATO",726,"Warm Bronze Brushed PVD",1957,"GPF635520P024G000","8056329562844"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63045,63045,"Verstelbare hoofddouche voor wandmontage.","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",720,"Nickel PVD",1715,"GPF630450P014G000","8055261729612"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO","030","Copper PVD",2338,"GPF637500P000G000","8055261728479"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",720,"Nickel PVD",2101,"GPF630530P014G000","8055261729278"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","031","Chrome",1488]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63549,63549,"Verstelbare hoofddouche aan de muur. RIGATO.","Pomme de douche latérale orientable. RIGATO.","Wall-mounted adjustable headshower. RIGATO.",299,"Matte Black",2717,"GPF635490C072G000","8055261241701"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",149,"Finox Brushed Nickel",2173]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63568,63568,"Verstelbare hoofddouche aan de muur. RIGATO.","Pomme de douche latérale orientable. RIGATO.","Wall-mounted adjustable headshower. RIGATO.",726,"Warm Bronze Brushed PVD",3371,"GPF635680P024G000","8055261241459"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63572,63572,"Verstelbare plafonddouche. RIGATO.","Pomme de douche au plafond orientable. RIGATO.","Ceiling-mounted adjustable headshower. RIGATO.",713,"Antique Brass",3179,"GPF635720V204G000","8055261241121"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63570,63570,"Verstelbare plafonddouche. lengte op aanvraag. RIGATO.","Pomme de douche au plafond avec bras orientable, longueur à la demande. RIGATO.","Ceiling-mounted adjustable headshower. Length on request. RIGATO.",706,"Black Metal PVD",3872,"GPF635700P001G000","8055261241350"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63582,63582,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m. RIGATO.","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée. RIGATO.","Sliding rail with antilimestone handshower, 1,50 m flexible hose and water outlet. RIGATO.",299,"Matte Black",1173,"GPF635820C072G000","8056329569928"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63584,63584,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m. RIGATO.","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m. RIGATO.","Sliding rail with antilimestone handshower, 1,50 m flexible hose. RIGATO.",726,"Warm Bronze Brushed PVD",1166,"GPF635840P024G000","8056329569713"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63329,63329,"Doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m.","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",710,"Brass PVD",658,"GPF633290P011G000","8056329592063"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",726,"Warm Bronze Brushed PVD",1003,"GPF630990P024G000","8056329215948"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",32971,32971,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",279,"Matte White",404,"GPF329710C071G000","8022692625813"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",32977,32977,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",707,"Black Metal Brushed PVD",411,"GPF329771P004G000","8022692889314"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","32985+32982",32982,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour douchette laterale orientable","External parts for adjustable lateral body jet",716,"Gold Brushed PVD",804,"GPF329820P005G000","8056603933162"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",65295,65295,"Afbouwdeel Voor Waterval Douche Uitloop Nog Compleet Te Maken Met Separate Bediening (Niet Inclusief)","Partie apparente pour bec cascade de douche murale. À compléter par commande séparée.","Waterfall shower spout to be completed with separate control (not included)",149,"Finox Brushed Nickel",1375,"GPF652950G002G000","8056603003971"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",65295,65295,"Afbouwdeel Voor Waterval Douche Uitloop Nog Compleet Te Maken Met Separate Bediening (Niet Inclusief)","Partie apparente pour bec cascade de douche murale. À compléter par commande séparée.","Waterfall shower spout to be completed with separate control (not included)",845,"Dark Bronze",1607,"GPF652950V221G000","8056603621922"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",20293,20293,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",735,"Warm Bronze PVD",2295,"GPF202930P037G000","8056329555822"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",63461,63461,"Wateraansluitpunt met houder handdouche","Sortie murale coudée avec support fixe pour douchette.","Water outlet and handshower hook",713,"Antique Brass",381,"GPF634610V204G000","8056329560956"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",58157,58157,"Vaste houder voor handdouche","Support fixe pour douchette.","Fixed handshower hook",845,"Dark Bronze",192,"GPF581570V221G000","8056603622639"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",58160,58160,"Oriënteerbare duplex houder voor handdouche","Support mural orientable pour douchette.","Adjustable handshower hook",713,"Antique Brass",338,"GPF581600V204G000","8022692872651"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",279,"Matte White",376,"GPF329290C071G000","8055261236257"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",246,"Gold PVD",413,"GPF329300P007G000","8055261227682"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",14371,14371,"Antikalk handdouche","Douchette anticalcaire.","Antilimestone handshower",246,"Gold PVD",234,"GPF143710P007G000","8055261239821"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",246,"Gold PVD",252,"GPF143700P007G000","8056603631839"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",707,"Black Metal Brushed PVD",346,"GPF143780P004G000","8056603633239"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",727,"Brass Brushed PVD",269,"GPF473510P025G000","8056603587013"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",149,"Finox Brushed Nickel",217,"GPF473500G002G000","8056603535731"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",845,"Dark Bronze",120,"GPF016370V221G000","8056603623247"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish",707,"Black Metal Brushed PVD",150,"GPF541370P004G000","8022692850161"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",845,"Dark Bronze",143,"GPF287460V221G000","8056603623186"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector","030","Copper PVD",152,"GPF017240P000G000","8055261240094"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63801,63801,"Wand-zeepbakje wit","Porte-savon mural blanc.","Wall-mounted soap dish, white",187,"Aged Bronze",447,"GPF638010G052G000","8056329586598"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63808,63808,"Wand-glashouder zwart","Porte-verre mural noir.","Wall-mounted holder, black",720,"Nickel PVD",471,"GPF638080P014G000","8056603494571"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63813,63813,"Wand-dispenserhouder wit","Distributeur de savon liquide mural blanc.","Wall-mounted liquid soap dispenser , white",299,"Matte Black",593,"GPF638130C072G000","8056329575103"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63814,63814,"Wand-dispenserhouder zwart","Distributeur de savon liquide mural noir.","Wall-mounted liquid soap dispenser - black",735,"Warm Bronze PVD",650,"GPF638140P037G000","8056329585935"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63819,63819,"Wand-toiletborstelhouder wit","Porte-balayette mural blanche.","Wall-mounted brush holder, white",726,"Warm Bronze Brushed PVD",683,"GPF638190P024G000","8056329585843"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63820,63820,"Wand-toiletborstelhouder zwart","Porte-balayette mural noir.","Wall-mounted brush holder, black",713,"Antique Brass",683,"GPF638200V204G000","8056329585720"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",58526,58526,"Zwarte Witte Staande Zeephouder","Porte-savon à poser noir","Standing soap holder, black",713,"Antique Brass",381,"GPF585260V204G000","8056329062283"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",58531,58531,"Witte Staande Bekerhouder","Porte-verre à poser blanc.","Standing tumbler holder, white",845,"Dark Bronze",417,"GPF585310V221G000","8056603622011"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",58532,58532,"Zwarte Staande Bekerhouder","Porte-verre à poser noir","Standing tumbler holder, black",246,"Gold PVD",444,"GPF585320P007G000","8056329062146"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",66437,66437,"staande witte zeep dispenser","Distributeur de savon liquide à poser blanc","Standing soap dispenser holder, white",727,"Brass Brushed PVD",589,"GPF664370P025G000","8056603572972"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",66438,66438,"staande zwarte zeep dispenser","Distributeur de savon liquide à poser noir","Standing soap dispenser holder, black",726,"Warm Bronze Brushed PVD",589,"GPF664380P024G000","8056603572880"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63743,63743,"Staande toiletborstelhouder wit","Porte-balayette à poser blanche.","Standing brush holder, white",710,"Brass PVD",464,"GPF637430P011G000","8056329590069"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63855,63855,"Horizontale of verticale wand-toiletrolhouder","Porte-papier mural horizontal ou vertical.","Paper-roll holder for horizontal/vertical installation",735,"Warm Bronze PVD",290,"GPF638550P037G000","8056329585232"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63897,63897,"Wand-handdoekhouder 30 cm","Porte-serviette 30 cm.","30 cm centre distance towel rail",735,"Warm Bronze PVD",485,"GPF638971P037G000","8056329585133"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63903,63903,"Wand-handdoekhouder 60 cm","Porte-serviette 60 cm.","60 cm centre distance towel rail",299,"Matte Black",468,"GPF639031C072G000","8056329574991"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63903,63903,"Wand-handdoekhouder 60 cm","Porte-serviette 60 cm.","60 cm centre distance towel rail",713,"Antique Brass",546,"GPF639031V204G000","8056329584921"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63821,63821,"Wand-kledinghaak","Patère.","Wall-mounted robe hook",726,"Warm Bronze Brushed PVD",198,"GPF638210P024G000","8056329585645"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",63926,63926,"Handdoekhouder 45 cm","Poignée et porte-serviette pour verre 45 cm","45 cm towel rail for glass fixing",707,"Black Metal Brushed PVD",875,"GPF639261P004G000","8056329584761"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",735,"Warm Bronze PVD",1465,"GPF584241P037G000","8056329556461"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",710,"Brass PVD",1465,"GPF584241P011G000","8056329595057"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.","031","Chrome",154,"GPF391840G001G000","8056603452038"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",726,"Warm Bronze Brushed PVD",260,"GPF391840P024G000","8056603451871"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",708,"Copper Brushed PVD",273,"GPF375842P006G000","8022692430080"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",147,"Chome Brushed",125,"GPF375870G006G000","8022692536164"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",149,"Finox Brushed Nickel",714,"GPF452300G002G000","8055261645677"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",707,"Black Metal Brushed PVD",758,"GPF451310P004G000","8055261227361"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1161,"GPF452270P001G000","8055261645806"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1152,"GPF451240P001G000","8056603615839"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",726,"Warm Bronze Brushed PVD",1029,"GPF451231P024G000","8056329013315"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1152,"GPF451260P011G000","8056603632898"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",650,"GPF143313G001G000","8022692049831"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",246,"Gold PVD",1092,"GPF143313P007G000","8056329223974"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1390,"GPF451220P011G000","8056603615983"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",54635,54635,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12. RIGATO","Plaques de déclenchement pour Geberit SIgma 8 e Sigma 12. RIGATO","Cover plate GEBERIT SIGMA 8 & 12. RIGATO",720,"Nickel PVD",976,"GPF546350P014G000","8056603606806"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",54639,54639,"Bedieningspaneel voor Geberit OMEGA 12. RIGATO","Plaques de déclenchement pour GEBERIT OMEGA 12. RIGATO","Cover plate GEBERIT OMEGA 12. RIGATO","031","Chrome",628,"GPF546390G001G000","8056329565760"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",54639,54639,"Bedieningspaneel voor Geberit OMEGA 12. RIGATO","Plaques de déclenchement pour GEBERIT OMEGA 12. RIGATO","Cover plate GEBERIT OMEGA 12. RIGATO","030","Copper PVD",927,"GPF546390P000G000","8056329565722"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",54643,54643,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600. RIGATO.","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600. RIGATO.","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600. RIGATO.",707,"Black Metal Brushed PVD",1451,"GPF546430P004G000","8056329565487"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",54645,54645,"Bedieningspaneel voor VIEGA PREVISTA 12. RIGATO","Plaques de déclenchement pour VIEGA PREVISTA 12. RIGATO","Cover plate VIEGA PREVISTA 12. RIGATO",707,"Black Metal Brushed PVD",1834,"GPF546451P004G000","8056329565371"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",54599,54599,"Afvoerplug \"Stop&Go\"","Bonde de lavabo “Stop & Go” 2 en 1 : un mécanisme d'ouverture et de fermeture dévissable et remplaçable avec un mécanisme toujours ouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",707,"Black Metal Brushed PVD",194,"GPF545990P004G000","8022692841794"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",727,"Brass Brushed PVD",169,"GPF014210P025G000","8056603964173"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK",28767,28767,"Verlengstuk buis voor sifon, lengte 40 cm","Tubelure prolongée pour siphone, longueur 40 cm","Syphon pipe extension, 40 cm length",706,"Black Metal PVD",84,"GPF287670P001G000","8056329062818"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK","01377","01377","1 1/4\" sifon","Siphon 1 1/4”.","1 1/4\" syphon",735,"Warm Bronze PVD",429,"GPF013771P037G000","8056329559196"]
["BATHROOM","INGRANAGGIO","INGRANAGGIO TOTAL LOOK","01411","01411","Onderbouwmengkraan met filter en 1/2\" aansluiting","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection",706,"Black Metal PVD",225,"GPF014110P001G000","8022692852035"]
["BATHROOM","HABITO","HABITO UNITO",70002,70002,"Wastafel mengkraan, Flexibele slangen, zonder plug","Mitigeur lavabo sans vidage avec flexibles de raccordement.","Basin mixer without waste and connecting flexibles.",761,"Coffee Bronze Brushed PVD",771,"GPF700020E059G000","8055261585645"]
["BATHROOM","HABITO","HABITO UNITO",70006,70006,"Medium versie Wastafel mengkraan, Flexibele slangen, zonder plug","Mitigeur lavabo moyen sans vidage avec flexibles de raccordement.","Medium version basin mixer without waste and connecting flexibles.",735,"Warm Bronze PVD",812,"GPF700060P037G000","8056603668347"]
["BATHROOM","HABITO","HABITO UNITO",70004,70004,"Hoge versie Wastafel mengkraan, Flexibele slangen, zonder plug","Mitigeur lavabo réhaussé sans vidage avec flexibles de raccordement.","High version basin mixer without waste and connecting flexibles.","031","Chrome",599,"GPF700040G001G000","8056603668729"]
["BATHROOM","HABITO","HABITO UNITO","54198+70088",70088,"afbouwdeel voor wandgemonteerde wastafel kraan","Partie apparente mitigeur lavabo mural.","External part for wall-mounted basin mixer.",707,"Black Metal Brushed PVD",715,"GPF700880P004G000","8056603667289"]
["BATHROOM","HABITO","HABITO UNITO",66102,66102,"wand-gemonteerde uitloop wastafel, medium uitloop","Bec de lavabo mural moyen","Wall-mounted medium spout basin",726,"Warm Bronze Brushed PVD",325,"GPF661020P024G000","8056603566612"]
["BATHROOM","HABITO","HABITO UNITO",63399,63399,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond à compléter par un mitigeur à commande séparée","Ceiling-mounted spout. To be completed with separate control.",708,"Copper Brushed PVD",1474,"GPF633990P006G000","8056329551497"]
["BATHROOM","HABITO","HABITO UNITO",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.",720,"Nickel PVD",1932,"GPF634990P014G000","8056603455817"]
["BATHROOM","HABITO","HABITO UNITO","54055+70099",70099,"afbouwdeel voor wandgemonteerde 1-weg mengkraan","Partie apparente pour mitigeur mural, 1 sortie.","External part for wall-mounted one-way mixer.",710,"Brass PVD",368,"GPF700990P011G000","8056603666985"]
["BATHROOM","HABITO","HABITO UNITO","46189+70095",70095,"afbouwdeel voor vrijstaande wastafelkraan zonder plug.","Partie apparente mitigeur de lavabo au sol sans vidage.","External part for freestanding basin mixer without waste.",299,"Matte Black",2151,"GPF700950C072G000","8056603667197"]
["BATHROOM","HABITO","HABITO UNITO","46189+70028",70028,"afbouwdeel Vrijstaande badkraan met automatische omstel","Partie apparente pour mitigeur bain-douche sur pied avec douchette et flexible et inveseur automatique.","External parts freestanding bath mixer with automatic diverter.",726,"Warm Bronze Brushed PVD",3338,"GPF700280P024G000","8056603677158"]
["BATHROOM","HABITO","HABITO UNITO",70033,70033,"Externe Thermostatische douche mengkraan.","Mitigeur thermostatique de baignoire avec prise d’eau et inverseur automatique.","External Thermostatic shower mixer.",727,"Brass Brushed PVD",1981,"GPF700330P025G000","8056603976930"]
["BATHROOM","HABITO","HABITO UNITO","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",299,"Matte Black",356,"GPF540580C072G000","8056329536968"]
["BATHROOM","HABITO","HABITO UNITO","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",710,"Brass PVD",388,"GPF540580P011G000","8056603627948"]
["BATHROOM","HABITO","HABITO UNITO","54169+70032",70032,"afbouwdeel voor thermostatische mengkraan, 1-weg","Partie apparente pour mitigeur thermostatique douche mural 1 sortie.","External parts for thermostatic mixer, one-way diverter.",149,"Finox Brushed Nickel",1038,"GPF700320G002G000","8056603685221"]
["BATHROOM","HABITO","HABITO UNITO","54169+70036",70036,"afbouwdeel wandgemonteerde thermostatische 3-weg douchemengkraan","Partie apparente pour mitigeur thermostatique douche mural 3 sorties.","External part wall-mounted thermostatic three-ways shower mixer.",761,"Coffee Bronze Brushed PVD",1292,"GPF700360E059G000","8055261585386"]
["BATHROOM","HABITO","HABITO UNITO","09269+70031",70031,"Afbouwdeel wand gemonteerd 2-weg douche mengkraan. UNITO.","Partie apparente mitigeur thermostatique 2 voies.","External part wall-mounted two ways shower mixer. UNITO.",708,"Copper Brushed PVD",1392,"GPF700310P006G000","8055261196735"]
["BATHROOM","HABITO","HABITO UNITO","09269+70039",70039,"Afbouwdeel wand gemonteerd 3-weg douche mengkraan. UNITO.","Partie apparente mitigeur thermostatique 3 voies.","External part wall-mounted three ways shower mixer. UNITO.",727,"Brass Brushed PVD",1392,"GPF700390P025G000","8055261192577"]
["BATHROOM","HABITO","HABITO UNITO",70042,70042,"Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose.",761,"Coffee Bronze Brushed PVD",1373,"GPF700420E059G000","8055261585324"]
["BATHROOM","HABITO","HABITO UNITO",70045,70045,"Glijrail met antikalk handdouche, 1,50 m flexibele slang.","Barre de douche complète avec douchette anticalcaire et flexibles 1,50 m.","Sliding rail with antilimestone handshower, 1,50 m flexible hose.",845,"Dark Bronze",1098,"GPF700450V221G000","8056603684958"]
["BATHROOM","HABITO","HABITO TRAME",70301,70301,"Wastafel mengkraan, Flexibele slangen, met vaste plug TRAME","Mitigeur lavabo avec vidage et flexibles de raccordement. TRAME","Basin mixer with waste and connecting flexibles. TRAME",706,"Black Metal PVD",797,"GPF703010P001G000","8056603664639"]
["BATHROOM","HABITO","HABITO TRAME",70306,70306,"Medium versie Wastafel mengkraan, Flexibele slangen, zonder plug TRAME","Mitigeur lavabo moyen sans vidage avec flexibles de raccordement. TRAME","Medium version basin mixer without waste and connecting flexibles. TRAME",727,"Brass Brushed PVD",921,"GPF703060P025G000","8056603663878"]
["BATHROOM","HABITO","HABITO TRAME",70304,70304,"Hoge versie Wastafel mengkraan, Flexibele slangen, zonder plug TRAME","Mitigeur lavabo réhaussé sans vidage avec flexibles de raccordement. TRAME","High version basin mixer without waste and connecting flexibles. TRAME",710,"Brass PVD",936,"GPF703040P011G000","8056603664189"]
["BATHROOM","HABITO","HABITO TRAME",66102,66102,"wand-gemonteerde uitloop wastafel, medium uitloop","Bec de lavabo mural moyen","Wall-mounted medium spout basin",273,"Matte Greige",278,"GPF661020T208G000","8056603568524"]
["BATHROOM","HABITO","HABITO TRAME",66104,66104,"wandgemonteerde wastafel uitloop. lengte op verzoek","Bec de lavabo mural. Bec avec longueur à la demande.","Wall-mounted basin spout, custom length",275,"Matte Cipria",555,"GPF661040T209G000","8056603588263"]
["BATHROOM","HABITO","HABITO TRAME",63399,63399,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond à compléter par un mitigeur à commande séparée","Ceiling-mounted spout. To be completed with separate control.","030","Copper PVD",1380,"GPF633990P000G000","8056329551527"]
["BATHROOM","HABITO","HABITO TRAME",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.",716,"Gold Brushed PVD",2193,"GPF634990P005G000","8055261230033"]
["BATHROOM","HABITO","HABITO TRAME","46189+70395",70395,"afbouwdeel voor vrijstaande wastafelkraan zonder plug. TRAME","Partie apparente mitigeur de lavabo au sol sans vidage. TRAME","External part for freestanding basin mixer without waste. TRAME",727,"Brass Brushed PVD",2571,"GPF703950P025G000","8056603662611"]
["BATHROOM","HABITO","HABITO TRAME",70307,70307,"Bidet kraan met plug en flexibele slangen TRAME","Mitigeur bidet avec vidage et flexibles de raccordement. TRAME","Bidet mixer with waste and connecting flexibles. TRAME",727,"Brass Brushed PVD",851,"GPF703070P025G000","8056603663731"]
["BATHROOM","HABITO","HABITO TRAME",70333,70333,"Externe Thermostatische douche mengkraan.","Partie apparente pour mitigeur douche.","External Thermostatic shower mixer.",708,"Copper Brushed PVD",2151,"GPF703330P006G000","8056603975025"]
["BATHROOM","HABITO","HABITO TRAME","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",708,"Copper Brushed PVD",388,"GPF540580P006G000","8056329025714"]
["BATHROOM","HABITO","HABITO TRAME","54073+70379",70379,"afbouwdeel wandgemonteerde tweeweg douchemengkraan met omstelling. TRAME","Partie apparente mitigeur de baignoire mural 2 sorties avec inverseur. TRAME","External part wall-mounted two-ways shower mixer with diverter. TRAME",710,"Brass PVD",943,"GPF703790P011G000","8056603662925"]
["BATHROOM","HABITO","HABITO TRAME","54169+70332",70332,"afbouwdeel voor thermostatische mengkraan, 1-weg TRAME","Partie apparente pour mitigeur thermostatique douche mural 1 sortie. TRAME","External parts for thermostatic mixer, one-way diverter. TRAME",735,"Warm Bronze PVD",1189,"GPF703320P037G000","8056603684521"]
["BATHROOM","HABITO","HABITO TRAME","54169+70336",70336,"afbouwdeel wandgemonteerde thermostatische 3-weg douchemengkraan TRAME","Partie apparente pour mitigeur thermostatique douche mural 3 sorties. TRAME","External part wall-mounted thermostatic three-ways shower mixer. TRAME",761,"Coffee Bronze Brushed PVD",1349,"GPF703360E059G000","8055261584396"]
["BATHROOM","HABITO","HABITO TRAME","09269+70339",70339,"Afbouwdeel wand gemonteerd 3-weg douche mengkraan. TRAME.","Partie apparente mitigeur thermostatique 3 voies.","External part wall-mounted three ways shower mixer. TRAME.",761,"Coffee Bronze Brushed PVD",1479,"GPF703390E059G000","8055261584358"]
["BATHROOM","HABITO","HABITO TRAME",70345,70345,"Glijrail met antikalk handdouche, 1,50 m flexibele slang. TRAME","Barre de douche complète avec douchette anticalcaire et flexibles 1,50 m. TRAME","Sliding rail with antilimestone handshower, 1,50 m flexible hose. TRAME",727,"Brass Brushed PVD",1168,"GPF703450P025G000","8056603684385"]
["BATHROOM","HABITO","HABITO INTRECCIO",70101,70101,"Wastafel mengkraan, Flexibele slangen, met vaste plug INTRECCIO","Mitigeur lavabo avec vidage et flexibles de raccordement. INTRECCIO","Basin mixer with waste and connecting flexibles. INTRECCIO",726,"Warm Bronze Brushed PVD",851,"GPF701010P024G000","8056603666824"]
["BATHROOM","HABITO","HABITO INTRECCIO",70102,70102,"Wastafel mengkraan, Flexibele slangen, zonder plug INTRECCIO","Mitigeur lavabo sans vidage avec flexibles de raccordement. INTRECCIO","Basin mixer without waste and connecting flexibles. INTRECCIO",845,"Dark Bronze",779,"GPF701020V221G000","8056603666640"]
["BATHROOM","HABITO","HABITO INTRECCIO",70106,70106,"Medium versie Wastafel mengkraan, Flexibele slangen, zonder plug INTRECCIO","Mitigeur lavabo moyen sans vidage avec flexibles de raccordement. INTRECCIO","Medium version basin mixer without waste and connecting flexibles. INTRECCIO",735,"Warm Bronze PVD",861,"GPF701060P037G000","8056603666107"]
["BATHROOM","HABITO","HABITO INTRECCIO",70103,70103,"Hoge versie Wastafel mengkraan, Flexibele slangen, met vaste plug INTRECCIO","Mitigeur lavabo réhaussé avec vidage et flexibles de raccordement. INTRECCIO","High version basin mixer with waste and connecting flexibles. INTRECCIO",761,"Coffee Bronze Brushed PVD",1138,"GPF701030E059G000","8055261585140"]
["BATHROOM","HABITO","HABITO INTRECCIO",66102,66102,"wand-gemonteerde uitloop wastafel, medium uitloop","Bec de lavabo mural moyen","Wall-mounted medium spout basin",706,"Black Metal PVD",305,"GPF661020P001G000","8056603566650"]
["BATHROOM","HABITO","HABITO INTRECCIO",66104,66104,"wandgemonteerde wastafel uitloop. lengte op verzoek","Bec de lavabo mural. Bec avec longueur à la demande.","Wall-mounted basin spout, custom length",726,"Warm Bronze Brushed PVD",649,"GPF661040P024G000","8056603588294"]
["BATHROOM","HABITO","HABITO INTRECCIO",63399,63399,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond à compléter par un mitigeur à commande séparée","Ceiling-mounted spout. To be completed with separate control.",246,"Gold PVD",1566,"GPF633990P007G000","8055261233799"]
["BATHROOM","HABITO","HABITO INTRECCIO","54055+70199",70199,"afbouwdeel voor wandgemonteerde 1-weg mengkraan INTRECCIO","Partie apparente pour mitigeur mural, 1 sortie. INTRECCIO","External part for wall-mounted one-way mixer. INTRECCIO",149,"Finox Brushed Nickel",380,"GPF701990G002G000","8056603683074"]
["BATHROOM","HABITO","HABITO INTRECCIO","54055+70199",70199,"afbouwdeel voor wandgemonteerde 1-weg mengkraan INTRECCIO","Partie apparente pour mitigeur mural, 1 sortie. INTRECCIO","External part for wall-mounted one-way mixer. INTRECCIO",726,"Warm Bronze Brushed PVD",446,"GPF701990P024G000","8056603664721"]
["BATHROOM","HABITO","HABITO INTRECCIO",70107,70107,"Bidet kraan met plug en flexibele slangen INTRECCIO","Mitigeur bidet avec vidage et flexibles de raccordement. INTRECCIO","Bidet mixer with waste and connecting flexibles. INTRECCIO",761,"Coffee Bronze Brushed PVD",903,"GPF701070E059G000","8055261585065"]
["BATHROOM","HABITO","HABITO INTRECCIO",70133,70133,"Externe Thermostatische douche mengkraan.","Partie apparente pour mitigeur douche.","External Thermostatic shower mixer.",707,"Black Metal Brushed PVD",2151,"GPF701330P004G000","8056603975476"]
["BATHROOM","HABITO","HABITO INTRECCIO",70133,70133,"Externe Thermostatische douche mengkraan.","Partie apparente pour mitigeur douche.","External Thermostatic shower mixer.",727,"Brass Brushed PVD",2151,"GPF701330P025G000","8056603975438"]
["BATHROOM","HABITO","HABITO INTRECCIO","54073+70179",70179,"afbouwdeel wandgemonteerde tweeweg douchemengkraan met omstelling. INTRECCIO","Partie apparente mitigeur de baignoire mural 2 sorties avec inverseur. INTRECCIO","External part wall-mounted two-ways shower mixer with diverter. INTRECCIO","031","Chrome",638,"GPF701790G001G000","8056603665223"]
["BATHROOM","HABITO","HABITO INTRECCIO","54169+70132",54169,"Inbouwdeel Thermostatische Mengkraan Wanddouche","Partie encastrée pour mitigeur thermostatique douche mural","Built-in part for wall-mounted thermostatic shower mixer.",239,"Steel Brushed",438,"GPF541690A000G000","8022692841398"]
["BATHROOM","HABITO","HABITO INTRECCIO","54169+70134",70134,"afbouwdeel wandgemonteerde thermostatische 2-weg douchemengkraan INTRECCIO","Partie apparente pour mitigeur thermostatique douche mural 2 sorties. INTRECCIO","External part wall-mounted thermostatic two-ways shower mixer. INTRECCIO",727,"Brass Brushed PVD",1268,"GPF701340P025G000","8056603665698"]
["BATHROOM","HABITO","HABITO INTRECCIO","54169+70136",70136,"afbouwdeel wandgemonteerde thermostatische 3-weg douchemengkraan INTRECCIO","Partie apparente pour mitigeur thermostatique douche mural 3 sorties. INTRECCIO","External part wall-mounted thermostatic three-ways shower mixer. INTRECCIO",845,"Dark Bronze",1268,"GPF701360V221G000","8056603665520"]
["BATHROOM","HABITO","HABITO INTRECCIO","09269+70131",70131,"Afbouwdeel wand gemonteerd 2-weg douche mengkraan. INTRECCIO.","Partie apparente mitigeur thermostatique 2 voies.","External part wall-mounted two ways shower mixer. INTRECCIO.",708,"Copper Brushed PVD",1392,"GPF701310P006G000","8055261196513"]
["BATHROOM","HABITO","HABITO INTRECCIO",70145,70145,"Glijrail met antikalk handdouche, 1,50 m flexibele slang. INTRECCIO","Barre de douche complète avec douchette anticalcaire et flexibles 1,50 m. INTRECCIO","Sliding rail with antilimestone handshower, 1,50 m flexible hose. INTRECCIO",707,"Black Metal Brushed PVD",1168,"GPF701450P004G000","8056603684736"]
["BATHROOM","HABITO","HABITO INTRECCIO",70144,70144,"Sliding rail. INTRECCIO","Barre de douche. INTRECCIO","Sliding rail. INTRECCIO",845,"Dark Bronze",953,"GPF701440V221G000","8056603665247"]
["BATHROOM","HABITO","HABITO RIGATO",70502,70502,"Wastafel mengkraan, Flexibele slangen, zonder plug RIGATO","Mitigeur lavabo sans vidage avec flexibles de raccordement. RIGATO","Basin mixer without waste and connecting flexibles. RIGATO",706,"Black Metal PVD",730,"GPF705020P001G000","8056603660013"]
["BATHROOM","HABITO","HABITO RIGATO",70505,70505,"Medium versie Wastafel mengkraan, Flexibele slangen, met vaste plug RIGATO","Mitigeur lavabo moyen avec vidage et flexibles de raccordement. RIGATO","Medium version basin mixer with waste and connecting flexibles. RIGATO",726,"Warm Bronze Brushed PVD",991,"GPF705050P024G000","8056603659543"]
["BATHROOM","HABITO","HABITO RIGATO",70503,70503,"Hoge versie Wastafel mengkraan, Flexibele slangen, met vaste plug RIGATO","Mitigeur lavabo réhaussé avec vidage et flexibles de raccordement. RIGATO","High version basin mixer with waste and connecting flexibles. RIGATO",299,"Matte Black",914,"GPF705030C072G000","8056603659918"]
["BATHROOM","HABITO","HABITO RIGATO",66102,66102,"wand-gemonteerde uitloop wastafel, medium uitloop","Bec de lavabo mural moyen","Wall-mounted medium spout basin",276,"Matte Agave",278,"GPF661020T210G000","8056603568500"]
["BATHROOM","HABITO","HABITO RIGATO",66104,66104,"wandgemonteerde wastafel uitloop. lengte op verzoek","Bec de lavabo mural. Bec avec longueur à la demande.","Wall-mounted basin spout, custom length",276,"Matte Agave",555,"GPF661040T210G000","8056603588256"]
["BATHROOM","HABITO","HABITO RIGATO",63399,63399,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond à compléter par un mitigeur à commande séparée","Ceiling-mounted spout. To be completed with separate control.",278,"Glossy Coral",1474,"GPF633990T212G000","8056603609463"]
["BATHROOM","HABITO","HABITO RIGATO",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.",277,"Glossy Ocra",2061,"GPF634990T211G000","8056603609418"]
["BATHROOM","HABITO","HABITO RIGATO",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.",727,"Brass Brushed PVD",2061,"GPF634990P025G000","8056329591257"]
["BATHROOM","HABITO","HABITO RIGATO","46189+70595",70595,"afbouwdeel voor vrijstaande wastafelkraan zonder plug. RIGATO","Partie apparente mitigeur de lavabo au sol sans vidage. RIGATO","External part for freestanding basin mixer without waste. RIGATO",706,"Black Metal PVD",2408,"GPF705950P001G000","8056603658195"]
["BATHROOM","HABITO","HABITO RIGATO","46189+70528",70528,"afbouwdeel Vrijstaande badkraan met automatische omstel RIGATO","Partie apparente pour mitigeur bain-douche sur pied avec douchette et flexible et inveseur automatique. RIGATO","External parts freestanding bath mixer with automatic diverter. RIGATO",735,"Warm Bronze PVD",3197,"GPF705280P037G000","8056603676571"]
["BATHROOM","HABITO","HABITO RIGATO",70533,70533,"Externe Thermostatische douche mengkraan. RIGATO.","Partie apparente pour mitigeur douche. RIGATO.","External Thermostatic shower mixer. RIGATO.",149,"Finox Brushed Nickel",1840,"GPF705330G002G000","8056603974172"]
["BATHROOM","HABITO","HABITO RIGATO","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",720,"Nickel PVD",388,"GPF540580P014G000","8056603627931"]
["BATHROOM","HABITO","HABITO RIGATO","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",710,"Brass PVD",388,"GPF540580P011G000","8056603627948"]
["BATHROOM","HABITO","HABITO RIGATO","54169+70532",70532,"afbouwdeel voor thermostatische mengkraan, 1-weg RIGATO","Partie apparente pour mitigeur thermostatique douche mural 1 sortie. RIGATO","External parts for thermostatic mixer, one-way diverter. RIGATO",710,"Brass PVD",1189,"GPF705320P011G000","8056603683968"]
["BATHROOM","HABITO","HABITO RIGATO","54169+70536",70536,"afbouwdeel wandgemonteerde thermostatische 3-weg douchemengkraan RIGATO","Partie apparente pour mitigeur thermostatique douche mural 3 sorties. RIGATO","External part wall-mounted thermostatic three-ways shower mixer. RIGATO",707,"Black Metal Brushed PVD",1268,"GPF705360P004G000","8056603658881"]
["BATHROOM","HABITO","HABITO RIGATO","09269+73533",73533,"afbouwdeel voor 1-uitgang thermostatische mengkraan.","Partie apparente pour mitigeur thermostatique mural 1 sortie.","External part for 1-outlet thermostatic mixer.",710,"Brass PVD",1304,"GPF735330P011G000","8055261232181"]
["BATHROOM","HABITO","HABITO RIGATO","09269+73537",73537,"afbouwdeel voor 3-uitgang thermostatische mengkraan.","Partie apparente pour mitigeur thermostatique mural 3 sortie.","External part for 3-outlet thermostatic mixer.",710,"Brass PVD",1304,"GPF735370P011G000","8055261231900"]
["BATHROOM","HABITO","HABITO RIGATO",63584,63584,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m. RIGATO.","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m. RIGATO.","Sliding rail with antilimestone handshower, 1,50 m flexible hose. RIGATO.","031","Chrome",738,"GPF635840G001G000","8056329569799"]
["BATHROOM","HABITO","HABITO RIGATO",63584,63584,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m. RIGATO.","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m. RIGATO.","Sliding rail with antilimestone handshower, 1,50 m flexible hose. RIGATO.",761,"Coffee Bronze Brushed PVD",1241,"GPF635840E059G000","8055261591721"]
["BATHROOM","HABITO","HABITO RIGATO",63585,63585,"Glijstang. RIGATO.","Barre de douche. RIGATO.","Sliding rail. RIGATO.",761,"Coffee Bronze Brushed PVD",1013,"GPF635850E059G000","8055261591707"]
["BATHROOM","HABITO","HABITO DIAMANTATO",70602,70602,"Wastafel mengkraan, Flexibele slangen, zonder plug DIAMANTATO","Mitigeur lavabo sans vidage avec flexibles de raccordement. DIAMANTATO","Basin mixer without waste and connecting flexibles. DIAMANTATO",710,"Brass PVD",730,"GPF706020P011G000","8056603657747"]
["BATHROOM","HABITO","HABITO DIAMANTATO",70605,70605,"Medium versie Wastafel mengkraan, Flexibele slangen, met vaste plug DIAMANTATO","Mitigeur lavabo moyen avec vidage et flexibles de raccordement. DIAMANTATO","Medium version basin mixer with waste and connecting flexibles. DIAMANTATO",845,"Dark Bronze",991,"GPF706050V221G000","8056603657266"]
["BATHROOM","HABITO","HABITO DIAMANTATO",70604,70604,"Hoge versie Wastafel mengkraan, Flexibele slangen, zonder plug DIAMANTATO","Mitigeur lavabo réhaussé sans vidage avec flexibles de raccordement. DIAMANTATO","High version basin mixer without waste and connecting flexibles. DIAMANTATO",845,"Dark Bronze",998,"GPF706040V221G000","8056603657402"]
["BATHROOM","HABITO","HABITO DIAMANTATO",66102,66102,"wand-gemonteerde uitloop wastafel, medium uitloop","Bec de lavabo mural moyen","Wall-mounted medium spout basin",707,"Black Metal Brushed PVD",325,"GPF661020P004G000","8056603566643"]
["BATHROOM","HABITO","HABITO DIAMANTATO",66104,66104,"wandgemonteerde wastafel uitloop. lengte op verzoek","Bec de lavabo mural. Bec avec longueur à la demande.","Wall-mounted basin spout, custom length",278,"Glossy Coral",649,"GPF661040T212G000","8056603588232"]
["BATHROOM","HABITO","HABITO DIAMANTATO",63399,63399,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond à compléter par un mitigeur à commande séparée","Ceiling-mounted spout. To be completed with separate control.",710,"Brass PVD",1380,"GPF633990P011G000","8056329591585"]
["BATHROOM","HABITO","HABITO DIAMANTATO",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.",845,"Dark Bronze",2061,"GPF634990V221G000","8056603609395"]
["BATHROOM","HABITO","HABITO DIAMANTATO","46189+70695",46189,"Inbouwdeel voor standaard bad","Partie encastrée tenue étanche pour mitigeur bain-douche sur pied.","Built-in part for freestanding basin/bath mixer with spout.","031","Chrome",457,"GPF461892G001G000","8022692601503"]
["BATHROOM","HABITO","HABITO DIAMANTATO","46189+70695",70695,"afbouwdeel voor vrijstaande wastafelkraan zonder plug. DIAMANTATO","Partie apparente mitigeur de lavabo au sol sans vidage. DIAMANTATO","External part for freestanding basin mixer without waste. DIAMANTATO",710,"Brass PVD",2408,"GPF706950P011G000","8056603655927"]
["BATHROOM","HABITO","HABITO DIAMANTATO","46189+70628",70628,"afbouwdeel Vrijstaande badkraan met automatische omstel DIAMANTATO","Partie apparente pour mitigeur bain-douche sur pied avec douchette et flexible et inveseur automatique. DIAMANTATO","External parts freestanding bath mixer with automatic diverter. DIAMANTATO",727,"Brass Brushed PVD",3414,"GPF706280P025G000","8056603676441"]
["BATHROOM","HABITO","HABITO DIAMANTATO","54139+70638",70638,"afbouwdeel wandgemonteerde 2-weg douchemengkraan met omstelling, waterafvoer, handdouchehaak en handdouche. DIAMANTATO","Partie apparente mitigeur de baignoire mural 2 sorties, avec inverseur, prise d'eau, support pour douchette et douchette. DIAMANTATO","External parts wall-mounted two-way shower mixer with diverter, water outlet, hand shower hook and hand shower. DIAMANTATO",708,"Copper Brushed PVD",1386,"GPF706380P006G000","8056603669276"]
["BATHROOM","HABITO","HABITO DIAMANTATO","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",713,"Antique Brass",388,"GPF540580V204G000","8056603509398"]
["BATHROOM","HABITO","HABITO DIAMANTATO","54073+70679",70679,"afbouwdeel wandgemonteerde tweeweg douchemengkraan met omstelling. DIAMANTATO","Partie apparente mitigeur de baignoire mural 2 sorties avec inverseur. DIAMANTATO","External part wall-mounted two-ways shower mixer with diverter. DIAMANTATO",735,"Warm Bronze PVD",943,"GPF706790P037G000","8056603656160"]
["BATHROOM","HABITO","HABITO DIAMANTATO","54169+70634",70634,"afbouwdeel wandgemonteerde thermostatische 2-weg douchemengkraan DIAMANTATO","Partie apparente pour mitigeur thermostatique douche mural 2 sorties. DIAMANTATO","External part wall-mounted thermostatic two-ways shower mixer. DIAMANTATO",708,"Copper Brushed PVD",1268,"GPF706340P006G000","8056603656771"]
["BATHROOM","HABITO","HABITO DIAMANTATO","54169+70636",70636,"afbouwdeel wandgemonteerde thermostatische 3-weg douchemengkraan DIAMANTATO","Partie apparente pour mitigeur thermostatique douche mural 3 sorties. DIAMANTATO","External part wall-mounted thermostatic three-ways shower mixer. DIAMANTATO",726,"Warm Bronze Brushed PVD",1268,"GPF706360P024G000","8056603656603"]
["BATHROOM","HABITO","HABITO DIAMANTATO","09269+73635",73635,"afbouwdeel voor 2-uitgang thermostatische mengkraan.","Partie apparente pour mitigeur thermostatique mural 2 sortie.","External part for 2-outlet thermostatic mixer.",187,"Aged Bronze",1392,"GPF736350G052G000","8055261231672"]
["BATHROOM","HABITO","HABITO DIAMANTATO",63482,63482,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m. DIAMANTATO.","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée. DIAMANTATO.","Sliding rail with antilimestone handshower, 1,50 m flexible hose and water outlet. DIAMANTATO.","031","Chrome",869,"GPF634820G001G000","8056329565258"]
["BATHROOM","HABITO","HABITO DIAMANTATO",63484,63484,"Glijstang met antikalk-handdouche en buigzame slang 1,50 m. DIAMANTATO.","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m. DIAMANTATO.","Sliding rail with antilimestone handshower, 1,50 m flexible hose. DIAMANTATO.","031","Chrome",738,"GPF634840G001G000","8056329565135"]
["BATHROOM","HABITO","HABITO DIAMANTATO",63485,63485,"Glijstang. DIAMANTATO.","Barre de douche. DIAMANTATO.","Sliding rail. DIAMANTATO.",720,"Nickel PVD",891,"GPF634850P014G000","8056603604970"]
["BATHROOM","HABITO","HABITO CESELLO",70401,70401,"Wastafel mengkraan, Flexibele slangen, met vaste plug CESELLO","Mitigeur lavabo avec vidage et flexibles de raccordement. CESELLO","Basin mixer with waste and connecting flexibles. CESELLO",299,"Matte Black",727,"GPF704010C072G000","8056603662437"]
["BATHROOM","HABITO","HABITO CESELLO",70402,70402,"Wastafel mengkraan, Flexibele slangen, zonder plug CESELLO","Mitigeur lavabo sans vidage avec flexibles de raccordement. CESELLO","Basin mixer without waste and connecting flexibles. CESELLO",727,"Brass Brushed PVD",779,"GPF704020P025G000","8056603662192"]
["BATHROOM","HABITO","HABITO CESELLO",70403,70403,"Hoge versie Wastafel mengkraan, Flexibele slangen, met vaste plug CESELLO","Mitigeur lavabo réhaussé avec vidage et flexibles de raccordement. CESELLO","High version basin mixer with waste and connecting flexibles. CESELLO",845,"Dark Bronze",1070,"GPF704030V221G000","8056603662024"]
["BATHROOM","HABITO","HABITO CESELLO","54198+70488",70488,"afbouwdeel voor wandgemonteerde wastafel kraan CESELLO","Partie apparente mitigeur lavabo mural. CESELLO","External part for wall-mounted basin mixer. CESELLO",726,"Warm Bronze Brushed PVD",768,"GPF704880P024G000","8056603660525"]
["BATHROOM","HABITO","HABITO CESELLO",66102,66102,"wand-gemonteerde uitloop wastafel, medium uitloop","Bec de lavabo mural moyen","Wall-mounted medium spout basin",278,"Glossy Coral",325,"GPF661020T212G000","8056603568487"]
["BATHROOM","HABITO","HABITO CESELLO",63399,63399,"Plafond Gemonteerde Uitloop. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond à compléter par un mitigeur à commande séparée","Ceiling-mounted spout. To be completed with separate control.","031","Chrome",932,"GPF633990G001G000","8056329551558"]
["BATHROOM","HABITO","HABITO CESELLO",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.",276,"Matte Agave",1762,"GPF634990T210G000","8056603609425"]
["BATHROOM","HABITO","HABITO CESELLO","54055+70499",70499,"afbouwdeel voor wandgemonteerde 1-weg mengkraan CESELLO","Partie apparente pour mitigeur mural, 1 sortie. CESELLO","External part for wall-mounted one-way mixer. CESELLO","031","Chrome",281,"GPF704990G001G000","8056603660327"]
["BATHROOM","HABITO","HABITO CESELLO","54055+70499",70499,"afbouwdeel voor wandgemonteerde 1-weg mengkraan CESELLO","Partie apparente pour mitigeur mural, 1 sortie. CESELLO","External part for wall-mounted one-way mixer. CESELLO",735,"Warm Bronze PVD",418,"GPF704990P037G000","8056603660228"]
["BATHROOM","HABITO","HABITO CESELLO",70407,70407,"Bidet kraan met plug en flexibele slangen CESELLO","Mitigeur bidet avec vidage et flexibles de raccordement. CESELLO","Bidet mixer with waste and connecting flexibles. CESELLO",735,"Warm Bronze PVD",797,"GPF704070P037G000","8056603661485"]
["BATHROOM","HABITO","HABITO CESELLO",70433,70433,"Externe Thermostatische douche mengkraan.","Partie apparente pour mitigeur douche.","External Thermostatic shower mixer.",706,"Black Metal PVD",2016,"GPF704330P001G000","8056603974608"]
["BATHROOM","HABITO","HABITO CESELLO","54057+54058",54057,"Inbouwdeel voor terugstroombeveiligingssysteem UNI EN 1717","Système anti-reflux UNI EN 1717,","Built-in part non-return system (optional), UNI EN 1717",239,"Steel Brushed",288,"GPF540570A000G000","8056329025745"]
["BATHROOM","HABITO","HABITO CESELLO","54073+70479",54073,"Inbouwdeel Voor Wandgemonteerde Douche Mengkraan, 2-Weg","Partie encastrée pour mitigeur douche mura deux sorties","Built-in part for wall-mounted shower mixer, two-ways.",239,"Steel Brushed",516,"GPF540731A000G000","8022692849813"]
["BATHROOM","HABITO","HABITO CESELLO","54073+70479",70479,"afbouwdeel wandgemonteerde tweeweg douchemengkraan met omstelling. CESELLO","Partie apparente mitigeur de baignoire mural 2 sorties avec inverseur. CESELLO","External part wall-mounted two-ways shower mixer with diverter. CESELLO",761,"Coffee Bronze Brushed PVD",1070,"GPF704790E059G000","8055261583771"]
["BATHROOM","HABITO","HABITO CESELLO","54169+70434",70434,"afbouwdeel wandgemonteerde thermostatische 2-weg douchemengkraan CESELLO","Partie apparente pour mitigeur thermostatique douche mural 2 sorties. CESELLO","External part wall-mounted thermostatic two-ways shower mixer. CESELLO",707,"Black Metal Brushed PVD",1268,"GPF704340P004G000","8056603661263"]
["BATHROOM","HABITO","HABITO CESELLO","54169+70436",70436,"afbouwdeel wandgemonteerde thermostatische 3-weg douchemengkraan CESELLO","Partie apparente pour mitigeur thermostatique douche mural 3 sorties. CESELLO","External part wall-mounted thermostatic three-ways shower mixer. CESELLO",727,"Brass Brushed PVD",1268,"GPF704360P025G000","8056603661072"]
["BATHROOM","HABITO","HABITO CESELLO","09269+70439",70439,"Afbouwdeel wand gemonteerd 3-weg douche mengkraan. CESELLO.","Partie apparente mitigeur thermostatique 3 voies.","External part wall-mounted three ways shower mixer. CESELLO.",710,"Brass PVD",1304,"GPF704390P011G000","8055261192263"]
["BATHROOM","HABITO","HABITO CESELLO",70442,70442,"Glijstang met waterafvoer, antikalk handdouche en 1,50 m flexibele slang CESELLO","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée. CESELLO","Sliding rail with water outlet, antilimestone handshower and 1,50 m flexible hose. CESELLO",761,"Coffee Bronze Brushed PVD",1460,"GPF704420E059G000","8055261583832"]
["BATHROOM","HABITO","HABITO CESELLO",70444,70444,"Sliding rail. CESELLO","Barre de douche. CESELLO","Sliding rail. CESELLO",727,"Brass Brushed PVD",953,"GPF704440P025G000","8056603660792"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",66103,66103,"wandfixing baduitloop","Bec de bagnoire mural","Wall-fixing bath spout",761,"Coffee Bronze Brushed PVD",449,"GPF661030E059G000","8055261588448"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","09266+63436",63436,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie externe mitigeur thermostatique mural à 3 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with three separate exits.",707,"Black Metal Brushed PVD",2069,"GPF634360P004G000","8056603618892"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","09263+63440",63440,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie externe mitigeur thermostatique mural à 5 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with five separate exits.",720,"Nickel PVD",2412,"GPF634400P014G000","8056603630344"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","43103+43064",43064,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",735,"Warm Bronze PVD",2172,"GPF430642P037G000","8056329555976"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","43103+43234",43234,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",299,"Matte Black",1889,"GPF432341C072G000","8022692584936"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","43103+43234",43234,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",761,"Coffee Bronze Brushed PVD",2607,"GPF432341E059G000","8055261603189"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","43105+43236",43236,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",706,"Black Metal PVD",2501,"GPF432361P001G000","8056329131385"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","43107+43068",43068,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",279,"Matte White",2486,"GPF430682C071G000","8022692655100"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","43107+43238",43238,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",720,"Nickel PVD",2858,"GPF432381P014G000","8056603456944"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","43109+43070",43070,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",187,"Aged Bronze",3472,"GPF430702G052G000","8056329562141"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","43109+43240",43240,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS",735,"Warm Bronze PVD",3153,"GPF432401P037G000","8056329556249"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","43281+43256",43256,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente mitigeur THERMOSTATIQUE douche haut débit","External parts wall-mounted thermostatic high-capacity mixer",147,"Chome Brushed",880,"GPF432561G006G000","8022692828412"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","43283+43268",43268,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur haut débit.","External parts for stop valve for thermostatic high-capacity mixer.",708,"Copper Brushed PVD",708,"GPF432680P006G000","8056329131163"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",66150,66150,"wandgemonteerde antikalk en verstelbare hoofddouche","Pomme de douche murale orientable.","Wall-mounted anti limestone and adjustable head shower",720,"Nickel PVD",2181,"GPF661500P014G000","8056603578646"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63352,63352,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable shower head","031","Chrome",507,"GPF633520G001G000","8056329552364"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63350,63350,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted showerhead, length on request",761,"Coffee Bronze Brushed PVD",1195,"GPF633500E059G000","8055261592995"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO","031","Chrome",1584,"GPF637450G001G000","8055261728677"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63645,63645,"Verstelbare hoofddouche voor wandmontage. DIAMANTATO","Pomme de douche murale orientable. DIAMANTATO","Wall-mounted adjustable headshower. DIAMANTATO","030","Copper PVD",2345,"GPF636450P000G000","8055261729155"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",761,"Coffee Bronze Brushed PVD",1834,"GPF630500E059G000","8055261729537"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63750,63750,"Verstelbare hoofddouche voor montage aan het plafond. RIGATO","Pomme de douche au plafond orientable. RIGATO","Ceiling-mounted adjustable headshower. RIGATO",726,"Warm Bronze Brushed PVD",2497,"GPF637500P024G000","8055261728417"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.","030","Copper PVD",2101,"GPF630530P000G000","8055261729322"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63653,63653,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. DIAMANTATO","Pomme de douche au plafond orientable, longueur à la demande. DIAMANTATO","Ceiling-mounted adjustable headshower, length on request. DIAMANTATO",726,"Warm Bronze Brushed PVD",3245,"GPF636530P024G000","8055261728752"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",66049,66049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",187,"Aged Bronze",2352,"GPF660490G052G000","8055261541337"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63549,63549,"Verstelbare hoofddouche aan de muur. RIGATO.","Pomme de douche latérale orientable. RIGATO.","Wall-mounted adjustable headshower. RIGATO.",735,"Warm Bronze PVD",2978,"GPF635490P037G000","8055261241589"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",66068,66068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",720,"Nickel PVD",2383]
["BATHROOM","HABITO","HABITO BATH-SHOWER",66068,66068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",187,"Aged Bronze",2543]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63568,63568,"Verstelbare hoofddouche aan de muur. RIGATO.","Pomme de douche latérale orientable. RIGATO.","Wall-mounted adjustable headshower. RIGATO.",735,"Warm Bronze PVD",3158,"GPF635680P037G000","8055261241435"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63468,63468,"Verstelbare hoofddouche aan de muur. DIAMANTATO.","Pomme de douche latérale orientable. DIAMANTATO.","Wall-mounted adjustable headshower. DIAMANTATO.",706,"Black Metal PVD",3158,"GPF634680P001G000","8055261242104"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",66072,66072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",727,"Brass Brushed PVD",2352]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63472,63472,"Verstelbare plafonddouche. DIAMANTATO.","Pomme de douche au plafond orientable. DIAMANTATO.","Ceiling-mounted adjustable headshower. DIAMANTATO.",149,"Finox Brushed Nickel",2717,"GPF634720G002G000","8055261241831"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",66070,66070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",149,"Finox Brushed Nickel",2824]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",707,"Black Metal Brushed PVD",3305]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63570,63570,"Verstelbare plafonddouche. lengte op aanvraag. RIGATO.","Pomme de douche au plafond avec bras orientable, longueur à la demande. RIGATO.","Ceiling-mounted adjustable headshower. Length on request. RIGATO.",706,"Black Metal PVD",3872,"GPF635700P001G000","8055261241350"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63470,63470,"Verstelbare plafonddouche. lengte op aanvraag. DIAMANTATO.","Pomme de douche au plafond avec bras orientable, longueur à la demande. DIAMANTATO.","Ceiling-mounted adjustable headshower. Length on request. DIAMANTATO.",726,"Warm Bronze Brushed PVD",4133,"GPF634700P024G000","8055261241909"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",716,"Gold Brushed PVD",1067,"GPF630990P005G000","8056329559301"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",32971,32971,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",845,"Dark Bronze",474,"GPF329710V221G000","8056603623179"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",32977,32977,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",726,"Warm Bronze Brushed PVD",411,"GPF329771P024G000","8056329006904"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","32985+32982",32982,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour douchette laterale orientable","External parts for adjustable lateral body jet",735,"Warm Bronze PVD",685,"GPF329820P037G000","8056329555945"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",13375,13375,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","Adjustable lateral body jet",720,"Nickel PVD",315,"GPF133750P014G000","8056603455992"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",20293,20293,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",238,"Mirror Steel",1550,"GPF202930A001G000","8022692642421"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63461,63461,"Wateraansluitpunt met houder handdouche","Sortie murale coudée avec support fixe pour douchette.","Water outlet and handshower hook","030","Copper PVD",357,"GPF634610P000G000","8056329550919"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",63469,63469,"Wateraansluitpunt","Sortie murale coudée.","Water outlet",149,"Finox Brushed Nickel",214,"GPF634690G002G000","8056329550834"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",58157,58157,"Vaste houder voor handdouche","Support fixe pour douchette.","Fixed handshower hook",727,"Brass Brushed PVD",192,"GPF581570P025G000","8022692872002"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",58160,58160,"Oriënteerbare duplex houder voor handdouche","Support mural orientable pour douchette.","Adjustable handshower hook",299,"Matte Black",290,"GPF581600C072G000","8022692874570"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",727,"Brass Brushed PVD",438,"GPF329290P025G000","8055261227804"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",32930,32930,"Black Kneipp handdouche","Douchette Kneipp noire.","Black Kneipp handshower.",279,"Matte White",332,"GPF329300C071G000","8055261236240"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",14371,14371,"Antikalk handdouche","Douchette anticalcaire.","Antilimestone handshower",845,"Dark Bronze",220,"GPF143710V221G000","8055261239753"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",726,"Warm Bronze Brushed PVD",346,"GPF143760P024G000","8056329652354"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",246,"Gold PVD",366,"GPF143760P007G000","8056603522571"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector","030","Copper PVD",252,"GPF473510P000G000","8056603587075"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",706,"Black Metal PVD",252,"GPF473500P001G000","8056603587174"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",720,"Nickel PVD",102,"GPF016370P014G000","8056329725720"]
["BATHROOM","HABITO","HABITO BATH-SHOWER",54137,54137,"Buigzame slang Darkflex lengte 1,50 m","Flexible darkflex 1,50 m","1,50 m Darkflex black flexible hose and cap in finish","031","Chrome",90,"GPF541370G001G000","8056329573116"]
["BATHROOM","HABITO","HABITO BATH-SHOWER","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",149,"Finox Brushed Nickel",130,"GPF017240G002G000","8055261240124"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66401,66401,"wandgemonteerde witte zeep dispenser","Porte-savon mural blanc","Wall-mounted soap dish, white",706,"Black Metal PVD",332,"GPF664010P001G000","8056603565950"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66401,66401,"wandgemonteerde witte zeep dispenser","Porte-savon mural blanc","Wall-mounted soap dish, white",845,"Dark Bronze",356,"GPF664010V221G000","8056603565899"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66407,66407,"wandgemonteerde witte beker houder","Porte-verre mural blanc","Wall-mounted holder, white",720,"Nickel PVD",388,"GPF664070P014G000","8056603565721"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66407,66407,"wandgemonteerde witte beker houder","Porte-verre mural blanc","Wall-mounted holder, white",716,"Gold Brushed PVD",443,"GPF664070P005G000","8055261229266"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66413,66413,"wandgemonteerde witte zeep houder","Distributeur de savon liquide mural blanc","Wall-mounted liquid soap dispenser , white",727,"Brass Brushed PVD",663,"GPF664130P025G000","8056603565509"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66413,66413,"wandgemonteerde witte zeep houder","Distributeur de savon liquide mural blanc","Wall-mounted liquid soap dispenser , white",761,"Coffee Bronze Brushed PVD",705,"GPF664130E059G000","8055261588202"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66419,66419,"wandgemonteerde witte borstel houder","Porte-balayette mural blanc","Wall-mounted brush holder, white",735,"Warm Bronze PVD",658,"GPF664190P037G000","8056603638050"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66420,66420,"wandgemonteerde zwarte borstel houder","Porte-balayette mural noir","Wall-mounted brush holder, black",845,"Dark Bronze",702,"GPF664200V221G000","8056603565196"]
["BATHROOM","HABITO","HABITO ACCESSORIES",58526,58526,"Zwarte Witte Staande Zeephouder","Porte-savon à poser noir","Standing soap holder, black",708,"Copper Brushed PVD",381,"GPF585260P006G000","8056329062269"]
["BATHROOM","HABITO","HABITO ACCESSORIES",58531,58531,"Witte Staande Bekerhouder","Porte-verre à poser blanc.","Standing tumbler holder, white",720,"Nickel PVD",391,"GPF585310P014G000","8056603455916"]
["BATHROOM","HABITO","HABITO ACCESSORIES",58531,58531,"Witte Staande Bekerhouder","Porte-verre à poser blanc.","Standing tumbler holder, white",845,"Dark Bronze",417,"GPF585310V221G000","8056603622011"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66437,66437,"staande witte zeep dispenser","Distributeur de savon liquide à poser blanc","Standing soap dispenser holder, white","031","Chrome",373,"GPF664370G001G000","8056603573047"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66438,66438,"staande zwarte zeep dispenser","Distributeur de savon liquide à poser noir","Standing soap dispenser holder, black",187,"Aged Bronze",589,"GPF664380G052G000","8056603609265"]
["BATHROOM","HABITO","HABITO ACCESSORIES",58543,58543,"Witte Staande Borstelhouder","Porte-balayette à poser blanche","Standing brush holder, white",761,"Coffee Bronze Brushed PVD",784,"GPF585431E059G000","8055261594210"]
["BATHROOM","HABITO","HABITO ACCESSORIES",58544,58544,"Zwarte Staande Borstelhouder","Porte-balayette à poser noir.","Standing brush holder, black",716,"Gold Brushed PVD",784,"GPF585441P005G000","8055261230149"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66455,66455,"toiletrol houder voor horizontaal/verticaal installatie","Porte-papier mural horizontal ou vertical","Horizontal/Vertical paper-roll holder",713,"Antique Brass",325,"GPF664550V204G000","8056603636773"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66500,66500,"Handdoekhouder 30 cm","Porte-serviette 30 cm","30 cm Towel rail",727,"Brass Brushed PVD",422,"GPF665000P025G000","8056603565004"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66502,66502,"45 cm Handdoekhouder","Porte-serviette 45 cm","45 cm Towel rail",726,"Warm Bronze Brushed PVD",451,"GPF665020P024G000","8056603564915"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66523,66523,"wand gemonteerde badjas haak.","Patère murale","Wall-mounted robe hook.",710,"Brass PVD",202,"GPF665230P011G000","8056603636230"]
["BATHROOM","HABITO","HABITO ACCESSORIES",70123,70123,"Kleding haak. INTRECCIO","Patère. INTRECCIO","Wall-mounted robe hook. INTRECCIO",149,"Finox Brushed Nickel",225,"GPF701230G002G000","8056603683173"]
["BATHROOM","HABITO","HABITO ACCESSORIES",70523,70523,"Kleding haak. RIGATO","Patère. RIGATO","Wall-mounted robe hook. RIGATO","031","Chrome",167,"GPF705230G001G000","8056603659208"]
["BATHROOM","HABITO","HABITO ACCESSORIES",70623,70623,"Kleding haak. DIAMANTATO","Patère. DIAMANTATO","Wall-mounted robe hook. DIAMANTATO",726,"Warm Bronze Brushed PVD",263,"GPF706230P024G000","8056603656887"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66511,66511,"30 cm Handdoekhouder voor glasmontage","Porte-serviette 30 cm à fixer sur le verre","30 cm Towel rail for glass fixing","030","Copper PVD",1012,"GPF665110P000G000","8056603636537"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66515,66515,"60 cm Handdoekhouder voor glasmontage","Porte-serviette 60 cm à fixer sur le verre","60 cm Towel rail for glass fixing",149,"Finox Brushed Nickel",1120,"GPF665150G002G000","8056603564564"]
["BATHROOM","HABITO","HABITO ACCESSORIES",66515,66515,"60 cm Handdoekhouder voor glasmontage","Porte-serviette 60 cm à fixer sur le verre","60 cm Towel rail for glass fixing",707,"Black Metal Brushed PVD",1312,"GPF665150P004G000","8056603564540"]
["BATHROOM","HABITO","HABITO ACCESSORIES",45590,45590,"Papierbak wit","Poubelle blanche.","White waste-paper basket",716,"Gold Brushed PVD",913,"GPF455900P005G000","8056603047562"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",239,"Steel Brushed",209,"GPF391840A000G000","8056603452069"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.","030","Copper PVD",257,"GPF375842P000G000","8022692674279"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",727,"Brass Brushed PVD",154,"GPF375870P025G000","8056329081987"]
["BATHROOM","HABITO","HABITO TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",299,"Matte Black",714,"GPF452300C072G000","8055261645714"]
["BATHROOM","HABITO","HABITO TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",708,"Copper Brushed PVD",758,"GPF451300P006G000","8055261227521"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1240,"GPF452270P006G000","8055261645783"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1230,"GPF451240P025G000","8056603615761"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1267,"GPF452260P037G000","8055261645882"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",187,"Aged Bronze",1230,"GPF451260G052G000","8056603632959"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",710,"Brass PVD",1060,"GPF144310P011G000","8055261646070"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1268,"GPF451220G002G000","8056603616065"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",54611,54611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",246,"Gold PVD",1055,"GPF546110P007G000","8056329070530"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",54613,54613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",720,"Nickel PVD",1495,"GPF546130P014G000","8056603456906"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",707,"Black Metal Brushed PVD",883,"GPF546150P004G000","8056329070264"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",187,"Aged Bronze",883,"GPF546150G052G000","8056329070318"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",54617,54617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",187,"Aged Bronze",988,"GPF546170G052G000","8056329098831"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",54621,54621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",273,"Matte Greige",1497,"GPF546211T208G000","8056603587969"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",54671,54671,"bedieningspaneel RIGATO voor GEBERIT SIGMA 8 & 12","Plaque de finissage RIGATO pour GEBRIT SIGMA 8 et 12","Cover plate RIGATO for GEBERIT SIGMA 8 & 12","030","Copper PVD",1960,"GPF546710P000G000","8056603458481"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",54671,54671,"bedieningspaneel RIGATO voor GEBERIT SIGMA 8 & 12","Plaque de finissage RIGATO pour GEBRIT SIGMA 8 et 12","Cover plate RIGATO for GEBERIT SIGMA 8 & 12",761,"Coffee Bronze Brushed PVD",2225]
["BATHROOM","HABITO","HABITO TOTAL LOOK",54681,54681,"bedieningspaneel DIAMANTATO voor GEBERIT SIGMA 8 & 12","Plaque de finissage DIAMANTATO pour GEBRIT SIGMA 8 et 12","Cover plate DIAMANTATO for GEBERIT SIGMA 8 & 12",761,"Coffee Bronze Brushed PVD",2225]
["BATHROOM","HABITO","HABITO TOTAL LOOK","01758","01758","Afwerkplaat 5 gaten voor secur box","Plaque de finition pour Secu Box robinetterie 5 trous","Five-holes finishing plate for mounting box",708,"Copper Brushed PVD",841,"GPF017580P006G000","8056329069275"]
["BATHROOM","HABITO","HABITO TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",276,"Matte Agave",168,"GPF014210T210G000","8056603964135"]
["BATHROOM","HABITO","HABITO TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",246,"Gold PVD",209,"GPF014210P007G000","8056603964210"]
["BATHROOM","HABITO","HABITO TOTAL LOOK",28767,28767,"Verlengstuk buis voor sifon, lengte 40 cm","Tubelure prolongée pour siphone, longueur 40 cm","Syphon pipe extension, 40 cm length",761,"Coffee Bronze Brushed PVD",94,"GPF287670E059G000","8055261577671"]
["BATHROOM","HABITO","HABITO TOTAL LOOK","01377","01377","1 1/4\" sifon","Siphon 1 1/4”.","1 1/4\" syphon",716,"Gold Brushed PVD",484,"GPF013771P005G000","8056329077638"]
["BATHROOM","RETTANGOLO","RETTANGOLO K",53002,53002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo, sans vidage, avec flexibles de raccordement.","Basin mixer, flexible connections, without waste","031","Chrome",559,"GPF530021G001G000","8022692696264"]
["BATHROOM","RETTANGOLO","RETTANGOLO K",53006,53006,"Mengkraan Wastafel hoog, zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, sans vidage, avec flexibles de raccordement.","High basin mixer, flexible connections, without waste",735,"Warm Bronze PVD",1007,"GPF530061P037G000","8056329601871"]
["BATHROOM","RETTANGOLO","RETTANGOLO K",20099,20099,"Plafonduitloop. Aan te vullen met afstandsbediening","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout to be completed with separate control",149,"Finox Brushed Nickel",1304,"GPF200990G002G000","8022692791198"]
["BATHROOM","RETTANGOLO","RETTANGOLO K",20199,20199,"Plafonduitloop aanpasbare hoogte. Aan te vullen met afstandsbediening","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout, length on request with separate control (not included)",299,"Matte Black",1695,"GPF201990C072G000","8022692466058"]
["BATHROOM","RETTANGOLO","RETTANGOLO K",20118,20118,"Wanduitloop uitloop aanpasbare lengte. Aan te vullen met afstandsbediening","Bec mural à compléter par un mitigeur à commande séparée, longueur à la demande.","Wall-mounted spout, length on request, with separate control","031","Chrome",695,"GPF201180G001G000","8022692625257"]
["BATHROOM","RETTANGOLO","RETTANGOLO K","44697+53088",53088,"Extern deel Wandmengkraan middelgrote uitloop zonder waste","Partie apparente mitigeur mural avec bec moyen sans vidage","External parts wall-mounted mixer, medium spout, without waste",708,"Copper Brushed PVD",1118,"GPF530880P006G000","8022692697186"]
["BATHROOM","RETTANGOLO","RETTANGOLO K","44697+53084",53084,"Extern deel Wand-Mengkraan uitloop aanpasbare lengte zonder waste","Partie apparente pour mitigeur lavabo mural avec bec longueuer à la demande sans vidage.","External parts for built-in mixer spout with length on request, without waste","031","Chrome",1568,"GPF530840G001G000","8022692697049"]
["BATHROOM","RETTANGOLO","RETTANGOLO K","46189+53095",53095,"Afbouwdelen voor vrijstaande wastafelmengkraan zonder afvoer","Partie externe mitigeur de lavabo au sol sans vidage","External parts for freestanding basin mixer without waste",710,"Brass PVD",2360,"GPF530950P011G000","8056603614849"]
["BATHROOM","RETTANGOLO","RETTANGOLO K",53007,53007,"Mengkraan Bidet met buigzame aansluitslangen","Mitigeur bidet avec vidage et flexibles de raccordement.","Bidet mixer with flexible connections","030","Copper PVD",860,"GPF530071P000G000","8022692696530"]
["BATHROOM","RETTANGOLO","RETTANGOLO K",20111,20111,"Thermostatische Mengkraan Extern bad met automatische omstelknop bad/douche","Mitigeur bain-douche apparent THERMOSTATIQUE avec inverseur automatique.","External bath thermostatic mixer with automatic bath/shower diverter",710,"Brass PVD",1549,"GPF201112P011G000","8056329613812"]
["BATHROOM","RETTANGOLO","RETTANGOLO K",20127,20127,"Conus handdouchehouder met antikalk-handdouche en buigzame slang 1,50 m","Support douchette avec douchette anticacaire et flexibles 1,5m","Conical shower hook with antilimestone handshower and 1,5 m flexible",149,"Finox Brushed Nickel",532,"GPF201270G002G000","8022692782684"]
["BATHROOM","RETTANGOLO","RETTANGOLO K","01663","01663","Drie-gats afwerkplaat voor montagebox","Plaque de finition 3 trous pour la boîte de sécurité","Three-holes finishing plate for mounting box","030","Copper PVD",736,"GPF016631P000G000","8022692877946"]
["BATHROOM","RETTANGOLO","RETTANGOLO K","01767","01767","Uittrekbare handdouchekit, zijrand installatie. Niet geschikt voor artikels 01669, 01658, 01663, 01664.","Système de récupération eau pour flexible de douchette bain-douche, installation sur plan de bagnoire. Non compatible avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, rim installation. Not fitting items 01669, 01658, 01663 and 01664.",720,"Nickel PVD",1124,"GPF017670P014G000","8056603608824"]
["BATHROOM","RETTANGOLO","RETTANGOLO K","01080","01080","Polyethyleen badafvoer met overloopdopvuller. Lengte van de aanvoer leiding 80 cm","Vidage en polyéthylène baignoire avec trop-plein. Longueur 80 cm","Polyethylene column bath waste with overflow cap filler. Length of control cable 80 cm",246,"Gold PVD",720,"GPF010802P007G000","8056329097605"]
["BATHROOM","RETTANGOLO","RETTANGOLO K",20191,20191,"Cascade-uitloop Badrand Aan te vullen met afstandsbediening","Bec cascade pour baignoire à compléter par un mitigeur à commande séparée.","Bath group waterfall spout to be completed with separate control",708,"Copper Brushed PVD",2673,"GPF201910P006G000","8022692224924"]
["BATHROOM","RETTANGOLO","RETTANGOLO K",20121,20121,"Wanduitloop Bad uitloop aanpasbare lengte Aan te vullen met afstandsbediening","Bec pour baignoire mural à compléter d'un mitigeur à commande séparée, longueur à la DEMANDE.","Bath spout with length on request with separate control (not included)","031","Chrome",695,"GPF201210G001G000","8022692625295"]
["BATHROOM","RETTANGOLO","RETTANGOLO K","44655+53061",53061,"Extern deel Wand-mengkraan 1-weg","Partie apparente pour mitigeur mural, 1 sortie.","External parts mixer one-way diverter",299,"Matte Black",595,"GPF530610C072G000","8022692876253"]
["BATHROOM","RETTANGOLO","RETTANGOLO K","44673+53079",53079,"Extern deel Wand-Mengkraan 2-weg met automatische omstelknop bad/douche","Partie apparente mitigeur mural avec inverseur automatique bain-douche 2 sorties","External parts for wall-mounted mixer two-way, automatic bath/ shower diverter","030","Copper PVD",730,"GPF530790P000G000","8022692696998"]
["BATHROOM","RETTANGOLO","RETTANGOLO K","44639+53141",53141,"Extern deel Wand-mengkraan Douche 2-weg met omstelknop, wateraansluitpunt en houder handdouche. Aan te vullen met handdouche enbuigzame slang","Partie apparente mitigeur douche mural deux sorties avec inverseur, alimentation de l’eau murale, support. À completer par fle xibles de raccondement 1,50 m et douchette anticalcaire","External parts for two-way built-in shower mixer with automatic diverter, water outlet, handshower hook. To be completed with flexible hose and handshower",708,"Copper Brushed PVD",1973,"GPF531410P006G000","8022692697827"]
["BATHROOM","RETTANGOLO","RETTANGOLO K","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",147,"Chome Brushed",81,"GPF016370G006G000","8056329136793"]
["BATHROOM","RETTANGOLO","RETTANGOLO K","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",279,"Matte White",134,"GPF016370C071G000","8022692891997"]
["BATHROOM","RETTANGOLO","RETTANGOLO",20002,20002,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen","Mitigeur lavabo, sans vidage, avec flexibles de raccordement.","Basin mixer, flexible connections, without waste",720,"Nickel PVD",828,"GPF200020P014G000","8056603608640"]
["BATHROOM","RETTANGOLO","RETTANGOLO",11922,11922,"Mengkraan Wastafel hoog, zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, sans vidage, avec flexibles de raccordement.","High basin mixer, flexible connections, without waste",735,"Warm Bronze PVD",1007,"GPF119221P037G000","8056329614567"]
["BATHROOM","RETTANGOLO","RETTANGOLO",20199,20199,"Plafonduitloop aanpasbare hoogte. Aan te vullen met afstandsbediening","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout, length on request with separate control (not included)",708,"Copper Brushed PVD",1981,"GPF201990P006G000","8022692226096"]
["BATHROOM","RETTANGOLO","RETTANGOLO",20118,20118,"Wanduitloop uitloop aanpasbare lengte. Aan te vullen met afstandsbediening","Bec mural à compléter par un mitigeur à commande séparée, longueur à la demande.","Wall-mounted spout, length on request, with separate control",706,"Black Metal PVD",1028,"GPF201180P001G000","8022692212372"]
["BATHROOM","RETTANGOLO","RETTANGOLO",20005,20005,"Afstandsbediening","Commande séparée.","Separate control",707,"Black Metal Brushed PVD",438,"GPF200050P004G000","8022692650297"]
["BATHROOM","RETTANGOLO","RETTANGOLO","44697+44836",44836,"Extern deel Wandmengkraan middelgrote uitloop zonder waste","Partie apparente mitigeur mural avec bec moyen sans vidage","External parts wall-mounted mixer, medium spout, without waste",720,"Nickel PVD",1031,"GPF448360P014G000","8056603607551"]
["BATHROOM","RETTANGOLO","RETTANGOLO","44697+44838",44838,"Extern deel Wand-Mengkraan lange uitloop zonder waste","Partie apparente pour mitigeur lavabo mural avec bec long sans vidage.","External parts for built-in mixer with long spout, without waste",149,"Finox Brushed Nickel",991,"GPF448380G002G000","8022692809510"]
["BATHROOM","RETTANGOLO","RETTANGOLO","46189+20092",20092,"Afbouwdelen voor vrijstaande wastafelmengkraan zonder afvoer","Partie externe mitigeur de lavabo au sol sans vidage","External parts for freestanding basin mixer without waste",727,"Brass Brushed PVD",2518,"GPF200920P025G000","8056603614955"]
["BATHROOM","RETTANGOLO","RETTANGOLO",20007,20007,"Mengkraan Bidet met waste met buigzame aansluitslangen","Mitigeur bidet, avec flexibles de raccordement et vidage.","Bidet mixer, flexible connections, with waste",707,"Black Metal Brushed PVD",918,"GPF200071P004G000","8022692203516"]
["BATHROOM","RETTANGOLO","RETTANGOLO",20111,20111,"Thermostatische Mengkraan Extern bad met automatische omstelknop bad/douche","Mitigeur bain-douche apparent THERMOSTATIQUE avec inverseur automatique.","External bath thermostatic mixer with automatic bath/shower diverter",726,"Warm Bronze Brushed PVD",1654,"GPF201112P024G000","8056329613805"]
["BATHROOM","RETTANGOLO","RETTANGOLO",20127,20127,"Conus handdouchehouder met antikalk-handdouche en buigzame slang 1,50 m","Support douchette avec douchette anticacaire et flexibles 1,5m","Conical shower hook with antilimestone handshower and 1,5 m flexible",720,"Nickel PVD",580,"GPF201270P014G000","8056603480000"]
["BATHROOM","RETTANGOLO","RETTANGOLO",20127,20127,"Conus handdouchehouder met antikalk-handdouche en buigzame slang 1,50 m","Support douchette avec douchette anticacaire et flexibles 1,5m","Conical shower hook with antilimestone handshower and 1,5 m flexible",735,"Warm Bronze PVD",580,"GPF201270P037G000","8056329613560"]
["BATHROOM","RETTANGOLO","RETTANGOLO","01766","01766","Uittrekbare handdouchekit, installatie op zijplan in de badkuip. Niet geschikt voor artikels 01669, 01658, 01663, 01664.","Système de récupération eau pour flexible de douchette bain-douche, installation sur plan latéral à la bagnoire. Non compatibleavec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, tile wall installation. Not fitting items 01669, 01658, 01663 and 01664.",708,"Copper Brushed PVD",1907,"GPF017660P006G000","8022692856309"]
["BATHROOM","RETTANGOLO","RETTANGOLO","01080","01080","Polyethyleen badafvoer met overloopdopvuller. Lengte van de aanvoer leiding 80 cm","Vidage en polyéthylène baignoire avec trop-plein. Longueur 80 cm","Polyethylene column bath waste with overflow cap filler. Length of control cable 80 cm",149,"Finox Brushed Nickel",504,"GPF010802G002G000","8022692791082"]
["BATHROOM","RETTANGOLO","RETTANGOLO",20191,20191,"Cascade-uitloop Badrand Aan te vullen met afstandsbediening","Bec cascade pour baignoire à compléter par un mitigeur à commande séparée.","Bath group waterfall spout to be completed with separate control","031","Chrome",1690,"GPF201910G001G000","8022692028911"]
["BATHROOM","RETTANGOLO","RETTANGOLO",20191,20191,"Cascade-uitloop Badrand Aan te vullen met afstandsbediening","Bec cascade pour baignoire à compléter par un mitigeur à commande séparée.","Bath group waterfall spout to be completed with separate control",845,"Dark Bronze",2673,"GPF201910V221G000","8056603634090"]
["BATHROOM","RETTANGOLO","RETTANGOLO","44655+44602",44602,"Extern deel Wand-mengkraan douche 1-weg","Partie apparente mitigeur douche mural une sorties","External parts wall-mounted shower mixer, one-way",727,"Brass Brushed PVD",723,"GPF446020P025G000","8056329608054"]
["BATHROOM","RETTANGOLO","RETTANGOLO",19431,19431,"Thermostatische Mengkraan extern douche","Mitigeur thermostatique douche apparent.","External shower thermostatic mixer",708,"Copper Brushed PVD",1424,"GPF194312P006G000","8022692875140"]
["BATHROOM","RETTANGOLO","RETTANGOLO","44639+44910",44910,"Extern deel Wand-mengkraan Douche 2-weg met omstelknop, wateraansluitpunt en houder handdouche. Aan te vullen met handdouche enbuigzame slang","Partie apparente mitigeur douche mural deux sorties avec inverseur, alimentation de l’eau murale, support. À completer par fle xibles de raccondement 1,50 m et douchette anticalcaire","External parts for two-way built-in shower mixer with diverter, water outlet, handshower hook. To be completed with flexible hose and handshower",735,"Warm Bronze PVD",1823,"GPF449100P037G000","8056329607729"]
["BATHROOM","RETTANGOLO","RETTANGOLO",20154,20154,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",299,"Matte Black",291,"GPF201540C072G000","8022692053500"]
["BATHROOM","RETTANGOLO","RETTANGOLO","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",726,"Warm Bronze Brushed PVD",120,"GPF016370P024G000","8056329555655"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","09269+20184",20184,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche mural 2 sorties.","External parts for thermostatic mixer, two-way diverter",708,"Copper Brushed PVD",1477,"GPF201840P006G000","8022692224252"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","09269+20190","09269","Inbouwdeel voor thermostatische mengkraan","Partie encastrée pour mitigeur de douche thermostatique mural","Built-in part for thermostatic mixer","031","Chrome",571,"GPF092691G001G000","8022692101652"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","09266+44336",44336,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie externe mitigeur thermostatique mural à 3 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with three separate exits.",299,"Matte Black",1768,"GPF443360C072G000","8056603620611"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","09268+44338",44338,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie externe mitigeur thermostatique mural à 4 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with four separate exits.",720,"Nickel PVD",2198,"GPF443380P014G000","8056603620369"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","43103+43024",43024,"Extern deel Thermostatische wand-mengkraan hoog debiet 2 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Deux sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with TWO SEPARATE EXITS",707,"Black Metal Brushed PVD",2389,"GPF430241P004G000","8022692580860"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","43105+43026",43026,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS",720,"Nickel PVD",2501,"GPF430261P014G000","8056603607742"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","43105+43216",43216,"Extern deel Thermostatische wand-mengkraan hoog debiet 3 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Trois sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with THREE SEPARATE EXITS","031","Chrome",1311,"GPF432161G001G000","8022692584219"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","43107+43028",43028,"Extern deel Thermostatische wand-mengkraan hoog debiet 4 onafhankelijke uitgangen. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Quatre sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FOUR SEPARATE EXITS",710,"Brass PVD",2858,"GPF430281P011G000","8056329608795"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","43109+43220",43109,"Inbouwdeel Thermostatische mengkraan hoog debiet 5 onafhankelijke uitgangen","Partie encastrée mitigeur THERMOSTATIQUE douche haut débit, cinq sorties indépendantes. Installation verticale/horizontale.","Built-in thermostatic high-capacity mixer with FIVE SEPARATE EXITS. Vertical/Horizontal installation.","031","Chrome",1547,"GPF431093G001G000","8022692583427"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","43111+43032",43032,"Extern deel Thermostatische wand-mengkraan hoog debiet 5 uitgangen met enkele selectie. Verticale/horizontale installatie.","Partie apparente mitigeur THERMOSTATIQUE douche haut débit. Cinq sorties avec manette selective. Installation verticale/horizontale.","External parts for wall-mounted thermostatic high-capacity mixer. Vertical/horizontal setting up with FIVE SEPARATE EXITS with single selection",710,"Brass PVD",2353,"GPF430321P011G000","8056329608733"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","43281+43252",43252,"Extern deel Thermostatische Wand-mengkraan hoog debiet","Partie apparente mitigeur THERMOSTATIQUE douche haut débit","External parts wall-mounted thermostatic high-capacity mixer",727,"Brass Brushed PVD",1127,"GPF432521P025G000","8056329608191"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","43283+43264",43264,"Extern deel Stopkraan hoog debiet.","Partie apparente robinet d’arrêt pour mitigeur haut débit.","External parts for stop valve for thermostatic high-capacity mixer.",761,"Coffee Bronze Brushed PVD",777,"GPF432640E059G000","8055261603066"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",33095,33095,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted shower head",279,"Matte White",3372,"GPF330951C071G000","8056329077584"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",20148,20148,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-fixing antilimestone and adjustable headshower",716,"Gold Brushed PVD",2219,"GPF201480P005G000","8055261231191"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",20151,20151,"Antikalk-hoofddouchekop plafond oriënteerbaar","Pomme de douche au plafond orientable.","Wall-mounted adjustable and antilimestone showerhead",279,"Matte White",1672,"GPF201510C071G000","8056329007314"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",15186,15186,"Antikalk-hoofddouchekop plafond oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead",187,"Aged Bronze",2499,"GPF151860G052G000","8056329653221"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",20150,20150,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",187,"Aged Bronze",2775,"GPF201500G052G000","8056603637589"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",15199,15199,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",246,"Gold PVD",3527,"GPF151990P007G000","8056329720282"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",20142,20142,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with antilimestone handshower, 1,50 m flexible hose and water outlet",299,"Matte Black",1348,"GPF201421C072G000","8022692215106"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet","031","Chrome",397,"GPF329840G001G000","8022692519334"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",32973,32973,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",726,"Warm Bronze Brushed PVD",474,"GPF329730P024G000","8056329529724"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",149,"Finox Brushed Nickel",351,"GPF329791G002G000","8022692800623"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",20172,20172,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","adjustable lateral body jet",707,"Black Metal Brushed PVD",388,"GPF201720P004G000","8022692223781"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",720,"Nickel PVD",1506,"GPF202950P014G000","8056603457231"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",20293,20293,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",716,"Gold Brushed PVD",2605,"GPF202930P005G000","8056603671729"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",20123,20123,"Doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m.","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",299,"Matte Black",734,"GPF201231C072G000","8022692068900"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",20169,20169,"Wateraansluitpunt","Sortie murale coudée.","water outlet",149,"Finox Brushed Nickel",243,"GPF201691G002G000","8022692783407"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",20157,20157,"Vaste houder voor handdouche","Support mural fixe pour douchette.","Fixed handshower hook",726,"Warm Bronze Brushed PVD",150,"GPF201570P024G000","8056329613270"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",706,"Black Metal PVD",223,"GPF143700P001G000","8056329015135"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",720,"Nickel PVD",325,"GPF143760P014G000","8056603631785"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",299,"Matte Black",278,"GPF143780C072G000","8056603633321"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",761,"Coffee Bronze Brushed PVD",367,"GPF143780E059G000","8055261609570"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",761,"Coffee Bronze Brushed PVD",284,"GPF473510E059G000","8055261602700"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",187,"Aged Bronze",133,"GPF016370G052G000","8056329008779"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",710,"Brass PVD",134,"GPF287460P011G000","8056329610750"]
["BATHROOM","RETTANGOLO","RETTANGOLO BATH-SHOWER","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",187,"Aged Bronze",162,"GPF017240G052G000","8055261240100"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20801,20801,"Wand-zeepbakje wit","Porte-savon mural blanc.","Wall-mounted soap dish, white","030","Copper PVD",491,"GPF208011P000G000","8022692243291"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20802,20802,"Wand-zeepbakje zwart","Porte-savon mural noir.","Wall-mounted soap dish, black",713,"Antique Brass",524,"GPF208020V204G000","8056603628709"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20813,20813,"Wand-dispenserhouder wit","Distributeur de savon liquide mural blanc.","Wall-mounted liquid soap dispenser , white",706,"Black Metal PVD",741,"GPF208132P001G000","8022692833867"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20814,20814,"Wand-dispenserhouder zwart","Distributeur de savon liquide mural noir.","Wall-mounted liquid soap dispenser - black",706,"Black Metal PVD",741,"GPF208141P001G000","8022692245875"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20820,20820,"Wand-toiletborstelhouder zwart","Porte-balayette mural noir.","Black wall-mounted brush holder",706,"Black Metal PVD",810,"GPF208202P001G000","8022692832846"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20820,20820,"Wand-toiletborstelhouder zwart","Porte-balayette mural noir.","Black wall-mounted brush holder",726,"Warm Bronze Brushed PVD",864,"GPF208202P024G000","8056329612235"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20826,20826,"Staand zeepbakje zwart","Porte-savon à poser noir.","Black standing soap holder",708,"Copper Brushed PVD",332,"GPF208260P006G000","8022692248777"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20832,20832,"Staande glashouder zwart","Porte-verre à poser noir.","Standing tumbler holder black",707,"Black Metal Brushed PVD",332,"GPF208320P004G000","8022692250138"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20837,20837,"Staande dispenserhouder wit","Distributeur de savon liquide à poser blanc.","Standing Soap dispenser white",707,"Black Metal Brushed PVD",574,"GPF208372P004G000","8022692833072"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20838,20838,"Staande dispenserhouder zwart","Distributeur de savon liquide à poser noir.","Black standing Soap dispenser",706,"Black Metal PVD",537,"GPF208381P001G000","8022692251982"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20843,20843,"Staande toiletborstelhouder wit","Porte-balayette à poser blanche.","White standing brush holder",710,"Brass PVD",557,"GPF208433P011G000","8056329611924"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20849,20849,"Wand-toiletrolhouder met deksel","Porte-papier mural à couvercle.","Wall-mounted paper roll holder with cover",761,"Coffee Bronze Brushed PVD",626,"GPF208491E059G000","8055261609099"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20867,20867,"Wandkolom met toiletrolhouder en toiletborstelhouder wit","Serviteur mural avec porte-papier et porte-balayette blanc.","Wall-mounted column with paper roll holder and white brush holder","030","Copper PVD",1093,"GPF208673P000G000","8022692257922"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20868,20868,"Wandkolom met toiletrolhouder en toiletborstelhouder zwart","Serviteur mural avec porte-papier et porte-balayette noir.","Wall-mounted column with paper roll holder and black brush holder",735,"Warm Bronze PVD",1093,"GPF208682P037G000","8056329611740"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20933,20933,"Vloerstandaard met toiletrolhouder en toiletborstelhouder wit","Serviteur sur pied avec porte-papier et porte-balayette blanc.","Standing set with paper roll holder and white brush holder",727,"Brass Brushed PVD",1199,"GPF209333P025G000","8056329611436"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20939,20939,"Vloerstandaard handdoekhouder","Serviteur sur pied porte-serviette.","Freestanding towel rail","031","Chrome",1020,"GPF209390G001G000","8022692021189"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20897,20897,"Wand-handdoekhouder 30 cm","Porte-serviette 30 cm.","30 cm centre distance towel rail",187,"Aged Bronze",544,"GPF208970G052G000","8056603628426"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20900,20900,"Wand-handdoekhouder 45 cm","Porte-serviette 45 cm.","45 cm centre distance towel rail",713,"Antique Brass",561,"GPF209000V204G000","8022692261523"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20909,20909,"Wand-handdoekhouder ringvorm","Anneau porte-serviette.","Towel ring",706,"Black Metal PVD",393,"GPF209091P001G000","8022692834253"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20909,20909,"Wand-handdoekhouder ringvorm","Anneau porte-serviette.","Towel ring",761,"Coffee Bronze Brushed PVD",446,"GPF209091E059G000","8055261608931"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20963,20963,"Handdoekhouder 45 cm","Porte-serviette 45 cm à fixer sur le verre.","45 cm towel rail for glass fixing",713,"Antique Brass",1102,"GPF209630V204G000","8056603628174"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20965,20965,"Handdoekhouder 60 cm","Porte-serviette 60 cm à fixer sur le verre.","60 cm towel rail for glass fixing",149,"Finox Brushed Nickel",995,"GPF209650G002G000","8056329539532"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20947,20947,"Wandrekje 30 cm","Console 30 cm.","Shelf 30 cm.",720,"Nickel PVD",614,"GPF209470P014G000","8056603608152"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm","031","Chrome",579,"GPF209450G001G000","8022692026955"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20945,20945,"Wandrekje 60 cm","Console 60 cm","Shelf 60 cm",706,"Black Metal PVD",856,"GPF209450P001G000","8022692272420"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20990,20990,"Papierbak wit","Poubelle blanche.","White waste-paper basket.",708,"Copper Brushed PVD",903,"GPF209901P006G000","8022692275469"]
["BATHROOM","RETTANGOLO","RETTANGOLO  ACCESSORIES",20893,20893,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip-handle for bathtub and shower enclosure, 45 cm length","031","Chrome",485,"GPF208930G001G000","8022692473629"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",37573,37573,"Wandtoilet van Keramiek (6 liter). Scharnieren met vertraagde sluiting opgenomen in afwerking 031","Cuvette suspendue en Céramique Blanc Europe (6 litres) avec abattant muni de système “SOFT CLOSE” ou assisté. Charnière en finiton 031 chromée","Wall hung WC (6 litres) in Ceramic. Soft-closing hardware included in 031 finishing",518,"White Ceramic",1140,"GPF375733C083G000","8022692429862"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",727,"Brass Brushed PVD",273,"GPF375842P025G000","8056329080393"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",845,"Dark Bronze",836,"GPF452300V221G000","8055261645578"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1205,"GPF591531E059G000","8055261577350"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",720,"Nickel PVD",1317,"GPF591511P014G000","8056603605656"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",54611,54611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",280,"Matte Ocra",848,"GPF546110T213G000","8056603609715"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",54613,54613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",239,"Steel Brushed",1011,"GPF546130A000G000","8056329070509"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",708,"Copper Brushed PVD",883,"GPF546150P006G000","8056329070240"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",54617,54617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",720,"Nickel PVD",988,"GPF546170P014G000","8056603456883"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",54617,54617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",761,"Coffee Bronze Brushed PVD",1057,"GPF546170E059G000","8055261574373"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",54619,54619,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaque de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",845,"Dark Bronze",1386,"GPF546190V221G000","8056603637701"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",54621,54621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",707,"Black Metal Brushed PVD",1749,"GPF546211P004G000","8056329540798"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.","031","Chrome",60,"GPF014210G001G000","8056603964326"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",277,"Glossy Ocra",194,"GPF014210T211G000","8056603964128"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK",28767,28767,"Verlengstuk buis voor sifon, lengte 40 cm","Tubelure prolongée pour siphone, longueur 40 cm","Syphon pipe extension, 40 cm length",727,"Brass Brushed PVD",88,"GPF287670P025G000","8056329198999"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK","01412","01412","Hoekstopkraan onder wastafel met filter en aansluiting van 1/2\"","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection",299,"Matte Black",281,"GPF014120C072G000","8022692122190"]
["BATHROOM","RETTANGOLO","RETTANGOLO TOTAL LOOK","01412","01412","Hoekstopkraan onder wastafel met filter en aansluiting van 1/2\"","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection",735,"Warm Bronze PVD",348,"GPF014120P037G000","8056329559141"]
["BATHROOM","GOCCIA","GOCCIA","33603",33603,"Mengkraan Wastafel, lange uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo avec bec long sans vidage avec flexibles de raccordement.","Basin mixer, long spout, flexible connections, without waste. Swivelling spout.","031","Chrome",754,"GPF336030G001G000","8022692056884"]
["BATHROOM","GOCCIA","GOCCIA","33603",33603,"Mengkraan Wastafel, lange uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo avec bec long sans vidage avec flexibles de raccordement.","Basin mixer, long spout, flexible connections, without waste. Swivelling spout.",845,"Dark Bronze",1192,"GPF336030V221G000","8055261478947"]
["BATHROOM","GOCCIA","GOCCIA","33605","33605","Middelgrote Mengkraan Wastafel, middelgrote uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo moyen avec bec moyen sans vidage avec flexibles de raccordement.","Medium version basin mixer, medium spout, flexible connections, without waste. Swivelling spout.",761,"Coffee Bronze Brushed PVD",1377,"GPF336050E059G000","8055261607385"]
["BATHROOM","GOCCIA","GOCCIA","33606","33606","Middelgrote Mengkraan Wastafel, lange uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo moyen avec bec long sans vidage avec flexibles de raccordement","Medium version basin mixer, long spout, flexible connections, without waste. Swivelling spout.",726,"Warm Bronze Brushed PVD",1452,"GPF336060P024G000","8055261607316"]
["BATHROOM","GOCCIA","GOCCIA","33610","33610","Mengkraan Wastafel hoog, lange uitloop zonder waste met buigzame aansluitslangen","Mitigeur lavabo réhaussé, bec long. Sans vidage, avec flexibles de raccordement.","High version basin mixer , long spout, flexible connections, without waste. Swivelling spout.",761,"Coffee Bronze Brushed PVD",1623,"GPF336101E059G000","8055261607101"]
["BATHROOM","GOCCIA","GOCCIA","46189+33626","33626","Extern deel Vloer-Mengkraan Wastafel, korte uitloop zonder waste","Partie apparente pour mitigeur de vasque au sol avec bec court sans vidage.","External parts for freestanding basin mixer, short spout without waste. Swivelling spout.",149,"Finox Brushed Nickel",1653,"GPF336260G002G000","8056603720625"]
["BATHROOM","GOCCIA","GOCCIA","46189+33630","33630","Extern deel Vloer-Mengkraan Wastafel, lange uitloop zonder waste","Partie apparente pour mitigeur de lavabo au sol avec bec long sans vidage.","External parts for freestanding basin mixer, long spout without waste. Swivelling spout.",706,"Black Metal PVD",1956,"GPF336300P001G000","8055261606920"]
["BATHROOM","GOCCIA","GOCCIA","33699","33699","Plafonduitloop. Aan te vullen met afstandsbediening of met en elektronische hoog.","Bec au plafond. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout to be completed with separate control",761,"Coffee Bronze Brushed PVD",1871,"GPF336990E059G000","8055261606500"]
["BATHROOM","GOCCIA","GOCCIA","33715","33715","Wanduitloop Wastafel middelgrote uitloop. Aan te vullen met afstandsbediening","Bec de lavabo mural moyen. À compléter par un mitigeur à commande séparée.","Wall-mounted spout, medium spout,with separate control (not included).",149,"Finox Brushed Nickel",400,"GPF337150G002G000","8056329013957"]
["BATHROOM","GOCCIA","GOCCIA","33723","33723","Wanduitloop Wastafel uitloop aanpasbare lengte. Aan te vullen met afstandsbediening","Bec de lavabo mural longueur à la demande. À compléter par un mitigeur à commande séparée.","Wall-mounted spout, spout length on request,with separate control (not included).",761,"Coffee Bronze Brushed PVD",985,"GPF337230E059G000","8055261606296"]
["BATHROOM","GOCCIA","GOCCIA","33745+33744","33744","Extern deel Wand-mengkraan 1-weg","Partie apparente pour mitigeur mural, 1 sortie.","External parts mixer one-way diverter",735,"Warm Bronze PVD",615,"GPF337440P037G000","8055261606197"]
["BATHROOM","GOCCIA","GOCCIA","09285+33044","33044","Afbouwdeel wand gemonteerde separate bediening.","Partie apparente mitigeur mural à 1 sortie","External part wall-mounted separate control.",706,"Black Metal PVD",744,"GPF330440P001G000","8055261608405"]
["BATHROOM","GOCCIA","GOCCIA","33687+33684","33684","Extern deel Wand-Mengkraan korte uitloop zonder waste","Partie apparente pour mitigeur lavabo mural avec bec court sans vidage.","External parts for built-in mixer with short spout, without waste",707,"Black Metal Brushed PVD",1154,"GPF336840P004G000","8056329099937"]
["BATHROOM","GOCCIA","GOCCIA","33687+33686","33686","Extern deel Wand-Mengkraan lange uitloop zonder waste","Partie apparente pour mitigeur lavabo mural avec bec long sans vidage.","External parts for built-in mixer with long spout, without waste",707,"Black Metal Brushed PVD",1154,"GPF336860P004G000","8055261606630"]
["BATHROOM","GOCCIA","GOCCIA","33687+33690","33690","Extern deel Wand-Mengkraan uitloop aanpasbare lengte zonder waste","Partie apparente pour mitigeur lavabo mural avec bec longueuer à la demande sans vidage.","External parts for built-in mixer spout with length on request, without waste",707,"Black Metal Brushed PVD",2502,"GPF336900P004G000","8055261606555"]
["BATHROOM","GOCCIA","GOCCIA","09283+33090","09283","Inbouwdeel voor eengreeps inbouw wastafelmengkraan voor wandmontage.","Partie encastrée pour mitigeur lavabo mural.","Built-in part for mixer with spout.","031","Chrome",405,"GPF092830G001G000","8055261029361"]
["BATHROOM","GOCCIA","GOCCIA","46189+33029","33029","Extern deel Externe Standaard bad","Partie apparente pour mitigeur bain-douche sur pied","External parts for freestanding external bath mixer",713,"Antique Brass",4478,"GPF330290V204G000","8056603720663"]
["BATHROOM","GOCCIA","GOCCIA","54055+33019","33019","Afbouwdeel wand gemonteerd 1-weg douche mengkraan.","Partie apparente mitigeur mural à 1 sortie","External part wall-mounted one way shower mixer.",279,"Matte White",540,"GPF330190C071G000","8055261195929"]
["BATHROOM","GOCCIA","GOCCIA","44673+44678","44678","Extern deel Wand-Mengkraan 2-weg met automatische omstelknop bad/douche","Partie apparente mitigeur mural avec inverseur automatique bain-douche deux sorties","External parts for wall-mounted mixer two-way, automatic bath/ shower diverter",707,"Black Metal Brushed PVD",751,"GPF446780P004G000","8056329099807"]
["BATHROOM","GOCCIA","GOCCIA","09269+33842","33842","Extern deel bad-/douche thermostaat 1-weg","Partie apparente pour mitigeur thermostatique douche mural 1 sortie.","External parts for thermostatic mixer, one-way diverter",713,"Antique Brass",905,"GPF338420V204G000","8056329609372"]
["BATHROOM","GOCCIA","GOCCIA","09269+33844","33844","Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche mural 2 sorties.","External parts for thermostatic mixer, two-way diverter",279,"Matte White",774,"GPF338440C071G000","8022692625929"]
["BATHROOM","GOCCIA","GOCCIA","54169+33132","33132","Afbouwdeel wand gemonteerde 1-wegthermostatische mengkraan.","Partie apparente mitigeur thermostatique mural 1 voie.","External part wall-mounted one way thermostatic mixer.",707,"Black Metal Brushed PVD",1328,"GPF331320P004G000","8055261607835"]
["BATHROOM","GOCCIA","GOCCIA","54169+33136","33136","Afbouwdeel wand gemonteerde 3-weg thermostatische mengkraan.","Partie apparente mitigeur thermostatique mural 3 voies.","External part wall-mounted three ways thermostatic mixer.",713,"Antique Brass",1328,"GPF331360V204G000","8055261234888"]
["BATHROOM","GOCCIA","GOCCIA","09266+63436",63436,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie externe mitigeur thermostatique mural à 3 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with three separate exits.",720,"Nickel PVD",1938,"GPF634360P014G000","8056603618861"]
["BATHROOM","GOCCIA","GOCCIA","09268+63438",63438,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie externe mitigeur thermostatique mural à 4 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with four separate exits.",720,"Nickel PVD",2198,"GPF634380P014G000","8056603618717"]
["BATHROOM","GOCCIA","GOCCIA","09263+63440",63440,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 5 uitgangen.","Partie externe mitigeur thermostatique mural à 5 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with five separate exits.",707,"Black Metal Brushed PVD",2574,"GPF634400P004G000","8056603630375"]
["BATHROOM","GOCCIA","GOCCIA","33642","33642","Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with antilimestone handshower, 1,50 m flexible hose and water outlet",761,"Coffee Bronze Brushed PVD",1406,"GPF336420E059G000","8055261606876"]
["BATHROOM","GOCCIA","GOCCIA",33655,33655,"Antikalk-hoofddouchekop Wanddouche oriënteerbaar","Pomme de douche murale orientable.","Wall-mounted adjustable and antilimestone showerhead",299,"Matte Black",1260]
["BATHROOM","GOCCIA","GOCCIA","33766",33766,"Antikalk-hoofddouchekop Plafonddouche oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead","031","Chrome",1182,"GPF337663G001G000","8022692404982"]
["BATHROOM","GOCCIA","GOCCIA",33664,33664,"Oriënteerbare antikalk hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable and antilimestone showerhead, length on request",299,"Matte Black",1769]
["BATHROOM","GOCCIA","GOCCIA","33768","33768","Oriënteerbare antikalk hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable and antilimestone showerhead, length on request",279,"Matte White",2344,"GPF337683C071G000","8022692060379"]
["BATHROOM","GOCCIA","GOCCIA","33751","33751","Antikalk-hoofddouchekop Plafonddouche","Pomme de douche au plafond.","Ceiling-mounted antilimestone showerhead",713,"Antique Brass",2034,"GPF337511V204G000","8056329071377"]
["BATHROOM","GOCCIA","GOCCIA","33753","33753","Antikalk-hoofddouchekop Plafonddouche arm aanpasbare hoogte","Pomme de douche au plafond, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",845,"Dark Bronze",2785,"GPF337532V221G000","8055261237070"]
["BATHROOM","GOCCIA","GOCCIA","33761","33761","Wateraansluitpunt met houder handdouche","Sortie murale coudée avec support fixe pour douchette.","water outlet and handshower hook",149,"Finox Brushed Nickel",232,"GPF337610G002G000","8056603999960"]
["BATHROOM","GOCCIA","GOCCIA","33761","33761","Wateraansluitpunt met houder handdouche","Sortie murale coudée avec support fixe pour douchette.","water outlet and handshower hook",735,"Warm Bronze PVD",255,"GPF337610P037G000","8055261605640"]
["BATHROOM","GOCCIA","GOCCIA","33757","33757","Vaste houder voor handdouche","Support fixe pour douchette.","Fixed handshower hook",708,"Copper Brushed PVD",190,"GPF337570P006G000","8055261605817"]
["BATHROOM","GOCCIA","GOCCIA","33760","33760","Oriënteerbare duplex houder voor handdouche","Support mural orientable pour douchette.","Adjustable handshower hook",279,"Matte White",241,"GPF337600C071G000","8022692060065"]
["BATHROOM","GOCCIA","GOCCIA",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",720,"Nickel PVD",325,"GPF143760P014G000","8056603631785"]
["BATHROOM","GOCCIA","GOCCIA",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",761,"Coffee Bronze Brushed PVD",367,"GPF143780E059G000","8055261609570"]
["BATHROOM","GOCCIA","GOCCIA",47351,47351,"3-jet anti-kalk handdouche met drukknop selectie","Douchette anticalcaire trois jets avec sélecteur à bouton","Three-jets anti-limescale hand shower with push button selector",713,"Antique Brass",269,"GPF473510V204G000","8056603586993"]
["BATHROOM","GOCCIA","GOCCIA","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",720,"Nickel PVD",102,"GPF016370P014G000","8056329725720"]
["BATHROOM","GOCCIA","GOCCIA",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",735,"Warm Bronze PVD",134,"GPF287460P037G000","8056329610736"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38007","38007","Wand-glashouder van wit GRES","Porte-verre mural en GRES blanc.","Wall-mounted holder, white","030","Copper PVD",379,"GPF380070P000G000","8055261604889"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38008","38008","Wand-glashouder van zwart GRES","Porte-verre mural en GRES noir.","Wall-mounted holder, black",735,"Warm Bronze PVD",379,"GPF380080P037G000","8055261604759"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38014","38014","Wand-dispenserhouder van zwart GRES","Distributeur de savon mural en GRES noir.","Wall-mounted liquid soap dispenser - black",706,"Black Metal PVD",602,"GPF380143P001G000","8055261604643"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38019","38019","Wand-toiletborstelhouder van wit GRES","Porte-balayette mural en GRES blanc.","Wall-mounted brush holder, white",706,"Black Metal PVD",523,"GPF380190P001G000","8055261604575"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38037","38037","Staande dispenserhouder van wit GRES","Distributeur de savon à poser en GRES blanc .","Standing soap dispenser holder, white",761,"Coffee Bronze Brushed PVD",491,"GPF380373E059G000","8055261604452"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38038",38038,"Staande dispenserhouder van zwart GRES","Distributeur de savon à poser en GRES noir.","Standing soap dispenser holder, black","031","Chrome",292,"GPF380383G001G000","8022692433050"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38044","38044","Staande toiletborstelhouder van zwart GRES","Porte-balayette à poser en GRES noir.","Black GRES standing brush holder","030","Copper PVD",346,"GPF380440P000G000","8055261604223"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38055","38055","Horizontale of verticale wand-toiletrolhouder","Porte-papier mural horizontal ou vertical.","Paper-roll holder for horizontal/vertical installation",735,"Warm Bronze PVD",364,"GPF380550P037G000","8055261604094"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38067","38067","Vloerstandaard met toiletrolhouder en toiletborstelhouder van wit GRES","Serviteur sur pied avec porte-papier et porte-balayette en GRES blanc.","White GRES Standing set with paper roll holder and brush holder",149,"Finox Brushed Nickel",945,"GPF380670G002G000","8056603967129"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38144","38144","Plafond-handdoekhouder 45 cm","Porte-serviette au plafond 45 cm.","45 cm ceiling-mounted towel rail",149,"Finox Brushed Nickel",1137,"GPF381440G002G000","8022692437287"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38097","38097","Handdoekhouder 30 cm","Porte-serviette 30 cm.","30 cm towel rail","030","Copper PVD",352,"GPF380970P000G000","8055261603929"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38100","38100","Handdoekhouder 45 cm","Porte-serviette 45 cm.","45 cm towel rail",735,"Warm Bronze PVD",473,"GPF381000P037G000","8055261603844"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38103","38103","Handdoekhouder 60 cm","Porte-serviette 60 cm.","60 cm towel rail",708,"Copper Brushed PVD",558,"GPF381030P006G000","8056329099296"]
["BATHROOM","GOCCIA","GOCCIA ACCESSORIES","38121","38121","Wand-kledinghaak","Patère.","Wall-mounted robe hook",706,"Black Metal PVD",158,"GPF381210P001G000","8055261603707"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",39113,39113,"Wandtoilet van Keramiek (6 liter) met geïntegreerde sifon. Scharnieren met vertraagde sluiting en laterale gatafdekkingen opgenomen in afwerking 031","Cuvette suspendue en Céramique (6 litres) avec abattant muni de système “SOFT CLOSE” ou assisté. Charnière et enjoliveurs latéraux en finition 031","Wall hung WC (6 litres) in Ceramic, integrated siphon. Soft-closing hardware and lateral holes plugs included in 031 finishing.",531,"Matte White Ceramic",1706,"GPF391133C288G000","8056329052512"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",29463,29463,"Toiletzitting van antibacteriële hars voor artikel 39114. Te completeren met zachtsluitend beslag 37584 (niet inbegrepen).","Siège en résine antibactérienne pour cuvette 39114. À combiner avec les charnières 37584 (non inclues).","Anti-bacterical resin WC seat for item 39114. To be completed with soft-closing hardware 37584 (not included).",279,"Matte White",411,"GPF294630C071G000","8056329097674"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",39115,39115,"Wandbidet van Keramiek met overloop. Met centraal gat voor kraanwerk. Dop overloop en laterale gatafdekkingen opgenomen in afwerking 031.","Bidet suspendu en Céramique Blanc Europe avec vidage et trop plein, percé monotrou pour la robinetterie, fourni avec cache de trop plein et enjoliveurs latéraux en finition 031.","Wall hung bidet in in White Europe Ceramic with overflow waste, with central hole for taps and fittings. Overflow cap and side covering caps included in 031 finishing",518,"White Ceramic",769,"GPF391150C083G000","8022692785302"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",37587,37587,"Afwerkingsdop waste overloop met zijdoppen gatafdekking","Kit de cache de trop plein et enjoliveurs latéraux.","Finished cover cap for overflow waste with lateral hole plugs",845,"Dark Bronze",154,"GPF375870V221G000","8055261076396"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",54613,54613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",706,"Black Metal PVD",1495,"GPF546130P001G000","8056329070448"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",54619,54619,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaque de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","031","Chrome",877,"GPF546190G001G000","8056329540965"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",54621,54621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",706,"Black Metal PVD",1641,"GPF546211P001G000","8056329540804"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",735,"Warm Bronze PVD",783,"GPF452300P037G000","8055261645585"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",707,"Black Metal Brushed PVD",758,"GPF451300P004G000","8055261227545"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",761,"Coffee Bronze Brushed PVD",806,"GPF451310E059G000","8055261577398"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1482,"GPF451220P004G000","8056603616010"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1354,"GPF452260P024G000","8055261645905"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",713,"Antique Brass",1408,"GPF591511V204G000","8056329057630"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",706,"Black Metal PVD",1059,"GPF591531P001G000","8056329057470"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK",39100,39100,"Opbouw wastafel Ø400 mm","Cuvette de support Ø400 mm","Counter washbasin Ø400 mm",532,"Matte Black Ceramic",1158,"GPF391000C289G000","8055261228061"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",149,"Finox Brushed Nickel",178,"GPF014230G002G000","8022692791822"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",713,"Antique Brass",161,"GPF013910V204G000","8022692633467"]
["BATHROOM","GOCCIA","GOCCIA TOTAL LOOK","01377","01377","1 1/4\" sifon","Siphon 1 1/4”.","1 1/4\" syphon",713,"Antique Brass",455,"GPF013771V204G000","8022692088557"]
["BATHROOM","RILIEVO","RILIEVO",59001,59001,"Mengkraan Wastafel met waste met buigzame aansluitslangen. Patroon Ø25 mm","Mitigeur lavabo, avec vidage et flexibles de raccordement. Cartouche Ø25 mm","Basin mixer, flexible connections, with waste. Ø25 mm cartridge",708,"Copper Brushed PVD",689,"GPF590011P006G000","8056329036963"]
["BATHROOM","RILIEVO","RILIEVO",59006,59006,"Mengkraan Wastafel zonder waste met buigzame aansluitslangen. Patroon Ø35 mm","Mitigeur lavabo, sans vidage, avec flexibles de raccordement. Cartouche Ø35 mm","Basin mixer, flexible connections, without waste. Ø35 mm cartridge",735,"Warm Bronze PVD",678,"GPF590061P037G000","8056329594296"]
["BATHROOM","RILIEVO","RILIEVO",59003,59003,"Mengkraan Wastafel hoog, met waste met buigzame aansluitslangen. Patroon Ø25 mm","Mitigeur lavabo réhaussé, avec vidage et flexibles de raccordement. Cartouche Ø25 mm","High basin mixer, flexible connections, with waste. Ø25 mm cartridge",735,"Warm Bronze PVD",929,"GPF590030P037G000","8056329594357"]
["BATHROOM","RILIEVO","RILIEVO",59009,59009,"Mengkraan Wastafel hoog, met waste met buigzame aansluitslangen. Patroon Ø35 mm","Mitigeur lavabo réhaussé, avec vidage et flexibles de raccordement. Cartouche Ø35 mm","High basin mixer, flexible connections, with waste. Ø35 mm cartridge","031","Chrome",649,"GPF590091G001G000","8056329005297"]
["BATHROOM","RILIEVO","RILIEVO",59010,59010,"Mengkraan Wastafel hoog, zonder waste met buigzame aansluitslangen. Patroon Ø35 mm","Mitigeur lavabo réhaussé, sans vidage, avec flexibles de raccordement. Cartouche Ø35 mm","High basin mixer, flexible connections, without waste. Ø35 mm cartridge","030","Copper PVD",930,"GPF590101P000G000","8056329036192"]
["BATHROOM","RILIEVO","RILIEVO","54198+59087",59087,"Afbouwdeel wand gemonteerd wastafelkraan.","Partie apparente mitigeur lavabo mural.","External part wall-mounted basin mixer.",720,"Nickel PVD",795,"GPF590870P014G000","8055261193130"]
["BATHROOM","RILIEVO","RILIEVO","44697+59089",59089,"Extern deel Wandmengkraan middelgrote uitloop zonder waste","Partie apparente mitigeur mural avec bec moyen sans vidage","External parts wall-mounted mixer, medium spout, without waste",708,"Copper Brushed PVD",894,"GPF590890P006G000","8056329064362"]
["BATHROOM","RILIEVO","RILIEVO","45089+59090",59090,"Extern deel Wand 3-gats wastafelmengkraan middelgrote uitloop zonder waste","Partie apparente mitigeur lavabo mural trois sorties avec bec moyen sans vidage","External parts three-holes basin mixer with medium spout, without waste.",710,"Brass PVD",987,"GPF590900P011G000","8056329593886"]
["BATHROOM","RILIEVO","RILIEVO",59100,59100,"Wanduitloop Wastafel middelgrote uitloop","Bec de lavabo mural moyen","Wall-mounted spout basin, medium spout",279,"Matte White",453,"GPF591000C071G000","8056329034754"]
["BATHROOM","RILIEVO","RILIEVO",63499,63499,"Plafond Gemonteerd Uitloop Met Lengte Op Aanvraag. Nog Compleet Te Maken Met Separate Bediening.","Bec au plafond, longueur à la demande. A compléter avec mitigeur à commande séparée.","Ceiling-mounted spout with length on request. To be completed with separate control.",275,"Matte Cipria",1762,"GPF634990T209G000","8056603609432"]
["BATHROOM","RILIEVO","RILIEVO","46112+59109",59109,"Extern deel Wand-mengkraan 1-weg","Partie apparente pour mitigeur mural, 1 sortie.","External parts mixer one-way diverter",735,"Warm Bronze PVD",435,"GPF591090P037G000","8056329593770"]
["BATHROOM","RILIEVO","RILIEVO","46112+59109",59109,"Extern deel Wand-mengkraan 1-weg","Partie apparente pour mitigeur mural, 1 sortie.","External parts mixer one-way diverter",710,"Brass PVD",435,"GPF591090P011G000","8056329593787"]
["BATHROOM","RILIEVO","RILIEVO",59013,59013,"Externe Mengkraan bad met automatische omstelknop bad/douche","Mitigeur bain-douche mural avec inverseur automatique.","External bath mixer with automatic bath/shower diverter",720,"Nickel PVD",697,"GPF590130P014G000","8056603605939"]
["BATHROOM","RILIEVO","RILIEVO",59037,59037,"Badrandgroep 3 gaten met wateruitloop, omstelknop, buigzame slang 1,50 m en antikalk-handdouche. Omstelknop ingebouwd in de uitloop","Mélangeur bain-douche trois trous avec bec, inverseur, flexibles de raccordement 1,50m et douchette anticalcaire. Inverseur surle bec.","Three-holes bath mixer with diverter in the spout, 1,50 m flexible hose and antilimestone handshower",707,"Black Metal Brushed PVD",2016,"GPF590370P004G000","8056329035690"]
["BATHROOM","RILIEVO","RILIEVO",59127,59127,"Conus handdouchehouder met antikalk-handdouche en buigzame slang 1,50 m","Support douchette avec douchette anticacaire et flexibles 1,5m","Conical shower hook with antilimestone handshower and 1,5 m flexible",710,"Brass PVD",530,"GPF591270P011G000","8056329593749"]
["BATHROOM","RILIEVO","RILIEVO",59170,59170,"Systeem voor terugwinning water Badrand voor buigzame slang handdouche","Système de récupération de l'eau pour flexible de douchette bain-douche.","Pull-out handshower drain kit",149,"Finox Brushed Nickel",1531,"GPF591700G002G000","8056329032446"]
["BATHROOM","RILIEVO","RILIEVO",59170,59170,"Systeem voor terugwinning water Badrand voor buigzame slang handdouche","Système de récupération de l'eau pour flexible de douchette bain-douche.","Pull-out handshower drain kit",726,"Warm Bronze Brushed PVD",1791,"GPF591700P024G000","8056329029637"]
["BATHROOM","RILIEVO","RILIEVO","01080","01080","Polyethyleen badafvoer met overloopdopvuller. Lengte van de aanvoer leiding 80 cm","Vidage en polyéthylène baignoire avec trop-plein. Longueur 80 cm","Polyethylene column bath waste with overflow cap filler. Length of control cable 80 cm",726,"Warm Bronze Brushed PVD",680,"GPF010802P024G000","8056329040007"]
["BATHROOM","RILIEVO","RILIEVO",59103,59103,"Wanduitloop. Aan te vullen met afstandsbediening","Bec mural à compléter par un mitigeur à commande séparée.","Wall-mounted spout to be completed with separate control","030","Copper PVD",519,"GPF591030P000G000","8056329034563"]
["BATHROOM","RILIEVO","RILIEVO","54139+59036",59036,"Afbouwdeel wand gemonteerd douche mengkraan met diverter, water uitgang, handdouche and support.","Partie apparente mitigeur douche mural 2 voies avec inverseur et douchette.","External part wall-mounted shower mixer with diverter, water outlet, handshower and support.",279,"Matte White",875,"GPF590360C071G000","8055261193550"]
["BATHROOM","RILIEVO","RILIEVO","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",761,"Coffee Bronze Brushed PVD",396,"GPF540580E059G000","8055261602076"]
["BATHROOM","RILIEVO","RILIEVO","54055+59019",59019,"Afbouwdeel wand gemonteerd 1-weg bath/douche mengkraan.","Partie apparente mitigeur douche mural 1 voie.","External part wall-mounted one way bath/shower mixer.",279,"Matte White",348,"GPF590190C071G000","8055261193710"]
["BATHROOM","RILIEVO","RILIEVO","44655+59061",59061,"Extern deel Wand-mengkraan 1-weg","Partie apparente pour mitigeur mural, 1 sortie.","External parts mixer one-way diverter",707,"Black Metal Brushed PVD",555,"GPF590610P004G000","8056329035379"]
["BATHROOM","RILIEVO","RILIEVO","44673+59079",59079,"Extern deel Wand-Mengkraan 2-weg met automatische omstelknop bad/douche","Partie apparente mitigeur mural avec inverseur automatique bain-douche deux sorties","External parts for wall-mounted mixer two-way, automatic bath/ shower diverter",708,"Copper Brushed PVD",650,"GPF590790P006G000","8056329035263"]
["BATHROOM","RILIEVO","RILIEVO","09269+59134",59134,"Extern deel bad-/douche thermostaat 2-weg","Partie apparente pour mitigeur thermostatique douche mural 2 sorties.","External parts for thermostatic mixer, two-way diverter",149,"Finox Brushed Nickel",931,"GPF591340G002G000","8056329034020"]
["BATHROOM","RILIEVO","RILIEVO","09269+59136",59136,"Extern deel bad-/douche thermostaat 3-weg","Partie apparente pour mitigeur thermostatique douche mural 3 sorties.","External parts for thermostatic mixer, three-way diverter","030","Copper PVD",1020,"GPF591360P000G000","8056329033887"]
["BATHROOM","RILIEVO","RILIEVO","09264+63434",63434,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 2 uitgangen.","Partie externe mitigeur thermostatique mural à 2 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with two separate exits.",187,"Aged Bronze",1779,"GPF634340G052G000","8056603619073"]
["BATHROOM","RILIEVO","RILIEVO","09266+63436",63436,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 3 uitgangen.","Partie externe mitigeur thermostatique mural à 3 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with three separate exits.","030","Copper PVD",1938,"GPF634360P000G000","8056603618915"]
["BATHROOM","RILIEVO","RILIEVO","09268+63438",63438,"afbouwdelen voor wand gemonteerde thermostatische mengkraan. Verticaal/horizontaal montage met 4 uitgangen.","Partie externe mitigeur thermostatique mural à 4 sorties indépendantes. Installation verticale/horizontale.","External parts for wall-mounted thermostatic mixer. Vertical/horizontal setting up with four separate exits.",761,"Coffee Bronze Brushed PVD",2494,"GPF634380E059G000","8055261592599"]
["BATHROOM","RILIEVO","RILIEVO","44639+59140",59140,"Extern deel Wand-mengkraan douche 2-weg met omstelknop, wateraansluitpunt, houder, buigzame slang 1,50 en antikalk-handdouche","Partie apparente mitigeur douche mural deux sorties avec inverseur, alimentation de l’eau murale, support, flexibles de raccon dement 1,50 m et douchette anticalcaire","External parts for two-way built-in shower mixer with automatic diverter, water outlet, handshower hook, flexible hose and antilimestone handshower",727,"Brass Brushed PVD",1408,"GPF591400P025G000","8056329030343"]
["BATHROOM","RILIEVO","RILIEVO","44639+59141",59141,"Extern deel Wand-mengkraan douche 2-weg met omstelknop, wateraansluitpunt, houder, buigzame slang 1,50 en antikalk-handdouche","Partie apparente mitigeur douche mural deux sorties avec inverseur, alimentation de l’eau murale, support, flexibles de raccon dement 1,50 m et douchette anticalcaire","External parts for two-way built-in shower mixer with automatic diverter, water outlet, handshower hook, flexible hose and antilimestone handshower",706,"Black Metal PVD",1319,"GPF591410P001G000","8056329033436"]
["BATHROOM","RILIEVO","RILIEVO",59158,59158,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-fixing antilimestone and adjustable headshower","031","Chrome",649,"GPF591580G001G000","8056329004771"]
["BATHROOM","RILIEVO","RILIEVO",59158,59158,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-fixing antilimestone and adjustable headshower",713,"Antique Brass",1024,"GPF591580V204G000","8056329029859"]
["BATHROOM","RILIEVO","RILIEVO",59159,59159,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",726,"Warm Bronze Brushed PVD",1378,"GPF591590P024G000","8056329037731"]
["BATHROOM","RILIEVO","RILIEVO",59148,59148,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-fixing antilimestone and adjustable headshower",187,"Aged Bronze",946,"GPF591480G052G000","8056329033054"]
["BATHROOM","RILIEVO","RILIEVO",59152,59152,"Antikalk-hoofddouchekop Plafonddouche oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead",726,"Warm Bronze Brushed PVD",842,"GPF591520P024G000","8056329029996"]
["BATHROOM","RILIEVO","RILIEVO",59150,59150,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",716,"Gold Brushed PVD",1344]
["BATHROOM","RILIEVO","RILIEVO",59242,59242,"Glijstang met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Barre de douche complète avec douchette anticalcaire, flexibles 1,50 m et sortie murale coudée.","Sliding rail with antilimestone handshower, 1,50 m flexible hose and water outlet",710,"Brass PVD",704,"GPF592420P011G000","8056329593268"]
["BATHROOM","RILIEVO","RILIEVO",59123,59123,"Doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m.","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",726,"Warm Bronze Brushed PVD",450,"GPF591230P024G000","8056329030763"]
["BATHROOM","RILIEVO","RILIEVO",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",187,"Aged Bronze",1003,"GPF630990G052G000","8056329216044"]
["BATHROOM","RILIEVO","RILIEVO",59169,59169,"Wateraansluitpunt","Sortie murale coudée.","water outlet",727,"Brass Brushed PVD",238,"GPF591690P025G000","8056329029682"]
["BATHROOM","RILIEVO","RILIEVO",59157,59157,"Vaste houder voor handdouche","Support fixe pour douchette.","Fixed handshower hook",707,"Black Metal Brushed PVD",246,"GPF591570P004G000","8056329032750"]
["BATHROOM","RILIEVO","RILIEVO",59160,59160,"Oriënteerbare duplex houder voor handdouche","Support mural orientable pour douchette.","Adjustable handshower hook",708,"Copper Brushed PVD",363,"GPF591600P006G000","8056329029774"]
["BATHROOM","RILIEVO","RILIEVO",32929,32929,"Rosewood Kneipp handdouche.","Douchette Kneipp en Palissandre.","Rosewood Kneipp handshower.",713,"Antique Brass",438,"GPF329290V204G000","8055261227781"]
["BATHROOM","RILIEVO","RILIEVO",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",246,"Gold PVD",259,"GPF143720P007G000","8056329037328"]
["BATHROOM","RILIEVO","RILIEVO",14370,14370,"Antikalk-handdouche","Douchette anticalcaire.","antilimestone handshower",716,"Gold Brushed PVD",252,"GPF143700P005G000","8055261231245"]
["BATHROOM","RILIEVO","RILIEVO",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",708,"Copper Brushed PVD",346,"GPF143760P006G000","8056329701915"]
["BATHROOM","RILIEVO","RILIEVO",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",710,"Brass PVD",325,"GPF143780P011G000","8056603633208"]
["BATHROOM","RILIEVO","RILIEVO",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",720,"Nickel PVD",252,"GPF473500P014G000","8056603631709"]
["BATHROOM","RILIEVO","RILIEVO",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",761,"Coffee Bronze Brushed PVD",284,"GPF473500E059G000","8055261602724"]
["BATHROOM","RILIEVO","RILIEVO",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections","030","Copper PVD",134,"GPF287460P000G000","8056329105157"]
["BATHROOM","RILIEVO","RILIEVO",28746,28746,"Buigzame slang Cromalux lengte 2,00 m met aansluiting van 1/2\" kegelvormig","Flexible cromalux avec raccord 1/2” conique, longueur 2,00 m.","2,00 m Cromalux flexible hose with conic 1/2\" connections",187,"Aged Bronze",167,"GPF287460G052G000","8056329105218"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59501,59501,"Wand-zeepbakje wit","Porte-savon mural blanc.","Wall-mounted soap dish, white",706,"Black Metal PVD",337,"GPF595010P001G000","8056329028340"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59507,59507,"Wand-glashouder wit","Porte-verre mural blanc.","Wall-mounted holder, white",149,"Finox Brushed Nickel",355,"GPF595070G002G000","8056329028265"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59508,59508,"Wand-glashouder zwart","Porte-verre mural noir.","Wall-mounted holder, black",708,"Copper Brushed PVD",414,"GPF595080P006G000","8056329056923"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59513,59513,"Wand-dispenserhouder wit","Distributeur de savon liquide mural blanc.","Wall-mounted liquid soap dispenser , white",707,"Black Metal Brushed PVD",586,"GPF595131P004G000","8056329027916"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59519,59519,"Wand-toiletborstelhouder","Porte-balayette mural.","Wall-mounted brush holder, white",720,"Nickel PVD",498,"GPF595192P014G000","8056603477413"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59538,59538,"Staande dispenserhouder zwart","Distributeur de savon liquide à poser noir.","Standing soap dispenser holder, black",720,"Nickel PVD",417,"GPF595381P014G000","8056603477376"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59543,59543,"Staande toiletborstelhouder","Porte-balayette à poser.","Standing brush holder, white",706,"Black Metal PVD",413,"GPF595432P001G000","8056329027091"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59455,59455,"Horizontale of verticale wand-toiletrolhouder","Porte-papier mural horizontal ou vertical.","Paper-roll holder for horizontal/vertical installation",726,"Warm Bronze Brushed PVD",189,"GPF594550P024G000","8056329028449"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59415,59415,"Wand-toiletrolhouder dubbel","Porte-papier mural double.","Double wall-mounted paper roll holder",727,"Brass Brushed PVD",232,"GPF594150P025G000","8056329026629"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59397,59397,"Wand-handdoekhouder 30 cm","Porte-serviette 30 cm.","30 cm centre distance towel rail",735,"Warm Bronze PVD",252,"GPF593970P037G000","8056329593190"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59397,59397,"Wand-handdoekhouder 30 cm","Porte-serviette 30 cm.","30 cm centre distance towel rail",710,"Brass PVD",252,"GPF593970P011G000","8056329593206"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59405,59405,"Dubbele wand-handdoekhouder 60 cm","Porte-serviette mural double 60cm.","60 cm wall-mounted double towel rail",706,"Black Metal PVD",441,"GPF594050P001G000","8056329029040"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59509,59509,"Wand-handdoekhouder ringvorm","Anneau porte-serviette.","Towel ring",706,"Black Metal PVD",249,"GPF595090P001G000","8056329028067"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59549,59549,"Plank 30 Cm","Console murale 30 cm","Shelf 30 cm","031","Chrome",406,"GPF595491G001G000","8056329027039"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59521,59521,"Wand-kledinghaak","Patère.","Wall-mounted robe hook","031","Chrome",77,"GPF595210G001G000","8056329027725"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59521,59521,"Wand-kledinghaak","Patère.","Wall-mounted robe hook",735,"Warm Bronze PVD",114,"GPF595210P037G000","8056329592865"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59562,59562,"Handdoekhouder 30 cm","Porte-serviette 30 cm à fixer sur le verre.","30 cm towel rail for glass fixing",726,"Warm Bronze Brushed PVD",462,"GPF595620P024G000","8056329116085"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",59564,59564,"Handdoekhouder 45 cm","Porte-serviette 45 cm à fixer sur le verre.","45 cm towel rail for glass fixing","030","Copper PVD",446,"GPF595640P000G000","8056329115989"]
["BATHROOM","RILIEVO","RILIEVO ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",707,"Black Metal Brushed PVD",1565,"GPF584241P004G000","8056329545519"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",37584,37584,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 29463, 42117, 46757.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour les sièges 29463, 42117, 46757.","Soft-closing hardware and lateral holes plugs for WC seat 29463, 42117, 46757.",246,"Gold PVD",290,"GPF375842P007G000","8056329097582"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","09276+45230","09276","Inbouwdeel voor afsluitbare douche met mengkraan.","Partie encastrée pour douchette shut-off avec mitigeur.","Built-in part for shut-off douchette with mixer.","031","Chrome",324,"GPF092760G001G000","8055261237261"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","09276+45130","09276","Inbouwdeel voor afsluitbare douche met mengkraan.","Partie encastrée pour douchette shut-off avec mitigeur.","Built-in part for shut-off douchette with mixer.","031","Chrome",324,"GPF092760G001G000","8055261237261"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",710,"Brass PVD",711,"GPF451300P011G000","8055261227507"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",716,"Gold Brushed PVD",807,"GPF451310P005G000","8055261227354"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1309,"GPF451240E059G000","8055261577459"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1230,"GPF451260P004G000","8056603632928"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",299,"Matte Black",967,"GPF144310C072G000","8055261646162"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",707,"Black Metal Brushed PVD",1029,"GPF143313P004G000","8056329192676"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",707,"Black Metal Brushed PVD",1127,"GPF591531P004G000","8056329057456"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1482,"GPF451220P025G000","8056603615952"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",54611,54611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12","030","Copper PVD",930,"GPF546110P000G000","8056329070608"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",54613,54613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",276,"Matte Agave",1364,"GPF546130T210G000","8056603588140"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",276,"Matte Agave",807,"GPF546150T210G000","8056603588096"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",246,"Gold PVD",1003,"GPF546150P007G000","8056329070233"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",54617,54617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",187,"Aged Bronze",988,"GPF546170G052G000","8056329098831"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",54619,54619,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaque de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",845,"Dark Bronze",1386,"GPF546190V221G000","8056603637701"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",54599,54599,"Afvoerplug \"Stop&Go\"","Bonde de lavabo “Stop & Go” 2 en 1 : un mécanisme d'ouverture et de fermeture dévissable et remplaçable avec un mécanisme toujours ouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",299,"Matte Black",199,"GPF545990C072G000","8056329228856"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK",54599,54599,"Afvoerplug \"Stop&Go\"","Bonde de lavabo “Stop & Go” 2 en 1 : un mécanisme d'ouverture et de fermeture dévissable et remplaçable avec un mécanisme toujours ouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",708,"Copper Brushed PVD",194,"GPF545990P006G000","8022692841800"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",708,"Copper Brushed PVD",161,"GPF013910P006G000","8022692883138"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.","031","Chrome",92,"GPF014230G001G000","8022692037562"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",149,"Finox Brushed Nickel",105,"GPF013760G002G000","8022692854039"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.","031","Chrome",90,"GPF014200G001G000","8022692033304"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",246,"Gold PVD",260,"GPF014200P007G000","8056329068698"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",727,"Brass Brushed PVD",84,"GPF013460P025G000","8056329184220"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","01377","01377","1 1/4\" sifon","Siphon 1 1/4”.","1 1/4\" syphon",187,"Aged Bronze",455,"GPF013771G052G000","8056329051744"]
["BATHROOM","RILIEVO","RILIEVO TOTAL LOOK","01411","01411","Onderbouwmengkraan met filter en 1/2\" aansluiting","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection",726,"Warm Bronze Brushed PVD",240,"GPF014110P024G000","8056329002562"]
["BATHROOM","EQUILIBRIO","EQUILIBRIO","52001+52002",52001,"Mengkraan Wastafel","Mitigeur lavabo","Basin mixer",722,"Materic Black Metal PVD",1112,"GPF520011P018G000","8022692690996"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",35173,35173,"Thermostatische Wand-Mengkraan met hoofddouchekop, automatische omstelknop bad/douche, buigzame slang 1,50 m, glijstang en antikalk-handdouche.","Colonne de douche THERMOSTATIQUE avec pomme de douche Ø200, inverseur automatique, support orientable sur barre de douche, flexibles 1,50 m et douchette anticalcaire.","Wall-mounted thermostatic mixer with Ø200 showerhead, automatic bath/shower diverter, 1,50 m flexible hose, sliding rail and antilimestone handshower.",708,"Copper Brushed PVD",2396,"GPF351730P006G000","8056329516106"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",35175,35175,"Thermostatische Wand-Mengkraan met hoofddouchekop, automatische omstelknop bad/douche, buigzame slang 1,50 m, glijstang en antikalk-handdouche","Colonne de douche THERMOSTATIQUE avec pomme de douche Ø250, inverseur automatique, support orientable sur barre de douche, flexibles 1,50 m et douchette anticalcaire.","Wall-mounted thermostatic shower column with Ø250 showerhead, automatic diverter, 1,50 m flexible hose, and antilimestone handshower",727,"Brass Brushed PVD",2518,"GPF351750P025G000","8056329515970"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",35177,35177,"Thermostatische Wand-Mengkraan met hoofddouchekop, automatische omstelknop bad/douche, buigzame slang 1,50 m, glijstang en antikalk-handdouche","Colonne de douche THERMOSTATIQUE avec pomme de douche Ø300, inverseur automatique, support orientable sur barre de douche, flexibles 1,50 m et douchette anticalcaire.","Wall-mounted thermostatic shower column with Ø300 showerhead, automatic diverter, 1,50 m flexible hose, and antilimestone handshower","030","Copper PVD",3024,"GPF351770P000G000","8056329515925"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",23447,23447,"Thermostatische Wand-Mengkraan met hoofddouchekop, automatische omstelknop bad/douche, buigzame slang 1,50 m en antikalk-handdouche","Mitigeur thermostatique mural avec pomme de douche, inverseur automatique, flexibles 1,50 m et douchette anticalcaire.","Wall-mounted thermostatic mixer with Ø306 showerhead, automatic bath/shower diverter, 1,50 m flexible hose and antilimestone handshower",720,"Nickel PVD",4871,"GPF234471P014G000","8055261113695"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",33095,33095,"Wand-hoofddouchekop","Pomme de douche murale.","Wall-mounted shower head",238,"Mirror Steel",2499,"GPF330951A001G000","8022692365436"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",66156,66156,"Verstelbare hoofddouche aan de muur.","Bec complet","Wall-mounted adjustable headshower.",845,"Dark Bronze",1494,"GPF661560V221G000","8055261232518"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",66158,66158,"Multi-functionele wandgemonteerde douche","Pomme de douche murale multifonction","Multifunction wall-mounted jet",707,"Black Metal Brushed PVD",1494,"GPF661580P004G000","8056603883016"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",54149,54149,"wandgemonteerde verstelbare hoofddouche","Pomme de douche au plafond orientable","Wall-fixing adjustable showerhead",761,"Coffee Bronze Brushed PVD",2338,"GPF541490E059G000","8055261601321"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",63348,63348,"Oriënteerbare wand-hoofddouchekop","Pomme de douche latérale orientable.","Wall-mounted adjustable showerhead","031","Chrome",572,"GPF633480G001G000","8056329552463"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",59148,59148,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-fixing antilimestone and adjustable headshower",246,"Gold PVD",1010,"GPF591480P007G000","8056329030060"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",58248,58248,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-fixing antilimestone and adjustable headshower",246,"Gold PVD",1867,"GPF582480P007G000","8056329066533"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",54148,54148,"Oriënteerbare wand-hoofddouchekop","Pomme de douche orientable anticalcaire avec bras mural.","Wall-mounted adjustable showerhead",761,"Coffee Bronze Brushed PVD",2931,"GPF541481E059G000","8055261601345"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",59158,59158,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-fixing antilimestone and adjustable headshower",706,"Black Metal PVD",961,"GPF591580P001G000","8056329032675"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",59158,59158,"Oriënteerbare antikalk-wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-fixing antilimestone and adjustable headshower",761,"Coffee Bronze Brushed PVD",1091,"GPF591580E059G000","8055261594098"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",54151,54151,"plafond-gemonteerde verstelbare hoofddouche","Pomme de douche au plafond orientable","Ceiling-mounted adjustable showerhead",239,"Steel Brushed",1080,"GPF541510A000G000","8056603563338"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",63352,63352,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable shower head",246,"Gold PVD",852,"GPF633520P007G000","8056603637336"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",59152,59152,"Antikalk-hoofddouchekop Plafonddouche oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead",727,"Brass Brushed PVD",842,"GPF591520P025G000","8056329029989"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",54146,54146,"Verstelbare plafonddouche.","Pomme de douche au plafond orientable","Ceiling-mounted adjustable headshower.",761,"Coffee Bronze Brushed PVD",2142,"GPF541460E059G000","8055261601383"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",54152,54152,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable showerhead",727,"Brass Brushed PVD",2414,"GPF541521P025G000","8056329068988"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",59155,59155,"Antikalk-hoofddouchekop Plafonddouche oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead",246,"Gold PVD",979,"GPF591550P007G000","8056329029941"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",15186,15186,"Antikalk-hoofddouchekop plafond oriënteerbaar","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable and antilimestone showerhead",246,"Gold PVD",2657,"GPF151860P007G000","8056329631427"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",58150,58150,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",761,"Coffee Bronze Brushed PVD",1957,"GPF581500E059G000","8055261595675"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",54153,54153,"plafond-gemonteerde verstelbare hoofddouche, lengte op verzoek","Pomme de douche au plafond orientable. Longueur à la demande","Ceiling-mounted adjustable showerhead with custom length",761,"Coffee Bronze Brushed PVD",2481,"GPF541530E059G000","8055261601246"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",63350,63350,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted showerhead, length on request",727,"Brass Brushed PVD",1122,"GPF633500P025G000","8056329591776"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",58250,58250,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",727,"Brass Brushed PVD",2452,"GPF582500P025G000","8056329069138"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",20150,20150,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",707,"Black Metal Brushed PVD",2775,"GPF201500P004G000","8022692220292"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",20150,20150,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",716,"Gold Brushed PVD",2953,"GPF201500P005G000","8055261231184"]
["BATHROOM","MINIMALISTIC SHOWER","MINIMALISTIC SHOWER",59159,59159,"Antikalk-hoofddouchekop plafond arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted antilimestone showerhead, length on request",761,"Coffee Bronze Brushed PVD",1468,"GPF591590E059G000","8055261594074"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63601,63601,"witte wandgemonteerde soap houder","Porte-savon mural blanc","Wall-mounted white soap holder",845,"Dark Bronze",312,"GPF636010V221G000","8056603637305"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66401,66401,"wandgemonteerde witte zeep dispenser","Porte-savon mural blanc","Wall-mounted soap dish, white",279,"Matte White",305,"GPF664010C071G000","8056603638524"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63602,63602,"zwarte wandgemonteerde soap houder","Porte-savon mural noir","Wall-mounted black soap holder",727,"Brass Brushed PVD",312,"GPF636020P025G000","8056329590595"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66402,66402,"wandgemonteerde zwarte zeep dispenser","Porte-savon mural noir","Wall-mounted soap dish, black",187,"Aged Bronze",356,"GPF664020G052G000","8056603638449"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63607,63607,"witte wandgemonteerde beker houder","Porte-verre mural blanc","Wall-mounted white tumbler holder",710,"Brass PVD",320,"GPF636070P011G000","8056329590564"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66407,66407,"wandgemonteerde witte beker houder","Porte-verre mural blanc","Wall-mounted holder, white",727,"Brass Brushed PVD",415,"GPF664070P025G000","8056603565707"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66408,66408,"wandgemonteerde zwarte beker houder","Porte-verre mural noir","Wall-mounted holder, black",726,"Warm Bronze Brushed PVD",415,"GPF664080P024G000","8056603565615"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63613,63613,"witte wandgemonteerde soap","Distributeur de savon liquide mural blanc","Wall-mounted white dispenser",726,"Warm Bronze Brushed PVD",557,"GPF636130P024G000","8056329547674"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66413,66413,"wandgemonteerde witte zeep houder","Distributeur de savon liquide mural blanc","Wall-mounted liquid soap dispenser , white","030","Copper PVD",622,"GPF664130P000G000","8056603638227"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63614,63614,"zwarte wandgemonteerde soap dispenser","Distributeur de savon liquide mural noir","Wall-mounted black dispenser",299,"Matte Black",476,"GPF636140C072G000","8056329547650"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66414,66414,"wandgemonteerde zwarte zeep houder","Distributeur de savon liquide mural noir","Wall-mounted liquid soap dispenser - black",707,"Black Metal Brushed PVD",663,"GPF664140P004G000","8056603565448"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66419,66419,"wandgemonteerde witte borstel houder","Porte-balayette mural blanc","Wall-mounted brush holder, white",149,"Finox Brushed Nickel",600,"GPF664190G002G000","8056603565363"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63620,63620,"zwarte wandgemonteerde borstel houder","Porte-balayette mural noir","Wall-mounted black toilet brush holder",708,"Copper Brushed PVD",532,"GPF636200P006G000","8056603452762"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63620,63620,"zwarte wandgemonteerde borstel houder","Porte-balayette mural noir","Wall-mounted black toilet brush holder",279,"Matte White",454,"GPF636200C071G000","8056603467063"]
["BATHROOM","ACCESSORIES","ACCESSORIES",58525,58525,"Witte Staande Zeephouder","Porte-savon à poser blanc","Standing soap holder, white","030","Copper PVD",357,"GPF585250P000G000","8022692861389"]
["BATHROOM","ACCESSORIES","ACCESSORIES",58526,58526,"Zwarte Witte Staande Zeephouder","Porte-savon à poser noir","Standing soap holder, black",246,"Gold PVD",406,"GPF585260P007G000","8056329062252"]
["BATHROOM","ACCESSORIES","ACCESSORIES",58531,58531,"Witte Staande Bekerhouder","Porte-verre à poser blanc.","Standing tumbler holder, white",246,"Gold PVD",444,"GPF585310P007G000","8022692860634"]
["BATHROOM","ACCESSORIES","ACCESSORIES",58532,58532,"Zwarte Staande Bekerhouder","Porte-verre à poser noir","Standing tumbler holder, black",299,"Matte Black",356,"GPF585320C072G000","8056329062238"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66437,66437,"staande witte zeep dispenser","Distributeur de savon liquide à poser blanc","Standing soap dispenser holder, white",726,"Warm Bronze Brushed PVD",589,"GPF664370P024G000","8056603572989"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63743,63743,"Staande toiletborstelhouder wit","Porte-balayette à poser blanche.","Standing brush holder, white",706,"Black Metal PVD",464,"GPF637430P001G000","8056329566927"]
["BATHROOM","ACCESSORIES","ACCESSORIES",58543,58543,"Witte Staande Borstelhouder","Porte-balayette à poser blanche","Standing brush holder, white",706,"Black Metal PVD",688,"GPF585431P001G000","8022692862195"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63744,63744,"Staande toiletborstelhouder zwart","Porte-balayette a poser noir","Standing brush holder, black",706,"Black Metal PVD",464,"GPF637440P001G000","8056329566811"]
["BATHROOM","ACCESSORIES","ACCESSORIES",58544,58544,"Zwarte Staande Borstelhouder","Porte-balayette à poser noir.","Standing brush holder, black","031","Chrome",467,"GPF585441G001G000","8056329062009"]
["BATHROOM","ACCESSORIES","ACCESSORIES",58544,58544,"Zwarte Staande Borstelhouder","Porte-balayette à poser noir.","Standing brush holder, black",845,"Dark Bronze",734,"GPF585441V221G000","8056603621960"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63655,63655,"wandgemonteerde paper roll houder","Porte-papier mural","Wall-mounted paper roll holder",761,"Coffee Bronze Brushed PVD",205,"GPF636550E059G000","8055261591387"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63697,63697,"30 cm Handdoekhouder","Porte-serviette 30 cm","30 cm Towel rail",713,"Antique Brass",262,"GPF636971V204G000","8056329560178"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63700,63700,"45 cm Handdoekhouder","Porte-serviette 45 cm","45 cm Towel rail",149,"Finox Brushed Nickel",271,"GPF637001G002G000","8056329546936"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63700,63700,"45 cm Handdoekhouder","Porte-serviette 45 cm","45 cm Towel rail",246,"Gold PVD",338,"GPF637001P007G000","8056603637015"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63703,63703,"60 cm Handdoekhouder","Porte-serviette 60 cm","60 cm Towel rail",710,"Brass PVD",324,"GPF637031P011G000","8056329590281"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63703,63703,"60 cm Handdoekhouder","Porte-serviette 60 cm","60 cm Towel rail",845,"Dark Bronze",346,"GPF637031V221G000","8056603636964"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63709,63709,"Handdoek ring","Anneau porte-serviette","Wall ring towel holder",708,"Copper Brushed PVD",338,"GPF637090P006G000","8056603452458"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63621,63621,"Wand-kledinghaak","Patère.","Wall-mounted robe hook",761,"Coffee Bronze Brushed PVD",127,"GPF636210E059G000","8055261591400"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66523,66523,"wand gemonteerde badjas haak.","Patère murale","Wall-mounted robe hook.",706,"Black Metal PVD",202,"GPF665230P001G000","8056603632805"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66511,66511,"30 cm Handdoekhouder voor glasmontage","Porte-serviette 30 cm à fixer sur le verre","30 cm Towel rail for glass fixing",299,"Matte Black",923,"GPF665110C072G000","8056603564786"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66511,66511,"30 cm Handdoekhouder voor glasmontage","Porte-serviette 30 cm à fixer sur le verre","30 cm Towel rail for glass fixing",187,"Aged Bronze",1081,"GPF665110G052G000","8056603636544"]
["BATHROOM","ACCESSORIES","ACCESSORIES",63726,63726,"45 cm Handdoekhouder voor glasmontage","Poignée et porte-serviette pour verre 45 cm","45 cm Towel rail for glass fixing",761,"Coffee Bronze Brushed PVD",655,"GPF637261E059G000","8055261574267"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66513,66513,"45 cm Handdoekhouder voor glasmontage","Porte-serviette 45 cm à fixer sur le verre","45 cm Towel rail for glass fixing",726,"Warm Bronze Brushed PVD",1280,"GPF665130P024G000","8056603564618"]
["BATHROOM","ACCESSORIES","ACCESSORIES",66515,66515,"60 cm Handdoekhouder voor glasmontage","Porte-serviette 60 cm à fixer sur le verre","60 cm Towel rail for glass fixing","031","Chrome",829,"GPF665150G001G000","8056603564571"]
["BATHROOM","ACCESSORIES","ACCESSORIES",45590,45590,"Papierbak wit","Poubelle blanche.","White waste-paper basket",279,"Matte White",734,"GPF455900C071G000","8022692815146"]
["BATHROOM","ACCESSORIES","ACCESSORIES",58424,58424,"Staande handgreep voor bad/douche 45 cm","Poignée de soutien pour baignoire/douche 45 cm.","Safety grip handle for bathtub and shower enclosure, 45 cm lenght.",845,"Dark Bronze",1565,"GPF584241V221G000","8056603637466"]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63745,63745,"Verstelbare hoofddouche voor wandmontage. RIGATO","Pomme de douche murale orientable. RIGATO","Wall-mounted adjustable headshower. RIGATO","031","Chrome",1584,"GPF637450G001G000","8055261728677"]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63645,63645,"Verstelbare hoofddouche voor wandmontage. DIAMANTATO","Pomme de douche murale orientable. DIAMANTATO","Wall-mounted adjustable headshower. DIAMANTATO",299,"Matte Black",2140,"GPF636450C072G000","8055261729216"]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63050,63050,"Verstelbare hoofddouche voor montage aan het plafond.","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",735,"Warm Bronze PVD",1616,"GPF630500P037G000","8055261729414"]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63053,63053,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag.","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.","030","Copper PVD",2101,"GPF630530P000G000","8055261729322"]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63753,63753,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. RIGATO","Pomme de douche au plafond orientable, longueur à la demande. RIGATO","Ceiling-mounted adjustable headshower, length on request. RIGATO",706,"Black Metal PVD",3040,"GPF637530P001G000","8055261728295"]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63653,63653,"Verstelbare hoofddouche voor montage aan het plafond, lengte op aanvraag. DIAMANTATO","Pomme de douche au plafond orientable, longueur à la demande. DIAMANTATO","Ceiling-mounted adjustable headshower, length on request. DIAMANTATO",726,"Warm Bronze Brushed PVD",3245,"GPF636530P024G000","8055261728752"]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.","031","Chrome",1488]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63049,63049,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",845,"Dark Bronze",2352]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63449,63449,"Verstelbare hoofddouche aan de muur. DIAMANTATO.","Pomme de douche latérale orientable. DIAMANTATO.","Wall-mounted adjustable headshower. DIAMANTATO.",708,"Copper Brushed PVD",3179,"GPF634490P006G000","8055261242234"]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63068,63068,"Oriënteerbare wand-hoofddouchekop","Pomme de douche murale orientable.","Wall-mounted adjustable headshower.",706,"Black Metal PVD",2383]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63568,63568,"Verstelbare hoofddouche aan de muur. RIGATO.","Pomme de douche latérale orientable. RIGATO.","Wall-mounted adjustable headshower. RIGATO.",735,"Warm Bronze PVD",3158,"GPF635680P037G000","8055261241435"]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",66072,66072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",706,"Black Metal PVD",2202]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",66072,66072,"Oriënteerbare plafond-hoofddouchekop","Pomme de douche au plafond orientable.","Ceiling-mounted adjustable headshower.",727,"Brass Brushed PVD",2352]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63572,63572,"Verstelbare plafonddouche. RIGATO.","Pomme de douche au plafond orientable. RIGATO.","Ceiling-mounted adjustable headshower. RIGATO.",727,"Brass Brushed PVD",3179,"GPF635720P025G000","8055261241145"]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",66070,66070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.",149,"Finox Brushed Nickel",2824]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63070,63070,"Plafond-hoofddouchekop arm aanpasbare hoogte","Pomme de douche au plafond orientable, longueur à la demande.","Ceiling-mounted adjustable headshower, length on request.","031","Chrome",2092]
["BATHROOM","TONDO SHOWER","TONDO SHOWER",63570,63570,"Verstelbare plafonddouche. lengte op aanvraag. RIGATO.","Pomme de douche au plafond avec bras orientable, longueur à la demande. RIGATO.","Ceiling-mounted adjustable headshower. Length on request. RIGATO.","030","Copper PVD",3872,"GPF635700P000G000","8055261241367"]
["HOME DECOR","HOME FRAGRANCES","HOME FRAGRANCES",68605,68605,"3000 ml Diffuser en parfum DIAMANTATO","Diffuseur et parfums d'ambiance DIAMANTATO 3000 ml","3000 ml Diffuser and fragrance DIAMANTATO",707,"Black Metal Brushed PVD",4481,"GPF686050P004G000","8056603563956"]
["HOME DECOR","HOME FRAGRANCES","HOME FRAGRANCES",68205,68205,"3000 ml Diffuser en parfum MECCANICA","Diffuseur et parfums d'ambiance MECCANICA 3000 ml","3000 ml Diffuser and fragrance MECCANICA",726,"Warm Bronze Brushed PVD",4481,"GPF682050P024G000","8056603564182"]
["HOME DECOR","HOME FRAGRANCES","HOME FRAGRANCES",68718,68718,"geurfles kist. RIGATO","Coffret parfum. RIGATO","Fragrance casket. RIGATO",726,"Warm Bronze Brushed PVD",820,"GPF687180P024G000","8056603580403"]
["HOME DECOR","HOME VASES","HOME VASES",68515,68515,"vaas RIGATO d.100 h.300 mm","Vase RIGATO d.100 h.300 mm","Vase RIGATO d.100 h.300 mm",726,"Warm Bronze Brushed PVD",1268,"GPF685150P024G000","8056603574266"]
["HOME DECOR","HOME VASES","HOME VASES",68617,68617,"vaas DIAMANTATO d.100 h.370 mm","Vase DIAMANTATO d.100 h.370 mm","Vase DIAMANTATO d.100 h.370 mm",726,"Warm Bronze Brushed PVD",1397,"GPF686170P024G000","8056603574129"]
["HOME DECOR","HOME VASES","HOME VASES",68217,68217,"vaas MECCANICA d.100 h.370 mm","Vase MECCANICA d.100 h.370 mm","Vase MECCANICA d.100 h.370 mm",726,"Warm Bronze Brushed PVD",1397,"GPF682170P024G000","8056603574600"]
["HOME DECOR","HOME VASES","HOME VASES",68734,68734,"Vaas kist. TRAME","Coffret vase. TRAME","Vase casket. TRAME",707,"Black Metal Brushed PVD",1306,"GPF687340P004G000","8056603580335"]
["PILLAR TAPS","PILLAR TAPS","PILLAR TAPS","00915","00915","Draaibare enkele waterkraan","Robinet à bec pivotant","Rotating single water tap",299,"Matte Black",280,"GPF009150C072G000","8056329012042"]
["PRIVATE WELLNESS","HI-FI","HI-FI","63001+63004",63004,"Extern deel bad-/douche thermostaat 2-weg, met drukknop aan / uit controle.","Partie apparente pour mitigeur thermostatique deux fonctions avec touche on/off","External parts for thermostatic mixer for two separate functions, with push-button on/off controls.",299,"Matte Black",1672,"GPF630040C072G000","8056329219885"]
["PRIVATE WELLNESS","HI-FI","HI-FI","63001+63006",63006,"Extern deel bad-/douche thermostaat 3-weg, met drukknop aan / uit controle.","Partie apparente pour mitigeur thermostatique trois fonctions avec touche on/off","External parts for thermostatic mixer for three separate functions, with push-button on/off controls.",716,"Gold Brushed PVD",2181,"GPF630060P005G000","8056603551083"]
["PRIVATE WELLNESS","HI-FI","HI-FI","63011+63012",63012,"Extern deel Thermostatische wand-mengkraan 2 onafhankelijke uitgangen, met drukknop aan / uit controle.","Partie apparente pour mitiguer thermostatique deux fonctions avec touche on/off","External parts for thermostatic mixer for two separate functions, with push-button on/off controls.",710,"Brass PVD",2299,"GPF630120P011G000","8056329592483"]
["PRIVATE WELLNESS","HI-FI","HI-FI","63013+63014",63014,"Extern deel Thermostatische wand-mengkraan 3 onafhankelijke uitgangen, met drukknop aan / uit controle.","Partie apparente pour mitiguer thermostatique trois fonctions avec touche on/off","External parts for thermostatic mixer for three separate functions, with push-button on/off controls.",149,"Finox Brushed Nickel",2468,"GPF630140G002G000","8056329219083"]
["PRIVATE WELLNESS","HI-FI","HI-FI","63015+63016",63016,"Extern deel Thermostatische wand-mengkraan 4 onafhankelijke uitgangen, met drukknop aan / uit controle.","Partie apparente pour mitiguer thermostatique quatre fonctions avec touche on/off","External parts for thermostatic mixer for four separate functions, with push-button on/off controls.",726,"Warm Bronze Brushed PVD",3384,"GPF630160P024G000","8056329218703"]
["PRIVATE WELLNESS","HI-FI","HI-FI","63021+63022",63022,"Extern deel Thermostatisch schap wandmontage 2 onafhankelijke uitgangen, met drukknop aan / uit controle.","Partie apparente pour mitiguer thermostatique avec support tablette, deux fonctions avec touche on/off. Support tablette en cr ystal trempé noir.","External parts for thermostatic shelf mixer for two separate functions, with push-button on/off controls. Shelf made of black frosted safety glass.",299,"Matte Black",3518,"GPF630220C072G000","8056329218345"]
["PRIVATE WELLNESS","HI-FI","HI-FI","63023+63024",63024,"Extern deel Thermostatisch schap wandmontage 3 onafhankelijke uitgangen, met drukknop aan / uit controle.","Partie apparente pour mitiguer thermostatique avec support tablette, trois fonctions avec touche on/off. Support tablette en c rystal trempé noir.","External parts for thermostatic shelf mixer for three separate functions, with push-button on/off controls. Shelf made of blackfrosted safety glass.",727,"Brass Brushed PVD",4266,"GPF630240P025G000","8056329217904"]
["PRIVATE WELLNESS","HI-FI","HI-FI","63025+63026",63026,"Extern deel Thermostatisch schap wandmontage 4 onafhankelijke uitgangen, met drukknop aan / uit controle.","Partie apparente pour mitiguer thermostatique avec support tablette, quatre fonctions avec touche on/off. Support tablette en crystal trempé noir.","External parts for thermostatic shelf mixer for four separate functions, with push-button on/off controls. Shelf made of black frosted safety glass.",720,"Nickel PVD",4939,"GPF630260P014G000","8056603605465"]
["PRIVATE WELLNESS","HI-FI","HI-FI","63027+63028",63028,"Extern deel Thermostatisch schap wandmontage 5 onafhankelijke uitgangen, met drukknop aan / uit controle.","Partie apparente pour mitiguer thermostatique avec support tablette, cinq fonctions avec touche on/off. Support tablette en cr ystal trempé noir.","External parts for thermostatic shelf mixer for five separate functions, with push-button on/off controls. Shelf made of black frosted safety glass.",710,"Brass PVD",5165,"GPF630280P011G000","8056329592414"]
["PRIVATE WELLNESS","HI-FI","HI-FI","63055+63079",63079,"Extern deel Wand-Mengkraan 2-weg, met drukknop aan / uit controle.","Partie apparente pour mitiguer monocommande deux fonctions avec touche on/off","External parts for single-lever mixer for two separate functions, with push-button on/off controls.",708,"Copper Brushed PVD",1574,"GPF630790P006G000","8056329216440"]
["PRIVATE WELLNESS","HI-FI","HI-FI",63099,63099,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m Cromalux","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m Cromalux.","Magnetic shower set with water outlet, 1,50 m Cromalux flexible hose and antilimestone handshower",708,"Copper Brushed PVD",1003,"GPF630990P006G000","8056329215962"]
["PRIVATE WELLNESS","HI-FI","HI-FI",63199,63199,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en Darkflex buigzame slang 1,50 m","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et Darkflex flexibles 1,50 m.","Magnetic shower set with water outlet, 1,50 m Darkflex flexible hose and antilimestone handshower",710,"Brass PVD",940,"GPF631990P011G000","8056329592339"]
["PRIVATE WELLNESS","HI-FI","HI-FI",63057,63057,"Oriënteerbare duplex houder voor handdouche","Support mural orientable pour douchette.","Adjustable handshower hook",735,"Warm Bronze PVD",893,"GPF630570P037G000","8056329558236"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02766","SP02766","Plaat met REGEN-symbool. Aanpasbaar met artikel 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Plaque avec symbole PLUIE. Adaptable à l'article 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Push-botton plate with RAINFALL symbol. To be combined with art. 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026,63028, 63061, 63079, 63041, 63043.",707,"Black Metal Brushed PVD",193,"GSP027660P004G000","8056329526570"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02767","SP02767","Plaat met CASCADE-symbool. Aanpasbaar met artikel 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Plaque avec symbole CASCADE. Adaptable à l'article 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061,63079, 63041, 63043.","Push-botton plate with WATERFALL symbol. To be combined with art. 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026,63028, 63061, 63079, 63041, 63043.","030","Copper PVD",181,"GSP027670P000G000","8056329526457"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02768","SP02768","Plaat met VERNEVELING-symbool. Aanpasbaar met artikel 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Plaque avec symbole BRUMISATION. Adaptable à l'article 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Push-botton plate with ATOMIZER symbol. To be combined with art. 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026,63028, 63061, 63079, 63041, 63043.",708,"Copper Brushed PVD",193,"GSP027680P006G000","8056329526273"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02770","SP02770","Plaat met hoofddouchekop symbool. Aanpasbaar met artikel 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Plaque avec symbole JETS LATERAUX. Adaptable à l'article 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Push-botton plate with BODY JETS symbol. To be combined with art. 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026,63028, 63061, 63079, 63041, 63043.",735,"Warm Bronze PVD",181,"GSP027700P037G000","8056329558106"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02771","SP02771","Plaat met VAN symbool. Aanpasbaar met artikel 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Plaque avec symbole BAIGNOIRE. Adaptable à l'article 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Push-botton plate with BATHTUB symbol. To be combined with art. 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.",246,"Gold PVD",210,"GSP027710P007G000","8056329529298"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02772","SP02772","Plaat met Wanduitloop Bad symbool. Aanpasbaar met artikel 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028,63061, 63079, 63041, 63043.","Plaque avec symbole BEC BAIGNOIRE. Adaptable à l'article 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Push-botton plate with FOOT SPOUT symbol. To be combined with art. 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.",720,"Nickel PVD",181,"GSP027720P014G000","8056603504799"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02773","SP02773","Plaat met WATER RUBE KNEIPP symbool. Aanpasbaar met artikel 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Plaque avec symbole WATER TUBE KNEIPP. Adaptable à l'article 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Push-botton plate with WATER TUBE KNEIPP symbol. To be combined with art. 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.",716,"Gold Brushed PVD",210,"GSP027730P005G000","8056329525580"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02783","SP02783","Plaat met WAND VERNEVELING-symbool. Aanpasbaar met artikel 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028,63061, 63079, 63041, 63043.","Plaque avec symbole BRUMISATION MURALE. Adaptable à l'article 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.","Push-botton plate with WALL-MOUNTED ATOMIZER symbol. To be combined with art. 63002, 63004, 63012, 63014, 63016, 63018, 63022, 63024, 63026, 63028, 63061, 63079, 63041, 63043.",707,"Black Metal Brushed PVD",163,"GSP027830P004G000","8056329524194"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02774","SP02774","Plaat met REGEN-symbool voor 63006, 63081","Plaque avec symbole PLUIE pour 63006 et 63081","Push-botton plate with RAINFALL symbol, for items 63006 and 63081.","030","Copper PVD",153,"GSP027740P000G000","8056329525474"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02774","SP02774","Plaat met REGEN-symbool voor 63006, 63081","Plaque avec symbole PLUIE pour 63006 et 63081","Push-botton plate with RAINFALL symbol, for items 63006 and 63081.",246,"Gold PVD",178,"GSP027740P007G000","8056329529236"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02776","SP02776","Plaat met VERNEVELING-symbool voor 63006, 63081","Plaque avec symbole BRUMISATION pour 63006 et 63081","Push-botton plate with ATOMIZER symbol, for items 63006 and 63081.",149,"Finox Brushed Nickel",140,"GSP027760G002G000","8056329525221"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02777","SP02777","Plaat met DOUCHESET symbool voor 63006, 63081","Plaque avec symbole ENSEMBLE DOUCHETTE pour 63006 et 63081","Push-botton plate with HANDSHOWER symbol, for items 63006 and 63081.",761,"Coffee Bronze Brushed PVD",184,"GSP027770E059G000","8055261581487"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02779","SP02779","Plaat met VAN symbool voor 63006, 63081","Plaque avec symbole BAIGNOIRE pour 63006 et 63081","Push-botton plate with BATHTUB symbol, for items 63006 and 63081.",720,"Nickel PVD",153,"GSP027790P014G000","8056603504720"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02780","SP02780","Plaat met Wanduitloop Bad symbool voor 63006, 63081","Plaque avec symbole BEC BAIGNOIRE pour 63006 et 63081","Push-botton plate with FOOT SPOUT symbol, for items 63006 and 63081.","031","Chrome",103,"GSP027800G001G000","8056329524675"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02780","SP02780","Plaat met Wanduitloop Bad symbool voor 63006, 63081","Plaque avec symbole BEC BAIGNOIRE pour 63006 et 63081","Push-botton plate with FOOT SPOUT symbol, for items 63006 and 63081.",845,"Dark Bronze",163,"GSP027800V221G000","8056603634588"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02781","SP02781","Plaat met WATER RUBE KNEIPP symbool voor 63006, 63081","Plaque avec symbole WATER TUBE KNEIPP pour 63006 et 63081","Push-botton plate with WATER TUBE KNEIPP symbol, for items 63006 and 63081.",761,"Coffee Bronze Brushed PVD",184,"GSP027810E059G000","8055261581401"]
["PRIVATE WELLNESS","HI-FI","HI-FI","SP02784","SP02784","Plaat met WAND CASCADE-symbool voor 63006, 63081","Plaque avec symbole CASCADE MURALE pour 63006 et 63081","Push-botton plate with WALL-MOUNTED WATERFALL symbol, for items 63006 and 63081.",761,"Coffee Bronze Brushed PVD",184,"GSP027840E059G000","8055261581340"]
["PRIVATE WELLNESS","HI-FI","HI-FI ORIGINI","63013+66224",66224,"Afbouwdeel Voor Thermostatische Mengkraan Drie Gelijktijdige Functies, Met Druk Knop Aan/Uit Bediening. Combineerbaar met verschillende afwerkingen met inleg 66600 of inleg art 66602","Partie apparente pour mitiguer thermostatique trois fonctions avectouche on/off. Combiner avec finitions differentes avec insert66600 ou insert ART 66602","External parts for thermostatic mixer for three separate functions, with push-button on/off controls. Can be combined with inserts with different finishes: art. 66600 and art. 66602.",708,"Copper Brushed PVD",2888,"GPF662240P006G000","8056603581097"]
["PRIVATE WELLNESS","HI-FI","HI-FI ORIGINI",66600,66600,"inleg","Insert","Insert","031","Chrome",65,"GPF666000G001G000","8056603572842"]
["PRIVATE WELLNESS","HI-FI","HI-FI ORIGINI",66602,66602,"inleg ART","Insert ART","Insert ART",290,"Materic",117,"GPF666020T219G000","8056603613897"]
["PRIVATE WELLNESS","HI-FI","HI-FI ORIGINI",66604,66604,"Kit 5 inleg","Kit 5 inserts","Kit 5 Insert",720,"Nickel PVD",410,"GPF666040P014G000","8056603626859"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","63001+65232",65232,"Afbouwdeel Voor Thermostatische Mengkraan Voor Twee Gelijktijdige Functies, Met Druk Knop Aan/Uit Bediening.","Partie apparente pour mitigeur thermostatique deux fonctions avectouche on/off","External part for thermostatic mixer for two separate functions, with push-button on/off controls","030","Copper PVD",1832,"GPF652320P000G000","8056603004602"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","63011+65222",65222,"Afbouwdeel Voor Thermostatische Mengkraan Twee Gelijktijdige Functies, Met Druk Knop Aan/Uit Bediening.","Partie apparente pour mitiguer thermostatique deux fonctions avectouche on/off","External part for thermostatic mixer two simultaneous functions, with push button on/off controls.",706,"Black Metal PVD",2298,"GPF652220P001G000","8056603004985"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","63013+65224",65224,"Afbouwdeel Voor Thermostatische Mengkraan Drie Gelijktijdige Functies, Met Druk Knop Aan/Uit Bediening.","Partie apparente pour mitiguer thermostatique trois fonctions avectouche on/off","External part for thermostatic mixer three simultaneous functions, with push button on/off controls.",735,"Warm Bronze PVD",2706,"GPF652240P037G000","8056603004787"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","63015+65226",65226,"Afbouwdeel Voor Thermostatische Mengkraan Vier Gelijktijdige Functies, Met Druk Knop Aan/Uit Bediening.","Partie apparente pour mitiguer thermostatique quatre fonctions avectouche on/off","External part for thermostatic mixer four simultaneous functions, with push button on/off controls.",149,"Finox Brushed Nickel",2891,"GPF652260G002G000","8056603004756"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","63015+65226",65226,"Afbouwdeel Voor Thermostatische Mengkraan Vier Gelijktijdige Functies, Met Druk Knop Aan/Uit Bediening.","Partie apparente pour mitiguer thermostatique quatre fonctions avectouche on/off","External part for thermostatic mixer four simultaneous functions, with push button on/off controls.",845,"Dark Bronze",3384,"GPF652260V221G000","8056603633543"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC",63199,63199,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en Darkflex buigzame slang 1,50 m","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et Darkflex flexibles 1,50 m.","Magnetic shower set with water outlet, 1,50 m Darkflex flexible hose and antilimestone handshower","030","Copper PVD",940,"GPF631990P000G000","8056329522411"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","SP03289","SP03289","druk knop plaatje met regendouche symbool","Boutoun icône PLUIE","Push-button plate with RAINFALL symbol","031","Chrome",98,"GSP032890G001G000","8056603463638"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","SP03289","SP03289","druk knop plaatje met regendouche symbool","Boutoun icône PLUIE","Push-button plate with RAINFALL symbol",708,"Copper Brushed PVD",166,"GSP032890P006G000","8056603464963"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","SP03292","SP03292","druk knop plaatje met waterval symbool","Boutoun icône CASCADE","Push-button plate with WATERFALL symbol",761,"Coffee Bronze Brushed PVD",175,"GSP032920E059G000","8055261581241"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","SP03291","SP03291","druk knop plaatje met verneveling symbool","Boutoun icône BRUMISATION","Push-button plate with ATOMIZER symbol",187,"Aged Bronze",166,"GSP032910G052G000","8056603464741"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","SP03295","SP03295","druk knop plaatje met body jets symbool","Boutoun icône BODY JETS","Push-button plate with BODY JETS symbol",710,"Brass PVD",154,"GSP032950P011G000","8056603464178"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","SP03296","SP03296","druk knop plaatje met bad symbool","Boutoun icône BAIGNOIRE","Push-button plate with BATHTUB symbol",845,"Dark Bronze",166,"GSP032960V221G000","8056603634458"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","SP03298","SP03298","druk knop plaatje met voet uitloop symbool","Boutoun icône LAVEUR","Push-button plate with FOOT SPOUT symbol",727,"Brass Brushed PVD",166,"GSP032980P025G000","8056603463768"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","SP03297","SP03297","druk knop plaatje met kneipp tube symbool","Boutoun icône WATER TUBE KNEIPP","Push-button plate with WATER TUBE KNEIPP symbol",727,"Brass Brushed PVD",166,"GSP032970P025G000","8056603463898"]
["PRIVATE WELLNESS","HI-FI","HI-FI ECLECTIC","SP03290","SP03290","druk knop plaatje met wand-gemonteerd verneveling symbool","Boutoun icône BRUMISATION MURALE","Push-button plate with WALL-MOUNTED ATOMIZER symbol",845,"Dark Bronze",166,"GSP032900V221G000","8056603634519"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","38266+38711",38711,"Extern deel bad-/douche thermostaat 1-weg, met drukknop aan / uit controle.","Partie apparente pour mitigeur thermostatique une fonction avec touche on/off","External parts for thermostatic mixer for one function, with push-button on/off control.",246,"Gold PVD",1064,"GPF387110P007G000","8056603701532"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","38266+38717",38717,"Extern deel bad-/douche thermostaat 1-weg, met drukknop aan / uit controle.","Partie apparente pour mitigeur thermostatique une fonction avec touche on/off","External parts for thermostatic mixer for one function, with push-button on/off control.",716,"Gold Brushed PVD",1064,"GPF387170P005G000","8055261230996"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","38267+38713",38713,"Extern deel bad-/douche thermostaat 2-weg, met drukknop aan / uit controle.","Partie apparente pour mitigeur thermostatique deux fonctions avec touche on/off","External parts for thermostatic mixer for two simultaneous functions, with push-button on/off controls.",187,"Aged Bronze",1138,"GPF387130G052G000","8056603650540"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","38267+38718",38718,"Extern deel bad-/douche thermostaat 2-weg, met drukknop aan / uit controle.","Partie apparente pour mitigeur thermostatique deux fonctions avec touche on/off","External parts for thermostatic mixer for two simultaneous functions, with push-button on/off controls.",735,"Warm Bronze PVD",1067,"GPF387180P037G000","8056603650045"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","38268+38716",38716,"Extern deel bad-/douche thermostaat 3-weg, met drukknop aan / uit controle.","Partie apparente pour mitigeur thermostatique trois fonctions avec touche on/off","External parts for thermostatic mixer for three simultaneous functions, with push-button on/off controls.",713,"Antique Brass",1418,"GPF387160V204G000","8056603650311"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","SP04254","SP04254","druk knop plaatje met regendouche symbool. te combineren met met art. 38711, 38713, 38716, 38717, 38718, 38719.","Boutoun icône PLUIE. Peut être combiné avec les articles 38711, 38713, 38716, 38717, 38718, 38719.","Push-botton plate with RAINFALL symbol. To be combined with art. 38711, 38713, 38716, 38717, 38718, 38719.",727,"Brass Brushed PVD",70,"GSP042540P025G000","8056603717823"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","SP04255","SP04255","druk knop plaatje met wand-gemonteerd verneveling symbool. te combineren met met art. 38711, 38713, 38716, 38717, 38718, 38719.","Boutoun icône BRUMISATION MURALE. Peut être combiné avec les articles 38711, 38713, 38716, 38717, 38718, 38719.","Push-botton plate with WALL-MOUNTED ATOMIZER symbol. To be combined with art. 38711, 38713, 38716, 38717, 38718, 38719.",716,"Gold Brushed PVD",74,"GSP042550P005G000","8056603717694"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","SP04257","SP04257","druk knop plaatje met waterval symbool. te combineren met met art. 38711, 38713, 38716, 38717, 38718, 38719.","Boutoun icône CASCADE. Peut être combiné avec les articles 38711, 38713, 38716, 38717, 38718, 38719.","Push-botton plate with WATERFALL symbol. To be combined with art. 38711, 38713, 38716, 38717, 38718, 38719.",706,"Black Metal PVD",67,"GSP042570P001G000","8056603717335"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","SP04258","SP04258","druk knop plaatje met wand-gemonteerd waterval symbool. te combineren met met art. 38711, 38713, 38716, 38717, 38718, 38719.","Boutoun icône CASCADE MURALE. Peut être combiné avec les articles 38711, 38713, 38716, 38717, 38718, 38719.","Push-botton plate with WALL-MOUNTED WATERFALL symbol. To be combined with art. 38711, 38713, 38716, 38717, 38718, 38719.",187,"Aged Bronze",70,"GSP042580G052G000","8056603717168"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","SP04259","SP04259","druk knop plaatje met handdouche symbool. te combineren met met art. 38711, 38713, 38716, 38717, 38718, 38719.","Boutoun icône DOUCHETTE. Peut être combiné avec les articles 38711, 38713, 38716, 38717, 38718, 38719.","Push-botton plate with HANDSHOWER symbol. To be combined with art. 38711, 38713, 38716, 38717, 38718, 38719.",708,"Copper Brushed PVD",70,"GSP042590P006G000","8056603716925"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","SP04260","SP04260","druk knop plaatje met body jets symbool. te combineren met met art. 38711, 38713, 38716, 38717, 38718, 38719.","Boutoun icône BODY JETS. Peut être combiné avec les articles 38711, 38713, 38716, 38717, 38718, 38719.","Push-botton plate with BODY JETS symbol. To be combined with art. 38711, 38713, 38716, 38717, 38718, 38719.",713,"Antique Brass",70,"GSP042600V204G000","8056603716666"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","SP04262","SP04262","druk knop plaatje met kneipp tube symbool. te combineren met met art. 38711, 38713, 38716, 38717, 38718, 38719.","Boutoun icône WATER TUBE KNEIPP. Peut être combiné avec les articles 38711, 38713, 38716, 38717, 38718, 38719.","Push-botton plate with WATER TUBE KNEIPP symbol. To be combined with art. 38711, 38713, 38716, 38717, 38718, 38719.",727,"Brass Brushed PVD",70,"GSP042620P025G000","8056603716307"]
["PRIVATE WELLNESS","HI-FI","HI-FI COMFORT","SP04262","SP04262","druk knop plaatje met kneipp tube symbool. te combineren met met art. 38711, 38713, 38716, 38717, 38718, 38719.","Boutoun icône WATER TUBE KNEIPP. Peut être combiné avec les articles 38711, 38713, 38716, 38717, 38718, 38719.","Push-botton plate with WATER TUBE KNEIPP symbol. To be combined with art. 38711, 38713, 38716, 38717, 38718, 38719.",761,"Coffee Bronze Brushed PVD",76,"GSP042620E059G000","8055261580947"]
["PRIVATE WELLNESS","SOGNI","SOGNI","57961+57963",57963,"Afbouwdeel voor multifunctioneel douchesysteem met chromotherapie-effect. Functies REGENVAL/WATERVAL/VERNEVELING.","Parties apparentes pour pomme de douche multifonction avec chromothérapie. Fonction PLUIE/CASCADE/BRUMISATION.","External parts for multifunctional shower system with chromotherapy. RAINFALL/WATERFALL/MIST functions.",279,"Matte White",10210,"GPF579630C071G000","8056603462990"]
["PRIVATE WELLNESS","SOGNI","SOGNI","01720","01720","Opti1-wegle kit capacitief toetsenbord voor chromotherapieregeling met IP-connector.","Kit optionnel clavier capacitif pour contrôle de la chromothérapie avec connecteur IP, pour système à installation au plafond.","Optional kit capacitive keyboard for chromotherapy control with IP connector.",246,"Gold PVD",913,"GPF017200P007G000","8055261240261"]
["PRIVATE WELLNESS","AFILO","AFILO","57301+57002","57002","Cover esthetische afwerking 300x300","Coque de finition esthétique 300X300","Cover for 300x300 shower system",735,"Warm Bronze PVD",1844,"GPF570020P037G000","8056329558663"]
["PRIVATE WELLNESS","AFILO","AFILO","57303+57002","57002","Cover esthetische afwerking 300x300","Coque de finition esthétique 300X300","Cover for 300x300 shower system",299,"Matte Black",1682,"GPF570020C072G000","8056329068629"]
["PRIVATE WELLNESS","AFILO","AFILO","57305+57004","57004","Cover esthetische afwerking 300x300","Coque de finition esthétique 300X300","Cover for 300x300 multifunction system",720,"Nickel PVD",1844,"GPF570040P014G000","8056603456845"]
["PRIVATE WELLNESS","AFILO","AFILO","57401+57006",57401,"Douchesysteem met Chromotherapie op verlaagd plafond 300x500 met REGEN-functie. Elektronica en hermetische multifunctionele afstandsbediening met houder inbegrepen. Te combineren met voedingseenheid 12 V 01723 (niet inbegrepen) en esthetische cover (nietinbegrepen)","Système douche avec Cromothérapie pour installation au faux plafond 300x500 fonction PLUIE. Electronique et télécommande multifonction étanche avec support inclus. A combiner avec alimentation 12 V 01723, non inclus. A compléter par une coque esthétique.","300X500 Built-in shower system, with rainfall function and chromotherapy effect, for false-ceiling installation. Electronic parts included with remote watertight control and hook. To be matched with 12V 01723 power supply, not included. To be completed with cover (not included).",279,"Matte White",4521,"GPF574010C071G000","8022692879483"]
["PRIVATE WELLNESS","AFILO","AFILO","57401+57006","57006","Cover esthetische afwerking 300x500","Coque de finition esthétique 300X500","Cover for 300x500 shower system",279,"Matte White",1784,"GPF570060C071G000","8056329152618"]
["PRIVATE WELLNESS","AFILO","AFILO","57403+57006","57006","Cover esthetische afwerking 300x500","Coque de finition esthétique 300X500","Cover for 300x500 shower system",845,"Dark Bronze",1955,"GPF570060V221G000","8056603633925"]
["PRIVATE WELLNESS","AFILO","AFILO","57409+57010","57010","Cover esthetische afwerking 300x500","Coque de finition esthétique 300X500","Cover for 300x500 multifunction system",845,"Dark Bronze",1955,"GPF570100V221G000","8056603633918"]
["PRIVATE WELLNESS","AFILO","AFILO","57411+57010","57010","Cover esthetische afwerking 300x500","Coque de finition esthétique 300X500","Cover for 300x500 multifunction system",726,"Warm Bronze Brushed PVD",1955,"GPF570100P024G000","8022692879315"]
["PRIVATE WELLNESS","AFILO","AFILO","57501+57012","57012","Cover esthetische afwerking 500x500","Coque de finition esthétique 500X500","Cover for 500x500 shower system",727,"Brass Brushed PVD",2161,"GPF570120P025G000","8056329068407"]
["PRIVATE WELLNESS","AFILO","AFILO","57509+57016","57016","Cover esthetische afwerking 500x500","Coque de finition esthétique 500X500","Cover for 500x500 multifunction system",238,"Mirror Steel",945,"GPF570160A001G000","8022692879384"]
["PRIVATE WELLNESS","AFILO","AFILO","57511+57016",57016,"Cover esthetische afwerking 500x500","Coque de finition esthétique 500X500","Cover for 500x500 multifunction system",239,"Steel Brushed",945,"GPF570160A000G000","8022692879377"]
["PRIVATE WELLNESS","AFILO","AFILO","57601+57018","57018","Cover esthetische afwerking Ø350","Coque de finition esthétique Ø350","Cover for Ø350 shower system","030","Copper PVD",1844,"GPF570180P000G000","8022692856927"]
["PRIVATE WELLNESS","AFILO","AFILO","57601+57018","57018","Cover esthetische afwerking Ø350","Coque de finition esthétique Ø350","Cover for Ø350 shower system",187,"Aged Bronze",1844,"GPF570180G052G000","8056329019775"]
["PRIVATE WELLNESS","AFILO","AFILO","01720","01720","Opti1-wegle kit capacitief toetsenbord voor chromotherapieregeling met IP-connector.","Kit optionnel clavier capacitif pour contrôle de la chromothérapie avec connecteur IP, pour système à installation au plafond.","Optional kit capacitive keyboard for chromotherapy control with IP connector.",299,"Matte Black",693,"GPF017200C072G000","8055261240339"]
["PRIVATE WELLNESS","MINIMALI","MINIMALI","57801+57871","57871","Cover esthetische afwerking 350x350","Coque de finition esthétique 350X350","Cover for 350x350 shower system",706,"Black Metal PVD",1844,"GPF578710P001G000","8022692856958"]
["PRIVATE WELLNESS","MINIMALI","MINIMALI","57807+57875","57875","Cover esthetische afwerking 350x350","Coque de finition esthétique 350X350","Cover for 350x350 multifunction system",720,"Nickel PVD",1844,"GPF578750P014G000","8056603456739"]
["PRIVATE WELLNESS","MINIMALI","MINIMALI","57805+57006","57006","Cover esthetische afwerking 300x500","Coque de finition esthétique 300X500","Cover for 300x500 shower system",187,"Aged Bronze",1955,"GPF570060G052G000","8056329068513"]
["PRIVATE WELLNESS","MINIMALI","MINIMALI","57811+57010","57010","Cover esthetische afwerking 300x500","Coque de finition esthétique 300X500","Cover for 300x500 multifunction system",187,"Aged Bronze",1955,"GPF570100G052G000","8056329068476"]
["PRIVATE WELLNESS","MINIMALI","MINIMALI","57901+57012","57012","Cover esthetische afwerking 500x500","Coque de finition esthétique 500X500","Cover for 500x500 shower system",246,"Gold PVD",2452,"GPF570120P007G000","8056329068414"]
["PRIVATE WELLNESS","MINIMALI","MINIMALI","57907+57016","57016","Cover esthetische afwerking 500x500","Coque de finition esthétique 500X500","Cover for 500x500 multifunction system",710,"Brass PVD",2161,"GPF570160P011G000","8056329598126"]
["PRIVATE WELLNESS","MINIMALI","MINIMALI","57803+57018","57018","Cover esthetische afwerking Ø350","Coque de finition esthétique Ø350","Cover for Ø350 shower system",726,"Warm Bronze Brushed PVD",1844,"GPF570180P024G000","8022692879452"]
["PRIVATE WELLNESS","MINIMALI","MINIMALI","57809+57873","57873","Cover esthetische afwerking Ø350","Coque de finition esthétique Ø350","Cover for Ø350 multifunction system",707,"Black Metal Brushed PVD",1844,"GPF578730P004G000","8022692879742"]
["PRIVATE WELLNESS","MINIMALI","MINIMALI","57909+57975","57975","Cover esthetische afwerking Ø500","Coque de finition esthétique Ø500","Cover for Ø500 multifunction system",238,"Mirror Steel",946,"GPF579750A001G000","8022692880687"]
["PRIVATE WELLNESS","COLOUR","COLOUR","57827+57876","57876","Cover esthetische afwerking met verlichting 350x350","Coque de finition esthétique avec éclairage 350X350","Cover with lighting system for 350x350 multifunction system",720,"Nickel PVD",2248,"GPF578760P014G000","8056603456722"]
["PRIVATE WELLNESS","COLOUR","COLOUR","57827+57876","57876","Cover esthetische afwerking met verlichting 350x350","Coque de finition esthétique avec éclairage 350X350","Cover with lighting system for 350x350 multifunction system",713,"Antique Brass",2248,"GPF578760V204G000","8056329068209"]
["PRIVATE WELLNESS","COLOUR","COLOUR","57927+57977","57977","Cover esthetische afwerking met verlichting 500x500","Coque de finition esthétique avec éclairage 500x500","Cover with lighting system for 500x500 multifunction system",299,"Matte Black",2369,"GPF579770C072G000","8056329061422"]
["PRIVATE WELLNESS","COLOUR","COLOUR","57927+57977","57977","Cover esthetische afwerking met verlichting 500x500","Coque de finition esthétique avec éclairage 500x500","Cover with lighting system for 500x500 multifunction system",246,"Gold PVD",2946,"GPF579770P007G000","8056329067547"]
["PRIVATE WELLNESS","COLOUR","COLOUR","57929+57980","57980","Cover esthetische afwerking met verlichting Ø500","Coque de finition esthétique avec éclairage Ø500","Cover with lighting system for Ø500 multifunction system",710,"Brass PVD",2834,"GPF579800P011G000","8056329597648"]
["PRIVATE WELLNESS","COLOUR","COLOUR","57929+57980","57980","Cover esthetische afwerking met verlichting Ø500","Coque de finition esthétique avec éclairage Ø500","Cover with lighting system for Ø500 multifunction system",761,"Coffee Bronze Brushed PVD",3026,"GPF579800E059G000","8055261596696"]
["PRIVATE WELLNESS","TREMILLIMETRI","TREMILLIMETRI",33051,33051,"Hoofddouchekop Wanddouche TONDO 200","Pomme de douche murale TONDO 200","TONDO 200 Wall-mounted shower head",706,"Black Metal PVD",2164,"GPF330512P001G000","8056329136502"]
["PRIVATE WELLNESS","TREMILLIMETRI","TREMILLIMETRI",33053,33053,"Multifunctioneel wandsysteem 200 met REGEN/CASCADE-functies. Aan te vullen met afstandsbediening twee uitgangen","Pomme de douche multifonction (PLUIE/CASCADE) murale TONDO 200 .","Wall-mounted multifunction system TONDO 200 with RAINFALL/WATERFALL. To complete with separate control",246,"Gold PVD",3448,"GPF330532P007G000","8056329136335"]
["PRIVATE WELLNESS","TREMILLIMETRI","TREMILLIMETRI",33063,33063,"Multifunctioneel wandsysteem 200 met REGEN/CASCADE-functies. Aan te vullen met afstandsbediening twee uitgangen","Pomme de douche multifonction (PLUIE/CASCADE) murale QUADRO 200.","Wall-mounted multifunction shower system 200 with RAINFALL/WATERFALL. To complete with separate control",720,"Nickel PVD",3036,"GPF330632P014G000","8056603457118"]
["PRIVATE WELLNESS","TREMILLIMETRI","TREMILLIMETRI",33063,33063,"Multifunctioneel wandsysteem 200 met REGEN/CASCADE-functies. Aan te vullen met afstandsbediening twee uitgangen","Pomme de douche multifonction (PLUIE/CASCADE) murale QUADRO 200.","Wall-mounted multifunction shower system 200 with RAINFALL/WATERFALL. To complete with separate control",761,"Coffee Bronze Brushed PVD",3241,"GPF330632E059G000","8055261608283"]
["PRIVATE WELLNESS","TREMILLIMETRI","TREMILLIMETRI",33071,33071,"Hoofddouchekop Wanddouche TONDO 300","Pomme de douche murale TONDO 300.","TONDO 300 Wall-mounted showerhead",246,"Gold PVD",2733,"GPF330713P007G000","8056329135680"]
["PRIVATE WELLNESS","TREMILLIMETRI","TREMILLIMETRI",33073,33073,"Multifunctioneel wandsysteem 300 met REGEN/CASCADE-functies. Aan te vullen met afstandsbediening twee uitgangen","Pomme de douche multifonction (PLUIE/CASCADE) murale TONDO 300 .","Wall-mounted multifunction system 300 with RAINFALL/WATERFALL. To complete with separate control",187,"Aged Bronze",3502,"GPF330732G052G000","8056329135611"]
["PRIVATE WELLNESS","TREMILLIMETRI","TREMILLIMETRI",33083,33083,"Multifunctioneel wandsysteem 300 met REGEN/CASCADE-functies. Aan te vullen met afstandsbediening twee uitgangen","Pomme de douche multifonction (PLUIE/CASCADE) murale QUADRO 300.","Wall-mounted multifunction system 300 with RAINFALL/WATERFALL. To complete with separate control",710,"Brass PVD",3281,"GPF330832P011G000","8056329609822"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57201,57201,"Oriënteerbare wand-hoofddouchekop FLESSA. Multispray-functie","Pomme de douche murale orientable FLESSA. Fonction Multi-spray","Wall-mounted adjustable showerhead FLESSA. Multi-spray function",239,"Steel Brushed",1048,"GPF572010A000G000","8056329107441"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57205,57205,"Oriënteerbare wand-hoofddouchekop FLESSA. VERNEVELING-functie","Pomme de douche murale orientable FLESSA. Fonction BRUMISATION","Wall-mounted adjustable showerhead FLESSA. Mist function",239,"Steel Brushed",1004,"GPF572050A000G000","8056329107366"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57249,57249,"wandgemonteerde verstelbare douche head FLESSA. 3 instellingen functie","Pomme de douche anticalcaire au plafond orientable FLESSA. Trois sorties","Wall-mounted adjustable shower head FLESSA. RAINFALL/SPRAY/MASSAGE function.",708,"Copper Brushed PVD",1825,"GPF572490P006G000","8056603579285"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57245,57245,"Oriënteerbare wand-hoofddouchekop TRAME. VERNEVELING-functie","Pomme de douche murale orientable TRAME. Fonction BRUMISATION","Wall-mounted adjustable showerhead TRAME. Mist function",726,"Warm Bronze Brushed PVD",1867,"GPF572450P024G000","8056329106697"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57211,57211,"Oriënteerbare wand-hoofddouchekop INTRECCIO. Multispray-functie","Pomme de douche murale orientable INTRECCIO. Fonction Multi-spray","Wall-mounted adjustable showerhead INTRECCIO. Multi-spray function",707,"Black Metal Brushed PVD",1934,"GPF572110P004G000","8056329107274"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57289,57289,"Oriënteerbare wand-hoofddouchekop RIGATO. Multispray-functie","Pomme de douche murale orientable RIGATO. Fonction Multi-spray","Wall-mounted adjustable showerhead RIGATO. Multi-spray function",761,"Coffee Bronze Brushed PVD",2064,"GPF572890E059G000","8055261596955"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57285,57285,"Oriënteerbare wand-hoofddouchekop RIGATO. CASCADE-functie","Pomme de douche murale orientable RIGATO. Fonction CASCADE","Wall-mounted adjustable showerhead RIGATO. Waterfall function",727,"Brass Brushed PVD",2109,"GPF572850P025G000","8056603686853"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57287,57287,"Oriënteerbare wand-hoofddouchekop DIAMANTATO. Multispray-functie","Pomme de douche murale orientable DIAMANTATO. Fonction Multi-spray","Wall-mounted adjustable showerhead DIAMANTATO. Multi-spray function",707,"Black Metal Brushed PVD",1934,"GPF572870P004G000","8056603693851"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57283,57283,"Oriënteerbare wand-hoofddouchekop DIAMANTATO. CASCADE-functie","Pomme de douche murale orientable DIAMANTATO. Fonction CASCADE","Wall-mounted adjustable showerhead DIAMANTATO. Waterfall function",239,"Steel Brushed",1425,"GPF572830A000G000","8056603686969"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57223,57223,"Oriënteerbare wand-hoofddouchekop MECCANICA. REGEN-functie","Pomme de douche murale orientable MECCANICA. Fonction PLUIE","Wall-mounted adjustable showerhead MECCANICA. Rain function",707,"Black Metal Brushed PVD",1934,"GPF572230P004G000","8056329107076"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57233,57233,"Oriënteerbare wand-hoofddouchekop CESELLO. REGEN-functie","Pomme de douche murale orientable CESELLO. Fonction PLUIE","Wall-mounted adjustable showerhead CESELLO. Rain function",239,"Steel Brushed",1306,"GPF572330A000G000","8056329106925"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER316",57233,57233,"Oriënteerbare wand-hoofddouchekop CESELLO. REGEN-functie","Pomme de douche murale orientable CESELLO. Fonction PLUIE","Wall-mounted adjustable showerhead CESELLO. Rain function",726,"Warm Bronze Brushed PVD",1934,"GPF572330P024G000","8056329106895"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER",57261,57261,"Oriënteerbare wand-hoofddouchekop. Multispray-functie","Pomme de douche murale orientable. Fonction Multi-spray","Wall-mounted adjustable showerhead. Multi-spray function",720,"Nickel PVD",1441,"GPF572610P014G000","8056603456791"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER",57263,57263,"Oriënteerbare wand-hoofddouchekop. REGEN-functie","Pomme de douche murale orientable. Fonction PLUIE","Wall-mounted adjustable showerhead. Rain function",713,"Antique Brass",1536,"GPF572630V204G000","8056329108257"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER",57267,57267,"Oriënteerbare wand-hoofddouchekop. CASCADE-functie","Pomme de douche murale orientable. Fonction CASCADE","Wall-mounted adjustable showerhead. Waterfall function",299,"Matte Black",1475,"GPF572670C072G000","8056329108028"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER",57267,57267,"Oriënteerbare wand-hoofddouchekop. CASCADE-functie","Pomme de douche murale orientable. Fonction CASCADE","Wall-mounted adjustable showerhead. Waterfall function",279,"Matte White",1475,"GPF572670C071G000","8056329108035"]
["PRIVATE WELLNESS","SPOTWATER","SPOTWATER",57269,57269,"wandgemonteerde verstelbare douche head. 3 instellingen functie","Pomme de douche murale orientable. Fonction à trois jets.","Wall-mounted adjustable shower head. RAINFALL/SPRAY/MASSAGE function.",246,"Gold PVD",2397,"GPF572690P007G000","8056603627559"]
["PRIVATE WELLNESS","CASCATA","CASCATA",20295,20295,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche ou bagnoire à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",187,"Aged Bronze",1607,"GPF202950G052G000","8056329085718"]
["PRIVATE WELLNESS","CASCATA","CASCATA",20293,20293,"Cascade-uitloop Wanddouche. Aan te vullen met afstandsbediening","Bec cascade mural pour douche à compléter par un mitigeur à commande séparée.","Wall-fixing cascade shower spout to be completed with separate control (not included)",187,"Aged Bronze",2295,"GPF202930G052G000","8056329044586"]
["PRIVATE WELLNESS","CASCATA","CASCATA",20191,20191,"Cascade-uitloop Badrand Aan te vullen met afstandsbediening","Bec cascade pour baignoire à compléter par un mitigeur à commande séparée.","Bath group waterfall spout to be completed with separate control",713,"Antique Brass",2673,"GPF201910V204G000","8056329562219"]
["PRIVATE WELLNESS","BODY JETS","BODY JETS",32975,32975,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",713,"Antique Brass",1029,"GPF329751V204G000","8056329006928"]
["PRIVATE WELLNESS","BODY JETS","BODY JETS","32987+32984",32984,"Extern deel Laterale oriënteerbare Hoofddouchekop","Partie apparente pour pomme de douche laterale orientable","External parts for adjustable lateral body jet",149,"Finox Brushed Nickel",607,"GPF329840G002G000","8022692797480"]
["PRIVATE WELLNESS","BODY JETS","BODY JETS",32979,32979,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",149,"Finox Brushed Nickel",351,"GPF329791G002G000","8022692800623"]
["PRIVATE WELLNESS","BODY JETS","BODY JETS",32971,32971,"Laterale hoofddouchekop","Pomme de douche laterale","Lateral body jet",720,"Nickel PVD",444,"GPF329710P014G000","8056603455985"]
["PRIVATE WELLNESS","BODY JETS","BODY JETS",32977,32977,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",149,"Finox Brushed Nickel",351,"GPF329771G002G000","8022692801057"]
["PRIVATE WELLNESS","BODY JETS","BODY JETS",32977,32977,"Laterale vernevelaar","Pomme de douche latérale avec jet de brumisation.","Lateral nebulizer",713,"Antique Brass",411,"GPF329771V204G000","8056329037236"]
["PRIVATE WELLNESS","BODY JETS","BODY JETS",13375,13375,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","Adjustable lateral body jet",708,"Copper Brushed PVD",337,"GPF133750P006G000","8056329007659"]
["PRIVATE WELLNESS","BODY JETS","BODY JETS",13375,13375,"Oriënteerbare laterale hoofddouchekop","Pomme de douche latérale orientable.","Adjustable lateral body jet",845,"Dark Bronze",337,"GPF133750V221G000","8056603623193"]
["PRIVATE WELLNESS","SHOWER SETS","SHOWER SETS",65123,65123,"Douche Set Met Water Uitgang, 1,50 M Flexibele Slang And Antikalk Handdouche","Ensemble comprenant: sortie coudée murale, douchette anticalcaire etflexibles 1,50 m","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",710,"Brass PVD",1046,"GPF651230P011G000","8056603007429"]
["PRIVATE WELLNESS","SHOWER SETS","SHOWER SETS",58123,58123,"Doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m.","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",726,"Warm Bronze Brushed PVD",777,"GPF581230P024G000","8056329191587"]
["PRIVATE WELLNESS","SHOWER SETS","SHOWER SETS",20123,20123,"Doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m.","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",727,"Brass Brushed PVD",853,"GPF201231P025G000","8056329515253"]
["PRIVATE WELLNESS","SHOWER SETS","SHOWER SETS",59123,59123,"Doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m.","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",708,"Copper Brushed PVD",450,"GPF591230P006G000","8056329030787"]
["PRIVATE WELLNESS","SHOWER SETS","SHOWER SETS","33773",33773,"Doucheset met wateraansluitpunt, antikalk-handdouche en buigzame slang 1,50 m","Ensemble comprenant: sortie coudée murale, douchette anticalcaire et flexibles 1,50 m.","Shower set with water outlet, 1,50 m flexible hose and antilimestone handshower",761,"Coffee Bronze Brushed PVD",913,"GPF337730E059G000","8055261605398"]
["PRIVATE WELLNESS","SHOWER SETS","SHOWER SETS",63199,63199,"Magnetisch doucheset met wateraansluitpunt, antikalk-handdouche en Darkflex buigzame slang 1,50 m","Ensemble magnétique comprenant: sortie coudée murale, douchette anticalcaire et Darkflex flexibles 1,50 m.","Magnetic shower set with water outlet, 1,50 m Darkflex flexible hose and antilimestone handshower",708,"Copper Brushed PVD",1003,"GPF631990P006G000","8056329522381"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67511,67511,"Rechterwand-glas scharnier met heffunctie bij opening.","Charnière droite mur-verre avec rehausseur sur l'ouverture. RIGATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg,largeur maximum 900mm.","Right wall-glass hinge with lifting function at opening. RIGATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.",187,"Aged Bronze",1842,"GPF675111G052G000","8056603673457"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67513,67513,"Linkerwand-glas scharnier met heffunctie bij opening.","Charnière gauche mur-verre avec rehausseur sur l'ouverture. RIGATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg,largeur maximum 900mm.","Left wall-glass hinge with lifting function at opening. RIGATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.","030","Copper PVD",1726,"GPF675131P000G000","8056603673303"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67593,67593,"rechts wand-glas scharnier met heffunctie bij het openen. RIGATO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière droite MUR-VERRE avec fonction d'élévation. RIGATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","Right wall-glass hinge with lifting function at opening. RIGATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.",708,"Copper Brushed PVD",1842,"GPF675930P006G000","8055261213722"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67595,67595,"links wand-glas scharnier met heffunctie bij het openen. RIGATO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière gauche MUR-VERRE avec fonction d'élévation. RIGATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","Left wall-glass hinge with lifting function at opening. RIGATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.",708,"Copper Brushed PVD",1842,"GPF675950P006G000","8055261213364"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67517,67517,"Linkerglas-glas scharnier met heffunctie bij opening.","Charnière gauche verre-verre avec rehausseur sur l'ouverture 180°. RIGATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte40Kg, largeur maximum 900mm.","180° Left glass-glass hinge with lifting function at opening. RIGATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.",707,"Black Metal Brushed PVD",2630,"GPF675171P004G000","8056603673006"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67585,67585,"90° rechts glas-glas scharnier met heffunctie bij het openen. RIGATO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière droite VERRE-VERRE avec fonction d'élévation 90°. RIGATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg,largeur maximum 900mm.","90° Right glass-glass hinge with lifting function at opening. RIGATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.","030","Copper PVD",2465,"GPF675850P000G000","8055261215207"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67587,67587,"90° links glas-glas scharnier met heffunctie bij het openen. RIGATO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière gauche VERRE-VERRE avec fonction d'élévation 90°. RIGATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg,largeur maximum 900mm.","90° Left glass-glass hinge with lifting function at opening. RIGATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximumwidth 900 mm.",706,"Black Metal PVD",2465,"GPF675870P001G000","8055261214835"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67589,67589,"90° rechts glas-glas scharnier met heffunctie bij het openen. RIGATO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière droite VERRE-VERRE avec fonction d'élévation 90°. RIGATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg,largeur maximum 900mm.","90° Right glass-glass hinge with lifting function at opening. RIGATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.","031","Chrome",1665,"GPF675890G001G000","8055261214521"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67591,67591,"90° links glas-glas scharnier met heffunctie bij het openen. RIGATO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière gauche VERRE-VERRE avec fonction d'élévation 90°. RIGATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg,largeur maximum 900mm.","90° Left glass-glass hinge with lifting function at opening. RIGATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximumwidth 900 mm.",720,"Nickel PVD",2465,"GPF675910P014G000","8055261214057"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67505,67505,"glas-wand Klem. RIGATO","Pince Mur-Verre. RIGATO. Epaisseur du verre 8-10-12 mm.","Wall-Glass clamp. RIGATO. 8-10-12 mm glass thickness.",761,"Coffee Bronze Brushed PVD",847]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67507,67507,"Glas-Glas Klem. RIGATO","Pince Verre-Verre 90°. RIGATO. Epaisseur du verre 8-10-12 mm.","Glass-Glass clamp 90°. RIGATO. 8-10-12 mm glass thickness.","031","Chrome",606,"GPF675071G001G000","8056603593854"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67599,67599,"glas-glas klem 90°. RIGATO. 8-10-12 mm glas dikte.","Pince Verre-Verre 90°. RIGATO. Epaisseur du verre 8-10-12 mm.","Glass-Glass clamp 90°. RIGATO. 8-10-12 mm glass thickness.",720,"Nickel PVD",896,"GPF675990P014G000","8055261212978"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67599,67599,"glas-glas klem 90°. RIGATO. 8-10-12 mm glas dikte.","Pince Verre-Verre 90°. RIGATO. Epaisseur du verre 8-10-12 mm.","Glass-Glass clamp 90°. RIGATO. 8-10-12 mm glass thickness.",727,"Brass Brushed PVD",957,"GPF675990P025G000","8055261212954"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67509,67509,"T-gevormd glas-glas klem. RIGATO. 8-10-12 mm glas dikte.","Pince Verre-Verre en T. RIGATO. Epaisseur du verre 8-10-12 mm.","T-shaped glass-glass clamp. RIGATO.• 5/16\" - 1/2\" (8-12mm) glass thickness.",147,"Chome Brushed",1574,"GPF675090G006G000","8055261218284"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67510,67510,"klem. vloer/plafond installatie. RIGATO. 8-10-12 mm glas dikte.","Pince. Installation au sol/au plafond. RIGATO. Epaisseur du verre 8-10-12 mm.","Floor/Ceiling Glass clamp. RIGATO.• 5/16\" - 1/2\" (8-12mm) glass thickness.",710,"Brass PVD",687,"GPF675100P011G000","8055261218024"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67571,67571,"glas stabilisatie arm RIGATO.","Barre de fixation du verre. RIGATO. Epaisseur du verre 8-10 mm.","Glass holding arm. RIGATO. 8-10 mm glass thickness.","030","Copper PVD",612,"GPF675710P000G000","8056603625159"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67575,67575,"T-shaped glas rod. lengte op aanvraag. RIGATO","Barre de fixation du verre. Longueur réglable. RIGATO. Epaisseur du verre 8-10 mm.","T-shaped adjustable glass rod Adjustable. RIGATO. 8-10 mm glass thickness.",299,"Matte Black",1051,"GPF675750C072G000","8056603624848"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM RIGATO",67577,67577,"plafond gemonteerd glas stabilisatie stang. RIGATO. 8-10 mm glas dikte.","Bras de fermeture du verre réglable, installation au plafond. RIGATO. Epaisseur du verre 8-10 mm.","Ceiling mounted glass stabilization arm for frameless shower enclosure.  Customizable length. RIGATO. • 5/16\" - 3/8\" (8-10mm) glass thickness • 3-15/16\" - 29-1/2\" length",707,"Black Metal Brushed PVD",775,"GPF675770P004G000","8055261216266"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67611,67611,"Rechterwand-glas scharnier met heffunctie bij opening.","Charnière droite mur-verre avec rehausseur sur l'ouverture. DIAMANTATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","Right wall-glass hinge with lifting function at opening. DIAMANTATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximumwidth 900 mm.",149,"Finox Brushed Nickel",1575,"GPF676111G002G000","8056603672900"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67613,67613,"Linkerwand-glas scharnier met heffunctie bij opening.","Charnière gauche mur-verre avec rehausseur sur l'ouverture. DIAMANTATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","Left wall-glass hinge with lifting function at opening. DIAMANTATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximumwidth 900 mm.",147,"Chome Brushed",1575,"GPF676131G006G000","8056603675512"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67613,67613,"Linkerwand-glas scharnier met heffunctie bij opening.","Charnière gauche mur-verre avec rehausseur sur l'ouverture. DIAMANTATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","Left wall-glass hinge with lifting function at opening. DIAMANTATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximumwidth 900 mm.",187,"Aged Bronze",1842,"GPF676131G052G000","8056603672757"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67695,67695,"links wand-glas scharnier met heffunctie bij het openen. DIAMANTATO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière gauche MUR-VERRE avec fonction d'élévation. DIAMANTATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","Left wall-glass hinge with lifting function at opening. DIAMANTATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximumwidth 900 mm.","031","Chrome",1166,"GPF676950G001G000","8055261207509"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67615,67615,"Rechterglas-glas scharnier met heffunctie bij opening.","Charnière droite verre-verre avec rehausseur sur l'ouverture 180°. DIAMANTATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","180° Right glass-glass hinge with lifting function at the opening. DIAMANTATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.",845,"Dark Bronze",2630,"GPF676151V221G000","8056603672511"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67617,67617,"Linkerglas-glas scharnier met heffunctie bij opening.","Charnière gauche verre-verre avec rehausseur sur l'ouverture 180°. DIAMANTATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","180° Left glass-glass hinge with lifting function at opening. DIAMANTATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.",716,"Gold Brushed PVD",2798,"GPF676171P005G000","8056603675369"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67685,67685,"90° rechts glas-glas scharnier met heffunctie bij het openen. DIAMANTATO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière droite VERRE-VERRE avec fonction d'élévation 90°. DIAMANTATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","90° Right glass-glass hinge with lifting function at opening. DIAMANTATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.",716,"Gold Brushed PVD",2798,"GPF676850P005G000","8055261209237"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67687,67687,"90° links glas-glas scharnier met heffunctie bij het openen. DIAMANTATO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière gauche VERRE-VERRE avec fonction d'élévation 90°. DIAMANTATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","90° Left glass-glass hinge with lifting function at opening. DIAMANTATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.",246,"Gold PVD",2798,"GPF676870P007G000","8055261208858"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67689,67689,"90° rechts glas-glas scharnier met heffunctie bij het openen. DIAMANTATO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière droite VERRE-VERRE avec fonction d'élévation 90°. DIAMANTATO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","90° Right glass-glass hinge with lifting function at opening. DIAMANTATO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.",710,"Brass PVD",2465,"GPF676890P011G000","8055261208483"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67605,67605,"glas-wand Klem. DIAMANTATO","Pince Mur-Verre. DIAMANTATO. Epaisseur du verre 8-10-12 mm.","Wall-Glass clamp. DIAMANTATO. 8-10-12 mm glass thickness.",735,"Warm Bronze PVD",747,"GPF676051P037G000","8056603591003"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67606,67606,"wand-glas klem DIAMANTATO","Pince Mur-Verre. DIAMANTATO. Epaisseur du verre 8-10-12 mm.","Wall-Glass clamp. DIAMANTATO. 8-10-12 mm glass thickness.",727,"Brass Brushed PVD",797,"GPF676061P025G000","8056603624503"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67607,67607,"Glas-Glas Klem. DIAMANTATO","Pince Verre-Verre 90°. DIAMANTATO. Epaisseur du verre 8-10-12 mm.","Glass-Glass clamp 90°. DIAMANTATO. 8-10-12 mm glass thickness.","030","Copper PVD",896,"GPF676071P000G000","8056603590914"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67699,67699,"glas-glas klem 90°. DIAMANTATO. 8-10-12 mm glas dikte.","Pince Verre-Verre 90°. DIAMANTATO. Epaisseur du verre 8-10-12 mm.","Glass-Glass clamp 90°. DIAMANTATO. 8-10-12 mm glass thickness.",727,"Brass Brushed PVD",957,"GPF676990P025G000","8055261207011"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67608,67608,"glas-glas klem 180°. DIAMANTATO. 8-10-12 mm glas dikte.","Pince Verre-Verre 180°. DIAMANTATO. Epaisseur du verre 8-10-12 mm.","Glass-Glass clamp 180°. DIAMANTATO. 8-10-12 mm glass thickness.",720,"Nickel PVD",1003,"GPF676080P014G000","8055261212435"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67610,67610,"klem. vloer/plafond installatie. DIAMANTATO. 8-10-12 mm glas dikte.","Pince. Installation au sol/au plafond. DIAMANTATO. Epaisseur du verre 8-10-12 mm.","Floor/Ceiling Glass clamp.   DIAMANATATO.• 5/16\" - 1/2\" (8-12mm) glass thickness.",299,"Matte Black",628,"GPF676100C072G000","8055261212190"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67610,67610,"klem. vloer/plafond installatie. DIAMANTATO. 8-10-12 mm glas dikte.","Pince. Installation au sol/au plafond. DIAMANTATO. Epaisseur du verre 8-10-12 mm.","Floor/Ceiling Glass clamp.   DIAMANATATO.• 5/16\" - 1/2\" (8-12mm) glass thickness.",708,"Copper Brushed PVD",734,"GPF676100P006G000","8055261212107"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67671,67671,"glas stabilisatie arm DIAMANTATO.","Barre de fixation du verre. DIAMANTATO. Epaisseur du verre 8-10 mm.","Glass holding arm. DIAMANTATO. 8-10 mm glass thickness.",761,"Coffee Bronze Brushed PVD",696,"GPF676710E059G000","8055261585881"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67675,67675,"T-gevormt glas stang, lengte op aanvraag. DIAMANTATO","Barre de fixation du verre. Longueur réglable. DIAMANTATO. Epaisseur du verre 8-10 mm.","T-shaped adjustable glass rod Adjustable. DIAMANTATO. 8-10 mm glass thickness.",726,"Warm Bronze Brushed PVD",1230,"GPF676750P024G000","8056603623384"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM DIAMANTATO",67677,67677,"plafond gemonteerd glas stabilisatie stang. DIAMANTATO. 8-10 mm glas dikte.","Bras de fermeture du verre réglable, installation au plafond. DIAMANTATO. Epaisseur du verre 8-10 mm.","Ceiling mounted glass stabilization arm for frameless shower enclosure.  Customizable length. DIAMANTATO. • 5/16\" - 3/8\" (8-10mm) glass thickness • 3-15/16\" - 29-1/2\" length",246,"Gold PVD",824,"GPF676770P007G000","8055261210295"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67011,67011,"rechts wand-glas scharnier met heffunctie bij het openen. UNITO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière droite mur-verre avec rehausseur sur l'ouverture. UNITO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","Right wall-glass hinge with lifting function at opening. UNITO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.",735,"Warm Bronze PVD",1726,"GPF670111P037G000","8055261224469"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67013,67013,"links wand-glas scharnier met heffunctie bij het openen. UNITO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte900 mm.","Charnière gauche mur-verre avec rehausseur sur l'ouverture. UNITO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","Left wall-glass hinge with lifting function at opening. UNITO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width900 mm.",726,"Warm Bronze Brushed PVD",1842,"GPF670131P024G000","8055261224124"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67093,67093,"rechts wand-glas scharnier met heffunctie bij het openen. UNITO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière droite MUR-VERRE avec fonction d'élévation. UNITO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeurmaximum 900mm.","Right wall-glass hinge with lifting function at opening. UNITO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width 900 mm.",726,"Warm Bronze Brushed PVD",1842,"GPF670930P024G000","8055261219625"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67095,67095,"links wand-glas scharnier met heffunctie bij het openen. UNITO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte900 mm.","Charnière gauche MUR-VERRE avec fonction d'élévation. UNITO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeurmaximum 900mm.","Left wall-glass hinge with lifting function at opening. UNITO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximum width900 mm.",706,"Black Metal PVD",1726,"GPF670950P001G000","8055261219335"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67017,67017,"180° links glas-glas scharnier met heffunctie bij het openen. UNITO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière gauche verre-verre avec rehausseur sur l'ouverture 180°. UNITO. Epaisseur du verre 8-10 mm. Poids maximum de la porte40Kg, largeur maximum 900mm.","180° Left glass-glass hinge with lifting function at opening. UNITO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximumwidth 900 mm.",706,"Black Metal PVD",2465,"GPF670171P001G000","8055261223479"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67085,67085,"90° rechts glas-glas scharnier met heffunctie bij het openen. UNITO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière droite VERRE-VERRE avec fonction d'élévation 90°. UNITO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","90° Right glass-glass hinge with lifting function at opening. UNITO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximumwidth 900 mm.","030","Copper PVD",2465,"GPF670850P000G000","8055261221147"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67087,67087,"90° links glas-glas scharnier met heffunctie bij het openen. UNITO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière gauche VERRE-VERRE avec fonction d'élévation 90°. UNITO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","90° Left glass-glass hinge with lifting function at opening. UNITO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximumwidth 900 mm.",299,"Matte Black",2248,"GPF670870C072G000","8055261220836"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67087,67087,"90° links glas-glas scharnier met heffunctie bij het openen. UNITO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière gauche VERRE-VERRE avec fonction d'élévation 90°. UNITO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","90° Left glass-glass hinge with lifting function at opening. UNITO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximumwidth 900 mm.",845,"Dark Bronze",2630,"GPF670870V221G000","8055261220669"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67091,67091,"90° links glas-glas scharnier met heffunctie bij het openen. UNITO. 8-10 mm glas dikte. maximale deurgewicht 40 kg, maximale breedte 900 mm.","Charnière gauche VERRE-VERRE avec fonction d'élévation 90°. UNITO. Epaisseur du verre 8-10 mm. Poids maximum de la porte 40Kg, largeur maximum 900mm.","90° Left glass-glass hinge with lifting function at opening. UNITO. 8-10 mm glass thickness. Maximum door weight 40 kg, maximumwidth 900 mm.",147,"Chome Brushed",2248,"GPF670910G006G000","8055261220089"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67005,67005,"glas-wand Klem","Pince Mur-Verre. UNITO. Epaisseur du verre 8-10-12 mm.","Wall-Glass clamp. UNITO. 8-10-12 mm glass thickness.",713,"Antique Brass",797,"GPF670051V204G000","8056603596756"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67006,67006,"wand-glas klem. UNITO. 8-10-12 mm glas dikte.","Pince Mur-Verre. UNITO. Epaisseur du verre 8-10-12 mm.","Wall-Glass clamp. UNITO. 8-10-12 mm glass thickness.",299,"Matte Black",681,"GPF670061C072G000","8055261234703"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67007,67007,"Glas-Glas Klem","Pince Verre-Verre 90°. UNITO. Epaisseur du verre 8-10-12 mm.","Glass-Glass clamp 90°. UNITO. 8-10-12 mm glass thickness.",246,"Gold PVD",1018,"GPF670071P007G000","8056603596626"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67008,67008,"glas-glas klem 180°. UNITO. 8-10-12 mm glas dikte.","Pince Verre-Verre 180°. UNITO. Epaisseur du verre 8-10-12 mm.","Glass-Glass clamp 180°. UNITO. 8-10-12 mm glass thickness.","031","Chrome",678,"GPF670080G001G000","8055261225145"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67008,67008,"glas-glas klem 180°. UNITO. 8-10-12 mm glas dikte.","Pince Verre-Verre 180°. UNITO. Epaisseur du verre 8-10-12 mm.","Glass-Glass clamp 180°. UNITO. 8-10-12 mm glass thickness.",726,"Warm Bronze Brushed PVD",1070,"GPF670080P024G000","8055261225022"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67010,67010,"klem. vloer/plafond installatie. UNITO. 8-10-12 mm glas dikte.","Pince. Installation au sol/au plafond. UNITO. Epaisseur du verre 8-10-12 mm.","Floor/Ceiling Glass clamp.  UNITO.• 5/16\" - 1/2\" (8-12mm) glass thickness.",708,"Copper Brushed PVD",734,"GPF670100P006G000","8055261224704"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67071,67071,"glas stabilisatie stang. UNITO. 8-10 mm glas dikte.","Barre de fixation du verre. UNITO. Epaisseur du verre 8-10 mm.","Glass holding arm. UNITO. 8-10 mm glass thickness.","031","Chrome",414,"GPF670710G001G000","8055261166868"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67073,67073,"glas verstelbare stabilisatie stang. UNITO. 8-10 mm glas dikte.","Barre de fixation du verre. Longueur réglable. UNITO. Epaisseur du verre 8-10 mm.","Glass holding adjustable arm. UNITO. 8-10 mm glass thickness.",706,"Black Metal PVD",774,"GPF670730P001G000","8055261238800"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G SWING SYSTEM UNITO",67075,67075,"T-gevormd verstelbare slang Adjustable. UNITO. 8-10 mm glas dikte.","Barre de fixation du verre. Longueur réglable. UNITO. Epaisseur du verre 8-10 mm.","T-shaped adjustable glass rod Adjustable. UNITO. 8-10 mm glass thickness.",845,"Dark Bronze",1230,"GPF670750V221G000","8055261238534"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67521,67521,"20 cm Greep. RIGATO","Poignée 20 cm. RIGATO","20 cm Handle. Vertical/horizontal installation. RIGATO",720,"Nickel PVD",815,"GPF675211P014G000","8056603636155"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67523,67523,"30 cm Greep. RIGATO","Poignée 30 cm. RIGATO","30 cm Handle. Vertical/horizontal installation. RIGATO","031","Chrome",641,"GPF675231G001G000","8056603593496"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67523,67523,"30 cm Greep. RIGATO","Poignée 30 cm. RIGATO","30 cm Handle. Vertical/horizontal installation. RIGATO",246,"Gold PVD",1076,"GPF675231P007G000","8056603593380"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67525,67525,"45 cm Greep. RIGATO","Poignée 45 cm. RIGATO","45 cm Handle. Vertical/horizontal installation. RIGATO",713,"Antique Brass",1159,"GPF675251V204G000","8056603593151"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67527,67527,"60 cm Greep. RIGATO","Poignée 60 cm. RIGATO","60 cm Handle. Vertical/horizontal installation. RIGATO",727,"Brass Brushed PVD",1230,"GPF675271P025G000","8056603592994"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67533,67533,"30 cm dubbele greep. RIGATO","Double poignée 30cm. Installation verticale/horizontale. RIGATO","30 cm Double handle. Vertical/horizontal installation. RIGATO",187,"Aged Bronze",1592,"GPF675331G052G000","8056603592727"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67535,67535,"45 cm dubbele greep. RIGATO","Double poignée 45cm. Installation verticale/horizontale. RIGATO","45 cm Double handle. Vertical/horizontal installation. RIGATO",710,"Brass PVD",1761,"GPF675351P011G000","8056603592475"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67537,67537,"60 cm dubbele greep. RIGATO","Double poignée 60cm. Installation verticale/horizontale. RIGATO","60 cm Double handle. Vertical/horizontal installation. RIGATO",710,"Brass PVD",1896,"GPF675371P011G000","8056603592291"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67541,67541,"30 cm Handdoekhouder. RIGATO","Porte serviette 30 cm. RIGATO","30 cm towel rail. RIGATO",708,"Copper Brushed PVD",1013,"GPF675411P006G000","8056603592130"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67543,67543,"45 cm Handdoekhouder. RIGATO","Porte serviette 45 cm. RIGATO","45 cm towel rail. RIGATO",726,"Warm Bronze Brushed PVD",1159,"GPF675431P024G000","8056603591928"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67542,67542,"30 cm greep en handdoek houder. RIGATO","Poignée et porte serviette 30 cm. RIGATO","30 cm Handle and towel rail. RIGATO","030","Copper PVD",1492,"GPF675421P000G000","8056603625722"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67544,67544,"45 cm greep en handdoek houder RIGATO","Poignée et porte serviette 45 cm. RIGATO","45 cm Handle and towel rail RIGATO",727,"Brass Brushed PVD",1881,"GPF675441P025G000","8056603625456"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67546,67546,"60 cm greep en handdoek houder RIGATO","Poignée et porte serviette 60 cm. RIGATO","60 cm Handle and towel rail RIGATO","031","Chrome",1281,"GPF675461G001G000","8056603625401"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67621,67621,"20 cm Greep. DIAMANTATO","Poignée 20 cm. DIAMANTATO","20 cm Handle. Vertical/horizontal installation. DIAMANTATO","031","Chrome",551,"GPF676211G001G000","8056603590792"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67623,67623,"30 cm Greep. DIAMANTATO","Poignée 30 cm. DIAMANTATO","30 cm Handle. Vertical/horizontal installation. DIAMANTATO",708,"Copper Brushed PVD",1013,"GPF676231P006G000","8056603590518"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67625,67625,"45 cm Greep. DIAMANTATO","Poignée 45 cm. DIAMANTATO","45 cm Handle. Vertical/horizontal installation. DIAMANTATO",716,"Gold Brushed PVD",1232,"GPF676251P005G000","8056603590341"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67627,67627,"60 cm Greep. DIAMANTATO","Poignée 60 cm. DIAMANTATO","60 cm Handle. Vertical/horizontal installation. DIAMANTATO","030","Copper PVD",1152,"GPF676271P000G000","8056603590198"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67631,67631,"20 cm dubbele greep. DIAMANTATO","Double poignée 20cm. Installation verticale/horizontale. DIAMANTATO","20 cm Double handle. Vertical/horizontal installation. DIAMANTATO",710,"Brass PVD",1219,"GPF676311P011G000","8056603589956"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67633,67633,"30 cm dubbele greep. DIAMANTATO","Double poignée 30cm. Installation verticale/horizontale. DIAMANTATO","30 cm Double handle. Vertical/horizontal installation. DIAMANTATO",710,"Brass PVD",1492,"GPF676331P011G000","8056603589772"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67637,67637,"60 cm dubbele greep. DIAMANTATO","Double poignée 60cm. Installation verticale/horizontale. DIAMANTATO","60 cm Double handle. Vertical/horizontal installation. DIAMANTATO",707,"Black Metal Brushed PVD",2023,"GPF676371P004G000","8056603589451"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67641,67641,"30 cm Handdoekhouder. DIAMANTATO","Porte serviette 30 cm. DIAMANTATO","30 cm towel rail. DIAMANTATO",707,"Black Metal Brushed PVD",1013,"GPF676411P004G000","8056603589277"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67643,67643,"45 cm Handdoekhouder. DIAMANTATO","Porte serviette 45 cm. DIAMANTATO","45 cm towel rail. DIAMANTATO",706,"Black Metal PVD",1086,"GPF676431P001G000","8056603589109"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67645,67645,"60 cm Handdoekhouder. DIAMANTATO","Porte serviette 60 cm. DIAMANTATO","60 cm towel rail. DIAMANTATO",147,"Chome Brushed",1051,"GPF676451G006G000","8056603588973"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67644,67644,"45 cm greep en handdoek houder DIAMANTATO","Poignée et porte serviette 45 cm. DIAMANTATO","45 cm Handle and towel rail DIAMANTATO",147,"Chome Brushed",1607,"GPF676441G006G000","8056603624251"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67646,67646,"60 cm greep en handdoek houder DIAMANTATO","Poignée et porte serviette 60 cm. DIAMANTATO","60 cm Handle and towel rail DIAMANTATO",299,"Matte Black",1729,"GPF676461C072G000","8056603624091"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67646,67646,"60 cm greep en handdoek houder DIAMANTATO","Poignée et porte serviette 60 cm. DIAMANTATO","60 cm Handle and towel rail DIAMANTATO",845,"Dark Bronze",2023,"GPF676461V221G000","8056603623919"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67023,67023,"30 cm Greep. UNITO","Poignée 30 cm. UNITO","30 cm Handle. Vertical/horizontal installation. UNITO",147,"Chome Brushed",865,"GPF670231G006G000","8056603596350"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67023,67023,"30 cm Greep. UNITO","Poignée 30 cm. UNITO","30 cm Handle. Vertical/horizontal installation. UNITO",716,"Gold Brushed PVD",1076,"GPF670231P005G000","8056603596282"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67025,67025,"45 cm Greep. UNITO","Poignée 45 cm. UNITO","45 cm Handle. Vertical/horizontal installation. UNITO",845,"Dark Bronze",1159,"GPF670251V221G000","8055261232426"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67031,67031,"20 cm dubbele greep. UNITO","Double poignée 20cm. Installation verticale/horizontale. UNITO","20 cm Double handle. Vertical/horizontal installation. UNITO",246,"Gold PVD",1386,"GPF670311P007G000","8056603595728"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67033,67033,"30 cm dubbele greep. UNITO","Double poignée 30cm. Installation verticale/horizontale. UNITO","30 cm Double handle. Vertical/horizontal installation. UNITO",735,"Warm Bronze PVD",1492,"GPF670331P037G000","8056603595506"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67037,67037,"60 cm dubbele greep. UNITO","Double poignée 60cm. Installation verticale/horizontale. UNITO","60 cm Double handle. Vertical/horizontal installation. UNITO",149,"Finox Brushed Nickel",1729,"GPF670371G002G000","8056603595285"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67037,67037,"60 cm dubbele greep. UNITO","Double poignée 60cm. Installation verticale/horizontale. UNITO","60 cm Double handle. Vertical/horizontal installation. UNITO",707,"Black Metal Brushed PVD",2023,"GPF670371P004G000","8056603595216"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67041,67041,"30 cm Handdoekhouder. UNITO","Porte serviette 30 cm. UNITO","30 cm towel rail. UNITO",187,"Aged Bronze",1013,"GPF670411G052G000","8056603595063"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67045,67045,"60 cm Handdoekhouder. UNITO","Porte serviette 60 cm. UNITO","60 cm towel rail. UNITO",706,"Black Metal PVD",1152,"GPF670451P001G000","8056603594684"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67045,67045,"60 cm Handdoekhouder. UNITO","Porte serviette 60 cm. UNITO","60 cm towel rail. UNITO",716,"Gold Brushed PVD",1306,"GPF670451P005G000","8056603594660"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67042,67042,"30 cm greep en handdoek houder UNITO","Poignée et porte serviette 30 cm. UNITO","30 cm Handle and towel rail UNITO",845,"Dark Bronze",1592,"GPF670421V221G000","8055261234338"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G ACCESSORIES",67044,67044,"45 cm greep en handdoek houder UNITO","Poignée et porte serviette 45 cm. UNITO","45 cm Handle and towel rail UNITO",845,"Dark Bronze",1881,"GPF670441V221G000","8055261234130"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G DRAINS",67051,67051,"60 cm drain voor GEBERIT Cleanline/VIEGA Advantix Cleviva","Vidage 60cm pour GEBERIT Cleanline/VIEGA Advantix Cleviva","Lateral cover for 67050 L=60cm",246,"Gold PVD",617,"GPF670510P007G000","8056603601764"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G DRAINS",67055,67055,"80 cm drain voor GEBERIT Cleanline/VIEGA Advantix Cleviva","Vidage 80cm pour GEBERIT Cleanline/VIEGA Advantix Cleviva","Lateral cover for 67050 L=80cm",706,"Black Metal PVD",679,"GPF670550P001G000","8056603601443"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G DRAINS",67057,67057,"90 cm drain voor GEBERIT Cleanline/VIEGA Advantix Cleviva","Vidage 90cm pour GEBERIT Cleanline/VIEGA Advantix Cleviva","Lateral cover for 67050 L=90cm",706,"Black Metal PVD",747,"GPF670570P001G000","8056603601269"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G DRAINS",67561,67561,"Cover voor waste RIGATO","Couverture pour vidage RIGATO","Central cover for 67050. RIGATO",706,"Black Metal PVD",380,"GPF675610P001G000","8056603591621"]
["PRIVATE WELLNESS","SHOWER G","SHOWER G DRAINS",67661,67661,"Cover voor waste DIAMANTATO","Couverture pour vidage DIAMANTATO","Central cover for 67050. DIAMANTATO",708,"Copper Brushed PVD",405,"GPF676610P006G000","8056603588713"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR ORIGINI","63215+63210","63210","Externe delen voor 2 uitgangen doucheset, compleet te maken met 66212 kit en douche in gewenste afwerking.","Parties apparentes pour colonne de douche pour l'extérieure 2 sorties, à compléter avec le kit 66212 et spotwater dans la finition souhaitée","External part for two exits outdoor shower column, to complete with 66212 kit and shower head in the desired finishing.",239,"Steel Brushed",4792,"GPF632100A000G000","8056603672047"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR ORIGINI",66152,66152,"Anti-kalk hoofddouche. Te combineren met artikel 63209, 63210.","Pomme de douche anticalcaire orientable. À combiner avec art. 63209, 63210.","Antilimestone adjustable shower head. To be matched with art. 63209, 63210.",707,"Black Metal Brushed PVD",2800,"GPF661520P004G000","8056603579247"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR ORIGINI",66600,66600,"inleg","Insert","Insert",761,"Coffee Bronze Brushed PVD",111,"GPF666000E059G000","8055261587946"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR","63215+63204",63204,"twee uitgangen thermostatische douchekolom, te completeren met 63216 kit en SpotWater in gewenste afwerking.","Colonne de douche thermostatique 2 voies pour extérne. À compléter avec le kit 63216 et SpotWater dans la finition souhaitée.","External part for two exits thermostatic shower column, to be completed with 63216 kit and SpotWater in desired finish.",856,"Corten",6500,"GPF632040T091G000","8055261234833"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",63213,63213,"Handgreepset voor artikel 63205 en 63231","Kit poignée pour articles 63205 et 63231","Lever kit for 63205 and 63231",761,"Coffee Bronze Brushed PVD",750,"GPF632130E059G000","8055261593572"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR","63215+63207",63207,"Externe onderdelen 2-weg buitendouchekolom, te completeren met kit 63214 en SpotWater, in de gewenste afwerking.","Partie apparente pour colonne de douche outdoor 2 sorties, à compléter par le kit 63214 et spotwater dans la finition souhaité e","External Parts for two exits shower column, to be completed with 63214 kit and SpotWater in the desired finish.",299,"Matte Black",7517,"GPF632070C072G000","8056329534452"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",57205,57205,"Oriënteerbare wand-hoofddouchekop FLESSA. VERNEVELING-functie","Pomme de douche murale orientable FLESSA. Fonction BRUMISATION","Wall-mounted adjustable showerhead FLESSA. Mist function",727,"Brass Brushed PVD",1483,"GPF572050P025G000","8056329598089"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",57245,57245,"Oriënteerbare wand-hoofddouchekop TRAME. VERNEVELING-functie","Pomme de douche murale orientable TRAME. Fonction BRUMISATION","Wall-mounted adjustable showerhead TRAME. Mist function",726,"Warm Bronze Brushed PVD",1867,"GPF572450P024G000","8056329106697"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",57247,57247,"Oriënteerbare wand-hoofddouchekop TRAME. CASCADE-functie","Pomme de douche murale orientable TRAME. Fonction CASCADE","Wall-mounted adjustable showerhead TRAME. Waterfall function",707,"Black Metal Brushed PVD",2110,"GPF572470P004G000","8056329106673"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",57217,57217,"Oriënteerbare wand-hoofddouchekop INTRECCIO. CASCADE-functie","Pomme de douche murale orientable INTRECCIO. Fonction CASCADE","Wall-mounted adjustable showerhead INTRECCIO. Waterfall function",299,"Matte Black",1924,"GPF572170C072G000","8056329598010"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",57277,57277,"Oriënteerbare wand-hoofddouchekop RIGATO. REGEN-functie","Pomme de douche murale orientable RIGATO. Fonction PLUIE","Wall-mounted adjustable showerhead RIGATO. Rain function",708,"Copper Brushed PVD",1934,"GPF572770P006G000","8056603687119"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",57285,57285,"Oriënteerbare wand-hoofddouchekop RIGATO. CASCADE-functie","Pomme de douche murale orientable RIGATO. Fonction CASCADE","Wall-mounted adjustable showerhead RIGATO. Waterfall function",726,"Warm Bronze Brushed PVD",2109,"GPF572850P024G000","8056603686860"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",57287,57287,"Oriënteerbare wand-hoofddouchekop DIAMANTATO. Multispray-functie","Pomme de douche murale orientable DIAMANTATO. Fonction Multi-spray","Wall-mounted adjustable showerhead DIAMANTATO. Multi-spray function",727,"Brass Brushed PVD",1934,"GPF572870P025G000","8056603693820"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",57223,57223,"Oriënteerbare wand-hoofddouchekop MECCANICA. REGEN-functie","Pomme de douche murale orientable MECCANICA. Fonction PLUIE","Wall-mounted adjustable showerhead MECCANICA. Rain function",726,"Warm Bronze Brushed PVD",1934,"GPF572230P024G000","8056329107052"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",57227,57227,"Oriënteerbare wand-hoofddouchekop MECCANICA. CASCADE-functie","Pomme de douche murale orientable MECCANICA. Fonction CASCADE","Wall-mounted adjustable showerhead MECCANICA. Waterfall function",726,"Warm Bronze Brushed PVD",2110,"GPF572270P024G000","8056329106970"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",57233,57233,"Oriënteerbare wand-hoofddouchekop CESELLO. REGEN-functie","Pomme de douche murale orientable CESELLO. Fonction PLUIE","Wall-mounted adjustable showerhead CESELLO. Rain function",726,"Warm Bronze Brushed PVD",1934,"GPF572330P024G000","8056329106895"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR",57237,57237,"Oriënteerbare wand-hoofddouchekop CESELLO. CASCADE-functie","Pomme de douche murale orientable CESELLO. Fonction CASCADE","Wall-mounted adjustable showerhead CESELLO. Waterfall function",727,"Brass Brushed PVD",2110,"GPF572370P025G000","8056329597860"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR L",63212,63212,"Handgreep / doucheset voor artikel 63203.","Kit poignée pour articles 63203 et 63229","Lever/handshower kit for 63203 and 63229",761,"Coffee Bronze Brushed PVD",2010,"GPF632120E059G000","8055261593596"]
["PRIVATE WELLNESS","OUTDOOR","OUTDOOR L",57703,57703,"Wand Gemonteerde Hoofddouche Met Chromotherapie Flessa. Regen Functie. Te combineren met artikel 63225, 63229, 63231, 63233 en voedingseenheid 12 V RIR5402, niet inbegrepen.","Pomme de douche murale orientable avec cromothérapie FLESSA. Fonction Pluie. À combiner avec art. 63225, 63229, 63231, 63233 etalimentation 12 V RIR5402, non inclus.","Wall-mounted adjustable showerhead with chromotherapy FLESSA. Rain function. To be matched with art. 63225, 63229, 63231, 63233and 12V RIR5402 power supply (not included).",707,"Black Metal Brushed PVD",2215,"GPF577030P004G000","8056603460743"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS",58023,58023,"Elektronische Wastafelkraan met temperatuur- en debietregeling via hoekstopkraan onder wastafel","Mitigeur lavabo electronique fourni avec 2 robinets sous-lavabo pour contrôle de la température et du débit.","Electronic basin mixer with temperature and water flow rate adjustment through under-basin control (included)",716,"Gold Brushed PVD",2672,"GPF580230P005G000","8056603908825"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44665+58105",58105,"Extern deel Elektronische Wastafelkraan","Partie apparente pour mitigeur lavabo ELECTRONIQUE mural","External part for wall-mounted electronic mixer",726,"Warm Bronze Brushed PVD",2441,"GPF581050P024G000","8056329596696"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44665+58107",58107,"Extern deel Elektronische Wastafelkraan","Partie apparente pour mitigeur lavabo ELECTRONIQUE mural","External part for wall-mounted electronic mixer",716,"Gold Brushed PVD",2594,"GPF581070P005G000","8055261230767"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+58024",58024,"Extern deel Elektronische Plafondwastafelkraan met temperatuur- en debietregeling via hoekstopkraan onder wastafel.","Partie apparente pour Robinet éléctronique avec fixation au plafond, réglage de la température et du débit avec robinets sous-lavabo","External part for Ceiling-mounted Electronic mixer with temperature and water flow rate adjustment through under-basin control (included)",735,"Warm Bronze PVD",3995,"GPF580240P037G000","8056329597259"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+58019",58019,"Extern deel Elektronische Wandafstandsbediening met box voor de regeling van temperatuur en debiet","Partie apparente pour commande séparée electronique murale, avec boîte pour le contrôle de la température et du débit.","External parts for built-in electronic separate control with temperature and flow rate setting box.",735,"Warm Bronze PVD",1375,"GPF580190P037G000","8056329597303"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+58019",58019,"Extern deel Elektronische Wandafstandsbediening met box voor de regeling van temperatuur en debiet","Partie apparente pour commande séparée electronique murale, avec boîte pour le contrôle de la température et du débit.","External parts for built-in electronic separate control with temperature and flow rate setting box.",246,"Gold PVD",1563,"GPF580190P007G000","8056329143180"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS",54181,54181,"Elektronische Wastafelkraan met temperatuur- en debietregeling via hoekstopkraan onder wastafel. INTRECCIO.","Mitigeur lavabo electronique fourni avec 2 robinets sous-lavabo pourcontrôle de la température et du débit. INTRECCIO.","Electronic basin mixer with temperature and water flow rate adjustment through under-basin control (included)",239,"Steel Brushed",1752,"GPF541810A000G000","8056329141322"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS",54481,54481,"Elektronische Wastafelkraan met temperatuur- en debietregeling via hoekstopkraan onder wastafel. CESELLO.","Mitigeur lavabo electronique fourni avec 2 robinets sous-lavabo pourcontrôle de la température et du débit. CESELLO.","Electronic basin mixer with temperature and water flow rate adjustment through under-basin control (included)",239,"Steel Brushed",1752,"GPF544810A000G000","8056329141087"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44665+54015",54015,"Extern deel Elektronische Wastafelkraan. FLESSA.","Partie apparente pour mitigeur lavabo ELECTRONIQUE mural FLESSA","External part for wall-mounted electronic mixer. FLESSA.",299,"Matte Black",2243,"GPF540150C072G000","8056329601109"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44665+54315",54315,"Extern deel Elektronische Wastafelkraan. TRAME.","Partie apparente pour mitigeur lavabo ELECTRONIQUE mural TRAME","External part for wall-mounted electronic mixer. TRAME.",761,"Coffee Bronze Brushed PVD",2889,"GPF543150E059G000","8055261600126"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44665+54115",54115,"Extern deel Elektronische Wastafelkraan. INTRECCIO.","Partie apparente pour mitigeur lavabo ELECTRONIQUE mural INTRECCIO","External part for wall-mounted electronic mixer. INTRECCIO.",239,"Steel Brushed",1828,"GPF541150A000G000","8056329141360"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44665+54414",54414,"Extern deel Elektronische Wastafelkraan. CESELLO.","Partie apparente pour mitigeur lavabo ELECTRONIQUE mural CESELLO","External part for wall-mounted electronic mixer. CESELLO.",299,"Matte Black",2304,"GPF544140C072G000","8056329599338"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44665+54415",54415,"Extern deel Elektronische Wastafelkraan. CESELLO.","Partie apparente pour mitigeur lavabo ELECTRONIQUE mural CESELLO","External part for wall-mounted electronic mixer. CESELLO.",727,"Brass Brushed PVD",2706,"GPF544150P025G000","8056329599307"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+54126",44679,"Inbouwdeel Elektronische Wandafstandsbediening","Partie encastrée pour commande séparée electronique murale.","Built-in part for wall-mounted electronic separate control","031","Chrome",552,"GPF446790G001G000","8056329141032"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+54226",54226,"Extern deel Elektronische Plafondwastafelkraan aanpasbare hoogte met temperatuur- en debietregeling via hoekstopkraan onder wastafel. MECCANICA","Partie apparente pour Robinet éléctronique avec fixation au plafond, longueur à la demande, réglage de la température et du débit avec robinets sous-lavabo MECCANICA","External part for Ceiling-mounted Electronic mixer, length on request, with temperature and water flow rate adjustment through under-basin control MECCANICA (included)",707,"Black Metal Brushed PVD",6214,"GPF542260P004G000","8056329541351"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+54426",54426,"Extern deel Elektronische Plafondwastafelkraan met temperatuur- en debietregeling via hoekstopkraan onder wastafel. CESELLO","Partie apparente pour Robinet éléctronique avec fixation au plafond, longueur à la demande, réglage de la température et du débit avec robinets sous-lavabo CESELLO","External part for Ceiling-mounted Electronic mixer, length on request, with temperature and water flow rate adjustment through under-basin control CESELLO (included)",707,"Black Metal Brushed PVD",6214,"GPF544260P004G000","8056329541276"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS",59023,59023,"Elektronische Wastafelkraan met temperatuur- en debietregeling via hoekstopkraan onder wastafel","Mitigeur lavabo electronique fourni avec 2 robinets sous-lavabo pour contrôle de la température et du débit.","Electronic basin mixer with temperature and water flow rate adjustment through under-basin control (included)",299,"Matte Black",1584,"GPF590230C072G000","8056329142756"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+59107",59107,"Extern deel Elektronische Wastafelkraan","Partie apparente pour mitigeur lavabo ELECTRONIQUE mural","External part for wall-mounted electronic mixer",710,"Brass PVD",1690,"GPF591070P011G000","8056329593800"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+59029",59029,"Extern deel Elektronische Wandafstandsbediening met box voor de regeling van temperatuur en debiet","Partie apparente pour commande séparée electronique murale, avec boîte pour le contrôle de la température et du débit.","External parts for built-in electronic separate control with temperature and flow rate setting box.",720,"Nickel PVD",1375,"GPF590290P014G000","8056603605892"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+20130",20130,"Extern deel Elektronische Wastafelkraan","Partie apparente pour mitigeur lavabo ELECTRONIQUE mural","External part for wall-mounted electronic mixer",299,"Matte Black",1705,"GPF201300C072G000","8056329160064"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+20024",44679,"Inbouwdeel Elektronische Wandafstandsbediening","Partie encastrée pour commande séparée electronique murale.","Built-in part for wall-mounted electronic separate control","031","Chrome",552,"GPF446790G001G000","8056329141032"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+20026",20026,"Extern deel Elektronische Plafondwastafelkraan aanpasbare hoogte met temperatuur- en debietregeling via hoekstopkraan onder wastafel.","Partie apparente pour Robinet éléctronique avec fixation au plafond, longueur à la demande, réglage de la température et du débit avec robinets sous-lavabo","External part for Ceiling-mounted Electronic mixer, length on request, with temperature and water flow rate adjustment through under-basin control (included)",149,"Finox Brushed Nickel",6352,"GPF200260G002G000","8056329541702"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS",30653,30653,"Elektronische Afstandsbediening voor uitloop met temperatuur- en debietregeling via hoekstopkraan onder wastafel","Commande séparée ELECTRONIQUE sur plan fournie avec flexibles de raccordement 3/8\", batterie et 2 robinets sous-lavabo pour controle de la température et du débit.","Electronic separate control with under-basin mixer to regulate flow rate and temperature (included)",761,"Coffee Bronze Brushed PVD",1522,"GPF306530E059G000","8055261608696"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+30654",30654,"Extern deel Elektronische Plafondwastafelkraan met temperatuur- en debietregeling via hoekstopkraan onder wastafel.","Partie apparente pour Robinet éléctronique avec fixation au plafond, réglage de la température et du débit avec robinets sous-lavabo","External part for Ceiling-mounted Electronic mixer with temperature and water flow rate adjustment through under-basin control (included)",708,"Copper Brushed PVD",3995,"GPF306540P006G000","8056329540392"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+30654",30654,"Extern deel Elektronische Plafondwastafelkraan met temperatuur- en debietregeling via hoekstopkraan onder wastafel.","Partie apparente pour Robinet éléctronique avec fixation au plafond, réglage de la température et du débit avec robinets sous-lavabo","External part for Ceiling-mounted Electronic mixer with temperature and water flow rate adjustment through under-basin control (included)",279,"Matte White",3414,"GPF306540C071G000","8056329540477"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+33724",33724,"Extern deel Elektronische Plafondwastafelkraan met temperatuur- en debietregeling via hoekstopkraan onder wastafel.","Partie apparente pour Robinet éléctronique avec fixation au plafond, réglage de la température et du débit avec robinets sous-lavabo","External part for Ceiling-mounted Electronic mixer with temperature and water flow rate adjustment through under-basin control (included)",707,"Black Metal Brushed PVD",3938,"GPF337240P004G000","8055261644373"]
["SENSOR TAPS","SENSOR TAPS","SENSOR TAPS","44679+33726",33726,"Extern deel Elektronische Plafondwastafelkraan aanpasbare hoogte met temperatuur- en debietregeling via hoekstopkraan onder wastafel.","Partie apparente pour Robinet éléctronique avec fixation au plafond, longueur à la demande, réglage de la température et du débit avec robinets sous-lavabo","External part for Ceiling-mounted Electronic mixer, length on request, with temperature and water flow rate adjustment through under-basin control (included)","030","Copper PVD",5133,"GPF337260P000G000","8055261644311"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","RI43127","RI43127","Verlengstuk hoogte 25 mm voor thermostaatmengkraan hoog debiet","Rallonge hauteur 25 mm pour mitigeur thermostatique haut débit.","25 mm height THERMOSTATIC HIGH-CAPACITY mixer extension","031","Chrome",414,"GRI431270G001G000","8022692797053"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","RIR4204","RIR4204","Verlengstuk hoogte 25 mm","Rallonge hauteur 25 mm.","25 mm height extension","031","Chrome",324,"GRIR42040G001G000","8022692622980"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","SP02810","SP02810","25-50 mm Verlengstuk voor wandgemonteerde uitloop Sensor kraan","Rallonge 25-50 mm pour bec de lavabo mural Sensor Taps","25-50 mm Extencion for wall-mounted spout Sensor Taps","031","Chrome",113,"GSP028100G001G000","8056329538085"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","SP02796","SP02796","0-25 mm Verlengstuk voor Hi-FI Compact/Linear","Rallonge 0-25 mm pour Hi Fi Compact/Linear","0-25 mm Extencion for Hi-FI Compact/Linear","031","Chrome",140,"GSP027960G001G000","8056329537972"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01785","01785","Uittrekbare handdouche afvoerset, tegelwandinstallatie. Niet passend op artikelen 01669, 01658, 01663 en 01664.","Système de récupération d'eau pour douchette flexible de bord de baignoire, installation murale. Ne peut être combiné avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, tile wall installation. Not fitting items 01669, 01658, 01663 and 01664.",708,"Copper Brushed PVD",1815,"GPF017850P006G000","8056329562592"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01786","01786","Uittrekbare handdouche afvoerset, randinstallatie. Niet passend op artikelen 01669, 01658, 01663 en 01664.","Système de récupération d'eau pour flexible de douchette, installation sur le bord de la baignoire. Ne peut être combiné avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, rim installation. Not fitting items 01669, 01658, 01663 and 01664.",713,"Antique Brass",1300,"GPF017860V204G000","8056329563650"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01766","01766","Uittrekbare handdouchekit, installatie op zijplan in de badkuip. Niet geschikt voor artikels 01669, 01658, 01663, 01664.","Système de récupération eau pour flexible de douchette bain-douche, installation sur plan latéral à la bagnoire. Non compatibleavec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, tile wall installation. Not fitting items 01669, 01658, 01663 and 01664.",708,"Copper Brushed PVD",1907,"GPF017660P006G000","8022692856309"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01767","01767","Uittrekbare handdouchekit, zijrand installatie. Niet geschikt voor artikels 01669, 01658, 01663, 01664.","Système de récupération eau pour flexible de douchette bain-douche, installation sur plan de bagnoire. Non compatible avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, rim installation. Not fitting items 01669, 01658, 01663 and 01664.",727,"Brass Brushed PVD",1455,"GPF017670P025G000","8056329614987"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01811","01811","Uittrekbare handdouchekit, zijrand installatie. Niet geschikt voor artikels 01669, 01658, 01663, 01664.","Système de récupération eau pour flexible de douchette bain-douche, installation sur plan de bagnoire. Non compatible avec 01669, 01658, 01663 et 01664.","Pull-out handshower drain kit, rim installation. Not fitting items 01669, 01658, 01663 and 01664.",147,"Chome Brushed",1038,"GPF018110G006G000","8022692882520"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01663","01663","Drie-gats afwerkplaat voor montagebox","Plaque de finition 3 trous pour la boîte de sécurité","Three-holes finishing plate for mounting box","030","Copper PVD",736,"GPF016631P000G000","8022692877946"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01758","01758","Afwerkplaat 5 gaten voor secur box","Plaque de finition pour Secu Box robinetterie 5 trous","Five-holes finishing plate for mounting box",720,"Nickel PVD",723,"GPF017580P014G000","8056603608848"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01758","01758","Afwerkplaat 5 gaten voor secur box","Plaque de finition pour Secu Box robinetterie 5 trous","Five-holes finishing plate for mounting box",761,"Coffee Bronze Brushed PVD",874,"GPF017580E059G000","8055261609839"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01411","01411","Onderbouwmengkraan met filter en 1/2\" aansluiting","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection","031","Chrome",103,"GPF014110G001G000","8022692037494"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01411","01411","Onderbouwmengkraan met filter en 1/2\" aansluiting","Robinet design carré sous-lavabo avec filtre, raccord mural 1/2\". Achat par deux pièces. Prix unitaire.","Underbasin mixer with filter and 1/2\" connection",727,"Brass Brushed PVD",240,"GPF014110P025G000","8056329068797"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01410","01410","Sifon van 1 1/4\"","Siphon 1 1/4”.","1 1/4\" syphon",716,"Gold Brushed PVD",670,"GPF014100P005G000","8022692622331"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01018","01018","Sifon van 1 1/4\"","Siphon 1 1/4”.","1 1/4\" syphon",149,"Finox Brushed Nickel",138,"GPF010180G002G000","8022692788792"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01018","01018","Sifon van 1 1/4\"","Siphon 1 1/4”.","1 1/4\" syphon",727,"Brass Brushed PVD",171,"GPF010180P025G000","8056329516250"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01374","01374","1-1/4\" sifon","Siphon de 1-1/4\"","1-1/4\" Syphon",726,"Warm Bronze Brushed PVD",308,"GPF013740P024G000","8055261227958"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES",28767,28767,"Verlengstuk buis voor sifon, lengte 40 cm","Tubelure prolongée pour siphone, longueur 40 cm","Syphon pipe extension, 40 cm length",187,"Aged Bronze",83,"GPF287670G052G000","8056329543799"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",277,"Glossy Ocra",150,"GPF014200T211G000","8056603635097"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01422","01422","Wastafelafvoer “Stop&Go”, met overloop. Plug in kleurafwerking. 'Geen zichtdelen' in finish 031, op aanvraag verkrijgbaar in kleurafwerking.","Bonde de lavabo \"Stop&Go\" avec trop-plein. Bouchon en finition. Partie sous-céramique en finition 031, disponible en finition àla demande.","Basin waste “Stop&Go”, with overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.","031","Chrome",92,"GPF014220G001G000","8022692031652"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01422","01422","Wastafelafvoer “Stop&Go”, met overloop. Plug in kleurafwerking. 'Geen zichtdelen' in finish 031, op aanvraag verkrijgbaar in kleurafwerking.","Bonde de lavabo \"Stop&Go\" avec trop-plein. Bouchon en finition. Partie sous-céramique en finition 031, disponible en finition àla demande.","Basin waste “Stop&Go”, with overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",713,"Antique Brass",221,"GPF014220V204G000","8022692089677"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",713,"Antique Brass",221,"GPF014230V204G000","8022692855944"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",726,"Warm Bronze Brushed PVD",161,"GPF013910P024G000","8056329000797"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01408","01408","Wastafelafvoer “Stop&Go”, met overloop. Plug in kleurafwerking. 'Geen zichtdelen' in finish 031, op aanvraag verkrijgbaar in kleurafwerking.","Bonde de lavabo \"Stop&Go\" avec trop-plein. Bouchon en finition. Partie sous-céramique en finition 031, disponible en finition àla demande.","Basin waste “Stop&Go”, with overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",710,"Brass PVD",219,"GPF014080P011G000","8056329615267"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",708,"Copper Brushed PVD",84,"GPF013460P006G000","8056329039957"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",727,"Brass Brushed PVD",136,"GPF013500P025G000","8056329184176"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES",29263,29263,"1 1/4\" klik waste met overflow.","Vidage pour lavabo 1 1/4\" avec trop plein.","1 1/4” basin pop-up waste with overflow.",299,"Matte Black",128,"GPF292630C072G000","8056329106000"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES",29264,29264,"2 1/4\" klik waste met overflow.","Vidage pour lavabo 1 1/4\" avec trop plein.","1 1/4” basin pop-up waste with overflow.",147,"Chome Brushed",83,"GPF292640G006G000","8056329183520"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",299,"Matte Black",114,"GPF143720C072G000","8022692435283"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES",14372,14372,"Handdouche los 1/2\" met antikalk.","Douchette anticalcaire.","Antilimestone handshower.",279,"Matte White",120,"GPF143720C071G000","8022692435276"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",707,"Black Metal Brushed PVD",346,"GPF143760P004G000","8056329700093"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES",14376,14376,"3 functies antikalk handdouche met witte inleg","Douchette anticalcaire à 3 jets avec insert blanc","Three-setting antilimestone handshower with white insert",246,"Gold PVD",366,"GPF143760P007G000","8056603522571"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES",14378,14378,"3 functies antikalk handdouche met zwarte inleg.","Douchette anticalcaire 3 jets avec insert noir","Three-setting antilimestone handshower with black insert.",761,"Coffee Bronze Brushed PVD",367,"GPF143780E059G000","8055261609570"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES",47350,47350,"2-jet anti-kalk handdouche met selectie wiel","Douchette anticalcaire trois jets avec sélecteur roulant","Two function anti-limescale hand shower with wheel selector with black insert.",735,"Warm Bronze PVD",252,"GPF473500P037G000","8056603587112"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01724","01724","Dubbelnaads flexibele slang, 1,5 m lengte, 1/2\" connector","Longueur de tuyau à double agrafage 1,50 m avec raccord conique 1/2","Double-seam flexible hose, 1,5 m length, 1/2\" connector",720,"Nickel PVD",152,"GPF017240P014G000","8055261240025"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",726,"Warm Bronze Brushed PVD",120,"GPF016370P024G000","8056329555655"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01637","01637","1,50 m Cromalux flexibele slang met conischee 1/2\" aansluitingen","Longueur du tuyau Cromalux 1,50 m avec raccord conique 1/2\"","1,50 m Cromalux flexible hose with conic 1/2\" connections",187,"Aged Bronze",133,"GPF016370G052G000","8056329008779"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01080","01080","Polyethyleen badafvoer met overloopdopvuller. Lengte van de aanvoer leiding 80 cm","Vidage en polyéthylène baignoire avec trop-plein. Longueur 80 cm","Polyethylene column bath waste with overflow cap filler. Length of control cable 80 cm",149,"Finox Brushed Nickel",504,"GPF010802G002G000","8022692791082"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01452","01452","Waste van polyethyleen Bad. Lengte kabel 700 mm","Vidage en polyéthyléne pour baignoire. Longueur 70 cm.","Polyethylene column bath waste. Length of control cable 70 cm",706,"Black Metal PVD",413,"GPF014521P001G000","8056329039759"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01415","01415","Staande koppeling 3/4\" met rozet voor vrijstaande montage van badmengkraan (hoogte 800 mm).","Raccord colonnette sur pied pour baignoire, hauteur 800 mm.","Floor-mounted bathfiller connector, 800 mm height.",149,"Finox Brushed Nickel",640,"GPF014150G002G000","8022692794113"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","01021","01021","Bevestigingsset voor 43281/43283.","Kit de fixation pour art. 43281/43283.","Fixing kit for 43281/43283.","031","Chrome",67,"GPF010210G001G000","8055261201002"]
["TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","TECHNICAL ACCESSORIES","54057+54058",54058,"Extern deel afdekking terugstroombeveiligingssysteem","Partie apparente couverture système anti-reflux","External parts non-return system",187,"Aged Bronze",388,"GPF540580G052G000","8056603627986"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54611,54611,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12","Plaque de déclenchement pour Geberit Sigma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",279,"Matte White",848,"GPF546110C071G000","8056329070646"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54613,54613,"Bedieningspaneel voor VIEGA 1H, 2H, 2L","Plaque de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA. Compatible with products VIEGA 1H, 2H, 2L.",727,"Brass Brushed PVD",1495,"GPF546130P025G000","8056329070363"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.","030","Copper PVD",883,"GPF546150P000G000","8056329070301"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54615,54615,"Bedieningspaneel voor Geberit Omega 12.","Plaque de déclenchement pour GEBERIT OMEGA 12.","Cover plate GEBERIT OMEGA 12.",761,"Coffee Bronze Brushed PVD",947,"GPF546150E059G000","8055261598850"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54617,54617,"Bedieningspaneel voor TECE","Plaque de déclenchement pour TECE","Cover plate TECE",716,"Gold Brushed PVD",1121,"GPF546170P005G000","8056329098770"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54619,54619,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Plaque de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600",727,"Brass Brushed PVD",1386,"GPF546190P025G000","8056329540880"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54621,54621,"Bedieningspaneel voor VIEGA PREVISTA 12.","Plaque de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",279,"Matte White",1497,"GPF546211C071G000","8056329540859"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54625,54625,"Bedieningspaneel voor VIEGA 1H, 2H, 2L. DIAMANTATO","Plaques de déclenchement pour Viega 1H, 2H, 2L. DIAMANTATO","Cover plate VIEGA 1H, 2H, 2L. DIAMANTATO",187,"Aged Bronze",1623,"GPF546250G052G000","8056329566514"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54627,54627,"Bedieningspaneel voor Geberit OMEGA 12. DIAMANTATO","Plaques de déclenchement pour GEBERIT OMEGA 12. DIAMANTATO","Cover plate GEBERIT OMEGA 12. DIAMANTATO",720,"Nickel PVD",927,"GPF546270P014G000","8056603606837"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54631,54631,"Bedieningspaneel voor SANIT, Villeroy&Boch ViConnect 92246100 e 92247600. DIAMANTATO.","Plaques de déclenchement pour SANIT, Villeroy&Boch ViConnect 92246100 e 92247600. DIAMANTATO.","Cover plate SANIT, Villeroy&Boch ViConnect 92246100 e 92247600. DIAMANTATO.",713,"Antique Brass",1451,"GPF546310V204G000","8056329566101"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54633,54633,"Bedieningspaneel voor VIEGA PREVISTA 12. DIAMANTATO","Plaques de déclenchement pour VIEGA PREVISTA 12. DIAMANTATO","Cover plate VIEGA PREVISTA 12. DIAMANTATO",707,"Black Metal Brushed PVD",1836,"GPF546331P004G000","8056329566033"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54635,54635,"Bedieningspaneel voor Geberit SIgma 8 e Sigma 12. RIGATO","Plaques de déclenchement pour Geberit SIgma 8 e Sigma 12. RIGATO","Cover plate GEBERIT SIGMA 8 & 12. RIGATO",761,"Coffee Bronze Brushed PVD",1108,"GPF546351E059G000","8055261598676"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54637,54637,"Bedieningspaneel voor VIEGA 1H, 2H, 2L. RIGATO","Plaques de déclenchement pour Viega 1H, 2H, 2L. RIGATO","Cover plate VIEGA 1H, 2H, 2L. RIGATO",187,"Aged Bronze",1623,"GPF546370G052G000","8056329565852"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54641,54641,"Bedieningspaneel voor TECE. RIGATO","Plaques de déclenchement pour TECE. RIGATO","Cover plate TECE. RIGATO",706,"Black Metal PVD",1036,"GPF546410P001G000","8056329565609"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54645,54645,"Bedieningspaneel voor VIEGA PREVISTA 12. RIGATO","Plaques de déclenchement pour VIEGA PREVISTA 12. RIGATO","Cover plate VIEGA PREVISTA 12. RIGATO",708,"Copper Brushed PVD",1834,"GPF546451P006G000","8056329565364"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54651,54651,"Bedieningsplaat Geberit Sigma 8 & 12","Plaques de déclenchement pour Geberit SIgma 8 e Sigma 12","Cover plate GEBERIT SIGMA 8 & 12",713,"Antique Brass",1287,"GPF546510V204G000","8056603012584"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54653,54653,"Bedieningsplaat Viega 1H, 2H, 2L","Plaques de déclenchement pour Viega 1H, 2H, 2L","Cover plate VIEGA 1H, 2H, 2L",716,"Gold Brushed PVD",1918,"GPF546530P005G000","8055261230934"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54655,54655,"Bedieningsplaat GEBERIT Omega 12","Plaques de déclenchement pour GEBERIT OMEGA 12","Cover plate GEBERIT OMEGA 12",713,"Antique Brass",1234,"GPF546550V204G000","8056603012324"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54661,54661,"Bedieningsplaat Viega Prevista 12.","Plaques de déclenchement pour VIEGA PREVISTA 12.","Cover plate VIEGA PREVISTA 12.",149,"Finox Brushed Nickel",1493,"GPF546611G002G000","8056603012041"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54671,54671,"bedieningspaneel RIGATO voor GEBERIT SIGMA 8 & 12","Plaque de finissage RIGATO pour GEBRIT SIGMA 8 et 12","Cover plate RIGATO for GEBERIT SIGMA 8 & 12",299,"Matte Black",1788,"GPF546710C072G000","8056603458535"]
["TOTAL LOOK","FLUSH PLATE","FLUSH PLATE",54681,54681,"bedieningspaneel DIAMANTATO voor GEBERIT SIGMA 8 & 12","Plaque de finissage DIAMANTATO pour GEBRIT SIGMA 8 et 12","Cover plate DIAMANTATO for GEBERIT SIGMA 8 & 12",706,"Black Metal PVD",1960,"GPF546810P001G000","8056603458269"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39118,39118,"Wandtoilet van Keramiek (6 liter) met geïntegreerde sifon. Scharnieren met vertraagde sluiting en laterale gatafdekkingen opgenomen in afwerking 031","Cuvette suspendue en Céramique (6 litres) avec abattant muni de système “SOFT CLOSE” ou assisté. Charnière et enjoliveurs latéraux en finition 031","Wall hung WC (6 litres) in Ceramic, integrated siphon. Soft-closing hardware and lateral holes plugs included in 031 finishing.",532,"Matte Black Ceramic",1711,"GPF391180C289G000","8056603448543"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39184,39184,"Zachtsluitende hardware en zijdelingse gatenpluggen voor WC-zitting 39168.","Charnières avec système \"SOFT CLOSE\" et caches latéraux pour le siège 39168.","Soft-closing hardware and lateral holes plugs for WC seat 39168.",727,"Brass Brushed PVD",260,"GPF391840P025G000","8056603451864"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",46754,46754,"wandgemonteerde WC (6 liters) in keramiek, geïntegreerde sifon. Hardware en pluggen voor laterale gaten niet inbegrepen.","Cuvette murale en céramique (6 litres) avec siphon intégré. Charnières et sièges non inclus.","Wall hung WC (6 litres) in Ceramic, integrated siphon. Hardware and lateral holes plugs not included.",518,"White Ceramic",1157,"GPF467540C083G000","8056603626941"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39115,39115,"Wandbidet van Keramiek met overloop. Met centraal gat voor kraanwerk. Dop overloop en laterale gatafdekkingen opgenomen in afwerking 031.","Bidet suspendu en Céramique Blanc Europe avec vidage et trop plein, percé monotrou pour la robinetterie, fourni avec cache de trop plein et enjoliveurs latéraux en finition 031.","Wall hung bidet in in White Europe Ceramic with overflow waste, with central hole for taps and fittings. Overflow cap and side covering caps included in 031 finishing",518,"White Ceramic",769,"GPF391150C083G000","8022692785302"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",46765,46765,"Afwerkingsdop waste overloop met zijdoppen gatafdekking voor 46755","Kit de cache de trop plein et enjoliveurs latéraux pour art. 46755","Finished cover cap for overflow waste with lateral hole plugs for 46755",761,"Coffee Bronze Brushed PVD",192,"GPF467650E059G000","8055261602748"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45230",45230,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",726,"Warm Bronze Brushed PVD",836,"GPF452300P024G000","8055261645608"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","031","Chrome",480,"GPF451300G001G000","8055261227606"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",149,"Finox Brushed Nickel",648,"GPF451300G002G000","8055261227590"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",299,"Matte Black",648,"GPF451300C072G000","8055261227613"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",147,"Chome Brushed",648,"GPF451300G006G000","8055261227583"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",720,"Nickel PVD",711,"GPF451300P014G000","8055261227491"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",706,"Black Metal PVD",711,"GPF451300P001G000","8055261227552"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",707,"Black Metal Brushed PVD",758,"GPF451300P004G000","8055261227545"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","030","Copper PVD",711,"GPF451300P000G000","8055261227569"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",708,"Copper Brushed PVD",758,"GPF451300P006G000","8055261227521"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",735,"Warm Bronze PVD",711,"GPF451300P037G000","8055261227460"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",726,"Warm Bronze Brushed PVD",758,"GPF451300P024G000","8055261227484"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",710,"Brass PVD",711,"GPF451300P011G000","8055261227507"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",727,"Brass Brushed PVD",758,"GPF451300P025G000","8055261227477"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",246,"Gold PVD",807,"GPF451300P007G000","8055261227514"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",716,"Gold Brushed PVD",807,"GPF451300P005G000","8055261227538"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",187,"Aged Bronze",758,"GPF451300G052G000","8055261227576"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",713,"Antique Brass",758,"GPF451300V204G000","8055261227453"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",279,"Matte White",648,"GPF451300C071G000","8055261236233"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45130",45130,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",761,"Coffee Bronze Brushed PVD",806,"GPF451300E059G000","8055261577411"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131","09276","Inbouwdeel voor afsluitbare douche met mengkraan.","Partie encastrée pour douchette shut-off avec mitigeur.","Built-in part for shut-off douchette with mixer.","031","Chrome",324,"GPF092760G001G000","8055261237261"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","031","Chrome",480,"GPF451310G001G000","8055261227422"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",149,"Finox Brushed Nickel",648,"GPF451310G002G000","8055261227415"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",299,"Matte Black",648,"GPF451310C072G000","8055261227439"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",147,"Chome Brushed",648,"GPF451310G006G000","8055261227408"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",720,"Nickel PVD",711,"GPF451310P014G000","8055261227316"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",706,"Black Metal PVD",711,"GPF451310P001G000","8055261227378"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",707,"Black Metal Brushed PVD",758,"GPF451310P004G000","8055261227361"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.","030","Copper PVD",711,"GPF451310P000G000","8055261227385"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",708,"Copper Brushed PVD",758,"GPF451310P006G000","8055261227347"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",735,"Warm Bronze PVD",711,"GPF451310P037G000","8055261227286"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",726,"Warm Bronze Brushed PVD",758,"GPF451310P024G000","8055261227309"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",710,"Brass PVD",711,"GPF451310P011G000","8055261227323"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",727,"Brass Brushed PVD",758,"GPF451310P025G000","8055261227293"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",246,"Gold PVD",807,"GPF451310P007G000","8055261227330"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",716,"Gold Brushed PVD",807,"GPF451310P005G000","8055261227354"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",187,"Aged Bronze",758,"GPF451310G052G000","8055261227392"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",713,"Antique Brass",758,"GPF451310V204G000","8055261227279"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",279,"Matte White",648,"GPF451310C071G000","8055261236226"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","09276+45131",45131,"Shut-off douchette met mengkraan.","Douchette shut-off avec mitigeur.","Shut-off douchette with mixer.",761,"Coffee Bronze Brushed PVD",806,"GPF451310E059G000","8055261577398"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI","031","Chrome",880,"GPF755270G001G000","8055261645530"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",149,"Finox Brushed Nickel",1189,"GPF755270G002G000","8055261645523"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",299,"Matte Black",1189,"GPF755270C072G000","8055261645561"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",720,"Nickel PVD",1303,"GPF755270P014G000","8055261645462"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",706,"Black Metal PVD",1303,"GPF755270P001G000","8055261645509"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",707,"Black Metal Brushed PVD",1390,"GPF755270P004G000","8055261645493"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI","030","Copper PVD",1303,"GPF755270P000G000","8055261645516"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",708,"Copper Brushed PVD",1390,"GPF755270P006G000","8055261645486"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",735,"Warm Bronze PVD",1303,"GPF755270P037G000","8055261645431"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",726,"Warm Bronze Brushed PVD",1390,"GPF755270P024G000","8055261645455"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",761,"Coffee Bronze Brushed PVD",1478,"GPF755270E059G000","8055261645547"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",710,"Brass PVD",1303,"GPF755270P011G000","8055261645479"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",727,"Brass Brushed PVD",1390,"GPF755270P025G000","8055261645448"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",75527,75527,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting. INCASTRI","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\". INCASTRI","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection. INCASTRI",845,"Dark Bronze",1390,"GPF755270V221G000","8055261645424"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","031","Chrome",785,"GPF452270G001G000","8055261645837"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1060,"GPF452270G002G000","8055261645820"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",299,"Matte Black",1060,"GPF452270C072G000","8055261645868"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",720,"Nickel PVD",1161,"GPF452270P014G000","8055261645769"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1161,"GPF452270P001G000","8055261645806"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1240,"GPF452270P004G000","8055261645790"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","030","Copper PVD",1161,"GPF452270P000G000","8055261645813"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1240,"GPF452270P006G000","8055261645783"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1161,"GPF452270P037G000","8055261645738"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1240,"GPF452270P024G000","8055261645752"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1319,"GPF452270E059G000","8055261645844"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1161,"GPF452270P011G000","8055261645776"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1240,"GPF452270P025G000","8055261645745"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45227,45227,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",845,"Dark Bronze",1240,"GPF452270V221G000","8055261645721"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","031","Chrome",779,"GPF451240G001G000","8056603615907"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1051,"GPF451240G002G000","8056603615891"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",299,"Matte Black",1051,"GPF451240C072G000","8056603615914"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",720,"Nickel PVD",1152,"GPF451240P014G000","8056603615785"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1152,"GPF451240P001G000","8056603615839"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1230,"GPF451240P004G000","8056603615822"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","030","Copper PVD",1152,"GPF451240P000G000","8056603615846"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1230,"GPF451240P006G000","8056603615815"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1152,"GPF451240P037G000","8056603615754"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1230,"GPF451240P024G000","8056603615778"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1152,"GPF451240P011G000","8056603615792"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1230,"GPF451240P025G000","8056603615761"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",246,"Gold PVD",1307,"GPF451240P007G000","8056603615808"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",716,"Gold Brushed PVD",1307,"GPF451240P005G000","8055261230972"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",187,"Aged Bronze",1230,"GPF451240G052G000","8056603615853"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",713,"Antique Brass",1230,"GPF451240V204G000","8056603615747"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",279,"Matte White",1051,"GPF451240C071G000","8056603615921"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45124,45124,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1309,"GPF451240E059G000","8055261577459"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",650,"GPF451231G001G000","8022692811681"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",878,"GPF451231G002G000","8022692811698"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",299,"Matte Black",878,"GPF451231C072G000","8022692811711"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",720,"Nickel PVD",962,"GPF451231P014G000","8056603455947"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",706,"Black Metal PVD",962,"GPF451231P001G000","8022692811728"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",707,"Black Metal Brushed PVD",1029,"GPF451231P004G000","8022692811735"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","030","Copper PVD",962,"GPF451231P000G000","8022692811674"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",708,"Copper Brushed PVD",1029,"GPF451231P006G000","8022692883466"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",735,"Warm Bronze PVD",962,"GPF451231P037G000","8056329556348"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",726,"Warm Bronze Brushed PVD",1029,"GPF451231P024G000","8056329013315"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",710,"Brass PVD",962,"GPF451231P011G000","8056329606890"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",727,"Brass Brushed PVD",1029,"GPF451231P025G000","8056329080515"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",246,"Gold PVD",1093,"GPF451231P007G000","8056603118019"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",716,"Gold Brushed PVD",1093,"GPF451231P005G000","8056329011694"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",187,"Aged Bronze",1029,"GPF451231G052G000","8056329561960"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",713,"Antique Brass",1029,"GPF451231V204G000","8056329561953"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",279,"Matte White",878,"GPF451231C071G000","8022692811704"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45123,45123,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1093,"GPF451231E059G000","8055261602809"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",717,"GPF591531G001G000","8056329057548"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",966,"GPF591531G002G000","8056329057531"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",299,"Matte Black",966,"GPF591531C072G000","8056329057555"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",720,"Nickel PVD",1059,"GPF591531P014G000","8056603605632"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",706,"Black Metal PVD",1059,"GPF591531P001G000","8056329057470"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",707,"Black Metal Brushed PVD",1127,"GPF591531P004G000","8056329057456"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","030","Copper PVD",1059,"GPF591531P000G000","8056329057487"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",708,"Copper Brushed PVD",1127,"GPF591531P006G000","8056329057432"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",735,"Warm Bronze PVD",1059,"GPF591531P037G000","8056329593459"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",726,"Warm Bronze Brushed PVD",1127,"GPF591531P024G000","8056329057418"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",710,"Brass PVD",1059,"GPF591531P011G000","8056329593466"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",727,"Brass Brushed PVD",1127,"GPF591531P025G000","8056329057401"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",279,"Matte White",966,"GPF591531C071G000","8056329057562"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59153,59153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1205,"GPF591531E059G000","8055261577350"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",717,"GPF581531G001G000","8056329020344"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",967,"GPF581531G002G000","8056329020337"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",299,"Matte Black",967,"GPF581531C072G000","8056329020351"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",720,"Nickel PVD",1059,"GPF581531P014G000","8056603606226"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",706,"Black Metal PVD",1059,"GPF581531P001G000","8056329020306"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",707,"Black Metal Brushed PVD",1127,"GPF581531P004G000","8056329020283"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","030","Copper PVD",1059,"GPF581531P000G000","8056329020313"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",708,"Copper Brushed PVD",1127,"GPF581531P006G000","8056329020276"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",735,"Warm Bronze PVD",1059,"GPF581531P037G000","8056329596054"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",726,"Warm Bronze Brushed PVD",1127,"GPF581531P024G000","8056329077720"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",710,"Brass PVD",1059,"GPF581531P011G000","8056329596061"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",727,"Brass Brushed PVD",1127,"GPF581531P025G000","8056329020252"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",246,"Gold PVD",1205,"GPF581531P007G000","8056329020269"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",716,"Gold Brushed PVD",1205,"GPF581531P005G000","8056329559332"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",187,"Aged Bronze",1127,"GPF581531G052G000","8056329020320"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",713,"Antique Brass",1127,"GPF581531V204G000","8056329020290"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",845,"Dark Bronze",1127,"GPF581531V221G000","8056603622646"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58153,58153,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1205,"GPF581531E059G000","8055261595613"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",20023,20023,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",688,"GPF200231G001G000","8022692461756"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",20023,20023,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",930,"GPF200231G002G000","8022692789645"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",20021,20021,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",650,"GPF200211G001G000","8022692461732"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",20021,20021,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",878,"GPF200211G002G000","8022692789638"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","031","Chrome",857,"GPF452260G001G000","8055261645981"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1157,"GPF452260G002G000","8055261645974"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",299,"Matte Black",1157,"GPF452260C072G000","8055261646018"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",720,"Nickel PVD",1267,"GPF452260P014G000","8055261645912"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1267,"GPF452260P001G000","8055261645950"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1354,"GPF452260P004G000","8055261645943"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","030","Copper PVD",1267,"GPF452260P000G000","8055261645967"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1354,"GPF452260P006G000","8055261645936"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1267,"GPF452260P037G000","8055261645882"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1354,"GPF452260P024G000","8055261645905"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1439,"GPF452260E059G000","8055261645998"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1267,"GPF452260P011G000","8055261645929"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1354,"GPF452260P025G000","8055261645899"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45226,45226,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",845,"Dark Bronze",1354,"GPF452260V221G000","8055261645875"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","031","Chrome",779,"GPF451260G001G000","8056603633000"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1051,"GPF451260G002G000","8056603632997"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",299,"Matte Black",1051,"GPF451260C072G000","8056603633017"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",720,"Nickel PVD",1152,"GPF451260P014G000","8056603632881"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1152,"GPF451260P001G000","8056603632935"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1230,"GPF451260P004G000","8056603632928"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.","030","Copper PVD",1152,"GPF451260P000G000","8056603632942"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1230,"GPF451260P006G000","8056603632911"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1152,"GPF451260P037G000","8056603632850"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1230,"GPF451260P024G000","8056603632874"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1152,"GPF451260P011G000","8056603632898"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1230,"GPF451260P025G000","8056603632867"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",246,"Gold PVD",1307,"GPF451260P007G000","8056603632904"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",716,"Gold Brushed PVD",1307,"GPF451260P005G000","8056603695046"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",187,"Aged Bronze",1230,"GPF451260G052G000","8056603632959"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",713,"Antique Brass",1230,"GPF451260V204G000","8056603632843"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",279,"Matte White",1051,"GPF451260C071G000","8056603633024"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45126,45126,"Wandgemonteerde drukknop Shut-Off douchette met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec vanne de sécurité, robinet d'arrêt et raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with safety valve, stop valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1309,"GPF451260E059G000","8055261577435"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",717,"GPF144310G001G000","8055261646131"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",967,"GPF144310G002G000","8055261646124"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",299,"Matte Black",967,"GPF144310C072G000","8055261646162"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",720,"Nickel PVD",1060,"GPF144310P014G000","8055261646063"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",706,"Black Metal PVD",1060,"GPF144310P001G000","8055261646100"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",707,"Black Metal Brushed PVD",1133,"GPF144310P004G000","8055261646094"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","030","Copper PVD",1060,"GPF144310P000G000","8055261646117"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",708,"Copper Brushed PVD",1133,"GPF144310P006G000","8055261646087"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",735,"Warm Bronze PVD",1060,"GPF144310P037G000","8055261646032"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",726,"Warm Bronze Brushed PVD",1133,"GPF144310P024G000","8055261646056"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1205,"GPF144310E059G000","8055261646148"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",710,"Brass PVD",1060,"GPF144310P011G000","8055261646070"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",727,"Brass Brushed PVD",1133,"GPF144310P025G000","8055261646049"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14431,14431,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",845,"Dark Bronze",1133,"GPF144310V221G000","8055261646025"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","031","Chrome",650,"GPF143313G001G000","8022692049831"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",149,"Finox Brushed Nickel",878,"GPF143313G002G000","8022692792669"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",299,"Matte Black",878,"GPF143313C072G000","8056329225343"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",147,"Chome Brushed",878,"GPF143313G006G000","8056329082557"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",720,"Nickel PVD",963,"GPF143313P014G000","8056603635639"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",706,"Black Metal PVD",963,"GPF143313P001G000","8056603447171"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",707,"Black Metal Brushed PVD",1029,"GPF143313P004G000","8056329192676"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.","030","Copper PVD",963,"GPF143313P000G000","8056329545854"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",708,"Copper Brushed PVD",1029,"GPF143313P006G000","8056329183179"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",735,"Warm Bronze PVD",963,"GPF143313P037G000","8056603635646"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",726,"Warm Bronze Brushed PVD",1029,"GPF143313P024G000","8056329723795"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",710,"Brass PVD",963,"GPF143313P011G000","8056329542099"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",727,"Brass Brushed PVD",1029,"GPF143313P025G000","8056329191044"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",246,"Gold PVD",1092,"GPF143313P007G000","8056329223974"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",716,"Gold Brushed PVD",1092,"GPF143313P005G000","8056329625204"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",187,"Aged Bronze",1029,"GPF143313G052G000","8056603507691"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",713,"Antique Brass",1029,"GPF143313V204G000","8056603507707"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",14331,14331,"Wandgemonteerde drukknop Shut-Off douchette met 1/2\" aansluiting.","Douchette Hygiénique Shut-Off murale avec raccord 1/2\".","Wall-mounted push-button Shut-Off douchette with 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1092,"GPF143313E059G000","8055261577916"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.","031","Chrome",940,"GPF451220G001G000","8056603616072"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",149,"Finox Brushed Nickel",1268,"GPF451220G002G000","8056603616065"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",299,"Matte Black",1268,"GPF451220C072G000","8056603616089"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",720,"Nickel PVD",1390,"GPF451220P014G000","8056603615976"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",706,"Black Metal PVD",1390,"GPF451220P001G000","8056603616027"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1482,"GPF451220P004G000","8056603616010"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.","030","Copper PVD",1390,"GPF451220P000G000","8056603616034"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",708,"Copper Brushed PVD",1482,"GPF451220P006G000","8056603616003"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",735,"Warm Bronze PVD",1390,"GPF451220P037G000","8056603615945"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1482,"GPF451220P024G000","8056603615969"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",710,"Brass PVD",1390,"GPF451220P011G000","8056603615983"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",727,"Brass Brushed PVD",1482,"GPF451220P025G000","8056603615952"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",246,"Gold PVD",1579,"GPF451220P007G000","8056603615990"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",716,"Gold Brushed PVD",1579,"GPF451220P005G000","8055261186811"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",187,"Aged Bronze",1482,"GPF451220G052G000","8056603616041"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",713,"Antique Brass",1482,"GPF451220V204G000","8056603615938"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",279,"Matte White",1268,"GPF451220C071G000","8056603616096"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45122,45122,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep, Stop Kraan en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec robinet d'arrêt, vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve, stop valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1579,"GPF451220E059G000","8055261577473"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.","031","Chrome",811,"GPF451211G001G000","8022692811612"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",149,"Finox Brushed Nickel",1095,"GPF451211G002G000","8022692811629"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",299,"Matte Black",1095,"GPF451211C072G000","8022692811643"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",720,"Nickel PVD",1199,"GPF451211P014G000","8056603455954"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",706,"Black Metal PVD",1199,"GPF451211P001G000","8022692822878"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",707,"Black Metal Brushed PVD",1281,"GPF451211P004G000","8022692822861"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.","030","Copper PVD",1199,"GPF451211P000G000","8022692811605"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",708,"Copper Brushed PVD",1281,"GPF451211P006G000","8056329014404"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",735,"Warm Bronze PVD",1199,"GPF451211P037G000","8056329556324"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1281,"GPF451211P024G000","8056329080287"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",710,"Brass PVD",1199,"GPF451211P011G000","8056329606906"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",727,"Brass Brushed PVD",1281,"GPF451211P025G000","8056329523838"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",246,"Gold PVD",1364,"GPF451211P007G000","8056603462327"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",716,"Gold Brushed PVD",1364,"GPF451211P005G000","8055261114449"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",187,"Aged Bronze",1281,"GPF451211G052G000","8056329561984"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",713,"Antique Brass",1281,"GPF451211V204G000","8056329561977"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",279,"Matte White",1095,"GPF451211C071G000","8022692811636"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45121,45121,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1364,"GPF451211E059G000","8055261602823"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.","031","Chrome",891,"GPF591511G001G000","8056329057715"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",149,"Finox Brushed Nickel",1201,"GPF591511G002G000","8056329057708"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",299,"Matte Black",1201,"GPF591511C072G000","8056329057722"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",720,"Nickel PVD",1317,"GPF591511P014G000","8056603605656"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",706,"Black Metal PVD",1317,"GPF591511P001G000","8056329057647"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",707,"Black Metal Brushed PVD",1406,"GPF591511P004G000","8056329057623"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.","030","Copper PVD",1317,"GPF591511P000G000","8056329057654"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",708,"Copper Brushed PVD",1406,"GPF591511P006G000","8056329057609"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",735,"Warm Bronze PVD",1317,"GPF591511P037G000","8056329593497"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1406,"GPF591511P024G000","8056329057586"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",710,"Brass PVD",1317,"GPF591511P011G000","8056329593503"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",727,"Brass Brushed PVD",1406,"GPF591511P025G000","8056329057579"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",279,"Matte White",1201,"GPF591511C071G000","8056329057739"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",59151,59151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1497,"GPF591511E059G000","8055261577374"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.","031","Chrome",891,"GPF581511G001G000","8056329020450"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",149,"Finox Brushed Nickel",1203,"GPF581511G002G000","8056329020443"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",299,"Matte Black",1203,"GPF581511C072G000","8056329020467"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",720,"Nickel PVD",1317,"GPF581511P014G000","8056603606240"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",706,"Black Metal PVD",1317,"GPF581511P001G000","8056329020412"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1406,"GPF581511P004G000","8056329020399"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.","030","Copper PVD",1317,"GPF581511P000G000","8056329020429"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",708,"Copper Brushed PVD",1406,"GPF581511P006G000","8056329020382"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",735,"Warm Bronze PVD",1317,"GPF581511P037G000","8056329596092"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1406,"GPF581511P024G000","8056329184558"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",710,"Brass PVD",1317,"GPF581511P011G000","8056329596108"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",727,"Brass Brushed PVD",1406,"GPF581511P025G000","8056329020368"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",246,"Gold PVD",1497,"GPF581511P007G000","8056329020375"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",716,"Gold Brushed PVD",1497,"GPF581511P005G000","8056603711425"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",187,"Aged Bronze",1406,"GPF581511G052G000","8056329020436"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",713,"Antique Brass",1406,"GPF581511V204G000","8056329020405"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",845,"Dark Bronze",1406,"GPF581511V221G000","8056603622660"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",58151,58151,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire avec raccordement 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1497,"GPF581511E059G000","8055261595651"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.","031","Chrome",811,"GPF338232G001G000","8022692803747"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",149,"Finox Brushed Nickel",1095,"GPF338232G002G000","8022692620351"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",299,"Matte Black",1095,"GPF338232C072G000","8056329006478"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",720,"Nickel PVD",1199,"GPF338232P014G000","8056603607803"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",706,"Black Metal PVD",1199,"GPF338232P001G000","8056329006461"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",707,"Black Metal Brushed PVD",1281,"GPF338232P004G000","8056329006454"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.","030","Copper PVD",1199,"GPF338232P000G000","8022692839371"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",708,"Copper Brushed PVD",1281,"GPF338232P006G000","8056329006447"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",735,"Warm Bronze PVD",1199,"GPF338232P037G000","8056329609396"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",726,"Warm Bronze Brushed PVD",1281,"GPF338232P024G000","8056329162907"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",710,"Brass PVD",1199,"GPF338232P011G000","8056329609419"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",727,"Brass Brushed PVD",1281,"GPF338232P025G000","8056329609402"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",33823,33823,"Wandgemonteerde Hydrobrush voor sanitaire keramiek met veiligheidsklep en 1/2\" aansluiting.","Balayette avec jet d'eau pour céramique sanitaire murale avec vanne de sécurité et raccord 1/2\".","Wall-mounted Hydrobrush for sanitary ceramics with safety valve and 1/2\" connection.",761,"Coffee Bronze Brushed PVD",1364,"GPF338232E059G000","8055261605329"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66601,66601,"waskom voor bladmontage in Cristalplant®, zonder overflow waste. Afvoerplug 01313 niet inbegrepen.","Vasque à poser en Cristalplant®, sans vidage, sans trop plein. Bonde 01313 non incluse.","Counter washbasin in Cristalplant®, without overflow waste. Basin waste 01313 not included.",521,"Cristalplant Matte White",1585,"GPF666010B017G000","8056603587624"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66601,66601,"waskom voor bladmontage in Cristalplant®, zonder overflow waste. Afvoerplug 01313 niet inbegrepen.","Vasque à poser en Cristalplant®, sans vidage, sans trop plein. Bonde 01313 non incluse.","Counter washbasin in Cristalplant®, without overflow waste. Basin waste 01313 not included.",511,"Cristalplant Matte Black",2408,"GPF666010B041G000","8056603587563"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66601,66601,"waskom voor bladmontage in Cristalplant®, zonder overflow waste. Afvoerplug 01313 niet inbegrepen.","Vasque à poser en Cristalplant®, sans vidage, sans trop plein. Bonde 01313 non incluse.","Counter washbasin in Cristalplant®, without overflow waste. Basin waste 01313 not included.",510,"Cristalplant Matte Coral",2408,"GPF666010B040G000","8056603587570"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66601,66601,"waskom voor bladmontage in Cristalplant®, zonder overflow waste. Afvoerplug 01313 niet inbegrepen.","Vasque à poser en Cristalplant®, sans vidage, sans trop plein. Bonde 01313 non incluse.","Counter washbasin in Cristalplant®, without overflow waste. Basin waste 01313 not included.",509,"Cristalplant Matte Ocra",2408,"GPF666010B039G000","8056603587587"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66601,66601,"waskom voor bladmontage in Cristalplant®, zonder overflow waste. Afvoerplug 01313 niet inbegrepen.","Vasque à poser en Cristalplant®, sans vidage, sans trop plein. Bonde 01313 non incluse.","Counter washbasin in Cristalplant®, without overflow waste. Basin waste 01313 not included.",508,"Cristalplant Matte Agave",2408,"GPF666010B038G000","8056603587594"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66601,66601,"waskom voor bladmontage in Cristalplant®, zonder overflow waste. Afvoerplug 01313 niet inbegrepen.","Vasque à poser en Cristalplant®, sans vidage, sans trop plein. Bonde 01313 non incluse.","Counter washbasin in Cristalplant®, without overflow waste. Basin waste 01313 not included.",507,"Cristalplant Matte Cipria",2408,"GPF666010B037G000","8056603587600"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66601,66601,"waskom voor bladmontage in Cristalplant®, zonder overflow waste. Afvoerplug 01313 niet inbegrepen.","Vasque à poser en Cristalplant®, sans vidage, sans trop plein. Bonde 01313 non incluse.","Counter washbasin in Cristalplant®, without overflow waste. Basin waste 01313 not included.",506,"Cristalplant Matte Greige",2408,"GPF666010B036G000","8056603587617"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66603,66603,"vrijstaene waskom in Cristalplant®, zonder overflow waste","Vasque au sol en Cristalplant®, sans trop plein","Freestanding washbasin in Cristalplant®, without overflow waste. Grille-plug and syphon included.",521,"Cristalplant Matte White",4748,"GPF666030B017G000","8056603587556"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66603,66603,"vrijstaene waskom in Cristalplant®, zonder overflow waste","Vasque au sol en Cristalplant®, sans trop plein","Freestanding washbasin in Cristalplant®, without overflow waste. Grille-plug and syphon included.",511,"Cristalplant Matte Black",6346,"GPF666030B041G000","8056603587495"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66603,66603,"vrijstaene waskom in Cristalplant®, zonder overflow waste","Vasque au sol en Cristalplant®, sans trop plein","Freestanding washbasin in Cristalplant®, without overflow waste. Grille-plug and syphon included.",510,"Cristalplant Matte Coral",6346,"GPF666030B040G000","8056603587501"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66603,66603,"vrijstaene waskom in Cristalplant®, zonder overflow waste","Vasque au sol en Cristalplant®, sans trop plein","Freestanding washbasin in Cristalplant®, without overflow waste. Grille-plug and syphon included.",509,"Cristalplant Matte Ocra",6346,"GPF666030B039G000","8056603587518"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66603,66603,"vrijstaene waskom in Cristalplant®, zonder overflow waste","Vasque au sol en Cristalplant®, sans trop plein","Freestanding washbasin in Cristalplant®, without overflow waste. Grille-plug and syphon included.",508,"Cristalplant Matte Agave",6346,"GPF666030B038G000","8056603587525"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66603,66603,"vrijstaene waskom in Cristalplant®, zonder overflow waste","Vasque au sol en Cristalplant®, sans trop plein","Freestanding washbasin in Cristalplant®, without overflow waste. Grille-plug and syphon included.",507,"Cristalplant Matte Cipria",6346,"GPF666030B037G000","8056603587532"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",66603,66603,"vrijstaene waskom in Cristalplant®, zonder overflow waste","Vasque au sol en Cristalplant®, sans trop plein","Freestanding washbasin in Cristalplant®, without overflow waste. Grille-plug and syphon included.",506,"Cristalplant Matte Greige",6346,"GPF666030B036G000","8056603587549"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54605,54605,"Opzetwastafel in roestvrij staal zonder overloop 400x400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 400x400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 400x400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",239,"Steel Brushed",1780,"GPF546050A000G000","8056329224964"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54605,54605,"Opzetwastafel in roestvrij staal zonder overloop 400x400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 400x400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 400x400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",299,"Matte Black",2385,"GPF546050C072G000","8056329225008"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54605,54605,"Opzetwastafel in roestvrij staal zonder overloop 400x400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 400x400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 400x400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",707,"Black Metal Brushed PVD",3957,"GPF546050P004G000","8056329224971"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54605,54605,"Opzetwastafel in roestvrij staal zonder overloop 400x400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 400x400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 400x400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",708,"Copper Brushed PVD",3957,"GPF546050P006G000","8056329224988"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54605,54605,"Opzetwastafel in roestvrij staal zonder overloop 400x400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 400x400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 400x400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",726,"Warm Bronze Brushed PVD",3957,"GPF546050P024G000","8056329224995"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54605,54605,"Opzetwastafel in roestvrij staal zonder overloop 400x400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 400x400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 400x400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",727,"Brass Brushed PVD",3957,"GPF546050P025G000","8056329533486"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54605,54605,"Opzetwastafel in roestvrij staal zonder overloop 400x400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 400x400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 400x400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",761,"Coffee Bronze Brushed PVD",4225,"GPF546050E059G000","8055261598935"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54606,54606,"Opzetwastafel in roestvrij staal 600x350mm zonder overloop 600x350mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 600x350mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 600x350mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",239,"Steel Brushed",2071,"GPF546060A000G000","8056329225015"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54606,54606,"Opzetwastafel in roestvrij staal 600x350mm zonder overloop 600x350mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 600x350mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 600x350mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",299,"Matte Black",2758,"GPF546060C072G000","8056329225053"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54606,54606,"Opzetwastafel in roestvrij staal 600x350mm zonder overloop 600x350mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 600x350mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 600x350mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",707,"Black Metal Brushed PVD",5094,"GPF546060P004G000","8056329225022"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54606,54606,"Opzetwastafel in roestvrij staal 600x350mm zonder overloop 600x350mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 600x350mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 600x350mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",708,"Copper Brushed PVD",5094,"GPF546060P006G000","8056329225039"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54606,54606,"Opzetwastafel in roestvrij staal 600x350mm zonder overloop 600x350mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 600x350mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 600x350mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",726,"Warm Bronze Brushed PVD",5094,"GPF546060P024G000","8056329225046"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54606,54606,"Opzetwastafel in roestvrij staal 600x350mm zonder overloop 600x350mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 600x350mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 600x350mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",727,"Brass Brushed PVD",5094,"GPF546060P025G000","8056329564534"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54606,54606,"Opzetwastafel in roestvrij staal 600x350mm zonder overloop 600x350mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser 600x350mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin 600x350mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",761,"Coffee Bronze Brushed PVD",5436,"GPF546060E059G000","8055261598911"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",239,"Steel Brushed",1280,"GPF546010A000G000","8022692851526"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",299,"Matte Black",1728,"GPF546010C072G000","8056329225565"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",707,"Black Metal Brushed PVD",3783,"GPF546010P004G000","8022692851533"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",708,"Copper Brushed PVD",3783,"GPF546010P006G000","8022692851540"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",726,"Warm Bronze Brushed PVD",3783,"GPF546010P024G000","8022692851557"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",727,"Brass Brushed PVD",3783,"GPF546010P025G000","8056329085220"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54601,54601,"Opzetwastafel in roestvrij staal zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel, without overflow waste. Without basin waste. It can be combined with waste 54599. 15 mm spacer RI01395 included.",761,"Coffee Bronze Brushed PVD",4037,"GPF546010E059G000","8055261598959"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",65601,65601,"Opzetwastafel in roestvrij staal RIGATO zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox RIGATO sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel RIGATO, without overflow waste. Waste not included. It can be combined with waste 54599. 15 mm spacer RI01395 included.",239,"Steel Brushed",3018,"GPF656010A000G000","8056603458139"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",65601,65601,"Opzetwastafel in roestvrij staal RIGATO zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox RIGATO sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel RIGATO, without overflow waste. Waste not included. It can be combined with waste 54599. 15 mm spacer RI01395 included.",707,"Black Metal Brushed PVD",5528,"GPF656010P004G000","8056603458122"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",65601,65601,"Opzetwastafel in roestvrij staal RIGATO zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox RIGATO sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel RIGATO, without overflow waste. Waste not included. It can be combined with waste 54599. 15 mm spacer RI01395 included.",708,"Copper Brushed PVD",5528,"GPF656010P006G000","8056603458115"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",65601,65601,"Opzetwastafel in roestvrij staal RIGATO zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox RIGATO sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel RIGATO, without overflow waste. Waste not included. It can be combined with waste 54599. 15 mm spacer RI01395 included.",726,"Warm Bronze Brushed PVD",5528,"GPF656010P024G000","8056603458108"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",65601,65601,"Opzetwastafel in roestvrij staal RIGATO zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox RIGATO sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel RIGATO, without overflow waste. Waste not included. It can be combined with waste 54599. 15 mm spacer RI01395 included.",727,"Brass Brushed PVD",5528,"GPF656010P025G000","8056603458092"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",65601,65601,"Opzetwastafel in roestvrij staal RIGATO zonder overloop Ø400mm. Afvoer niet inbegrepen. Te combineren met afvoer 54599. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser Ø400mm en acier Inox RIGATO sans trop-plein. La bonde n'est pas incluse. Combinable avec la bonde 54599. Entretoise de 15 mm RI01395 incluse.","Counter washbasin Ø400mm in stainless steel RIGATO, without overflow waste. Waste not included. It can be combined with waste 54599. 15 mm spacer RI01395 included.",761,"Coffee Bronze Brushed PVD",5900,"GPF656010E059G000","8055261588486"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01578","01578","Onderbouw wastafelbeugels voor 54601, 54605, 54606.","Supports lavabo sous-plan pour 54601, 54605, 54606.","Undermounted washbasin brackets for 54601, 54605, 54606.","031","Chrome",209,"GPF015780G001G000","8055261057487"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54603,54603,"Vloerhouder voor installatie op vloer artikel 54601, 65601. Sifon en verlengbare afvoerleiding inbegrepen. Waste naar vloer.","Support au sol in Cristalplant® pour installation art. 54601, 65601. Sifon et tuyau extensible de vidage inclus","Freestanding support in Cristalplant® for floor installation art 54601, 65601. Siphon and extensible drainage-pipe included. Floor drainage.",850,"Cristalplant Dark Metal",6667,"GPF546030T088G000","8056329008731"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01712","01712","Bevestigingsset voor Installatie onder het blad, item 46803, 46805","Kit de fixation pour installation sous-plan art. 43803, 46805","Fixing kit for under counter installation item 46803, 46805","031","Chrome",215,"GPF017120G001G000","8055261240445"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45911,45911,"Vloerwastafel van Cristalplant zonder overloop. Zonder gaten voor kraanwerk. Waste naar vloer. Afvoerplug met rooster en sifon inbegrepen","Vasque au sol en Cristalplant® sans trop plein. Sans percement pour la robinetterie. Vidage au sol, grille et siphon inclus","Freestanding washbasin in Cristalplant® without overflow waste. Floor drainage. No brassware seat-holes. Grille-plug and syphonincluded",521,"Cristalplant Matte White",4593,"GPF459110B017G000","8022692815344"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45907,45907,"Vloerwastafel van Cristalplant zonder overloop. Met gat voor kraanwerk. Waste in wand. Afvoerplug met rooster en sifon inbegrepen","Vasque au sol en Cristalplant® sans trop plein. Avec percement pour la robinetterie. Vidage murale, grille et siphon inclus","Freestanding washbasin in Cristalplant® without overflow waste. Wall drainage. With brassware seat-holes. Grille-plug and syphonincluded",521,"Cristalplant Matte White",5009,"GPF459070B017G000","8022692815283"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",45903,45903,"Staande wastafel van Cristalplant zonder overloop. Zonder gaten voor kraanwerk","Vasque à poser en Cristalplant® sans trop plein. Sans percement pour la robinetterie.","counter console in Cristalplant® without overflow waste. No holes for taps and fittings",521,"Cristalplant Matte White",1275,"GPF459030B017G000","8022692815269"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39100,39100,"Opbouw wastafel Ø400 mm","Cuvette de support Ø400 mm","Counter washbasin Ø400 mm",525,"Bright Copper",2514,"GPF391000B045G000","8055261073708"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39100,39100,"Opbouw wastafel Ø400 mm","Cuvette de support Ø400 mm","Counter washbasin Ø400 mm",524,"Bright Platinum",2514,"GPF391000B044G000","8055261073715"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39100,39100,"Opbouw wastafel Ø400 mm","Cuvette de support Ø400 mm","Counter washbasin Ø400 mm",526,"Bright Bronze",2514,"GPF391000B046G000","8055261737839"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39100,39100,"Opbouw wastafel Ø400 mm","Cuvette de support Ø400 mm","Counter washbasin Ø400 mm",531,"Matte White Ceramic",1158,"GPF391000C288G000","8055261228078"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39100,39100,"Opbouw wastafel Ø400 mm","Cuvette de support Ø400 mm","Counter washbasin Ø400 mm",532,"Matte Black Ceramic",1158,"GPF391000C289G000","8055261228061"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39102,39102,"Opbouw wastafel Ø500 mm","Cuvette de support Ø500 mm","Counter washbasin Ø500 mm",525,"Bright Copper",3388,"GPF391020B045G000","8055261073661"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39102,39102,"Opbouw wastafel Ø500 mm","Cuvette de support Ø500 mm","Counter washbasin Ø500 mm",524,"Bright Platinum",3388,"GPF391020B044G000","8055261073678"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39102,39102,"Opbouw wastafel Ø500 mm","Cuvette de support Ø500 mm","Counter washbasin Ø500 mm",526,"Bright Bronze",3388,"GPF391020B046G000","8055261737846"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39102,39102,"Opbouw wastafel Ø500 mm","Cuvette de support Ø500 mm","Counter washbasin Ø500 mm",531,"Matte White Ceramic",1408,"GPF391020C288G000","8055261228054"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",39102,39102,"Opbouw wastafel Ø500 mm","Cuvette de support Ø500 mm","Counter washbasin Ø500 mm",532,"Matte Black Ceramic",1408,"GPF391020C289G000","8055261228047"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",43460,43460,"Opzetwastafel zonder overloop, afstandshouder 15 mm inbegrepen. Voor installatie onder het aanrecht is bevestigingsset art. R4267 vereist. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser sans trop-plein, entretoise de 15 mm incluse. Pour l'installation sous plan, le kit de fixation art. R4267 est nécessaire.","Deck-mounted washbasin without overflow waste. For under counter installation fixing kit item R4267 required. 15 mm spacer RI01395 included.",516,"White Ceramic",632,"GPF434600B014G000","8056603599221"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",43456,43456,"Opzetwastafel zonder overloop, afstandshouder 15 mm inbegrepen. Voor installatie onder het aanrecht is bevestigingsset art. R4267 vereist. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser sans trop-plein, entretoise de 15 mm incluse. Pour l'installation sous plan, le kit de fixation art. R4267 est nécessaire.","Deck-mounted washbasin without overflow waste. For under counter installation fixing kit item R4267 required. 15 mm spacer RI01395 included.",516,"White Ceramic",632,"GPF434560B014G000","8056603599214"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",43458,43458,"Opzetwastafel zonder overloop, afstandshouder 15 mm inbegrepen. Voor installatie onder het aanrecht is bevestigingsset art. R4267 vereist. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser sans trop-plein, entretoise de 15 mm incluse. Pour l'installation sous plan, le kit de fixation art. R4267 est nécessaire.","Deck-mounted washbasin without overflow waste. For under counter installation fixing kit item R4267 required. 15 mm spacer RI01395 included.",516,"White Ceramic",696,"GPF434580B014G000","8056603599191"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01711","01711","Installatie onder het blad, Bevestigingsset voor item 43456, 43458, 43460.","Kit de fixation pour installation sous le plancher pour 43456, 43458, 43460.","Under counter installation fixing kit for item 43456, 43458, 43460.","031","Chrome",208,"GPF017110G001G000","8055261240452"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",43462,43462,"Opzetwastafel zonder overloop. Afstandshouder 15mm RI01395 inbegrepen.","Vasque à poser sans trop-plein, entretoise de 15 mm incluse.","Deck-mounted washbasin without overflow waste. 15 mm spacer RI01395 included.",516,"White Ceramic",923,"GPF434620B014G000","8056603609098"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow","031","Chrome",72,"GPF013910G001G000","8022692037463"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",275,"Matte Cipria",208,"GPF013910T209G000","8056603635172"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",273,"Matte Greige",208,"GPF013910T208G000","8056603635189"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",277,"Glossy Ocra",161,"GPF013910T211G000","8056603635158"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",278,"Glossy Coral",161,"GPF013910T212G000","8056603635141"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",276,"Matte Agave",208,"GPF013910T210G000","8056603635165"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",149,"Finox Brushed Nickel",136,"GPF013910G002G000","8022692788778"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",299,"Matte Black",208,"GPF013910C072G000","8056329039858"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",147,"Chome Brushed",136,"GPF013910G006G000","8022692121476"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",720,"Nickel PVD",150,"GPF013910P014G000","8056329183100"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",706,"Black Metal PVD",150,"GPF013910P001G000","8022692088816"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",707,"Black Metal Brushed PVD",161,"GPF013910P004G000","8022692852431"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow","030","Copper PVD",150,"GPF013910P000G000","8022692629651"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",708,"Copper Brushed PVD",161,"GPF013910P006G000","8022692883138"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",735,"Warm Bronze PVD",150,"GPF013910P037G000","8056329559189"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",726,"Warm Bronze Brushed PVD",161,"GPF013910P024G000","8056329000797"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",710,"Brass PVD",150,"GPF013910P011G000","8022692833010"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",727,"Brass Brushed PVD",161,"GPF013910P025G000","8056329025288"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",246,"Gold PVD",176,"GPF013910P007G000","8022692633450"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",716,"Gold Brushed PVD",128,"GPF013910P005G000","8056603965316"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",187,"Aged Bronze",161,"GPF013910G052G000","8056329068872"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",713,"Antique Brass",161,"GPF013910V204G000","8022692633467"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",845,"Dark Bronze",161,"GPF013910V221G000","8056603635134"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01391","01391","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","Basin waste always open, without overflow",761,"Coffee Bronze Brushed PVD",169,"GPF013910E059G000","8055261610033"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.","031","Chrome",92,"GPF014230G001G000","8022692037562"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",149,"Finox Brushed Nickel",178,"GPF014230G002G000","8022692791822"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",299,"Matte Black",270,"GPF014230C072G000","8056329039780"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",147,"Chome Brushed",178,"GPF014230G006G000","8022692122695"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",720,"Nickel PVD",196,"GPF014230P014G000","8056603530347"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",706,"Black Metal PVD",196,"GPF014230P001G000","8022692852738"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",707,"Black Metal Brushed PVD",221,"GPF014230P004G000","8022692848731"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.","030","Copper PVD",196,"GPF014230P000G000","8022692628913"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",708,"Copper Brushed PVD",221,"GPF014230P006G000","8022692847833"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",735,"Warm Bronze PVD",196,"GPF014230P037G000","8056329559110"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",726,"Warm Bronze Brushed PVD",221,"GPF014230P024G000","8056329002654"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",710,"Brass PVD",196,"GPF014230P011G000","8056329615212"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",727,"Brass Brushed PVD",221,"GPF014230P025G000","8056329068636"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",246,"Gold PVD",243,"GPF014230P007G000","8056329068643"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",716,"Gold Brushed PVD",164,"GPF014230P005G000","8055261231306"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",187,"Aged Bronze",221,"GPF014230G052G000","8056329068650"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",713,"Antique Brass",221,"GPF014230V204G000","8022692855944"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",279,"Matte White",270,"GPF014230C071G000","8056329152090"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01423","01423","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",761,"Coffee Bronze Brushed PVD",233,"GPF014230E059G000","8055261609969"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow","031","Chrome",55,"GPF013760G001G000","8022692035537"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",149,"Finox Brushed Nickel",105,"GPF013760G002G000","8022692854039"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",299,"Matte Black",159,"GPF013760C072G000","8056329039865"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",147,"Chome Brushed",105,"GPF013760G006G000","8022692120929"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",720,"Nickel PVD",157,"GPF013760P014G000","8056603530330"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",706,"Black Metal PVD",157,"GPF013760P001G000","8022692633337"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",707,"Black Metal Brushed PVD",174,"GPF013760P004G000","8022692633344"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow","030","Copper PVD",157,"GPF013760P000G000","8022692088380"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",708,"Copper Brushed PVD",174,"GPF013760P006G000","8022692890631"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",735,"Warm Bronze PVD",157,"GPF013760P037G000","8056329559202"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",726,"Warm Bronze Brushed PVD",174,"GPF013760P024G000","8056329002661"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",710,"Brass PVD",157,"GPF013760P011G000","8056329615281"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",727,"Brass Brushed PVD",174,"GPF013760P025G000","8056329068902"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",246,"Gold PVD",192,"GPF013760P007G000","8056329068919"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",716,"Gold Brushed PVD",97,"GPF013760P005G000","8056603686488"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",187,"Aged Bronze",174,"GPF013760G052G000","8056329063976"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",713,"Antique Brass",174,"GPF013760V204G000","8022692633351"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01376","01376","Wastafel afvoerplug altijd open, zonder overloop","Vidage avec sortie libre Lavabo sans trop-plein","basin waste always open, without overflow",761,"Coffee Bronze Brushed PVD",97,"GPF013760E059G000","8055261610057"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.","031","Chrome",90,"GPF014200G001G000","8022692033304"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",275,"Matte Cipria",121,"GPF014200T209G000","8056603635110"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",273,"Matte Greige",262,"GPF014200T208G000","8056603635127"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",277,"Glossy Ocra",150,"GPF014200T211G000","8056603635097"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",278,"Glossy Coral",150,"GPF014200T212G000","8056603635080"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",276,"Matte Agave",121,"GPF014200T210G000","8056603635103"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",149,"Finox Brushed Nickel",175,"GPF014200G002G000","8022692788464"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",299,"Matte Black",262,"GPF014200C072G000","8056329039803"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",147,"Chome Brushed",175,"GPF014200G006G000","8022692122596"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",720,"Nickel PVD",219,"GPF014200P014G000","8022692089653"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",706,"Black Metal PVD",219,"GPF014200P001G000","8022692877021"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",707,"Black Metal Brushed PVD",236,"GPF014200P004G000","8022692840704"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.","030","Copper PVD",219,"GPF014200P000G000","8022692633689"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",708,"Copper Brushed PVD",236,"GPF014200P006G000","8056329002586"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",735,"Warm Bronze PVD",219,"GPF014200P037G000","8056329559134"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",726,"Warm Bronze Brushed PVD",236,"GPF014200P024G000","8056329002630"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",710,"Brass PVD",219,"GPF014200P011G000","8056329615236"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",727,"Brass Brushed PVD",236,"GPF014200P025G000","8056329068681"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",246,"Gold PVD",260,"GPF014200P007G000","8056329068698"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",716,"Gold Brushed PVD",159,"GPF014200P005G000","8056329222816"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",187,"Aged Bronze",236,"GPF014200G052G000","8056329068704"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",713,"Antique Brass",236,"GPF014200V204G000","8022692089646"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",845,"Dark Bronze",236,"GPF014200V221G000","8056603635073"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01420","01420","Wastafel afvoerplug “Stop&Go”, zonder overloop. Plug in kleurafwerking. Onderkeramisch onderdeel in kleurafwerking 031, kleurafwerking op aanvraag.","Bonde « Stop&Go » sans trop-plein. Bouchon en finition. Pièce sous-céramique en finition 031, disponible en finition sur demande.","Basin waste “Stop&Go”, without overflow. Plug in finish. Under-ceramic part in finish 031, on request avaiable in finish.",761,"Coffee Bronze Brushed PVD",159,"GPF014200E059G000","8055261610002"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54599,54599,"Afvoerplug \"Stop&Go\"","Bonde de lavabo “Stop & Go” 2 en 1 : un mécanisme d'ouverture et de fermeture dévissable et remplaçable avec un mécanisme toujours ouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",239,"Steel Brushed",69,"GPF545990A000G000","8022692841787"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54599,54599,"Afvoerplug \"Stop&Go\"","Bonde de lavabo “Stop & Go” 2 en 1 : un mécanisme d'ouverture et de fermeture dévissable et remplaçable avec un mécanisme toujours ouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",299,"Matte Black",199,"GPF545990C072G000","8056329228856"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54599,54599,"Afvoerplug \"Stop&Go\"","Bonde de lavabo “Stop & Go” 2 en 1 : un mécanisme d'ouverture et de fermeture dévissable et remplaçable avec un mécanisme toujours ouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",707,"Black Metal Brushed PVD",194,"GPF545990P004G000","8022692841794"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54599,54599,"Afvoerplug \"Stop&Go\"","Bonde de lavabo “Stop & Go” 2 en 1 : un mécanisme d'ouverture et de fermeture dévissable et remplaçable avec un mécanisme toujours ouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",708,"Copper Brushed PVD",194,"GPF545990P006G000","8022692841800"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54599,54599,"Afvoerplug \"Stop&Go\"","Bonde de lavabo “Stop & Go” 2 en 1 : un mécanisme d'ouverture et de fermeture dévissable et remplaçable avec un mécanisme toujours ouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",726,"Warm Bronze Brushed PVD",194,"GPF545990P024G000","8022692841817"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54599,54599,"Afvoerplug \"Stop&Go\"","Bonde de lavabo “Stop & Go” 2 en 1 : un mécanisme d'ouverture et de fermeture dévissable et remplaçable avec un mécanisme toujours ouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",727,"Brass Brushed PVD",194,"GPF545990P025G000","8056329085329"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",54599,54599,"Afvoerplug \"Stop&Go\"","Bonde de lavabo “Stop & Go” 2 en 1 : un mécanisme d'ouverture et de fermeture dévissable et remplaçable avec un mécanisme toujours ouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",761,"Coffee Bronze Brushed PVD",206,"GPF545990E059G000","8055261598973"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.","031","Chrome",60,"GPF014210G001G000","8056603964326"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",239,"Steel Brushed",60,"GPF014210A000G000","8055261077515"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",275,"Matte Cipria",168,"GPF014210T209G000","8056603964142"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",273,"Matte Greige",168,"GPF014210T208G000","8056603964159"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",277,"Glossy Ocra",194,"GPF014210T211G000","8056603964128"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",278,"Glossy Coral",194,"GPF014210T212G000","8056603964111"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",276,"Matte Agave",168,"GPF014210T210G000","8056603964135"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",299,"Matte Black",172,"GPF014210C072G000","8056603964333"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",720,"Nickel PVD",169,"GPF014210P014G000","8056603964197"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",706,"Black Metal PVD",169,"GPF014210P001G000","8056603964258"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",707,"Black Metal Brushed PVD",169,"GPF014210P004G000","8056603964241"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.","030","Copper PVD",169,"GPF014210P000G000","8056603964265"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",708,"Copper Brushed PVD",169,"GPF014210P006G000","8056603964227"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",735,"Warm Bronze PVD",169,"GPF014210P037G000","8056603964166"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",726,"Warm Bronze Brushed PVD",194,"GPF014210P024G000","8056603964180"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",710,"Brass PVD",169,"GPF014210P011G000","8056603964203"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",727,"Brass Brushed PVD",169,"GPF014210P025G000","8056603964173"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",246,"Gold PVD",209,"GPF014210P007G000","8056603964210"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",716,"Gold Brushed PVD",209,"GPF014210P005G000","8056603964234"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",187,"Aged Bronze",194,"GPF014210G052G000","8056603964272"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",713,"Antique Brass",194,"GPF014210V204G000","8056603964104"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",845,"Dark Bronze",169,"GPF014210V221G000","8056603964098"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01421","01421","2-in-1 'Stop&Go' wastafelafvoer: een afschroefbaar en vervangbaar altijd-geopend mechanisme in één pakket.","Bonde de lavabo 2 en 1 « Stop&Go » : un mécanisme d'ouverture et de fermeture dévissable et remplaçable et un mécanisme toujoursouvert dans le même emballage.","2-in-1 'Stop&Go' washbasin outlet: an unscrewable and replaceable always-opened mechanism all in one package.",761,"Coffee Bronze Brushed PVD",179,"GPF014210E059G000","8055261574069"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation","031","Chrome",77,"GPF013500G001G000","8022692013344"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",149,"Finox Brushed Nickel",109,"GPF013500G002G000","8022692794472"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",299,"Matte Black",208,"GPF013500C072G000","8056329039933"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",147,"Chome Brushed",109,"GPF013500G006G000","8022692120370"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",720,"Nickel PVD",127,"GPF013500P014G000","8056603608879"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",706,"Black Metal PVD",127,"GPF013500P001G000","8056329039919"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",707,"Black Metal Brushed PVD",136,"GPF013500P004G000","8056329039902"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation","030","Copper PVD",127,"GPF013500P000G000","8056329039926"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",708,"Copper Brushed PVD",136,"GPF013500P006G000","8056329039896"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",735,"Warm Bronze PVD",127,"GPF013500P037G000","8056329559226"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",726,"Warm Bronze Brushed PVD",136,"GPF013500P024G000","8056329039889"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",710,"Brass PVD",127,"GPF013500P011G000","8056329615304"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",727,"Brass Brushed PVD",136,"GPF013500P025G000","8056329184176"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",246,"Gold PVD",147,"GPF013500P007G000","8056329184183"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",716,"Gold Brushed PVD",136,"GPF013500P005G000","8055261231320"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",187,"Aged Bronze",136,"GPF013500G052G000","8056329184190"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",713,"Antique Brass",136,"GPF013500V204G000","8022692846157"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01350","01350","Wastafel pop-up afvoerplug met handbediening aan bovenkant","Bonde de lavabo . Vidage à ouverture par le haut","basin pop-up waste with upper manual operation",761,"Coffee Bronze Brushed PVD",136,"GPF013500E059G000","8055261610088"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation","031","Chrome",49,"GPF013460G001G000","8022692013733"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",149,"Finox Brushed Nickel",72,"GPF013460G002G000","8022692794465"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",299,"Matte Black",120,"GPF013460C072G000","8056329039995"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",147,"Chome Brushed",72,"GPF013460G006G000","8022692888553"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",720,"Nickel PVD",74,"GPF013460P014G000","8056603608886"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",706,"Black Metal PVD",80,"GPF013460P001G000","8056329039971"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",707,"Black Metal Brushed PVD",84,"GPF013460P004G000","8056329039964"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation","030","Copper PVD",80,"GPF013460P000G000","8056329039988"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",708,"Copper Brushed PVD",84,"GPF013460P006G000","8056329039957"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",735,"Warm Bronze PVD",80,"GPF013460P037G000","8056329559233"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",726,"Warm Bronze Brushed PVD",84,"GPF013460P024G000","8056329039940"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",710,"Brass PVD",80,"GPF013460P011G000","8056329615311"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",727,"Brass Brushed PVD",84,"GPF013460P025G000","8056329184220"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",246,"Gold PVD",88,"GPF013460P007G000","8056329184237"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",716,"Gold Brushed PVD",88,"GPF013460P005G000","8055261228993"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",187,"Aged Bronze",80,"GPF013460G052G000","8056329184244"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",713,"Antique Brass",80,"GPF013460V204G000","8056329179110"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01346","01346","Wastafel pop-up afvoerplug met handbediening aan voorkant","Bonde de lavabo . Vidage à ouverture frontale","basin pop-up waste with frontal manual operation",761,"Coffee Bronze Brushed PVD",88,"GPF013460E059G000","8055261610101"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01313","01313","Afvoerplug met vrije waste Wastafel","Grille pour lavabo sortie libre","Basin waste always open","031","Chrome",110,"GPF013130G001G000","8022692788723"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK",29454,29454,"Sifon van polyethyleen","Siphon en polyéthylène","Polyethylene syphon","031","Chrome",67,"GPF294540G001G000","8022692506969"]
["TOTAL LOOK","TOTAL LOOK","TOTAL LOOK","01713","01713","Polyethyleen uitschuifbare afvoerbuis, aansluiting 1 1/4\", Ø32/40","Tubelure extensible pour trop plein en polyéthylène 1 1/4\" pour vidage Ø32/40 mm","Polyethylene extensible drainage-pipe, 1 1/4\" connection, Ø32/40","031","Chrome",38,"GPF017130G001G000","8055261240438"]